{"text_format":"1","workbook":"xlsx","n_sheets":40,"sheets":["Alliance Selection Guide Index","Master cross Reference","SDRAM","SDRAM Cross Reference","DDR1  SDRAM","DDR1 SDRAM Cross Reference","DDR2 SDRAM","DDR2 SDRAM Cross Reference","DDR3 SDRAM ","DDR3 SDRAM Cross Reference","DDR4 SDRAM","DDR4 SDRAM Cross Reference","Mobile LP DRAM-SDRAM","Mobile LP DRAM Cross Reference","LPDDR4-LPDDR4X","LPDDR4-LPDDR4X cross Reference","pSRAM","pSRAM Cross Reference","Fast Asynchronous SRAM","Fast Asyn SRAM Cross Reference","Low Power Asynchronous SRAM","Low Power Asyn SRAM Cross Refer","Parallel 5V NOR Flash","Parallel 5V NOR Falsh Cross Ref","SLC Parallel NAND Flash","SLC Parallel NAND Flash.Cross R","Serial NOR Flash","Serial NOR Flash Cross Ref","Serial NAND Flash","Serial NAND Flash Cross Ref","eMMC","eMMC Cross Reference","Part Numbering System - SRAM ","Part Numbering System - DRAM ","Part Numbering System- P.NAND","Part Numbering System - P.NOR","Part Numbering System - S.NAND","Part Numbering System-S.NOR","Part Numbering System-eMMC","Alliance Memory Contact"],"not_rendered":{"charts":0,"images":9,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Alliance Selection Guide Index","index":0,"n_rows":12,"n_cols":2,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,0,0,1],[33,0,34,0]]}
[" "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Last Update:",{"$f":"TODAY()","v":"2026-02-27"}]
["Last Update by:","VB-RV-GH"]

{"sheet":"Master cross Reference","index":1,"n_rows":396,"n_cols":15,"rows_kept":396,"cut":false,"hidden":false,"merged":[[56,5,56,6]]}
["Synchronous DRAM 3.3V Cross Reference"]
["DENSITY","ORG","ALLIANCE","SAMSUNG (EOL)","MICRON (EOL)","SK HYNIX (EOL)","ISSI","WINBOND","NANYA (EOL)","ELITE (ESMT)","ELPIDA (EOL)"]
["16Mb","1M x 16","AS4C1M16S-6/7TxN","K4S161622E","MT48LC1M16A1 (EOL)","HY57V161610","IS42S16100","W9816G6TH","NT56V1616AOT","M12L16161A-xTG2Q","EDS1616AGTA"]
["64Mb","4M x 16","AS4C4M16SA-5/6/7TxN\nAS4C4M16SB-6TIN","K4S641632N-UCxx","MT48LC4M16A2P (EOL)","HY57V641620","IS42S16400\nIS45S16400","W9864G6JH","NT56V6620C0T-xxB","M12L64164A-xTG2U","uPD4564163G5-Axx"]
["64Mb","4M x 16","AS4C4M16SA-6/7BxN",null,"MT48LCM16A2B4(EOL)","HY5V66D","IS42S16400\nIS45S16400","W9864G6JT",null,"M12L64154A-xBG2C"]
["64Mb","2M x 32","AS4C2M32S-6/7BxN",null,"MT48LC2M32B2B5 (EOL)","HY5V62","IS42S32200","W9864G2IB-x",null,null,"EDS6432AFBH"]
["64Mb","2M x 32","AS4C2M32SA-6/7TxN","K4S643232H-Ucxx","MT48LC2M32B2P-x (EOL)","HY57V643220","IS42S32200","W9864G2J(G,I)H-x",null,"M12L64322A-xTG2U","EDS6432AFTA"]
["128Mb","8M x 16","AS4C8M16SA-6/7TxN\nAS4C8M16SB-6TIN","K4S281632K-UCxx","MT48LC8M16A2P(EOL)","HY57V281620","IS42S16800\nIS45S16800","W9812G6K(G,I)H","NT5SV8M16AT-xxB","M12L128168A-xTG2N","uPD45128163G5-Axx"]
["128Mb","8M x 16","AS4C8M16SA-6/7BxN","K4S281632D-RL75","MT48LC8M16A2B4 (EOL)","HY5V26","IS42S16800\nIS45S16800","W9812G6JB",null,"M12L128168A-xBG2N"]
["128Mb","4M x 32","AS4C4M32S-6/7BxN",null,"MT48LC4M32B2B5 (EOL)","HY5V22","IS42S32400","W9812G21(G)B-x",null,"M12L128324-xBG2E","EDS1232AHBH"]
["128Mb","4M x 32","AS4C4M32SA-6/7TxN",null,"MT48LC4M32B2P-x (EOL)","HY57V283220T","IS42S32400","W9812G2GH",null,null,"EDS1232AHTA"]
["256Mb","16M x 16","AS4C16M16SA/B-6/7TxN","K4S561632N-UCxx","MT48LC16M16A2P (EOL)","H57V2562GTR","IS42S16160\nIS45S16160","W9825G6K(D,E,J)H","NT5SV16M16AT-xxB","M12L2561616A-xTG2A","EDS2516AP(AF,AC)TA-xx"]
["256Mb","16M x 16","AS4C16M16SA/B-6/7BxN","K4S561632D-RL75","MT48LC16M16A2B4 (EOL)","HY5V56","IS42S16160\nIS45S16160","W9825G6JB",null,"M12L2561616A-xBG2A","EDS2516EE(JE)BH"]
["256Mb","8M x 32","AS4C8M32S-6/7TxN",null,"MT48LC8M32B2B5-x (EOL)","HY5V52","IS42S32800","W9825G2J(D)B-x",null,null,"EDS2532EEBH"]
["256Mb","8M x 32","AS4C8M32SA-6/7BxN",null,"MT48LC8M32B2B5-x (EOL)","HY5V52","IS42S32800","W9825G2J(D)B-x",null,null,"EDS2532EEBH"]
["256Mb","32M X 8","AS4C32M8SA-6/7TxN",null,"MT48LC32M8A2P (EOL)",null,"IS42S83200J"]
["256Mb","64M x 4","AS4C64M4SA-6/7TxN",null,"MT48LC64M4A2P (EOL)",null,"IS42S32800"]
["512Mb","32M x 16","AS4C32M16SB-7BIN",null,null,null,"IS42S16320",null,null,"M12L5121632A"]
["512Mb","32M x 16","AS4C32M16SB-6/7TxN","K4S511632M-TC75","MT48LC32M16A2 (EOL)",null,"IS42S16320",null,null,"M12L5121632A","EDS5116ABTA"]
["512Mb","32M x 16","AS4C32M16SC-7TIN","K4S511632M-TC75","MT48LC32M16A2 (EOL)",null,"IS42S16320",null,null,"M12L5121632A","EDS5116ABTA"]
["512Mb","16M x 32","AS4C16M32SB-6BxN",null,"MT48LC16M32S2 (EOL)",null,"IS42S32160"]
["512Mb","16M x 32","AS4C16M32SC-7TIN",null,null,null,"IS42S32160"]
["512Mb","64M x 8","AS4C64M8SC-7TIN",null,"MT48LC64M8A2P-75:C (EOL)",null,"IS42S86400"]
["512Mb","64M x 8","AS4C64M8SD-7TCN",null,"MT48LC64M8A2P-75:C (EOL)",null,"IS42S86400"]
[]
["DDR1       2.5V SDRAM Cross Reference"]
["DENSITY","ALLIANCE","SAMSUNG (EOL)","MICRON (EOL)","ISSI","HYNIX - ALL EOL","WINBOND","NANYA","ELITE (ESMT)","ELPIDA"]
["64Mb","AS4C4M16D1A-5TxN","K4H641638N","MT46V4M16TG (EOL)","IS43R16400B",null,"W9464G6K(I,J)H",null,"M13S64164A-5TG2Y","(EOL)"]
["64Mb","AS4C2M32D1A-5BxN"]
["128Mb","AS4C8M16D1-5BXN","K4H281638D",null,"IS43R16800E-5BL",null,"W9412G6JB",null,"M13S128168A-5BG2N","EDD1216A"]
["128Mb","AS4C8M16D1A-5TxN","K4H281638D","MT46V8M16 (EOL)","IS43R16800E-5TL","HY5DU1281622","W9412G6K(I,J)H",null,"M13S128168A-5TG2N","EDD1216A"]
["128Mb","AS4C4M32D1A-5BxN",null,"MT46V4M32FK (EOL)","IS43R32400E-5BL",null,"W9412GIB",null,"M13S128324A-5BG2M","EDD1232A"]
["256Mb","AS4C32M8D1-5TxN","K4H560838N","MT46V32M8P (EOL)","IS43R83200","HY5DU56822",null,"NT5DS32M8ES",null,"EDD2508A"]
["256Mb","AS4C16M16D1-5BxN","K4H561638D","MT46V16M16CY(EOL)","IS43R16160\nIS46R16160","HY5DU561622","W9425G6JB",null,"M13S2561616A-xBG2A"]
["256Mb","AS4C16M16D1A-5TxN","KH561638D","MT46V16M16P (EOL)","IS43R16160","HY5DU561622","W945G6K(D,E,J)H",null,"M13S2561616A-xTG2A","EDD2516A"]
["512Mb","AS4C32M16D1-5BxN","K4H511638J","MT46V32M16CY(EOL)","IS43R16320\nIS46R16320","HY5DU121622",null,null,null,"EDD5116"]
["512Mb","AS4C32M16D1A-5TxN","K4H511638J","MT46V32M16P(EOL)","IS43R16320\nIS46R16320","HY5DU121622",null,"NT5DS32M16ES","M13S5121632A-5TG2S","EDD5116A"]
["512Mb","AS4C64M8D1-5TxN","K4H510838J","MT46V64M8P (EOL)","IS43R86400","HY5DU12822",null,"NT5DS64M8ES",null,"EDD5108A"]
["512Mb","AS4C64M8D1-5BxN","K4H510838J","MT46V64M8CY(EOL)","IS43R86400","HY5DU12822"]
["1Gb","AS4C64M16D1-6TxN",null,"MT46V64M16P (EOL)"]
["1Gb","AS4C64M16D1A-6BIN"]
[]
["DDR2    1.8V SDRAM Cross Reference"]
["DENSITY","ALLIANCE","SAMSUNG (EOL)","MICRON","ISSI","WINBOND","NANYA","ELITE (ESMT)","HYNIX (EOL)"]
["256Mb","AS4C16M16D2-25BxN","K4T56163Q","MT47H16M16BG","IS43DR16160","W9725G6K(J)B","NT5TU16M16BG","M14D2561616A-2.5BG","HY5PS561621"]
["512Mb","AS4C32M16D2A/C-25BxN","K4T51163Q","MT47H32M16HR(NF)-25E","IS43DR16320\nIS46DR16320","W9751G6K(J)B","NT5TU32M16GG","M14D5121632A-2.5BG","HY5PS121621"]
["512Mb","AS4C64M8D2-25BxN","K4T51083Q","MT47H64M8CF(SH)-25E","IS43DR86400\nIS46DR86400","W9751G8K(J)B","NT5TU64M8EE",null,"H5PS5182KFR"]
["1Gb","AS4C64M16D2A-25BxN","K4T1G164Q","MT47H64M16HR(NF)-25E","IS43DR16640\nIS46DR16640","W971GG6JB","NT5TU64M16HG","M14D1G1664A-2.5BG","H5PS1G63"]
["1Gb","AS4C64M16D2B-25BCN","K4T1G164Q","MT47H64M16HR(NF)-25E","IS43DR16640","W971GG6JB","NT5TU64M16HG","M14D1G1664A-2.5BG","H5PS1G63"]
["1Gb","AS4C128M8D2A-25BxN","K4T1G084Q","MT47H128M8SH-25E","IS43DR81280","W971GG8JB","NT5TU128M8HE","M14D1G8128A","H5PS1G83"]
["2Gb","AS4C128M16D2-25BxN",null,"MT47H128M16RT-25E (EOL)","IS43DR16128","W972GG6JB"]
["2Gb","AS4C128M16D2A-25BxN",null,"MT47H128M16RT-25E (EOL)","IS43DR16128\nIS46DR16128","W972GG6JB"]
[]
["DDR3 SDRAM Cross Reference"]
["DENSITY","ALLIANCE","MICRON","SAMSUNG(EOL)","ISSI","HYNIX","WINBOND","ELITE (ESMT)","ELPIDA","NANYA"]
["512Mb","AS4C32M16D3-12BxN\nAS4C32M16D3-10BCN",null,null,null,null,"W6351G6KB-x","M15T5121632A","EDJ5316BASE"]
["512Mb","AS4C64M8D3-12BxN",null,null,null,null,null,null,"EDJ5308BASE"]
["512Mb","AS4C32M16D3L-12BxN",null,null,null,null,null,"M15T5121632A","EDJ5316BASE"]
["512Mb","AS4C64M8D3L-12BxN",null,null,null,null,null,null,"EDJ5308BASE"]
["1Gb","AS4C64M16D3B-12BxN AS4C64M16D3W-12BCN","MT41J64M16JT(TW)-125 (EOL)","K4B1G1646E(G)","IS43TR16640\nIS46TR16640","H5TQ1G63D","W631GG6KB-x","M15F1G1664A","EDJ1116DJ(BA) BG","NT5CB64M16F(G)P"]
["1Gb","AS4C64M16D3LB/C-12BxN AS4C64M16D3LW-10BCN","MT41K64M16JT-125 (EOL)\nMT41K64M16TW-125 ","K4B1G1646E(G)","IS43TR16640xL\nIS46TR16640xL","H5TC1G63EFR (EOL)","W631GU6KB-x","M15T1G1664A-(2C)","EDJ1116EJBG","NT5CC64M16F(G)P-DI"]
["1Gb","AS4C64M16D3LW-10BCN","MT41K64M16JT-125 (EOL)\nMT41K64M16TW-125\nMT41K64M16TW-107 ","K4B1G1646E(G)","IS43TR16640xL\nIS46TR16640xL","H5TC1G63EFR (EOL)","W631GU6KB-x","M15T1G1664A-(2C)","EDJ1116EJBG","NT5CC64M16F(G)P-DI"]
["1Gb","AS4C128M8D3B-12BxN","MT41J128M8JP(DA)-125","K4B1G0846E(F,G)","IS43TR81280\nIS46TR81280","H5TQ1G83","W631GG8KB-x","M15T1G8128A","EDJ1108DJ(BA) BG","NT5CB128M8F(G)N-DI"]
["1Gb","AS4C128M8D3LB/C-12BxN","MT41K128M8JP(DA)-125","K4B1G0846G-BY","IS43TR81280xL\nIS46TR81280xL","H5TC1G83EFR (EOL)","W631GU8KB-x","M15T1G8128A","EDJ1108EJBG","NT5CC128M8F(G)N-DI"]
["2Gb","AS4C128M16D3C-93BxN","MT41J128M16JT(TW)-125","K4B2G1646E-B","IS43TR16128","H5TQ2G63","W632GG6KB-x","M15F2G16128A","EDJ2116DEBG","NT5CB128M16I(F)P-DI"]
["2Gb","AS4C128M16D3LC-12BxN","MT41K128M16JT-125","K4B2G1646Q-B","IS43TR16128xL\nIS46TR16128xL","H5TC2G63","W632GU6KB-x","M15F2G16128A","EDJ2116EEBG","NT5CC128M16I(F)P-DI"]
["2Gb","AS4C256M8D3LC-12BxN","MT41K256M8DA-125","K4B2G0846Q-BCK","IS43TR82560xL\nIS46TR82560xL","H5TQ2G83FFR-x","W632GG8KB-x","M15T2G8256A","EDJ2108DEBG","NT5CB256M8IN-FL"]
["4Gb","AS4C256M16D3C-93BCN AS4C256M16D3C-10BxN AS4C256M16D3C-12BxN","MT41J256M16HA-107 MT41J256M16HA-125","K4B4G1646B(D)","IS43TR16256","H5TQ4G63","W634GG6MB/ NB","M15F4G16256A","EDJ4216BFBG (BASE)","NT5CB256M16C(D,E) P-DI"]
["4Gb","AS4C256M16D3LC-10BxN AS4C256M16D3LC-12BxN AS4C256M16D3LD-10BxN","MT41K256M16HA-107/125 MT41K256M16TW-107/125","K4B4G1646E(Q)","IS43TR16256xL\nIS46TR16256xL","H5TC4G63","W634GU6MB/NB","M15T4G16256A","EDJ4216EFBG","NT5CC256M16C(D,E) P-DI"]
["4Gb","AS4C512M8D3LC-10BAN\nAS4C512M8D3LC-12BxN","MT41K512M8DA-125","K4B4G0846B(C,D)","IS43TR85120xL\nIS46TR85120xL","H5TC4G83","W634GU8MB/NB","M15T4G8512A","EDJ4208EFBG","NT5CC512M8C(D,E) N-DI"]
["8Gb","AS4C512M16D3LA-10BxN","MT41K512M16VRN-107 MT41K512M16VRP-107 MT41K512M16HA-125 (EOL)","K4B8G1646x","IS43TR16512","H5TC8G63CMR","W638GU6QB","M15T8G16512A–DE",null,"NT5CC512T16EH-DI/A/H\nNT5CC512T16EH-EK/A/H"]
["8Gb","AS4C512M16D3LB-12BxN","MT41K512M16HA-125 (EOL)","K4B8G1646x","IS43TR16512","H5TC8G63CMR","W638GU6QB","M15T8G16512A–BD",null,"NT5CC512T16EH-DI/A/H"]
["8Gb","AS4C512M16D3LC-10BxN\nAS4C512M16D3LC-12BxN ","MT41K512M16VRN-107 MT41K512M16VRP-107 MT41K512M16HA-125 (EOL)","K4B8G1646x","IS43TR16512","H5TC8G63CMR","W638GU6QB","M15T8G16512A–BD\nM15T8G16512A–DE",null,"NT5CC512T16EH-DI/A/H\nNT5CC512T16EH-EK/A/H"]
["8Gb","AS4C1G8D3LA-10BxN","MT41K1G8SN-107/125:E","K4B8G0846x","IS43TR81024","H5TC8G83BMR"]
["8Gb","MT41K512M16HA-125","MT41K512M16HA-125","K4B8G1646x","IS43TR16512","H5TC8G63CMR","W638GU6QB","M15T8G16512A–BD",null,"NT5CC512T16EH-DI/A/H"]
[]
["DDR4 SDRAM Cross Reference"]
["DENSITY","ORG","ALLIANCE","MICRON","NANYA","SAMSUNG","HYNIX","ISSI"]
["4Gb","256M x 16","AS4C256M16D4-83BxN\nAS4C256M16D4-75BxN","MT40A256M16GE","NT5AD256M16D4-HR/I/T\nNT5AD256M16E4-HR/I/T","K4A4G165WE-BxRC/PB/TD\nK4A4G165WF-BxTD","H5AN4G6NBJR-VKC\nH5AN4G6NBJR-VKI","IS43QR16256B-083RBL/I\nIS43QR16256B-075UBL/I"]
["4Gb","512M x 8","AS4C512M8D4-83BxN\nAS4C512M8D4-75BxN","MT40A512M8RH","NT5AD512M8D3-HR/I/T\nNT5AD512M8E3-HR/I/T","K4A4G085WE-BxRC/PB/TD\nK4A4G085WF-BxTD","H5AN4G8NBJR-VKC\nH5AN4G8NBJR-VKI","IS43QR85120B-083RBL/I\nIS43QR85120B-075UBL/I"]
["4Gb","256M x 16","AS4C256M16D4A-62BxN\nAS4C256M16D4A-75BxN","MT40A256M16GE","NT5AD256M16D4-HR/I/T\nNT5AD256M16E4-HR/I/T\nNT5AD256M16D4-JR/I/T\nNT5AD256M16E4-JR/I/T","K4A4G165WE-BxRC/PB/TD/WE\nK4A4G165WF-BxTD/WE\nK4A4G165WG-BxWE","H5AN4G6NBJR-VKC\nH5AN4G6NBJR-VKI","IS43QR16256B-083RBL/I\nIS43QR16256B-075UBL/I"]
["4Gb","512M x 8","AS4C512M8D4A-75BxN","MT40A512M8RH","NT5AD512M8D3-HR/I/T\nNT5AD512M8D3-JR/I/T\nNT5AD512M8E3-HR/I/T\nNT5AD512M8E3-JR/I/T","K4A4G085WE-BxRC/PB/TD\nK4A4G085WF-BxTD/WE\nK4A4G085WF-BxWE","H5AN4G8NBJR-VKC\nH5AN4G8NBJR-VKI","IS43QR85120B-083RBL/I\nIS43QR85120B-075UBL/I"]
["8Gb","512M x 16","AS4C512M16D4A-62BxN","MT40A512M16LY\nMT40A512M16JY\nMT40A512M16HA\nMT40A512M16TB","NT5AD512M16C4-HR/I/T\nNT5AD512M16C4-JR/I/T\nNT5AD512M16H4-HR/I/T\nNT5AD512M16H4-JR/I/T","K4A8G165WB-BxPB/RC/TD\nK4A8G165WC-BxTD/WE\nK4A8G165WG-BxWE","H5AN8G6NCJR-XNC/I\nH5AN8G6NCJR-WNC/I\nH5AN8G6NCJR-VNC\nH5AN8G6NDJR-WNC","IS43QR16512A-083TBL/I\nIS43QR16512A-075VBL/I"]
["8Gb","1G x 8","AS4C1G8D4A-62BxN","MT40A1G8SA\nMT40A1G8WE\nMT40A1G8PM","NT5AD1024M8C3-HR/I/T\nNT5AD1024M8C3-JR/I/T\nNT5AD1024M8H3-HR/I/T\nNT5AD1024M8H3-JR/I/T","K4A8G085WB-BxPB/RC/TD\nK4A8G085WC-BxPB/RC/TD/WE\nK4A8G085WG-BxWE","H5AN8G8NCJR-XNC\nH5AN8G8NDJR-XNC\nH5AN8G8NCJR-VKC/WNC/I\nH5AN8G8NDJR-VKC/WNC/I","IS43QR81024A-083TBL/I\nIS43QR81024A-075VBL/I"]
["8Gb","512M x 16","AS4C512M16D4B-62BCN AS4C512M16D4C-62BCN\nAS4C512M16D4D-62BCN","MT40A512M16LY\nMT40A512M16JY\nMT40A512M16HA\nMT40A512M16TB","NT5AD512M16C4-HR/JR\nNT5AD512M16H4-HR/JR","K4A8G165WB-BCPB/RC/TD\nK4A8G165WC-BCTD/WE\nK4A8G165WG-BCWE","H5AN8G6NCJR-XNC/VNC\nH5AN8G6NCJR-WNC\nH5AN8G6NDJR-WNC","IS43QR16512A-083TBL\nIS43QR16512A-075VBL"]
["8Gb","512M x 16","MT40A512M16TD-062E:R","MT40A512M16LY\nMT40A512M16JY\nMT40A512M16HA\nMT40A512M16TB","NT5AD512M16C4-HR/JR\nNT5AD512M16H4-HR/JR","K4A8G165WB-BCPB/RC/TD\nK4A8G165WC-BCTD/WE\nK4A8G165WG-BCWE","H5AN8G6NCJR-XNC/VNC\nH5AN8G6NCJR-WNC\nH5AN8G6NDJR-WNC","IS43QR16512A-083TBL\nIS43QR16512A-075VBL"]
["8Gb","1G x 8","AS4C1G8D4B-62BCN AS4C1G8D4D-62BCN\nMT40A1G8AG-062E","MT40A1G8SA\nMT40A1G8WE\nMT40A1G8PM","NT5AD1024M8C3-HR/JR\nNT5AD1024M8H3-HR/JR","K4A8G085WB-BCPB/RC/TD\nK4A8G085WC-BCPB/RC/TD/WE\nK4A8G085WG-BCWE","H5AN8G8NCJR-XNC\nH5AN8G8NDJR-XNC\nH5AN8G8NCJR-VKC/WNC\nH5AN8G8NDJR-VKC/WNC","IS43QR81024A-083TBL\nIS43QR81024A-075VBL"]
["16Gb","1G x 16","AS4C1G16D4-062BCN\nMT40A1G16KH-062E\nMT40A1G16KD-062E\nMT40A1G16TD-062E","MT40A1G16KH/KB/RC\nMT40A1G16TB/TD/TBB",null,"K4AAG165WA-BCWE\nK4AAG165WB-MCPB/RC/TD\nK4AAG165WC-BCWE","H5ANAG6NCMR-XNC\nH5ANAG6NCMR-WMC/VKC\nH5ANAG6NDMR-XNC\nH5ANAG6NDMR-WMC/VKC"]
["16Gb","1G x 16","AS4C1G16D4A-62BCN","MT40A1G16KH/KB\nMT40A1G16TB/TD\nMT40A1G16RC",null,"K4AAG165WA-BCWE\nK4AAG165WB-MCPB/RC/TD\nK4AAG165WC-BCWE","H5ANAG6NCMR-XNC\nH5ANAG6NCMR-WMC/VKC\nH5ANAG6NDMR-XNC\nH5ANAG6NDMR-WMC/VKC"]
["16Gb","2G x 8","AS4C2G8D4A-62BCN\nMT40A2G8JC-062E\nMT40A2G8JE-062E\nMT40A2G8AG-062E","MT40A2G8AG\nMT40A2G8SA/VA\nMT40A2G8JC/JE",null,"K4AAG085WA-BCWE/TD\nK4AAG085WB-BCWE\nK4AAG085WB-MCPB/RC\nK4AAG085WC-BCWE","H5ANAG8NCMR-XNC\nH5ANAG8NCMR-VKC/WMC\nH5ANAG8NDMR-XNC\nH5ANAG8NDMR-VKC/WMC","IS43QR8K02S2A-083TBL"]
["32Gb","2G x 16","AS4C2G16D4-62BCN","MT40A2G16TBB\nMT40A2G16SKL",null,"K4ABG165WA-MCTD\nK4ABG165WA-MCWE K4ABG165WB-MCWE","H5ANBG6NAMR-XNC\nH5ANBG6NAMR-WNC\nH5ANBG6NAMR-VKC"]
["32Gb","4G x 8","AS4C4G8D4-62BCN","MT40A4G8NEA\nMT40A4G8BAF",null,"K4ABG085WA-MCWE\nK4ABG085WA-MCTD ","H5ANBG8NABR-XNC\nH5ANBG8NABR-WNC\nH5ANBG8NABR-VKC"]
[]
["MOBILE LOW POWER SDRAM Cross Reference"]
["DENSITY","ALLIANCE","MICRON","ISSI","NANYA","WINBOND"]
["128Mb","AS4C8M16MSA-6BIN","MT48H8M16LFB4 (EOL)","IS42VM16800H",null,"W987D6HBGX"]
["256Mb","AS4C16M16MSA-6BIN","MT48H16M16LFBF (EOL)","IS42VM16160K",null,"W988D6FBGX"]
["256Mb","AS4C8M32MSB-6BIN","MT48H8M32LFB5 (EOL)","IS42VM32800K",null,"W988D2FBJX"]
["512Mb","AS4C32M16MSA-6BIN","MT48H32M16LFB4-6 IT (EOL)","IS42VM16320E","NT6SM32M16BG-S1","W989D6DBGX"]
["512Mb","AS4C16M32MSA-6BIN","MT48H16M32LFB5-6 IT (EOL)","IS42VM32160E","NT6SM16M32BK-S1","W989D2DBJX"]
[]
["MOBILE LP DDR1 Cross Reference"]
["DENSITY","ALLIANCE","MICRON","SAMSUNG","ISSI","HYNIX","NANYA","ELITE (ESMT)","WINBOND"]
["256Mb","AS4C16M16MD1-6BCN","MT46H16M16LFBF-6 (EOL)","K4X56163SPN","IS43LR16160","HY5MS5B6/ H5MS2562","NT6DM16M16AD-T1","M53D2561616A-6BG2F","W948D6FBHX"]
["512Mb","AS4C32M16MD1B-5BIN","MT46H32M16LFBF-5","K4X51163PI","IS43R16320B","HY5MS7B6/ H5MS5162","NT6DM32M16A(B)D-T1","M53D5121632A-5BG2T","W949D6DBHX"]
["512Mb","AS4C16M32MD1B-5BIN","MT46H16M32LFB5-5","K4X51323PI","IS43LR32160B","H5MS5132/ H5MS5122","NT6DM16M32A(B)C-T1","M53D5123216A-5BG2S","W949D2DBJX"]
["2Gb","AS4C64M32MD1-5BxN","MT46H64M32LFKQ-5","K4X2G323PC","IS43LR32640A","H5M52G22"]
["2Gb","AS4C64M32MD1A-5BIN","MT46H64M32LFKQ-5","K4X2G323PC","IS43LR32640A","H5M52G22"]
[]
["MOBILE LP DDR2 Cross Reference"]
["DENSITY","ALLIANCE","MICRON","SAMSUNG","ISSI","HYNIX","NANYA","ELITE (ESMT)","WINBOND"]
["256Mb","AS4C8M32MD2A-25B(P)CN",null,null,"IS43LD32800A-25BLx\nIS43LD32800B-25BLx",null,null,null,"W978H2KBVX2E"]
["1Gb","AS4C64M16MD2A-25BIN","MT42L64M16D1HE-25",null,"IS43LD16640C/A",null,"NT6TL64M16BA(I)-G0",null,"W97AH6KBVX2"]
["1Gb","AS4C32M32MD2A-25BIN","MT42L32M32D1HE-25",null,"IS43LD32320C/A",null,"NT6TL32M32BI(A)-G0",null,"W97AH2KBVX2"]
["2Gb","AS4C128M16MD2A-25BIN","MT42L128M16D1TK-25",null,"IS43LD16128B",null,"NT6TL128M16CI(A)-G0",null,"W97BH6KBVX2"]
["2Gb","AS4C64M32MD2A-25BIN","MT42L64M32D1TK-25",null,"IS43LD32640B",null,"NT6TL64M32CI(A)-G0",null,"W97BH2KBVX2"]
["4Gb","AS4C128M32MD2A-18BIN","MT42L128M32D1GU-18",null,"IS43LD32128A",null,"NT6TL128M32BI(A)-G0"]
["4Gb","AS4C128M32MD2A-25BIN","MT42L128M32D1GU-18",null,"IS43LD32128A",null,"NT6TL128M32BI(A)-G0"]
[]
["LPDDR4 Cross Reference "]
["DENSITY","ORG","ALLIANCE","MICRON","SAMSUNG","HYNIX","NANYA","ISSI","WINBOND","IM"]
["2Gb","128M x 16","AS4C128M16MD4-062BAN","MT53E128M16D1DS",null,"H9HCNNNBKUMLXR/HR","NT6AN128M16AV","IS43/46LQ16128A\nIS43/46LQ16128EA","W66BL6NBU\nW66BP6NBU"]
["2Gb","64M x 32","AS4C64M32MD4-062BAN",null,null,null,null,"IS43/46LQ32640A\nIS43/46LQ32640EA","W66CL2NQU\nW66CP2NQU\nW66CP2NQQ"]
["4Gb","128M x 32","AS4C128M32MD4-062BAN\nAS4C128M32MD4A-062BIN","MT53B128M32D1DS\nMT53E128M32D2DS\nMT53E128M32D2FW","K4F4E3S4HF-GFCJ\nK4F4E3S4HF-GHCJ",null,"NT6AN128T32AV","IS43/46LQ32128A\nIS43/46LQ32128EA","W66CL2NQU\nW66CP2NQU","IME4G32L4HABG"]
["4Gb","256M x 16","AS4C256M16MD4-062BAN\nAS4C256M16MD4A-046BIN","MT53E256M16D1DS\nMT53E256M16D1FW",null,"H9HCNNN4KUMLHR","NT6AN256M16AV","IS43/46LQ16256A\nIS43/46LQ16256EA","W66CP6NBU\nW66CL6NBU"]
["8Gb","256M x 32","AS4C256M32MD4-062BAN\nAS4C256M32MD4A-046BIN","MT53B256M32D1DS\nMT53E256M32D2DS\nMT53E256M32D2FW","K4F8E304HB-MGCJ\nK4F8E3S4HB-MFCJ\nK4F8E3S4HB-MHCJ","H9HCNNN8KUMLHR","NT6AN256T32AV","IS43/46LQ32256A\nIS43/46LQ32256EA","W66DP2NQU\nW66DL2NQU","IME8G32L4HADG"]
[]
["LPDDR4X Cross Reference "]
["DENSITY","ORG","ALLIANCE","MICRON","SAMSUNG","HYNIX","NANYA","ISSI","WINBOND","IM"]
["2Gb","128M x 16","AS4C128M16MD4V-062BAN",null,null,null,null,"IS43/46LQ16128AL\nIS43/46LQ16128EA","W66BQ6NBU"]
["4Gb","256M x 16","AS4C256M16MD4V-062BAN\nAS4C256M16MD4VA-046BIN","MT53E256M16D1DS\nMT53E256M16D1FW","K4U8E3S4AD-GFCL\nK4U8E3S4AD-GHC","H9HCNNN4KMMLHR","NT6AP256M16AV","IS43/46LQ16256AL\nIS43/46LQ16256EA","W66CQ6NQU","IM4G16L4JCBG"]
["4Gb","128M x 32","AS4C128M32MD4VA-062BIN","MT53B128M32D1DS\nMT53E128M32D2DS\nMT53E128M32D2FW","K4U4E3S4x",null,"NT6AP128T32AV","IS43/46LQ32128AL","W66CQ2NQU","IME4G32L4JCBG"]
["8Gb","256M x 32","AS4C256M32MD4V-062BAN\nAS4C256M32MD4VA-046BIN","MT53B256M32D1DS\nMT53E256M32D2DS\nMT53E256M32D2FW","K4U8E3S4Ax",null,"NT6AP256T32AV","IS43/46LQ32256AL\nIS43/46LQ32256EAL","W66DQ2NQU","IM8G32L4JCBG"]
["8Gb","512M x 16","AS4C512M16MD4V-053BIN\nAS4C512M16MD4VA-046BIN","MT53D512M16D1DS\nMT53E512M16D1FW",null,null,"NT6AP512M16AV","IS43LQ16512AL",null,"IM8G16L4JCBG-046"]
["16Gb","1G x 16","AS4C1G16MD4V-046BIN\nAS4C1G16MD4VA-046BIN","MT53E1G16D1ZW-046",null,null,"NT6AT1024M16AV",null,null,"IMAG16L4HBBG"]
["16Gb","512M x 32","AS4C512M32MD4V-053BIN","MT53D512M32D2Dx\nMT53D512M32D1ZW\nMT53D512M32D2FW","K4U6E3S4Ax","H9HCNNNBPUMLHR\n","NT6AP512T32BY",null,null,"IMAG32L4JCBG-046"]
["16Gb","512M x 32","AS4C512M32MD4V-046BIN\nAS4C512M32MD4VA-046BIN","MT53D512M32D2Dx\nMT53E512M32D2FW\nMT53E512M32D1ZW","K4U6E3S4Ax","H9HCNNNBKMMLXR\nH9HCNNNBPUMLHR\n","NT6AP512T32BY",null,null,"IMAG32L4JCBG-046"]
["32Gb","1G x 32","AS4C1G32MD4V-046BIN","MT53D1024M32D4Dx\nMT53E1G32D2FW\nMT53E1G32D2Nx","K4UBE3D4Ax","H9HCNNNCPMMLXR\nH9HCNNNCPMMLXR","NT6AP1024F32B",null,null,"IMBG32L4KBBG\nIMBG32L4KDDG"]
["Fast Asynchronous SRAM Cross Reference"]
["64K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS (EOL)","IDT","ISSI"]
["8K x 8","5V","28pin SOJ (300mil)",15,"AS7C164A-15JxN",null,"CY7C185-xxVI/VC (EOL)","7164SxxYG              \n7164LxxYG","IS61C64AL-xxJLI (EOL)"]
["8K x 8","5V","28pin Skinny PDIP 300mil",15,"AS7C164A-15PxN",null,"CY7C185-xxPC (EOL)","7164S20TPG"]
["256K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS (EOL)","IDT","ISSI"]
["32K x 8","5V","28pin SOJ","10,12,15,20","AS7C256A-xxJCN/JIN","K6E0808C1E-J (EOL)","CY7C199D-10VXI(EOL)   CY7C199CN–xxVXI/VXC(EOL) ","71256LxxYG                 71256SAxxYG","IS61C256AL-xxJL/JLI"]
["32K x 8","5V","28pin TSOP I","10,12,15,20","AS7C256A-xxTCN/TIN","K6E0808C1E-T (EOL)","CY7C199D-10ZXI(EOL)   CY7C199CN–xxZXC/ZXI(EOL)  ","71256SAxxPZG","IS61C256AL-xxTL/TLI"]
["32K x 8","3.3V","28pin SOJ","10,12,15,20","AS7C3256A-xxJCN/JIN","K6E0808V1E-J (EOL)","CY7C1399BN-xxVXC(EOL)","71V256SAxxYG","IS61LV256AL-10JL/JLI"]
["32K x 8","3.3V","28pin TSOP I","10,12,15,20","AS7C3256A-xxTCN/TIN","K6E0808V1E-T (EOL)","CY7C1399BN-xxZXI/ZXC(EOL)","71V256SAxxPZG","IS61LV256AL-10TL/TLI"]
["32K x 8","5V","28pin DIP",15,"AS7C256C-xxPCN",null,"CY7C199CN-15/25PXC (EOL)","71256LxxTDB     \n71256SxxTDB  \n71256SAxxTPG"]
["512K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI"]
["32K x 16","5V","44pin SOJ (400mil)",15,"AS7C513B-xxJCN",null,"CY7C1020D-10VXI(EOL)",null,"IS61C3216AL-12KLI "]
["32K x 16","5V","44pin TSOP II (400mil)","12,15","AS7C513B-xxTCN",null,"CY7C1020D-10ZSXI",null,"IS61C3216AL-12TLI"]
["32K x 16","3.3V","44pin TSOP II (400mil)","12,15,20","AS7C3513B-xxTCN",null,"CY7C1020DV33-10ZSXI",null,"IS61WV3216BLL-xxTLI"]
["32K x 16","3.3V","44pin SOJ (400mil)","10,12,15","AS7C3513B-xxJCN",null,"CY7C1020DV33-10VXI"]
["1M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG (EOL)","CYPRESS","IDT","ISSI","GSI"]
["128K x 8","5V","32pin SOJ (400mil)","12,15,20","AS7C1025B-xxJCN/JIN","K6R1008C1D-KI10","CY7C1019D-10VXI(EOL)","71124SxxYG(EOL)"]
["128K x 8","3.3V","32pin SOJ (400mil)","10,12,15,20","AS7C31025B-xxJCN/JIN","K6R1008V1D-KI10","CY7C1019DV33-10VXI","71V124SAxxYG","IS63LV1024-xxK/KI (EOL)"]
["128K x 8","5V","32pin SOJ (300mil)","10,12,15,20","AS7C1025B-xxTJCN"]
["128K x 8","3.3V","32pin SOJ (400mil)",12,"AS7C31025B-xxJIN",null,"CY7C1019DV33-10VXI"]
["128K x 8","3.3V","32pin SOJ (300mil)","10,12,15,20","AS7C31025B-xxTJCN/-12TJIN",null,"CY7C1018DV33-10VXI(EOL)","71V124SAxxTYG","IS63WV1288DBLL-xxJLI             IS63LV1024L-10JLI(EOL)"]
["128K x 8","5V","32pin SOJ (400mil)","12,15,20","AS7C1024D-12JIN",null,"CY7C109D-10VXI","71024SxxYG","IS61C1024AL-12KLI (EOL)"]
["128K x 8","5V","32pin TSOP I","12,15,20","AS7C1024B-xxTCN",null,"CY7C109D-10ZXI",null,"IS61C1024AL-12TLI"]
["128K x 8","5V","32pin SOJ (300mil)","12,15,20","AS7C1024D-12TJIN",null,"CY7C1009D-10VXI(EOL)","71024SxxTYG","IS61C1024AL-12JLI"]
["128K x 8","3.3V","32pin SOJ (400mil)","12,15,20","AS7C31024B-xxJCN"]
["128K x 8","3.3V","32pin TSOP I","10,12,15,20","AS7C31024B-xxTCN"]
["128K x 8","3.3V","32pin SOJ (300mil)","10,12,15,20","AS7C31024B-xxTJCN"]
["64K x 16","5V","44pin SOJ (400mil)","10,12,15,20","AS7C1026B-xxJCN/JIN","K6R1016C1D-KI10","CY7C1021D-10VXI","71016SxxYG","IS61C6416AL-12KLI"]
["64K x 16","5V","44pin TSOP II (400mil)","10,12,15,20","AS7C1026B-xxTCN/TIN","K6R1016C1D-UI10","CY7C1021D-10ZSXI/A(EOL)","71016SxxPHG","IS61C6416AL-12TLI"]
["64K x 16","3.3V","44pin SOJ (400mil)","10,12,15,20","AS7C31026B-xxJCN/TIN","K6R1016V1D-KI10","CY7C1021DV33-10VXI","71V016SAxxYG","IS61WV6416DBLL-xxKLI IS61LV6416-xxKL/KLI"]
["64K x 16","3.3V","44pin TSOP II (400mil)","10,12,15,20","AS7C31026B-xxTCN/TIN","K6R1016V1D-UI10","CY7C1021DV33-10ZSXI   CY7C1021DV33-10ZSXA(EOL)","71V016SAxxPHG","IS61WV6416DBLL-xxTLI IS61WV6416EEBLL-xxTLI IS61LV6416-xxT/TL/TI/TLI","GS71116AGP-xx"]
["2M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["128K x 16","3.3V","44pin TSOP II","10,12,15,20","AS7C32098A-xxTxN",null,"CY7C1011G30-10ZSXA     CY7C1011DV33-10ZSXI",null,"IS61WV12816EDBLL-xxTLI    IS64WV12816EDBLL-10CTLA1 IS61WV12816EFBLL-10TLI IS61WV12816FBLL-10TLI IS61WV12816DBLS-35TLI(EOL) IS61WV12816DBLL-10TL/TLI/TI(EOL) ","GS72116AGP-xx                                  GS72116ATP-xx(EOL)"]
["256K x 8","3.3V","44pin TSOP II","10,12,15,20","AS7C32096A-xxTxN",null,null,null,"IS61WV2568EDBLL-xxTLI IS64WV2568EDBLL-10CTLA1 IS61WV2568EFBLL-10TLI  IS61WV2568FBLL-10TLI ","GS72108AGP-xx                            GS72108ATP-xx(EOL)"]
["4M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["512K x 8","5V","36pin SOJ (400mil)","10,12,15,20","AS7C4096A-xxJxN","K6R4008C1D-KI10","CY7C1049D-10VXI(EOL)\nCY7C1049G-10VXI                   \nCY7C1049GN-10VXI","R1RP0408DGE-2LR(PI/PR)#B1","IS61C5128AL-10KLI"]
["512K x 8","5V","44pin TSOP II (400mil)","10,12,15,20","AS7C4096A-xxTxN","K6R4008C1D-UI10","CY7C1049G-10ZSXI",null,"IS61C5128AL-10TLI"]
["512K x 8","3.3V","36pin SOJ (400mil)","8,10,12,15,20","AS7C34096A-xxJxN","K6R4008V1D-KI10","CY7C1049DV33-10VXI (EOL)\nCY7C1049G30-10VXI                      CY7C1049GN30-10VXI ","71V424LxxYG      \n71V424SxxYG\nR1RW0408DGE-2LR(PI/PR)#B1","IS61WV5128FBLL-10KLI  IS64WV5128EFBLL-10KLA3  IS61WV5128EDBLL-10KLI/KLA1 IS61WV5128BLL-10KLI "]
["512K x 8","3.3V","44pin TSOP II (400mil)","10,12,15,20","AS7C34096A-xxTxN","K6R4008V1D-UI10","CY7C1049DV33-10ZSXI(EOL)\nCY7C1049G30-10ZSXI                      CY7C1049GN30-10ZSXI ","71V424LxxPHG    \n71V424SxxPHG","IS61WV5128FBLL-10TLI  IS64WV5128EFBLL-10CTLA3 IS61WV5128EDBLL-10TLI  IS64WV5128EDBLL-10CTA1/CTLA1 IS61WV5128BLL-10TL/TLI    IS61WV5128BLS-25TLI "]
["512K x 8","2.7 ~ 3.6V","44pin TSOP II",10,"AS7C34096B-10TIN",null,"CY7C1049G30-10ZSXI                      CY7C1049GN30-10ZSXI ","71V424LxxPHG     \n71V424SxxPHG","IS61WV5128FBLL-10TLI  IS64WV5128EFBLL-10CTLA3 IS61WV5128EDBLL-10TLI  IS64WV5128EDBLL-10CTA1/CTLA1 IS61WV5128BLL-10TL/TLI    IS61WV5128BLS-25TLI "]
["512K x 8","2.7 ~ 3.6V","36ball TFBGA",10,"AS7C34096B-10BIN",null,null,null,"IS61WV5128FBLL-10BI/BLI IS64WV5128EFBLL-10BA3/BLA3 IS61WV5128EDBLL-10BI/BLI IS64WV5128EDBLL-10BA1/BLA1  IS61WV5128BLL-10BI/BLI "]
["256K x 16","5V","44pin SOJ (400mil)","10,12,15,20","AS7C4098A-xxJxN","K6R4016C1D-KI10","CY7C1041D-10VXI(EOL)\nCY7C1041G-10VXI","R1RP0416DGE-2LR(PI/PR)#B1","IS61C25616AL-10KLI                  IS61C25616AS-25KLI"]
["256K x 16","5V","44pin TSOP II (400mil)","10,12,15,20","AS7C4098A-xxTxN","K6R4016C1D-UI10","CY7C1041D-10ZSXI(EOL)\nCY7C1041G-10ZSXI                          CY7C1041GN-10ZSXI ","R1RP0416DSB-0PI(PR)#D1     R1RP0416DSB-2LR(PI/PR/SR)#D1  R1RP0416DSB-2LR(PR)#S1","IS61C25616AL-10TL/TLI                 IS61C25616AS-25TLI"]
["256K x 16","3.3V","44pin SOJ (400mil)","10,12,15,20","AS7C34098A-xxJxN","K6R4016V1D-KI10","CY7C1041DV33-10VXI (EOL)\nCY7C1041GN30-10VXI(EOL)\nCY7C1041G30-10VXI","71V416LxxYG   \n71V416SxxYG\nR1RW0416DGE-2LR(PI/PR)#B1","IS61WV25616BLL-xxKLI(EOL)"]
["256K x 16","3.3V","44pin TSOP II (400mil)","8,10,12,15,20","AS7C34098A-xxTxN","K6R4016V1D-UI10","CY7C1041DV33-10ZSXI(EOL)\nCY7C1041G30-10ZSXI/A\n","71V416LxxPHG   \n71V416SxxPHG\nR1RW0416DSB-0PI(PR)#D1  R1RW0416DSB-0PI(PR)#S1  R1RW0416DSB-2LR(PI/PR/SR)#D1 R1RW0416DSB-2PI(PR)#S1","IS61WV25616EDBLL-xxTLI/CTLA1   IS61WV25616EFBLL-10TLI IS61WV25616FBLL-10TL    IS61WV25616BLL-xxTL/TLI(EOL)   IS61WV25616BLS-25TLI(EOL)","GS74116AGP-xx"]
["256K x 16","3.3V","48ball TFBGA",10,"AS7C34098A-xxBIN",null,"CY7C1041DV33-10BVXI(EOL)\nCY7C1041G30-10BVJXI\n","71V416LxxBE  \n71V416SxxBE","IS61WV25616EDBLL-xxBLI/BLA1   IS61WV25616EFBLL-10BLI IS61WV25616FBLL-10BI/BLI   IS61WV25616BLL-xxBLI (EOL)","GS74117AX-xx  GS74117AGX-xx"]
["256K x 16","2.7 ~ 3.6V","44pin TSOP II",10,"AS7C34098B-10TIN",null,"CY7C1041DV33-10ZSXI(EOL)\nCY7C1041G30-10ZSXI/A\n","71V416LxxPHG   \n71V416SxxPHG\nR1RW0416DSB-0PI(PR)#D1  R1RW0416DSB-0PI(PR)#S1  R1RW0416DSB-2LR(PI/PR/SR)#D1 R1RW0416DSB-2PI(PR)#S1","IS61WV25616EDBLL-xxTLI/CTLA1   IS61WV25616EFBLL-10TLI IS61WV25616FBLL-10TL    IS61WV25616BLL-xxTL/TLI(EOL)   IS61WV25616BLS-25TLI(EOL)","GS74116AGP-xx"]
["256K x 16","2.7 ~ 3.6V","48ball TFBGA",10,"AS7C34098B-10BIN",null,"CY7C1041DV33-10BVXI(EOL)\nCY7C1041G30-10BVJXI","71V416LxxBE   \n71V416SxxBE","IS61WV25616EDBLL-xxBLI/BLA1   IS61WV25616EFBLL-10BLI IS61WV25616FBLL-10BLI   IS61WV25616BLL-xxBLI (EOL)","GS74117AX-xx  GS74117AGX-xx"]
["8M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI"]
["512K x 16","3.3V","44pin TSOP II",10,"AS7C38098A-10TIN",null,"CY7C1051DV33-10/12ZSXI(EOL)\nCY7C1051H30-10ZSXI",null,"IS61WV51216EEBLL-xxTLI     IS61WV51216EDBLL-xxTLI    IS61WV51216BLL-xxTLI"]
["512K x 16","3.3V","48ball TFBGA",10,"AS7C38098A-10BIN",null,"CY7C1051DV33-10BAXI (EOL)\nCY7C1051H30-10BVXI",null,"IS61WV51216EEBLL-xxBLI   IS61WV51216EDBLL-xxBLI  IS61WV51216BLL-xxMLI"]
["256K x 32","3.3V","90ball TFBGA",10,"AS7C325632-10BIN",null,null,null,"IS61WV25632BLL-10BLI"]
["1M x 8","3.3V","44pin TSOP II",10,"AS7C38096A-10TIN",null,"CY7C1059DV33-10ZSXI(EOL)\nCY7C1059DV33-12ZSXI/Q(EOL)                      CY7C1059H30-10ZSXI",null,"IS61WV10248BLL-xxTLI   IS61WV10248EEBLL-8TLI   IS61WV10248EDBLL-xxTLI"]
["1M x 8","3.3V","48ball TFBGA (different pinout)",10,"AS7C38096A-10BIN"]
["1M x 8","3.3V","48ball TFBGA (different pinout)",10,"AS7C38096B-10BIN",null,null,null,"IS61WV10248BLL-xxMLI  IS61WV10248EEBLL-xxBLI  IS61WV10248EDBLL-xxBLI "]
["16M  FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI"]
["1M x 16","3.3V","48pin TSOP I",10,"AS7C316098A-10TIN",null,"CY7C1061GN30-10ZXI\n CY7C1061G30-10ZXI",null,"IS61WV102416BLL-xxTLI(EOL)  IS61WV102416DALL-12TLI  IS62WV102416BLL-25TLI   IS61WV102416EDBLL-10TL/TLI   IS61WV102416FBLL-xxTLI "]
["1M x 16","3.3V","48ball TFBGA",10,"AS7C316098A-10BIN",null,"CY7C1061GN30-10BV1XI (EOL)    CY7C1061G30-10BV1X",null,"IS61WV102416BLL-10MLI(EOL)    IS61WV102416DALL-12BLI    IS61WV102416EDBLL-10BL/BLI  IS61WV102416FBLL-xxBLI"]
["1M x 16","3.3V","54pin TSOP II",10,"AS7C316098B-10TIN",null,"CY7C1061GN30-10ZSXI \nCY7C1061G30-10ZSXI\nCY7C10612G30-10ZSXI   ",null,"IS61WV102416FBLL-xxT2LI"]
["1M x 16","3.3V","48ball TFBGA",10,"AS7C316098B-10BIN",null,"CY7C1061GN30-10BVJXI             CY7C1061GN30-10BVXI             CY7C1061G30-10BVJXI",null,"IS62WV102416BLL-25MLI    IS61WV102416FBLL-xxB2LI"]
["2M x 8","3.3V","48pin TSOP I",10,"AS7C316096A-10TIN"]
["2M x 8","3.3V","54pin TSOP II",10,"AS7C316096B-10TIN",null,"CY7C1069DV33-10ZSXI (EOL)\nCY7C1069GN30-10ZSXI\nCY7C1069G30-10ZSXI   ",null,"IS61WV20488FBLL-xxT2LI"]
["2M x 8","3.3V","44pin TSOP II",10,"AS7C316096C-10TIN",null,null,null,"IS61WV20488FBLL-xxTLI  IS61WV20488BLL-xxTLI (EOL)    IS62WV20488BLL-25TLI "]
["2M x 8","3.3V","48ball TFBGA (1CE)",10,"AS7C316096C-10BIN",null,null,null,"IS61WV20488BLL-xxMLI(EOL)  IS61WV20488FBLL-xxBLI"]
["2M x 8","3.3V","48ball TFBGA (2CE)",10,"AS7C316096B-10BIN",null,"CY7C1069GN30-10BVXI   CY7C1069G30-10BVXI     CY7C1069DV33-10BVXI(EOL)"]
[]
["32M  FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI"]
["2M x 16","1.8V/2.5V/3.3V","48b FBGA (6x8mm)",10,"AS7CW2M16-10BIN",null,"CY7C1071DV33-12BAXI (3.3V)",null,"IS61WV204816ALL-10BL/I (1.8V) IS61WV204816BLL-10BL/I (3.3V) "]
[]
["Low Power Asynchronous SRAM Cross Reference"]
["64K"]
["ORG","VCC","PACKAGE","ALLIANCE","ZMD","CYPRESS (EOL)","HITACHI (EOL)","NEC (EOL)","HYNIX (EOL)"]
["8K x 8","2.7V ~ 5.5V","28pin 600mil DIP","AS6C6264-55PCN / PIN","U6264BDC07LLG1",null,"HM6264BLP",null,"HY6264P"]
["8K x 8","2.7V ~ 5.5V","28pin 330mil SOP","AS6C6264-55SCN / SIN","U6264BS2C07LLG1","CY6264-55SNXC/I(EOL)             CY6264-70SNXC/I(EOL)","HM6264BLFP","uPD4464","HY6264G"]
["8K x 8","2.7V ~ 5.5V","28pin STSOP (8 x 13.4 mm)","AS6C6264-55STCN"]
["256K"]
["ORG","VCC","PACKAGE","ALLIANCE","ZMD","SAMSUNG (EOL)","CYPRESS (EOL)","RENESAS","BRILLIANCE (EOL)","ISSI"]
["32K x 8","2.7V ~ 5.5V","28pin 600mil DIP","AS6C62256-55PCN","U62256ADC07LLG1","K6X0808C1D-DF55","CY62256NLL-70PXC(EOL)",null,"BS62LV256PCP-55"]
["32K x 8","2.7V ~ 5.5V","28pin 330mil SOP","AS6C62256-55SxN","U62256AS2C07LLG1","K6X0808C1D-BF55","CY62256NLL-55SNXI(EOL)  CY62256NLL-70SNXA(EOL)  CY62256NVLL-70SNXI(EOL)","R1LP5256ESP-5SI   \nR1LV5256ESP-5SI","BS62LV256SCP-55","IS62C256AL-xxULI/UL IS62LV256AL-45ULI"]
["32K x 8","2.4V ~ 3.6V","28pin 330mil SOP","AS62V256-70SIN",null,null,"CY62256NVLL-70SNXI(EOL)","R1LV5256ESP-5SI","BS62LV256SCP-55","IS62LV256AL-45ULI"]
["32K x 8","2.7V ~ 5.5V","28pin STSOP (8 x 13.4 mm)","AS6C62256-55STxN",null,"K6X0808C1D-LF55","CY62256NLL-70ZRXI(EOL)\nCY62256NLL-55ZXI/A(EOL)  CY62256VNLL-70ZXC/I(EOL) ","R1LP5256ESA-5SI   \nR1LV5256ESA-5SI","BS62LV256STCP-55","IS62LV256AL-xxTL/TLI   IS62C256AL-45TL/TLI"]
["1M"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","BRILLIANCE (EOL)","NEC (EOL)","ISSI"]
["128K x 8","2 .7V ~ 5.5V","32pin 600mil DIP","AS6C1008-55PCN / PIN","K6X1008C2D-DB55",null,null,"BS62LV1027PCP-55","uPD431000ACZ-70L"]
["128K x 8","2.7V ~ 5.5V","32pin 450mil SOP","AS6C1008-55SIN","K6X1008C2D-GF55(Lead)/BF","CY62128ELL-45SXI/A    CY62128EV30LL-45SXI","M5M51008DFP-55HI\nR1LP0108ESN-5SI   \nR1LV0108ESN-5SI","BS62LV1027SIP-55","uPD431000AGW-70L","IS62C1024AL-35QLI IS62WV1288FBLL-45QLI    IS62WV1288BLL-45/55QLI (EOL) IS62WV1288DBLL-45QLI(EOL)"]
["128K x 8","2.7V ~ 5.5V","32pin TSOP I (8 x 20 mm)","AS6C1008-55TIN","K6X1008C2D-TF55 or PF","CY62128ELL-45ZXI/A   CY62128EV30LL-45ZXI","M5M51008DVP-55HI\nR1LP0108ESF-5SI   \nR1LV0108ESF-5SI","BS62LV1027TIP-55","uPD431000AGZ-70LL-KKH","IS62C1024AL-35TLI   IS62WV1288FBLL-45TLI  IS62WV1288BLL-45/55TLI(EOL)   IS65WV1288BLL-55TLA1(EOL)    IS62WV1288DBLL-45TLI(EOL)"]
["128K x 8","2.7V ~ 5.5V","32pin STSOP (8 x 13.4 mm)","AS6C1008-55STIN",null,"CY62128EV30LL-45ZAXI     CY62128ELL-45ZAXI(EOL)  ","M5M51008DKV-55HI\nR1LP0108ESA-5SI   \nR1LV0108ESA-5SI","BS62LV1027STIP-55","uPD431000AGU-B10-9JH"," IS62WV1288FBLL-45HLI    IS62WV1288BLL-45/55HLI(EOL)  IS65WV1288BLL-55HLA1(EOL) S62WV1288DBLL-45HLI(EOL)"]
["64K x 16","2.7V ~ 5.5V","48ball TFBGA","AS6C1016-55BIN","K6F1016U4C-EF55"," CY62126EV30LL-45BVXI",null,"BS616LV1010AI-70",null,"IS62WV6416FBLL-45BLI    IS62WV6416DBLL-45BLI(EOL)    IS62WV6416BLL-45/55BLI(EOL)"]
["64K x 16","2.7V ~ 5.5V","44pin TSOP II","AS6C1016-55ZIN",null,"CY62126EV30LL-45ZSXI/A",null,"BS616LV1010EI-70",null,"IS62WV6416FBLL-45TLI      IS62WV6416DBLL-45TLI(EOL)   IS62WV6416BLL-45/55TLI(EOL)"]
["64K x 16","2.7V ~3.6V","44pin TSOP II","AS6CE1016A-45ZIN",null,null,null,null,null,"IS61WV6416EEBLL"]
["2M"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["256K x 8","2.7V ~ 3.6V","32pin 450mil SOP","AS6C2008-55SIN",null,"CY62138FLL-45SXI    CY62138FV30LL-45SXI(EOL)",null,"BS62LV2006SIP-55"]
["256K x 8","2.7V ~ 3.6V","32pin TSOP I (8 x 20 mm)","AS6C2008-55TIN",null,"CY62138FV30LL-45ZXI",null,"BS62LV2006TIP-55","IS62WV2568BLL-45/55TLI  IS62WV2568EBLL-45TLI   IS62WV2568FBLL-45TLI "]
["256K x 8","2.7V ~ 3.6V","32pin STSOP (8 x 13.4 mm)","AS6C2008-55STIN","K6F2008V2E-LF70000","CY62138FV30LL-45ZAXI/A","M5M5V208AKV-55HI\nR1LV0208BSA-5SI","BS62LV2006STIP-55","IS62WV2568BLL-45/55HLI     IS62WV2568EBLL-45HLI   IS62WV2568FBLL-45HLI"]
["256K x 8","2.7V ~ 3.6V","36ball TFBGA (6mm x 8mm)","AS6C2008-55BIN",null,"CY62138FV30LL-45BVXI   ",null,null,"IS62WV2568BLL-45/55BLI     IS62WV2568EBLL-45BLI   IS62WV2568FBLL-45BLI"]
["128K x 16","2.7V ~ 5.5V","44pin TSOP II","AS6C2016-55ZIN",null,"CY62136VLL-70ZSXI(EOL)\nCY62136E/FV30LL-55ZSXI\nCY62136E/FV30LL-45ZSXI\nCY62137FV30LL-45ZSXI","M5M5V216ATP-70HI\nR1LV0216BSB-5SI","BS616LV2016EIP-55","IS62WV12816BLL-45/55TLI IS62WV12816EBLL-45/55TLI  IS62WV12816FBLL-45TLI    IS62WV12816DBLL-35/45/55TLI "]
["128K x 16","2.7V ~ 3.6V","48ball TFBGA","AS6C2016-55BIN","K6F2016U4E-EF55000","CY62136E/FV30LL-45BVXI\nCY62137FV30LL-45BVXI\nCY62137EV30LL-45BVXI(EOL)",null,"BS616LV2019AIG-55","IS62WV12816BLL-45/55BLI  IS62WV12816EBLL-45/55BLI   IS62WV12816FBLL-45BLI    IS62WV12816DBLL-35/45/55BLI"]
["256K x 8","2.7V ~ 5.5V","32pin 450mil SOP","AS6C2008A-55SIN",null,"CY62138FLL-45SXI    CY62138FV30LL-45SXI(EOL)",null,"BS62LV2006SIP-55"]
["256K x 8","2.7V ~ 5.5V","32pin TSOP I (8 x 20mm)","AS6C2008A-55TIN",null,"CY2138FV30LL-45ZXI",null,"BS62LV2006TIP-55","IS62WV2568BLL-45/55TLI  IS62WV2568EBLL-45TLI   IS62WV2568FBLL-45TLI "]
["256K x 8","2.7V ~ 5.5V","36ball TFBGA (6mm x 8mm)","AS6C2008A-55BIN",null,"CY62138FV30LL-45BVXI   ",null,null,"IS62WV2568BLL-45/55BLI     IS62WV2568EBLL-45BLI   IS62WV2568FBLL-45BLI"]
["4M"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["512K x 8","2.7V ~ 5.5V","32pin 600mil DIP","AS6C4008-55PCN","K4X4008C1F-DB55",null,null,"BS62LV4006PCP-55"]
["512K x 8","2.7V ~ 5.5V","32pin 450mil SOP","AS6C4008-55SIN","K6X4008C1F-GF55 or BF","CY62148ELL-55SXI      CY62148EV30LL-55SXI      CY62148G30-45SXI\nCY62148G-45SXI(EOL)             ","R1LP0408DSP-5SI          RMLV0408EGSP-4S2               ","BS62LV4006SIP-55","IS62C5128EL-45QLI      IS62WV5128DBLL-45QLI    IS62WV5128EBLL-45QLI   IS62WV5128BLL-55QLI "]
["512K x 8","2.7V ~ 5.5V","32pin STSOP (8 x 13.4mm)","AS6C4008-55STIN",null,"CY62148ESL-55ZAXI/A      ","RMLV0408EGSA-4S2","BS62LV4006STIP-55","IS62C5128EL-45HLI     IS62WV5128DBLL-45HLI   IS62WV5128EBLL-45HLI  IS62WV5128EHBLL-45HLI/HL  IS62WV5128BLL-55HLI "]
["512K x 8","2.7V ~ 5.5V","32pin TSOP I (8 x 20mm)","AS6C4008-55TIN",null,null,null,null,"IS62WV5128DBLL-45TLI  IS62WV5128EBLL-45TLI  IS62WV5128EHBLL-45TLI/TL  IS62WV5128BLL-55TLI "]
["512K x 8","2.7V ~ 5.5V","32pin TSOP II","AS6C4008-55ZIN","K6X4008C1F-VF55","CY62148ELL-45ZSXI    \nCY62148EV30LL-45ZSXI    \nCY62148G30-45ZSXI                CY62148G-45ZSXI(EOL)\nCY62148GN-45ZSXIT(EOL)\nCY62148GN30-45ZSXIT(EOL)","R1LP0408DSB-5SI        RMLV0408EGSB-4S2","BS62LV4006ECP55","IS62WV5128DBLL-45T2LI  IS62C5128EL-45TLI   IS62WV5128EBLL-45T2LI   IS62WV5128EHBLL-45T2LI/T2L IS62WV5128BLL-55T2LI"]
["512K x 8","2.7V ~ 5.5V","36pin TFBGA (6mm x 8mm)","AS6C4008-55BIN",null,"CY62148EV30LL-45BVXI     ",null,null,"IS62WV5128EBLL-45BLI  IS62WV5128DBLL-45BLI   IS62WV5128EHBLL-45BLI/BL   IS62WV5128BLL-55BLI "]
["256K x 16","2.7V ~ 5.5V","44pin TSOP II","AS6C4016-55ZIN","K6X4016C3F-TF70000","CY62146ELL-45ZSXI                    CY62146ESL-45ZSXI               CY62146EV30LL-45ZSXI\nCY62147EV30LL-45ZSXI      \nCY62146G-45ZSXI                \nCY62147G-45ZSXI                        CY62147G30-45ZSXI/A     \nCY62147GN30-45ZSXI                         \nCY62146GN-45ZSXI(EOL)\nCY62147GE-45ZSXI(EOL)   ","RMLV0414EGSB-4S2       RMLV0416EGSB-4S2","BS616LV4017EIP-55","IS62WV25616BLL-55TLI   IS62WV25616DBLL-45/55TLI   IS65WV25616DBLL-45CTLA1   IS62WV25616EBLL-45/55TLI   IS65WV25616EBLL-45CTLA1"]
["256K x 16","2.7V ~ 3.6V","44pin TSOP II","AS6C4016B-45ZIN","K6X4016T3F-TF70000","CY62146EV30LL-45ZSXI  \nCY62147EV30LL-45ZSXI     \nCY62147G30-45ZSXI/A    \nCY62147GN30-45ZSXI  \nCY62146GN30-45ZSXI(EOL)","RMLV0414EGSB-4S2        RMLV0416EGSB-4S2","BS616LV4017EIP-55","IS62WV25616BLL-55TLI   IS62WV25616DBLL-45/55TLI   IS65WV25616DBLL-45CTLA1   IS62WV25616EBLL-45/55TLI   IS65WV25616EBLL-45CTLA1"]
["256K x 16","2.7V ~ 3.6V","48ball  TFBGA","AS6C4016B-45BIN","K6F4016U6G-EF70000","CY62146EV30LL-45BVXI  \nCY62147EV30LL-45BVXI  \nCY62147G30-45BVXI                 \nCY62147G30-45BVXA(EOL)\nCY62146GN30-45BVXI (EOL)\nCY62147GN30-45BVXI(EOL)","RMLV0416EGBG-4S2","BS616LV4017AIP-55","IS62WV25616BLL-55BLI   IS62WV25616DBLL-45BLI   IS62WV25616EBLL-45/55BLI  IS65WV25616EBLL-45BLA1"]
["256K x 16","2.7V ~ 3.6V","44pin TSOP II","AS6CE4016B-45ZIN","K6X4016T3F-TF70000","CY62146G30-45ZSXI           \nCY62146G-45ZSXA                  \nCY62147G30-45ZSXA                 CY621472G30-45ZSXI/A         \nCY62147GE30-45ZSXI(EOL)","RMLV0414EGSB-4S2        RMLV0416EGSB-4S2","BS616LV4017EIP-55","IS62WV25616EHBLL-45TL/TLI  IS65WV25616EHBLL- 45CTLA1"]
["256K x 16","2.7V ~ 3.6V","48ball  TFBGA","AS6CE4016B-45BIN","K6F4016U6G-EF70000","CY62146G30-45BVXI  \nCY62147EV30LL-45BVXI\nCY62146GE30-45BVXI(EOL)","RMLV0416EGBG-4S2","BS616LV4017AIP-55","IS62WV25616EHBLL-45BLI"]
["8M"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","BRILLIANCE","ISSI"]
["1M x 8","2.7 ~ 5.5V","44pin TSOP II","AS6C8008-55ZIN","K6X8008(C/T)2B-UF55","CY62158EV30LL-45ZSXI   CY62158G30-45ZSXI  \nCY62158ELL-45ZSXI ","RMLV0808BGSB-4S2\nHM62V8100LTTI-5SL","BS62LV8001ECP-55","IS62C10248AL-55TLI   IS62WV10248EBLL-45/55TLI  IS62WV10248EFBLL-45TLI   IS62WV10248HBLL-45TL/TLI  IS62WV10248DBLL-55TLI"]
["1M x 8","2.7 ~ 5.5V","44pin TSOP II","AS6C8008B-45/55ZIN","K6X8008(C/T)2B-UF55","CY62158EV30LL-45ZSXI     CY62158G30-45ZSXI  \nCY62158ELL-45ZSXI   ","RMLV0808BGSB-4S2\nHM62V8100LTTI-5SL","BS62LV8001ECP-55","IS62C10248AL-55TLI   IS62WV10248EBLL-45/55TLI  IS62WV10248EFBLL-45TLI   IS62WV10248HBLL-45TL/TLI  IS62WV10248DBLL-55TLI"]
["1M x 8","2.7 ~ 5.5V","48ball TFBGA","AS6C8008-55BIN",null,"CY62158EV30LL-45BVXI    CY62158G30-45BVXI   CY62158GE30-45BVXI","HM62V8100LBPI-5SL","BS62LV8001ECP-55","IS62C10248AL-55MLI   IS62WV10248EBLL-45/55BLI  IS62WV10248EFBLL-45BLI     IS62WV10248HBLL-45B2L/B2LI  IS62WV10248DBLL-55MLI   IS62WV10248BLL-55BLI "]
["1M x 8","2.7 ~ 3.6V","48ball TFBGA","AS6C8008B-45BIN",null,"CY62158EV30LL-45BVXI","HM62V8100LBPI-5SL","BS62LV8001FIP-55","IS62WV10248EBLL-45/55BLI  IS62WV10248EFBLL-45BLI     IS62WV10248HBLL-45B2L/B2LI  IS62WV10248DBLL-55MLI   IS62WV10248BLL-55BLI "]
["512K x 16","2.7 ~ 5.5V","48ball TFBGA (6 x 8mm)*","AS6C8016-55BIN*","K6F8016U6G-FF55",null,"M5M5W816WG-55HI","BS616LV8017ECP55","IS62WV51216HBLL-45BL/BLI"]
["512K x 16","2.7 ~3.6V","48ball TFBGA (6 x 8mm)**","AS6C8016B-45/55BIN",null,"CY62157EV30LL-45BVXI/A    CY62157G30-45BVXI  ","RMLV0816BGBG-4S2",null,"IS62WV51216EBLL-45/55BLI   IS62WV51216EFBLL-45/55BLI   IS62WV51216HBLL-45B2L/B2LI"]
["512K x 16","2.7 ~ 5.5V","44pin TSOP II","AS6C8016 -55ZIN","K6X8016(C/T)3B-UF55","CY62157EV30LL-45ZSXI/A CY62157ESL-45ZSXI     CY62157ELL-45ZSXI\nCY62157G30-45ZSXI","RMLV0816BGSB-4S2\nHM62165I14LTT-5SL\nM5M5W816TP-55HI","BS616LV8017FCP70","IS62C51216AL-55TLI    IS62WV51216EBLL-45/55TLI   IS62WV51216EFBLL-45/55TLI   IS62WV51216HBLL-45/55TL "]
["512K x 16","2.7 ~3.6V","44pin TSOP II","AS6C8016B-45/55ZIN",null,"CY62157EV30LL-45ZSXI/A   CY62157ESL-45ZSXI    CY62157EV30LL-45ZSXI    CY62157G30-45ZSXI","RMLV0816BGSB-4S2",null,"IS62WV51216EFBLL-45/55TLI    IS62WV51216HBLL-45TL/TLI"]
["512K x 16","2.7 ~ 5.5V","48pin TSOP I","AS6C8016-55TIN",null,"CY62157EV30LL-45ZXI/A    CY62157G30-45ZXI","RMLV0816BGSA-4S2",null,"IS62WV51216GBLL-45TLI   "]
["* = one chip select pin:B5 ** = two chip select pins: B5 and A6"]
["16M"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["1M x 16","2.7 ~ 3.6V","48pin TSOP I","AS6C1616-55TIN\nAS6C1616B-45/55TIN","CY62167E30LL-45/55ZXI   CY62167EV30LL-45/55ZXI    CY62167DV30LL-55ZXI  CY62167EV30LL-45ZXI/A   CY62167G30-45ZXI/A   CY62167GN30-45ZXI ","RMLV1616AGSA-4/5U2   RMLV1616AGBG-5S2    RMLV1616AGSA-5S2 R1LV1616RSA-5/7/8S(EOL)","BS6216LV1611TCP55","IS62WV102416DBLL-45/55TLI     IS62WV102416GBLL-45TLI"]
["1M x 16","2.7 ~ 3.6V","48pin TSOP I","AS6C1616C-45TIN","CY62167E30LL-45/55ZXI\nCY62167EV30LL-45/55ZXI    CY62167DV30LL-55ZXI  CY62167EV30LL-45ZXI/A    CY62167G30-45ZXI/A     CY62167GN30-45ZXI ","RMLV1616AGSA-4/5U2   RMLV1616AGBG-5S2    RMLV1616AGSA-5S2 R1LV1616RSA-5/7/8S(EOL)","BS6216LV1611TCP55","IS62WV102416DBLL-45/55TLI     IS62WV102416GBLL-45TLI"]
["1M x 16","2.7 ~ 3.6V","48ball TFBGA","AS6C1616B-45/55BIN","CY62167DV30LL-70BVXI(EOL)\nCY62167DV30LL-55BVXI    CY62167EV30LL-45BVXI/A   CY62167G30-45BVX/A    CY62167GN30-45BVXI","R1LV1616HBG-4/5SI(EOL)   RMLV1616AGBG-4/5U2  RMLV1616AGBG-5S2","BS6216LV1611FCP70","IS62WV102416FBLL-45/55BLI   IS62WV102416EBLL-45/55BLI"]
["2M x 8","2.7 ~ 3.6V","44pin TSOP I","AS6C1608B-45TIN",null,null,"BS6216LV1600EIP55"]
["2M x 8","2.7 ~ 3.6V","48ball TFBGA","AS6C1608B-45BIN","CY62168EV30LL-45BVXI   CY62168G30-45BVXI   CY62168GN30-45BVXI",null,null,"IS62WV20488EBLL-45/55BLI     IS62WV20488FBLL-45/55BLI"]
["32M"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS"]
["2M x 16","2.7 ~ 3.6V","48pin TSOP I","AS6C3216A-55TIN*","CY62177EV30LL-55ZXI     CY62177G30-55ZXI","RMLV3216AGSA-5S2    R1LV3216RSA-5/7S(EOL)   "]
["2M x 16","2.7 ~ 3.6V","48ball TFBGA","AS6C3216A-55BIN","CY62177EV30LL-55BAXI   CY62177G30-55BAXI        CY62177G30-55BKXI   ","RMWV3216AGBG-5S2 RMLV3216AGBG-5S2"]
["*48pin TSOP I (please note: dual chip select 2Mx16 or 4Mx8)"]
["64M"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS"]
["4M x 16","2.7V ~ 3.6V","48pin TSOP I","AS6C6416-55TIN",null,"RMWV6416AGSA-5S2     R1WV6416RSA-5/7S(EOL)"]
["4M x 16","2.7V ~ 3.6V","48ball BGA","AS6C6416-55BIN","CY62187EV30LL-55BAXI     CY62187G30-55BAXI","RMWV6416AGBG-5S2     R1WV6416RBG-5/7S(EOL)"]
["*48pin TSOP I (please note: dual chip select 4Mx16 or 8Mx8)"]
["Sync SRAM Cross Reference"]
["ORG","DENSITY","PACKAGE","MODE","ALLIANCE","IDT","SAMSUNG","CYPRESS","GSI","ISSI"]
["4M","128K x 36","100TQFP","SPB","AS8C403600-QC150N","71V3576SxxxPFG","K7A403600B-QCxx","CY7C1347G-xxxAX","GS84036AGT-xxx","IS61LPS12836A-xxxTQ"]
["4M","256K x 16","100TQFP",null,"AS8C401800-QC150N","71V3578SxxxPFG","K7A401800B-QCxx","CY7C1327G-xxxAX","GS84018AGT-xxx","IS61LPS25618A-xxxTQ"]
["4M","128K x 36","100TQFP","SB","AS8C403625-QC75N","71V3577SxxPFG","K7B403625B-QCxx","CY7C1345G-xxxAX","GS84036AGT-xxx","IS61LF12836A-xxxTQ"]
["4M","256K x 18","100TQFP",null,"AS8C401825-QC75N","71V3579SxxPFG","K7B401825B-QCxx","CY7C1325G-xxxAX","GS84018AGT-xxx","IS61LF25618A-xxxTQ"]
["4M","128K x 36","100TQFP","ZBT/SPB","AS8C403601-QC166N","71V3556SxxxPFG","K7N403601B-QCxx","CY7C1350G-xxxAX","GS840Z36AGT-xxx","IS61NLP12836A-xxxTQ"]
["4M","256K x 18","100TQFP",null,"AS8C401801-QC166N","71V3558SxxxPFG","K7N401801B-QCxx","CY7C1352G-xxxAX","GS840Z18AGT-xxx","IS61NLP25618A-xxxTQ"]
["9M","256K x 36","100TQFP","SPB","AS8C803600-QC150N","71V67603SxxxPFG","K7A803600B-QCxx","CY7C1360C-xxxAJX","GS88036CT-xxx","IS61LPS25636A-xxxTQ"]
["9M","512K x 18","100TQFP",null,"AS8C801800-QC150N","71V67803SxxxPFG","K7A801800B-QCxx","CY7C1362C-xxxAJX","GS88018CT-xxx","IS61LPS51218A-xxxTQ"]
["9M","256K x 36","100TQFP","SB","AS8C803625-QC75N","71V67703SxxPFG","K7B803625B-QCxx","CY7C1361C-xxxAJX","GS88036CT-xxx","IS61LPS25636A-xxxTQ"]
["9M","256K x 36","100TQFP",null,"AS8C801825-QC75N","71V67903SxxPFG","K7B801825B-QCxx","CY7C1363C-xxxAJX","GS88018CT-xxx","IS61LPS51218A-xxxTQ"]
["9M","512K x 18","100TQFP","ZBT/SPB","AS8C803601-QC150N","71V65603SxxxPFG","K7N803601B-QCxx","CY7C1354C-xxxAJX","GS880Z36CT-xxx","IS61NLP25636A-xxxTQ"]
["9M","512K x 18","100TQFP",null,"AS8C801801-QC150N","71V65803SxxxPFG","K7N801801B-QCxx","CY7C1356C-xxxAJX","GS880Z18CT-xxx","IS61NLP51218A-xxxTQ"]
["9M","256K x 36","100TQFP","ZBT/SB","AS8C803625A-QC75N","71V65703SxxPFG","K7M803625B-QCxx","CY7C1351C-xxxAJX","GS880Z36CT-xxx","N/A"]
["9M","512K x 18","100TQFP",null,"AS8C801825A-QC75N","71V65903SxxPFG","K7M801825B-QCxx","CY7C1353C-xxxAJX","GS880Z18CT-xxx","N/A"]
["18M","512K x 36","100TQFP","ZBT/SPB","AS8C163631-QC166N","71T75602SxxxPFG","K7N163631B-QCxx","CY7C1370D-xxxAX","GS880Z36CT-xxx","IS61LPS12836A-xxxTQ"]
["18M","1M x 18","100TQFP",null,"AS8C161831-QC166N","71T75802SxxxPFG","K7N161831B-QCxx","CY7C1372D-xxxAX","GS880Z18CT-xxx","IS61LPS102418A-xxxTQ"]
[]
["pSRAM Cross Reference"]
["ORG","DENSITY","PACKAGE","COMMENTS/ PREV REV","ALLIANCE","JSC/JEJU","ISSI","FIDELIX","AP MEMORY"]
["8Mb","512K x 16","48 FPBGA","page mode & Non-DPD","AS1C512K16PL-70BIN","EM784SP16BPP-70LF","IS66WV51216EALL-70BLI"]
["8Mb","512K x 16","48 FPBGA","Non-page mode & Non-DPD","AS1C512K16P-70BIN","JS784SU16BSP-70LFI","IS66/67WV51216EBLL-70BL","FMP0817CAx"]
["16Mb","1M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C1M16PL-70BIN","EM7164SP16CSP-70LFI","IS66W1M16EALL-70BLI","FMP1617CCx"]
["16Mb","1M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C1M16P-70BIN","JS164SU16BSP-70LFI","IS66/67WV1M16EBLL-70BL","FMP1617CAx"]
["32Mb","2M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C2M16P-70BIN","JS7324SU16BSP-70LFI","IS66WVE2M16EBLL-70B","FMP3217CAx"]
["64Mb","4M X16","49 FBGA","DPD mode","AS1C4M16PL-70BIN","EMC643SP16CKDT-70LF"]
["128Mb\n(*2-stacked die)","8M X16","49 FBGA","DPD mode","AS1C8M16PL-70BIN","JSC283SP16ATDT-70LF",null,null,"APS128XX"]
[]
["Parallel 5V NOR Flash Cross Reference"]
["DENSITY","VCC","PACKAGE","SPEED (NS)","ALLIANCE","MICRON","CYPRESS/SPANSION","MACRONIX"]
["1Mb","5V","PLCC 32",55,"AS29CF010-55CCIN",null,"AM29F010B* (EOL)"]
["4Mb","5V","PLCC 32",55,"AS29CF040-55CCIN","M29F040","AM29F040B","MX29F040C"]
["4Mb","5V","TSOP 48pin",55,"M29F400FB55N3E2 \nM29F400FB55N3F2","M29F400F","AM29F400BB* (EOL)","MX29F400CBT"]
["4Mb","5V","TSOP 48pin",55,"M29F400FT5AN6E2","M29F400F","AM29F400BT* (EOL)","MX29F400CTT"]
["8Mb","5V","TSOP 48pin",55,"AS29CF800T-55TIN","M29F800F","AM29F800BT* (EOL)","MX29F800C T/B"]
["8Mb","5V","TSOP 48pin",55,"AS29CF800B-55TIN","M29F800F","AM29F800BB* (EOL)","MX29F800C T/B"]
["8Mb","5V","TSOP 48pin",55,"M29F800FB5AN6E2\nM29F800FB5AN6F2","M29F800F","AM29F800BB* (EOL)","MX29F800CBT"]
["8Mb","5V","TSOP 48pin",55,"M29F800FT55N3E2","M29F800F","AM29F800BT* (EOL)","MX29F800CTT"]
["16Mb","5V","TSOP 48pin",55,"AS29CF160T-55TIN","M29F160F","AM29F160DT* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"AS29CF160B-55TIN","M29F160F","AM29F160DB* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"M29F160FB5AN6F2","M29F160F","AM29F160DB* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"M29F160FT55N3E2","M29F160F","AM29F160DT* (EOL)"]
[]
["SLC Parallel NAND Flash Cross Reference"]
["DENSITY","VCC","BUS WIDTH","PACKAGE","TEMPERATURE","ALLIANCE","MICRON","SKY HIGH","CYPRESS","WINBOND","MACRONIX","KIOXIA","ISSI","GIGA DEVICES","ESMT"]
["1Gb","3.3V","x8","63b FBGA","-40°C to 85°C","AS9F31G08SA-25BIN","MT29F1G08ABADAH4\nMT29F1G08ABAEAH4","S34SL01G200BFI\nS34ML01G200BFI\nS34ML01G300BFI","S34ML01G100BFI","W29N01HV\nW29N01GV","MX30LF1G18AC","TC58NVG0S3HBA","IS34ML01G084","GD9FU1G8F3AL","F59L1G81MB"]
["2Gb","3.3V","x8","63b FBGA","-40°C to 85°C","AS9F32G08SA-25BIN","MT29F2G08ABAEAH4\nMT29F2G08ABAGAH4","S34SL02G200BFI\nS34ML02G200BFI\nS34ML02G300BFI","S34ML02G100BFI","W29N02GV\nW29N02KV","MX30LF2G18AC","TC58NVG1S3HBA","IS34ML02G084","GD9FU2G8F2AL","F59L2G81A\nF59L2G81KA"]
["4Gb","3.3V","x8","63b FBGA","-40°C to 85°C","AS9F34G08SA-25BIN","MT29F4G08ABADAH4\nMT29F4G08ABAEAH4\nMT29F4G08ABAFAH4","S34SL04G200BFI\nS34ML04G200BFI","S34ML04G100BFI","W29N04GV","MX30LF4G18AC","TC58NVG2S0HBA","IS34ML04G084","GD9FU4G8F2AL","F59L4G81XB"]
["8Gb","3.3V","x8","63b FBGA","-40°C to 85°C","AS9F38G08SA-25BIN","MT29F8G08ADACAH4","S34ML08G201BFI","S34ML08G101BFI","W29N08GV","MX60LF8G18AC","TH58NVG3S0HBA","IS34ML08G088\nIS34ML08G168","GD9FU8G8E2AL","F59D4G81XB\nF59D4G-81KA"]
["4Gb","1.8V","x8","63b FBGA","-40°C to 85°C","AS9F14G08SA-45BIN","MT29F4G08ABBDAH4\nMT29F4G08ABBEAH4\nMT29F4G08ABBFAH4","S34MS04G200BFI","S34MS04G100BFI","W29N04GZ\nW29N04GW","MX30UF4G18AC","TC58NYG2S0HBA","IS34MW04G164","GD9FS4G8F2AL","F59D8G81XB"]
["8Gb","1.8V","x8","63b FBGA","-40°C to 85°C","AS9F18G08SA-45BIN","MT29F8G08ADBCAH4\nMT29F8G08ADBDAH4\nMT29F8G08ABBCAH4\nMT29F8G08ABBDAH4","S34MS08G201BFI","S34MS08G101BFI","W29N08GW\nW29N08GZ","MX60UF8G18AC","TH58NYG3S0HBA","IS34MW08G088\nIS34MW08G168","GD9FS8G8E2AL"]
["4Gb","1.8V","x8","63b FBGA","-40°C to 105°C","AS9F14G08SA-45BAN","MT29F4G08ABBDAH4-A\nMT29F4G08ABBEAH4-A","S34MS04G200BFI","S34MS04G100BFV","W29N04GZ\nW29N04GW",null,null,"IS35MW04G084","GD9FS4G8F2AL"]
["8Gb","1.8V","x8","63b FBGA","-40°C to 105°C","AS9F18G08SA-45BAN","MT29F8G08ADBDAH4-A","S34MS08G201BFA","S34MS08G101BFA","W29N08GW\nW29N08GZ",null,null,null,"GD9FS8G8E2AL"]
[]
["Serial NOR Flash Cross Reference"]
["DENSITY","VCC","PACKAGES","ALLIANCE","MICRON","ADESTO","SPANSION","WINBOND","MACRONIX","ISSI","GIGA DEVICES"]
["2Mb","3.3V","8pin SOIC (150mils)","M45PE20-VMN6P","M45PE20-VMN6","AT45DB021E"]
["8Mb","3.3V","8pin DFN (6x5mm)","M45PE80-VMP6G","M45PE80-VMP6","AT45DB081E"]
["8Mb","3.3V","8pin DFN (6x5mm)","M45PE80-VMP6TG","M45PE80-VMP6","AT45DB081E"]
["16Mb","3.3V","8pin SOIC (208mils)","M45PE16-VMW6TG","M45PE16-VMW6","AT45DB161E"]
["4Mb","3.3V","8pin SOIC (150mils)","AS25F304MD-10S1IN","M25P40-AVMN6","AT25SF041","S25FL040","W25Q40","MX25L40\nMX25V40","IS25LP040\nIS25LQ040","GD25Q40\nGD25B40\nGD25D40"]
["16Mb","3.3V","8pin SOIC (150mils)","AS25F316MQ-10S1IN","M25P16-AVMN6\nM25PX16","AT25SF161\nAT25FF161","S25FL016","W25Q16","MX25L16\nMX25V16","IS25LP016\nIS25LQ016","GD25Q16\nGD25B16"]
["32Mb","3.3V","8pin DFN (4x3mm)","N25Q032A13EF440F","N25Q032A13EF4","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3.3V","8pin DFN (4x3mm)","N25Q032A13EF4A0F","N25Q032A13EF4","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3.3V","8pin DFN (6x5mm)","N25Q032A13EF640F","N25Q032A13EF6","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3.3V","8pin SOIC (150mils)","N25Q032A13ESC40G","N25Q032A13ESC","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3.3V","8pin SOIC (150mils)","N25Q032A13ESCA0F","N25Q032A13ESC","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3.3V","16pin SOIC (300mils)","N25Q032A13ESFA0F","N25Q032A13ESF","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["64Mb","1.8V","8pin SOIC (208mils)","N25Q064A11ESEA0F","N25Q064A11ESE","AT25SL64/AT25QL64",null,"W25Q64","MX25U64","IS25WP064","GD25LQ64"]
["64Mb","3.3V","8pin DFN (6x5mm)","N25Q064A13EF640E","N25Q064A13EF6","AT25SF64/AT25QF64","S25FL064A/P","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","8pin DFN (8x6mm)","N25Q064A13EF8A0E","N25Q064A13EF8","AT25SF64/AT25QF64","S25FL064A/P","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","8pin DFN (8x6mm)","N25Q064A13EF8A0F","N25Q064A13EF8","AT25SF64/AT25QF64","S25FL064A/P","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","8pin DFN (8x6mm)","N25Q064A13EF8H0E","N25Q064A13EF8","AT25SF64/AT25QF64","S25FL064A/P","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","16pin SOIC (300mils)","N25Q064A13ESFA0F","N25Q064A13ESF","AT25SF64/AT25QF64","S25FL064A/P","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","8pin SOIC (208mils)","AS25F364MQ-10SIN","N25Q064A13ESE","AT25QF64","S25FL064","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","8L WSON (6x5mm)","AS25F364MQ-10WIN","N25Q064A13EF6","AT25QF64","S25FL064","W25Q64","MX25L64","IS25L064","GD25Q64"]
["128Mb","1.8V","8pin SOIC (208mils)","AS25F1128MQ-70SIN","MT25QU128ABA1ESE","AT25SL128A-SUE","S25FS128SDSMFI","W25Q128JWSIM","MX25U12832FM2I","IS25WP128-JBLE","GD25LB128ESIG"]
["128Mb","1.8V","8L WSON (6x5mm)","AS25F1128MQ-70WIN","MT25QU128ABA1EW7","AT25SL128A-MHE","S25FS128SDSNFI","W25Q128JWPIM","MX25U12832FZNI","IS25WP128-JKLE","GD25LB128EWIG"]
["128Mb","3V","8pin SOP(208mils)","AS25F3128MQ-7SIN","MT25QL128ABA1ESE\nMT25QL128ABA8ESE","AT25QF128A-SHB","S25FL128LAGM","W25Q128JVSIQ","MX25L12833FM2I-10G\nMX25L12845GM2I-08G\nMX25L12873GM2I-08G","IS25LP128F-JBL","GD25B128ESIGR"]
["128Mb","3V","8L WSON (6x5mm)","AS25F3128MQ-6WINTR","MT25QL128ABA1EW7","AT25QF128A-MHB","S25FL128LAGN","W25Q128JVPIQ","MX25L12833FZNI-10G\nMX25L12845GZNI-08G\nMX25L12873GZNI-08G","IS25LP128F-JKL","GD25B128EWIGR"]
["256Mb","3V","16pin SOP (300mils)","AS25F3256MQ-7S2INTR","MT25QL256ABA8ESF","AT25SF2561C-SXUB\nAT25QF2561C-SXUB","S25FL256SAGM","W25Q256JVFIQ","MX25L25645GMI-08G\nMX25L25673GMI-10G","IS25LP256D-JML","GD25B256EFIGR"]
["256Mb","3V","8L WSON (6x8mm)","AS25F3256MQ-7W2INTR","MT25QL256ABA1EW9","AT25SF2561C-MWUB\nAT25QF2561C-MWUB","S25FL256SAGN","W25Q256JVEIQ","MX25L25645GZ2I-08G\nMX25L25645GZ4I-10G","IS25LP256D-JJL","GD25B256EYIGR"]
["512Mb","3V","16pin SOP (300mils)","AS25F3512MQ-7S2INTR","MT25QL512ABB8ESF",null,null,"W25Q512JVFIQ","MX25L51245GMI-08G\nMX25L51273GMI-08G","IS25LP512M-JML","GD25B512MFFIGR"]
["512Mb","3V","8L WSON (6x8mm)","AS25F3512MQ-7W2INTR","MT25QL512ABB1EW9",null,null,"W25Q512JVEIQ","MX25L51245GZ2I-08G\nMX25L51273GZ4I-08G","IS25LP512M-JLL","GD25B512MFYIGR"]
[]
["Serial NAND Flash Cross Reference"]
["DENSITY","SPEED (NS)","VCC","ALLIANCE","MICRON","TOSHIBA/KIOXIA","WINBOND","MACRONIX","GIGA DEVICES","ISSI"]
["1Gb","120Mhz","3V","AS5F31G04SND-08LIN","MT29F1G01ABAFDWB-IT","TC58CVG0S3HRAIJ","W25N01GV\nW25N01KV","MX35LF1GE4AB\nMX35LF1G24AD","GD5F1GQ4Ux\nGD5F1GQ5Ux\nGD5F1GM7Ux","IS37SML01G1-LLI\nIS37SML01G8A-JJLI"]
["2Gb","100Mhz","1.8V","AS5F12G04SND-10LIN","MT29F2G01ABBGDWB-IT:G","TC58CYG1S3HRAIJ","W25N02JW\nW25M02GW","MX35UF2G14AC\nMX35UF2G24AD\nMX35UF2GE4AC\nMX35UF2GE4AD","GD5F2GQ4Rx\nGD5F2GQ5Rx\nGD5F2GM7Rx","IS37SMW02G8A-JJLI"]
["2Gb","120Mhz","3V","AS5F32G04SNDA-08LIN AS5F32G04SNDB-08LIN","MT29F2G01ABAGDWB-IT","TC58CVG1S3HRAIJ","W25M02GV","MX35LF2G14AC\nMX35LF2GE4AD\nMX35LF2G24AD","GD5F2GQ4Ux\nGD5F2GQ5Ux\nGD5F2GM7Ux","IS37SML02G8A-JJLI"]
["4Gb","100Mhz","1.8V","AS5F14G04SND-10LIN","MT29F4G01ABBFDWB-IT","TC58CYG2S0HRAIJ","W25N04KW","MX35UF4G24AD\nMX35UF4GE4AD","GD5F4GQ6Rx\nGD5F4GM8Rx","IS37SMW04G8A-JJLI"]
["4Gb","120Mhz","3V","AS5F34G04SNDA-08LIN AS5F34G04SNDB-08LIN","MT29F4G01ABAFDWB","TC58CVG2S0HRAIJ","W25N04KV","MX35LF4G24AD\nMX35LF4GE4AD","GD5F4GQ6Ux\nGD5F4GM8Ux","IS37SML04G8A-JJLI"]
["8Gb","100Mhz","1.8V","AS5F18G04SND-10LIN AS5F18G04SNDB-10LIN",null,"TH58CYG3S0HRAIJ",null,null,null,"IS37SMW08G8A-JJLI"]
["8Gb","120Mhz","3V","AS5F38G04SND-08LIN AS5F38G04SNDA-08LIN",null,"TH58CVG3S0HRAIJ",null,null,null,"IS37SML08G8A-JJLI"]
[]
["eMMC Cross Reference"]
["DENSITY","Package Type","Temp Grade","ALLIANCE","MICRON","SAMSUNG","KINGSTON","KIOXIA","ISSI","SANDISK","SK HYNIX","MACRONIX","SKY-HIGH","GREENLIANT"]
["4GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC4G31MA-51BIN","MTFC4GACAJCN (EOL)\nMTFC4GLGDQ (EOL)\nMTFC4GLWDM (EOL)\nMTFC4GMWDM (EOL)","KLM4G1GXXX (EOL)","EMMC04GMK27\nEMMC04GM627\nEMMC04G-W627","THGBMNG5D1LBA","IS21ES04G-JCLI\nIS21ES04G-BCLI","X","H26M31001HPR","MX52LM04A11X","S40FC004C1B","GLS85VM1004"]
["5GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC5G31P3-51BIN","MTFC4GACAJCN (EOL)\nMTFC4GLGDQ (EOL)\nMTFC4GLWDM (EOL)\nMTFC4GMWDM (EOL)","KLM4G1GXXX (EOL)","EMMC04GMK27\nEMMC04GM627\nEMMC04G-W627","THGBMNG5D1LBA","IS21ES04G-JCLI\nIS21ES04G-BCLI","X","H26M31001HPR","MX52LM04A11X","S40FC004C1B","GLS85VM1004"]
["8GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","\nASFC8G31M-51BIN\nASFC8G31MA-51BIN\nASFC8G31MB-51BIN","MTFC8GACAENS (EOL)\nMTFC8GAKAJCN (EOL)\nMTFC8GAMALBH(EOL)\nMTFC8GAMALGT (EOL)\nMTFC8GLWDM (EOL)","KLM8G1GEUF\nKLM8G1GETF\nKLM8G1GESD (EOL)","EMMC08GML36","THGBMJG6C1LBA","IS21ES08GA-JCLI\nIS21ES08GA-BCLI","SDINBDG4-8G","H26M41208HPR","MX52LM08A11X","S40FC008C3B","GLS85VM1008C-M"]
["10GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC10G31P3-51BIN","MTFC8GACAENS (EOL)\nMTFC8GAKAJCN (EOL)\nMTFC8GAMALBH (EOL)\nMTFC8GAMALGT (EOL)\nMTFC8GLWDM (EOL)","KLM8G1GEUF\nKLM8G1GETF\nKLM8G1GESD (EOL)","EMMC08GML36","THGBMJG6C1LBA","IS21ES08GA-JCLI\nIS21ES08GA-BCLI","SDINBDG4-8G","H26M41208HPR","MX52LM08A11X","S40FC008C3B","GLS85VM1008E-S"]
["16GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC16G31TA-51BCN","MTFC16GAKAECN (EOL)\nMTFC16GAKAEJP (EOL)\nMTFC16GAPALBH (EOL)","KLMAG1JETD\nKLMAG2GEUF\nKLMAG2GESD (EOL)","EMMC16G-TB29\nEMMC16G-IB29","THGBMUG7C1LBA\nTHGAMVG7T13BA","IS21TF16G-JCLI\nIS21TF16G-BCLI","SDINBDA6-16G","H26M51002KPR","X","S40FC016C3B","GLS85VM1016C-M"]
["32GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC32G31T3-51BIN","MTFC32GAKAECN (EOL)\nMTFC32GAKAEJP (EOL)\nMTFC32GAZAQHD(EOL)\nMTFC32GAPALBH (EOL)","KLMBG2JETD\nKLMBG4GESD (EOL)","EMMC32G-TX29\nEMMC32G-IX29","THGBMUG8C2LBA\nTHGAMVG8T13BA\nTHGBMJG88C4LBA","IS21TF32G-JCLI\nIS21TF32G-BCLI","SDINBDA6-32G\nSDINBDG4-32G","H26M62002JPR\nH26M64208EM","X","X","GLS85VM1032C-M"]
["64GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC64G31T5-51BIN","MTFC64GAZAQHD (EOL)\nMTFC64GAPALBH (EOL)","KLMCG2KCTA\nKLMCG2UCTA\nKLMCG4JEUD\nKLMCG2UCTB (EOL)\nKLMCG8GESD (EOL)","EMMC64G-TY29\nEMMC64G-IY29","THGAMVG9T23BA\nTHGBMJG9C8LBA","IS21TF64G-JCLI\nIS21TF64G-BCLI","SDINBDA6-64G\nSDINBDG4-64G","H26M74002HMR\nH26M78208CMR","X","X","GLS85VM1064C-M-I"]
["128GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC128G32T5-51BIN","MTFC128GAPALNS(EOL)\nMTFC128GAZAQJP(EOL)","KLMDG4UCTA\nKLMDG8JEUD\nKLMDG4UCTB(EOL)","EMMC128-TY29\nEMMC128-IY29","THGAMVT0T43BA","IS21TF128G-JCLI\nIS21TF128G-BCLI","SDINBDA6-128G","X","X","X","X"]

{"sheet":"SDRAM","index":2,"n_rows":27,"n_cols":7,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
[]
["Synchronous DRAM 3.3V  x8,  x16  and  x32"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY (MHz)","TEMPERATURE","ALLIANCE"]
["16Mb","1M x 16","3.3V","50pin TSOP II","143/166 MHz","Commercial, Industrial","AS4C1M16S-6/7 TxN"]
["64Mb","4M x 16","3.3V","54-pin TSOP II / 54-ball TFBGA / 60-ball FBGA","143/166/200 MHz","Commercial, Industrial, Automotive","AS4C4M16SA-5/6/7 TxN"]
["64Mb","4M x 16","3.3V","54pin TSOP II","166 MHz","Industrial","AS4C4M16SB-6TIN"]
["64Mb","4M x 16","3.3V","54-ball FBGA / 60-ball FBGA","143/166 MHz","Commercial, Industrial, Automotive","AS4C4M16SA-6/7 BxN, B2xN"]
["64Mb","2M x 32","3.3V","90-ball TFBGA","143/166 MHz","Commercial, Industrial","AS4C2M32S-6/7 BxN"]
["64Mb","2M x 32","3.3V","86pin TSOP II","143/166 MHz","Commercial, Industrial","AS4C2M32SA-6/7 TxN"]
["128Mb","8M x 16","3.3V","54pin TSOP II/54-ball FBGA","143/166 MHz","Commercial, Industrial, Automotive","AS4C8M16SA-6/7 TxN/BxN"]
["128Mb","8M x 16","3.3V","54pin TSOP II","166 MHz","Inudstrial","AS4C8M16SB-6TIN"]
["128Mb","4M x 32","3.3V","90-ball TFBGA","143/166 MHz","Commercial, Industrial","AS4C4M32S-6/7 BxN"]
["128Mb","4M x 32","3.3V","86pin TSOP II","143/166 MHz","Commercial, Industrial","AS4C4M32SA-6/7 TxN"]
["256Mb","16M x 16","3.3V","54pin TSOP II/54-ball FBGA","143/166 MHz","Commercial, Industrial","AS4C16M16SA-6/7 TxN/BxN"]
["256Mb","16M x 16","3.3V","54pin TSOP II/54-ball FBGA","143/166 MHz","Commercial, Industrial","AS4C16M16SB-6/7 TxN/BxN"]
["256Mb","8M x 32","3.3V","86pin TSOP II","143/166 MHz","Commercial, Industrial","AS4C8M32S-6/7 TxN"]
["256Mb","8M x 32","3.3V","90-ball TFBGA","143/166 MHz","Commercial, Industrial","AS4C8M32SA-6/7 BxN"]
["256Mb","32M x 8","3.3V","54pin TSOP II","143/166 MHz","Commercial, Industrial","AS4C32M8SA-6/7 TxN"]
["256Mb","64M x 4","3.3V","54pin TSOP II","143/166 MHz","Commercial, Industrial","AS4C64M4SA-6/7 TxN"]
["512Mb","32M x 16","3.3V","54-ball FBGA","143 MHz","Industrial","AS4C32M16SB-7BIN"]
["512Mb","32M x 16","3.3V","54pin TSOP II","143 MHz/166 MHz","Commercial, Industrial","AS4C32M16SB-6/7 TxN"]
["512Mb","32M x 16","3.3V","54pin TSOP II","143 MHz","Industrial","AS4C32M16SC-7TIN"]
["512Mb","16M x 32","3.3V","86pin TSOP II","143 MHz","Industrial","AS4C16M32SC-7TIN"]
["512Mb","16M x 32","3.3V","90ball TFBGA","166MHz","Commercial, Industrial","AS4C16M32SB-6BxN"]
["512Mb","64M x 8","3.3V","54pin TSOP II","143 MHz","Industrial","AS4C64M8SC-7TIN"]
["512Mb","64M x 8","3.3V","54pin TSOP II","133 MHz","Commercial","AS4C64M8SD-7TCN"]
["* X= TEMPERATURE GRADE; C = COMMERCIAL ; I = INDUSTRIAL; A = AUTOMOTIVE"]

{"sheet":"SDRAM Cross Reference","index":3,"n_rows":25,"n_cols":11,"rows_kept":25,"cut":false,"hidden":false,"merged":[[27,0,27,2],[30,0,30,2],[1,0,1,2]]}
[]
["Synchronous DRAM 3.3V Cross Reference"]
["DENSITY","ORG","ALLIANCE","SAMSUNG (EOL)","MICRON (EOL)","SK HYNIX (EOL)","ISSI","WINBOND","NANYA (EOL)","ELITE (ESMT)","ELPIDA (EOL)"]
["16Mb","1M x 16","AS4C1M16S-6/7TxN","K4S161622E","MT48LC1M16A1 (EOL)","HY57V161610","IS42S16100","W9816G6TH","NT56V1616AOT","M12L16161A-xTG2Q","EDS1616AGTA"]
["64Mb","4M x 16","AS4C4M16SA-5/6/7TxN\nAS4C4M16SB-6TIN","K4S641632N-UCxx","MT48LC4M16A2P (EOL)","HY57V641620","IS42S16400\nIS45S16400","W9864G6JH","NT56V6620C0T-xxB","M12L64164A-xTG2U","uPD4564163G5-Axx"]
["64Mb","4M x 16","AS4C4M16SA-6/7BxN",null,"MT48LCM16A2B4(EOL)","HY5V66D","IS42S16400\nIS45S16400","W9864G6JT",null,"M12L64154A-xBG2C"]
["64Mb","2M x 32","AS4C2M32S-6/7BxN",null,"MT48LC2M32B2B5 (EOL)","HY5V62","IS42S32200","W9864G2IB-x",null,null,"EDS6432AFBH"]
["64Mb","2M x 32","AS4C2M32SA-6/7TxN","K4S643232H-Ucxx","MT48LC2M32B2P-x (EOL)","HY57V643220","IS42S32200","W9864G2J(G,I)H-x",null,"M12L64322A-xTG2U","EDS6432AFTA"]
["128Mb","8M x 16","AS4C8M16SA-6/7TxN\nAS4C8M16SB-6TIN","K4S281632K-UCxx","MT48LC8M16A2P(EOL)","HY57V281620","IS42S16800\nIS45S16800","W9812G6K(G,I)H","NT5SV8M16AT-xxB","M12L128168A-xTG2N","uPD45128163G5-Axx"]
["128Mb","8M x 16","AS4C8M16SA-6/7BxN","K4S281632D-RL75","MT48LC8M16A2B4 (EOL)","HY5V26","IS42S16800\nIS45S16800","W9812G6JB",null,"M12L128168A-xBG2N"]
["128Mb","4M x 32","AS4C4M32S-6/7BxN",null,"MT48LC4M32B2B5 (EOL)","HY5V22","IS42S32400","W9812G21(G)B-x",null,"M12L128324-xBG2E","EDS1232AHBH"]
["128Mb","4M x 32","AS4C4M32SA-6/7TxN",null,"MT48LC4M32B2P-x (EOL)","HY57V283220T","IS42S32400","W9812G2GH",null,null,"EDS1232AHTA"]
["256Mb","16M x 16","AS4C16M16SA/B-6/7TxN","K4S561632N-UCxx","MT48LC16M16A2P (EOL)","H57V2562GTR","IS42S16160\nIS45S16160","W9825G6K(D,E,J)H","NT5SV16M16AT-xxB","M12L2561616A-xTG2A","EDS2516AP(AF,AC)TA-xx"]
["256Mb","16M x 16","AS4C16M16SA/B-6/7BxN","K4S561632D-RL75","MT48LC16M16A2B4 (EOL)","HY5V56","IS42S16160\nIS45S16160","W9825G6JB",null,"M12L2561616A-xBG2A","EDS2516EE(JE)BH"]
["256Mb","8M x 32","AS4C8M32S-6/7TxN",null,"MT48LC8M32B2B5-x (EOL)","HY5V52","IS42S32800","W9825G2J(D)B-x",null,null,"EDS2532EEBH"]
["256Mb","8M x 32","AS4C8M32SA-6/7BxN",null,"MT48LC8M32B2B5-x (EOL)","HY5V52","IS42S32800","W9825G2J(D)B-x",null,null,"EDS2532EEBH"]
["256Mb","32M X 8","AS4C32M8SA-6/7TxN",null,"MT48LC32M8A2P (EOL)",null,"IS42S83200J"]
["256Mb","64M x 4","AS4C64M4SA-6/7TxN",null,"MT48LC64M4A2P (EOL)",null,"IS42S32800"]
["512Mb","32M x 16","AS4C32M16SB-7BIN",null,null,null,"IS42S16320",null,null,"M12L5121632A"]
["512Mb","32M x 16","AS4C32M16SB-6/7TxN","K4S511632M-TC75","MT48LC32M16A2 (EOL)",null,"IS42S16320",null,null,"M12L5121632A","EDS5116ABTA"]
["512Mb","32M x 16","AS4C32M16SC-7TIN","K4S511632M-TC75","MT48LC32M16A2 (EOL)",null,"IS42S16320",null,null,"M12L5121632A","EDS5116ABTA"]
["512Mb","16M x 32","AS4C16M32SB-6BxN",null,"MT48LC16M32S2 (EOL)",null,"IS42S32160"]
["512Mb","16M x 32","AS4C16M32SC-7TIN",null,null,null,"IS42S32160"]
["512Mb","64M x 8","AS4C64M8SC-7TIN",null,"MT48LC64M8A2P-75:C (EOL)",null,"IS42S86400"]
["512Mb","64M x 8","AS4C64M8SD-7TCN",null,"MT48LC64M8A2P-75:C (EOL)",null,"IS42S86400"]

{"sheet":"DDR1  SDRAM","index":4,"n_rows":17,"n_cols":8,"rows_kept":17,"cut":false,"hidden":false,"merged":[[11,0,12,0],[11,1,12,1],[11,2,12,2]]}
[]
["DDR1 2.5V SDRAM"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY (MHz)","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE"]
["64Mb","4M x 16","2.5V","66pin TSOP II","200 MHz","400 Mbps","Commercial, Industrial, Automotive","AS4C4M16D1A-5TxN"]
["64Mb","2M x 32","2.5V","144-ball FBGA","200 MHz","400 Mbps","Commercial, Industrial","AS4C2M32D1A-5BxN"]
["128Mb","8M x 16","2.5V","66pin TSOP II","200 MHz","400 Mbps","Commercial, Industrial","AS4C8M16D1A-5TxN"]
["128Mb","8M x 16","2.5V","60-ball FBGA","200 MHz","400 Mbps","Commercial, Industrial","AS4C8M16D1-5BxN"]
["128Mb","4M x 32","2.5V","144-ball FBGA","200 MHz","400 Mbps","Commercial, Industrial","AS4C4M32D1A-5BxN"]
["256Mb","16M x 16","2.5V","60-ball FBGA","200 MHz","400 Mbps","Commercial, Industrial, Automotive","AS4C16M16D1-5BxN"]
["256Mb","16M x 16","2.5V","66pin TSOP II","200 MHz","400 Mbps","Commercial, Industrial","AS4C16M16D1A-5TxN"]
["512Mb","32M x 16","2.5V","66pin TSOP II","200 MHz","400 Mbps","Commercial, Industrial, Automotive","AS4C32M16D1A-5TxN"]
["512Mb","32M x 16","2.5V","60-ball FBGA","200 MHz","400 Mbps","Commercial, Industrial, Automotive","AS4C32M16D1-5BxN"]
[null,null,null,"66pin TSOP II","200 MHz","400 Mbps","Commercial, Industrial","AS4C32M16D1-5TxN"]
["512Mb","64M x 8","2.5V","66pin TSOP II\n60-ball FBGA","200 MHz","400 Mbps","Commercial, Industrial","AS4C64M8D1-5TxN\nAS4C64M8D1-5BxN"]
["1Gb","64M x 16","2.5V","66pin TSOP II","166 MHz","333Mbps","Commercial, Industrial","AS4C64M16D1-6TxN"]
["1Gb","64M x 16","2.5V","60-ball FBGA","166 MHz","333Mbps","Industrial","AS4C64M16D1A-6BIN"]
["* X= TEMPERATURE GRADE; C = COMMERCIAL ; I = INDUSTRIAL; A = AUTOMOTIVE"]

{"sheet":"DDR1 SDRAM Cross Reference","index":5,"n_rows":17,"n_cols":10,"rows_kept":17,"cut":false,"hidden":false,"merged":[[1,0,1,2]]}
[]
["DDR1       2.5V SDRAM Cross Reference"]
["DENSITY","ALLIANCE","SAMSUNG (EOL)","MICRON (EOL)","ISSI","HYNIX - ALL EOL","WINBOND","NANYA","ELITE (ESMT)","ELPIDA"]
["64Mb","AS4C4M16D1A-5TxN","K4H641638N","MT46V4M16TG (EOL)","IS43R16400B",null,"W9464G6K(I,J)H",null,"M13S64164A-5TG2Y","(EOL)"]
["64Mb","AS4C2M32D1A-5BxN"]
["128Mb","AS4C8M16D1-5BXN","K4H281638D",null,"IS43R16800E-5BL",null,"W9412G6JB",null,"M13S128168A-5BG2N","EDD1216A"]
["128Mb","AS4C8M16D1A-5TxN","K4H281638D","MT46V8M16 (EOL)","IS43R16800E-5TL","HY5DU1281622","W9412G6K(I,J)H",null,"M13S128168A-5TG2N","EDD1216A"]
["128Mb","AS4C4M32D1A-5BxN",null,"MT46V4M32FK (EOL)","IS43R32400E-5BL",null,"W9412GIB",null,"M13S128324A-5BG2M","EDD1232A"]
["256Mb","AS4C32M8D1-5TxN","K4H560838N","MT46V32M8P (EOL)","IS43R83200","HY5DU56822",null,"NT5DS32M8ES",null,"EDD2508A"]
["256Mb","AS4C16M16D1-5BxN","K4H561638D","MT46V16M16CY(EOL)","IS43R16160\nIS46R16160","HY5DU561622","W9425G6JB",null,"M13S2561616A-xBG2A"]
["256Mb","AS4C16M16D1A-5TxN","KH561638D","MT46V16M16P (EOL)","IS43R16160","HY5DU561622","W945G6K(D,E,J)H",null,"M13S2561616A-xTG2A","EDD2516A"]
["512Mb","AS4C32M16D1-5BxN","K4H511638J","MT46V32M16CY(EOL)","IS43R16320\nIS46R16320","HY5DU121622",null,null,null,"EDD5116"]
["512Mb","AS4C32M16D1A-5TxN","K4H511638J","MT46V32M16P(EOL)","IS43R16320\nIS46R16320","HY5DU121622",null,"NT5DS32M16ES","M13S5121632A-5TG2S","EDD5116A"]
["512Mb","AS4C64M8D1-5TxN","K4H510838J","MT46V64M8P (EOL)","IS43R86400","HY5DU12822",null,"NT5DS64M8ES",null,"EDD5108A"]
["512Mb","AS4C64M8D1-5BxN","K4H510838J","MT46V64M8CY(EOL)","IS43R86400","HY5DU12822"]
["1Gb","AS4C64M16D1-6TxN",null,"MT46V64M16P (EOL)"]
["1Gb","AS4C64M16D1A-6BIN"]

{"sheet":"DDR2 SDRAM","index":6,"n_rows":13,"n_cols":8,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
[]
["DDR2   1.8V SDRAM"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY (MHz)","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE"]
["256Mb","16M x 16","1.8V","84-ball FBGA","400 MHz","800 Mbps","Commercial, Industrial","AS4C16M16D2-25BxN"]
["512Mb","32M x 16","1.8V","84-ball FBGA","400 MHz","800Mbps","Commercial, Industrial, Automotive","AS4C32M16D2A/C-25BxN"]
["512Mb","64M x 8","1.8V","60-ball FBGA","400 MHz","800 Mbps","Commercial, Industrial, Automotive","AS4C64M8D2-25BxN"]
["1Gb","64M x 16","1.8V","84-ball FBGA","400 MHz","800Mbps","Commercial, Industrial, Automotive","AS4C64M16D2A-25BxN"]
["1Gb","64M x 16","1.8V","84-ball FBGA","400 MHz","800 Mbps","Commercial","AS4C64M16D2B-25BCN"]
["1Gb","128M x 8","1.8V","60-ball FBGA","400 MHz","800Mbps","Commercial, Industrial","AS4C128M8D2A-25BxN"]
["2Gb","128M x 16","1.8V","84-ball FBGA","400 MHz","800 Mbps","Commercial, Industrial","AS4C128M16D2-25BxN"]
["2Gb","128M x 16","1.8V","84-ball FBGA","400 MHz","800Mbps","Commercial, Industrial","AS4C128M16D2A-25BxN"]
[]
["* X= TEMPERATURE GRADE; C = COMMERCIAL ; I = INDUSTRIAL; A = AUTOMOTIVE"]

{"sheet":"DDR2 SDRAM Cross Reference","index":7,"n_rows":11,"n_cols":9,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
[]
["DDR2    1.8V SDRAM Cross Reference"]
["DENSITY","ALLIANCE","SAMSUNG (EOL)","MICRON","ISSI","WINBOND","NANYA","ELITE (ESMT)","HYNIX (EOL)"]
["256Mb","AS4C16M16D2-25BxN","K4T56163Q","MT47H16M16BG","IS43DR16160","W9725G6K(J)B","NT5TU16M16BG","M14D2561616A-2.5BG","HY5PS561621"]
["512Mb","AS4C32M16D2A/C-25BxN","K4T51163Q","MT47H32M16HR(NF)-25E","IS43DR16320\nIS46DR16320","W9751G6K(J)B","NT5TU32M16GG","M14D5121632A-2.5BG","HY5PS121621"]
["512Mb","AS4C64M8D2-25BxN","K4T51083Q","MT47H64M8CF(SH)-25E","IS43DR86400\nIS46DR86400","W9751G8K(J)B","NT5TU64M8EE",null,"H5PS5182KFR"]
["1Gb","AS4C64M16D2A-25BxN","K4T1G164Q","MT47H64M16HR(NF)-25E","IS43DR16640\nIS46DR16640","W971GG6JB","NT5TU64M16HG","M14D1G1664A-2.5BG","H5PS1G63"]
["1Gb","AS4C64M16D2B-25BCN","K4T1G164Q","MT47H64M16HR(NF)-25E","IS43DR16640","W971GG6JB","NT5TU64M16HG","M14D1G1664A-2.5BG","H5PS1G63"]
["1Gb","AS4C128M8D2A-25BxN","K4T1G084Q","MT47H128M8SH-25E","IS43DR81280","W971GG8JB","NT5TU128M8HE","M14D1G8128A","H5PS1G83"]
["2Gb","AS4C128M16D2-25BxN",null,"MT47H128M16RT-25E (EOL)","IS43DR16128","W972GG6JB"]
["2Gb","AS4C128M16D2A-25BxN",null,"MT47H128M16RT-25E (EOL)","IS43DR16128\nIS46DR16128","W972GG6JB"]

{"sheet":"DDR3 SDRAM ","index":8,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[[3,3,4,3],[1,0,1,1],[12,0,12,1],[3,0,4,0],[3,1,4,1],[3,2,4,2]]}
[]
["DDR3 1.5V SDRAM"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY (MHz)","DATA RATE","TEMPERATURE  OPTIONS","ALLIANCE"]
["512Mb","32M x 16","1.5V","96-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial","AS4C32M16D3-12BxN"]
[null,null,null,null,"933 MHz","1866 Mbps","Commercial","AS4C32M16D3-10BCN"]
["512Mb","64M x 8","1.5V","78-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial","AS4C64M8D3-12BxN"]
["1Gb","64M x 16","1.5V","96-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial, Automotive","AS4C64M16D3B-12BxN"]
["1Gb","64M x 16","1.5V","96-ball FBGA","800 MHz","1600 Mbps","Commercial","AS4C64M16D3W-12BCN"]
["1Gb","128M x 8","1.5V","78-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial, Automotive","AS4C128M8D3B-12BxN"]
["2Gb","128M x 16","1.5V","96-ball FBGA","1066 MHz","2133 Mbps","Commercial, Industrial","AS4C128M16D3C-93BxN"]
["4Gb","256M x 16","1.5V","96-ball FBGA","800 MHz\n933 MHz\n1066 MHz","1600 Mbps\n1866 Mbps\n2133 Mbps","Commercial, Industrial","AS4C256M16D3C-12BxN \nAS4C256M16D3C-10BxN\nAS4C256M16D3C-93BxN"]
["* X= TEMPERATURE GRADE; C = COMMERCIAL ; I = INDUSTRIAL; A = AUTOMOTIVE"]
["DDR3L 1.35V SDRAM"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY (MHz)","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE"]
["512Mb","32M x 16","1.35V","96-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial","AS4C32M16D3L-12BxN"]
["512Mb","64M x 8","1.35V","78-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial","AS4C64M8D3L-12BxN"]
["1Gb","64M x 16","1.35V","96-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial, Automotive","AS4C64M16D3LB-12BxN\nAS4C64M16D3LC-12BxN"]
["1Gb","64M x 16","1.35V","96-ball FBGA","933 MHz","1866 Mbps","Commercial","AS4C64M16D3LW-10BCN"]
["1Gb","128M x 8","1.35V","78-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial, Automotive","AS4C128M8D3LB-12BxN\nAS4C128M8D3LC-12BxN"]
["2Gb","128M x 16","1.35V","96-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial, Automotive","AS4C128M16D3LC-12BxN"]
["2Gb","256M x 8","1.35V","78-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial, Automotive","AS4C256M8D3LC-12BxN"]
["4Gb","256M x 16","1.35V","96-ball FBGA","800 MHz\n933 MHz","1600 Mbps\n1866 Mbps","Commercial, Industrial, Automotive","AS4C256M16D3LC-12BxN AS4C256M16D3LC-10BxN"]
["4Gb","256M x 16","1.35V","96-ball FBGA","933MHz","1866 Mbps","Commercial, Industrial, Automotive","AS4C256M16D3LD-10BxN"]
["4Gb","512M x 8","1.35V","78-ball FBGA","800 MHz\n933 MHz","1600 Mbps\n1866 Mbps","Commercial, Industrial, Automotive","AS4C512M8D3LC-12BxN AS4C512M8D3LC-10BAN"]
["8Gb","512M x 16","1.35V","96-ball FBGA","933 MHz","1866 Mbps","Commercial, Industrial, Automotive","AS4C512M16D3LA-10BxN"]
["8Gb","512M x 16","1.35V","96-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial","AS4C512M16D3LB-12BxN"]
["8Gb","512M x 16","1.35V","96-ball FBGA","800 MHz\n933 MHz","1600 Mbps\n1866 Mbps","Commercial, Industrial","AS4C512M16D3LC-10BxN\nAS4C512M16D3LC-12BxN"]
["8Gb","1G x 8","1.35V","78-ball FBGA","933 MHz","1866 Mbps","Commercial, Industrial, Automotive","AS4C1G8D3LA-10BxN"]
["* X= TEMPERATURE GRADE; C = COMMERCIAL ; I = INDUSTRIAL; A = AUTOMOTIVE"]

{"sheet":"DDR3 SDRAM Cross Reference","index":9,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[[4,5,4,6]]}
[]
["DDR3 SDRAM Cross Reference"]
["DENSITY","ALLIANCE","MICRON","SAMSUNG(EOL)","ISSI","HYNIX","WINBOND","ELITE (ESMT)","ELPIDA","NANYA"]
["512Mb","AS4C32M16D3-12BxN\nAS4C32M16D3-10BCN",null,null,null,null,"W6351G6KB-x","M15T5121632A","EDJ5316BASE"]
["512Mb","AS4C64M8D3-12BxN",null,null,null,null,null,null,"EDJ5308BASE"]
["512Mb","AS4C32M16D3L-12BxN",null,null,null,null,null,"M15T5121632A","EDJ5316BASE"]
["512Mb","AS4C64M8D3L-12BxN",null,null,null,null,null,null,"EDJ5308BASE"]
["1Gb","AS4C64M16D3B-12BxN AS4C64M16D3W-12BCN","MT41J64M16JT(TW)-125 (EOL)","K4B1G1646E(G)","IS43TR16640\nIS46TR16640","H5TQ1G63D","W631GG6KB-x","M15F1G1664A","EDJ1116DJ(BA) BG","NT5CB64M16F(G)P"]
["1Gb","AS4C64M16D3LB/C-12BxN AS4C64M16D3LW-10BCN","MT41K64M16JT-125 (EOL)\nMT41K64M16TW-125 ","K4B1G1646E(G)","IS43TR16640xL\nIS46TR16640xL","H5TC1G63EFR (EOL)","W631GU6KB-x","M15T1G1664A-(2C)","EDJ1116EJBG","NT5CC64M16F(G)P-DI"]
["1Gb","AS4C64M16D3LW-10BCN","MT41K64M16JT-125 (EOL)\nMT41K64M16TW-125\nMT41K64M16TW-107 ","K4B1G1646E(G)","IS43TR16640xL\nIS46TR16640xL","H5TC1G63EFR (EOL)","W631GU6KB-x","M15T1G1664A-(2C)","EDJ1116EJBG","NT5CC64M16F(G)P-DI"]
["1Gb","AS4C128M8D3B-12BxN","MT41J128M8JP(DA)-125","K4B1G0846E(F,G)","IS43TR81280\nIS46TR81280","H5TQ1G83","W631GG8KB-x","M15T1G8128A","EDJ1108DJ(BA) BG","NT5CB128M8F(G)N-DI"]
["1Gb","AS4C128M8D3LB/C-12BxN","MT41K128M8JP(DA)-125","K4B1G0846G-BY","IS43TR81280xL\nIS46TR81280xL","H5TC1G83EFR (EOL)","W631GU8KB-x","M15T1G8128A","EDJ1108EJBG","NT5CC128M8F(G)N-DI"]
["2Gb","AS4C128M16D3C-93BxN","MT41J128M16JT(TW)-125","K4B2G1646E-B","IS43TR16128","H5TQ2G63","W632GG6KB-x","M15F2G16128A","EDJ2116DEBG","NT5CB128M16I(F)P-DI"]
["2Gb","AS4C128M16D3LC-12BxN","MT41K128M16JT-125","K4B2G1646Q-B","IS43TR16128xL\nIS46TR16128xL","H5TC2G63","W632GU6KB-x","M15F2G16128A","EDJ2116EEBG","NT5CC128M16I(F)P-DI"]
["2Gb","AS4C256M8D3LC-12BxN","MT41K256M8DA-125","K4B2G0846Q-BCK","IS43TR82560xL\nIS46TR82560xL","H5TQ2G83FFR-x","W632GG8KB-x","M15T2G8256A","EDJ2108DEBG","NT5CB256M8IN-FL"]
["4Gb","AS4C256M16D3C-93BCN AS4C256M16D3C-10BxN AS4C256M16D3C-12BxN","MT41J256M16HA-107 MT41J256M16HA-125","K4B4G1646B(D)","IS43TR16256","H5TQ4G63","W634GG6MB/ NB","M15F4G16256A","EDJ4216BFBG (BASE)","NT5CB256M16C(D,E) P-DI"]
["4Gb","AS4C256M16D3LC-10BxN AS4C256M16D3LC-12BxN AS4C256M16D3LD-10BxN","MT41K256M16HA-107/125 MT41K256M16TW-107/125","K4B4G1646E(Q)","IS43TR16256xL\nIS46TR16256xL","H5TC4G63","W634GU6MB/NB","M15T4G16256A","EDJ4216EFBG","NT5CC256M16C(D,E) P-DI"]
["4Gb","AS4C512M8D3LC-10BAN\nAS4C512M8D3LC-12BxN","MT41K512M8DA-125","K4B4G0846B(C,D)","IS43TR85120xL\nIS46TR85120xL","H5TC4G83","W634GU8MB/NB","M15T4G8512A","EDJ4208EFBG","NT5CC512M8C(D,E) N-DI"]
["8Gb","AS4C512M16D3LA-10BxN","MT41K512M16VRN-107 MT41K512M16VRP-107 MT41K512M16HA-125 (EOL)","K4B8G1646x","IS43TR16512","H5TC8G63CMR","W638GU6QB","M15T8G16512A–DE",null,"NT5CC512T16EH-DI/A/H\nNT5CC512T16EH-EK/A/H"]
["8Gb","AS4C512M16D3LB-12BxN","MT41K512M16HA-125 (EOL)","K4B8G1646x","IS43TR16512","H5TC8G63CMR","W638GU6QB","M15T8G16512A–BD",null,"NT5CC512T16EH-DI/A/H"]
["8Gb","AS4C512M16D3LC-10BxN\nAS4C512M16D3LC-12BxN ","MT41K512M16VRN-107 MT41K512M16VRP-107 MT41K512M16HA-125 (EOL)","K4B8G1646x","IS43TR16512","H5TC8G63CMR","W638GU6QB","M15T8G16512A–BD\nM15T8G16512A–DE",null,"NT5CC512T16EH-DI/A/H\nNT5CC512T16EH-EK/A/H"]
["8Gb","AS4C1G8D3LA-10BxN","MT41K1G8SN-107/125:E","K4B8G0846x","IS43TR81024","H5TC8G83BMR"]
["8Gb","MT41K512M16HA-125","MT41K512M16HA-125","K4B8G1646x","IS43TR16512","H5TC8G63CMR","W638GU6QB","M15T8G16512A–BD",null,"NT5CC512T16EH-DI/A/H"]

{"sheet":"DDR4 SDRAM","index":10,"n_rows":27,"n_cols":8,"rows_kept":27,"cut":false,"hidden":false,"merged":[[1,0,1,1]]}
[]
["DDR4 SDRAM"]
["DENSITY","ORG","VCC","PACKAGES","CLOCK FREQUENCY","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE PART#"]
["4Gb","256M x 16","1.2V","96-ball FBGA (7.5x13.5mm)","1333 MHz\n1200 MHz","2666 Mbps\n2400 Mbps","Commercial, Industrial","AS4C256M16D4-75BxN\nAS4C256M16D4-83BxN"]
["4Gb","512M x 8","1.2V","78-ball FBGA\n(7.5x10.6mm)","1333 MHz\n1200 MHz","2666 Mbps\n2400 Mbps","Commercial, Industrial","AS4C512M8D4-75BxN\nAS4C512M8D4-83BxN"]
["4Gb","256M x 16","1.2V","96-ball FBGA (7.5x13mm)","1600 MHz\n1333 MHz","3200 Mbps\n2666 Mbps","Commercial, Industrial","AS4C256M16D4A-62BxN\nAS4C256M16D4A-75BxN"]
["4Gb","512M x 8","1.2V","78-ball FBGA\n(7.5x11mm)","1333 MHz","2666 Mbps","Commercial, Industrial","AS4C512M8D4A-75BxN"]
["8Gb","512M x 16","1.2V","96-ball FBGA\n(7.5x13mm)","1600 MHz","3200 Mbps","Commercial, Industrial","AS4C512M16D4A-62BxN"]
["8Gb","1G x 8","1.2V","78-ball FBGA\n(7.5x12mm)","1600 MHz","3200 Mbps","Commercial, Industrial","AS4C1G8D4A-62BxN"]
["8Gb","512M x 16","1.2V","96-ball FBGA\n(7.5x13mm)","1600 MHz","3200 Mbps","Commercial","AS4C512M16D4B-62BCN"]
["8Gb","1G x 8","1.2V","78-ball FBGA\n(7.5x11mm)","1600 MHz","3200 Mbps","Commercial","AS4C1G8D4B-62BCN"]
["8Gb","512M x 16","1.2V","96-ball FBGA\n(7.5 x 12mm)","1600 MHz","3200 Mbps","Commercial","AS4C512M16D4C-62BCN"]
["8Gb","512M x 16","1.2V","96-ball FBGA","1600 MHz","3200 Mbps","Commercial","AS4C512M16D4D-62BCN"]
["8Gb","1G x 8","1.2V","78-ball FBGA","1600 MHz","3200 Mbps","Commercial","AS4C1G8D4D-62BCN"]
["8Gb","512M x16","1.2V","96-ball FBGA \n(7.5 x 13mm)","1600 MHz","3200 Mbps","Commercial","MT40A512M16TD-062E:R"]
["8Gb","1G x 8","1.2V","78-ball FBGA\n(7.5x11mm)","1600 MHz","3200 Mbps","Commercial","MT40A1G8AG-062E:R"]
["16Gb","1G x 16","1.2V","96-ball FBGA\n(9x13mm)","1600 MHz","3200 Mbps","Commercial","MT40A1G16KH-062E:E"]
["16Gb","1G x 16","1.2V","96-ball FBGA\n(9x13mm)","1600 MHz","3200 Mbps","Commercial","MT40A1G16KD-062E:E"]
["16Gb","1G x 16","1.2V","96-ball FBGA\n(7.5x13mm)","1600 MHz","3200 Mbps","Commercial","MT40A1G16TD-062E:F"]
["16Gb","1G x 16","1.2V","96-ball FBGA\n(9x13mm)","1600 MHz","3200 Mbps","Commercial","AS4C1G16D4-062BCN"]
["16Gb","1G x 16","1.2V","96-ball FBGA\n(7.5x13mm)","1600 MHz","3200 Mbps","Commercial","AS4C1G16D4A-62BCN"]
["16Gb","2G x 8","1.2V","78-ball FBGA\n(7.5x11mm)","1600 MHz","3200 Mbps","Commercial","AS4C2G8D4A-62BCN"]
["16Gb","2G x 8","1.2V","78-ball FBGA\n(9x11mm)","1600 MHz","3200 Mbps","Commercial","MT40A2G8JC-062E:E"]
["16Gb","2G x 8","1.2V","78-ball FBGA\n(9x11mm)","1600 MHz","3200 Mbps","Commercial","MT40A2G8JE-062E:E"]
["16Gb","2G x 8","1.2V","78-ball FBGA\n(7.5x11mm)","1600 MHz","3200 Mbps","Commercial","MT40A2G8AG-062E:F"]
["32Gb","2G x 16","1.2V","96-ball FBGA\n(7.5x13mm)","1600 MHz","3200 Mbps","Commercial","AS4C2G16D4-62BCN"]
["32Gb","4G x 8","1.2V","78-ball FBGA\n(7.5x11mm)","1600 MHz","3200 Mbps","Commercial","AS4C4G8D4-62BCN"]

{"sheet":"DDR4 SDRAM Cross Reference","index":11,"n_rows":17,"n_cols":8,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
[]
["DDR4 SDRAM Cross Reference"]
["DENSITY","ORG","ALLIANCE","MICRON","NANYA","SAMSUNG","HYNIX","ISSI"]
["4Gb","256M x 16","AS4C256M16D4-83BxN\nAS4C256M16D4-75BxN","MT40A256M16GE","NT5AD256M16D4-HR/I/T\nNT5AD256M16E4-HR/I/T","K4A4G165WE-BxRC/PB/TD\nK4A4G165WF-BxTD","H5AN4G6NBJR-VKC\nH5AN4G6NBJR-VKI","IS43QR16256B-083RBL/I\nIS43QR16256B-075UBL/I"]
["4Gb","512M x 8","AS4C512M8D4-83BxN\nAS4C512M8D4-75BxN","MT40A512M8RH","NT5AD512M8D3-HR/I/T\nNT5AD512M8E3-HR/I/T","K4A4G085WE-BxRC/PB/TD\nK4A4G085WF-BxTD","H5AN4G8NBJR-VKC\nH5AN4G8NBJR-VKI","IS43QR85120B-083RBL/I\nIS43QR85120B-075UBL/I"]
["4Gb","256M x 16","AS4C256M16D4A-62BxN\nAS4C256M16D4A-75BxN","MT40A256M16GE","NT5AD256M16D4-HR/I/T\nNT5AD256M16E4-HR/I/T\nNT5AD256M16D4-JR/I/T\nNT5AD256M16E4-JR/I/T","K4A4G165WE-BxRC/PB/TD/WE\nK4A4G165WF-BxTD/WE\nK4A4G165WG-BxWE","H5AN4G6NBJR-VKC\nH5AN4G6NBJR-VKI","IS43QR16256B-083RBL/I\nIS43QR16256B-075UBL/I"]
["4Gb","512M x 8","AS4C512M8D4A-75BxN","MT40A512M8RH","NT5AD512M8D3-HR/I/T\nNT5AD512M8D3-JR/I/T\nNT5AD512M8E3-HR/I/T\nNT5AD512M8E3-JR/I/T","K4A4G085WE-BxRC/PB/TD\nK4A4G085WF-BxTD/WE\nK4A4G085WF-BxWE","H5AN4G8NBJR-VKC\nH5AN4G8NBJR-VKI","IS43QR85120B-083RBL/I\nIS43QR85120B-075UBL/I"]
["8Gb","512M x 16","AS4C512M16D4A-62BxN","MT40A512M16LY\nMT40A512M16JY\nMT40A512M16HA\nMT40A512M16TB","NT5AD512M16C4-HR/I/T\nNT5AD512M16C4-JR/I/T\nNT5AD512M16H4-HR/I/T\nNT5AD512M16H4-JR/I/T","K4A8G165WB-BxPB/RC/TD\nK4A8G165WC-BxTD/WE\nK4A8G165WG-BxWE","H5AN8G6NCJR-XNC/I\nH5AN8G6NCJR-WNC/I\nH5AN8G6NCJR-VNC\nH5AN8G6NDJR-WNC","IS43QR16512A-083TBL/I\nIS43QR16512A-075VBL/I"]
["8Gb","1G x 8","AS4C1G8D4A-62BxN","MT40A1G8SA\nMT40A1G8WE\nMT40A1G8PM","NT5AD1024M8C3-HR/I/T\nNT5AD1024M8C3-JR/I/T\nNT5AD1024M8H3-HR/I/T\nNT5AD1024M8H3-JR/I/T","K4A8G085WB-BxPB/RC/TD\nK4A8G085WC-BxPB/RC/TD/WE\nK4A8G085WG-BxWE","H5AN8G8NCJR-XNC\nH5AN8G8NDJR-XNC\nH5AN8G8NCJR-VKC/WNC/I\nH5AN8G8NDJR-VKC/WNC/I","IS43QR81024A-083TBL/I\nIS43QR81024A-075VBL/I"]
["8Gb","512M x 16","AS4C512M16D4B-62BCN AS4C512M16D4C-62BCN\nAS4C512M16D4D-62BCN","MT40A512M16LY\nMT40A512M16JY\nMT40A512M16HA\nMT40A512M16TB","NT5AD512M16C4-HR/JR\nNT5AD512M16H4-HR/JR","K4A8G165WB-BCPB/RC/TD\nK4A8G165WC-BCTD/WE\nK4A8G165WG-BCWE","H5AN8G6NCJR-XNC/VNC\nH5AN8G6NCJR-WNC\nH5AN8G6NDJR-WNC","IS43QR16512A-083TBL\nIS43QR16512A-075VBL"]
["8Gb","512M x 16","MT40A512M16TD-062E:R","MT40A512M16LY\nMT40A512M16JY\nMT40A512M16HA\nMT40A512M16TB","NT5AD512M16C4-HR/JR\nNT5AD512M16H4-HR/JR","K4A8G165WB-BCPB/RC/TD\nK4A8G165WC-BCTD/WE\nK4A8G165WG-BCWE","H5AN8G6NCJR-XNC/VNC\nH5AN8G6NCJR-WNC\nH5AN8G6NDJR-WNC","IS43QR16512A-083TBL\nIS43QR16512A-075VBL"]
["8Gb","1G x 8","AS4C1G8D4B-62BCN AS4C1G8D4D-62BCN\nMT40A1G8AG-062E","MT40A1G8SA\nMT40A1G8WE\nMT40A1G8PM","NT5AD1024M8C3-HR/JR\nNT5AD1024M8H3-HR/JR","K4A8G085WB-BCPB/RC/TD\nK4A8G085WC-BCPB/RC/TD/WE\nK4A8G085WG-BCWE","H5AN8G8NCJR-XNC\nH5AN8G8NDJR-XNC\nH5AN8G8NCJR-VKC/WNC\nH5AN8G8NDJR-VKC/WNC","IS43QR81024A-083TBL\nIS43QR81024A-075VBL"]
["16Gb","1G x 16","AS4C1G16D4-062BCN\nMT40A1G16KH-062E\nMT40A1G16KD-062E\nMT40A1G16TD-062E","MT40A1G16KH/KB/RC\nMT40A1G16TB/TD/TBB",null,"K4AAG165WA-BCWE\nK4AAG165WB-MCPB/RC/TD\nK4AAG165WC-BCWE","H5ANAG6NCMR-XNC\nH5ANAG6NCMR-WMC/VKC\nH5ANAG6NDMR-XNC\nH5ANAG6NDMR-WMC/VKC"]
["16Gb","1G x 16","AS4C1G16D4A-62BCN","MT40A1G16KH/KB\nMT40A1G16TB/TD\nMT40A1G16RC",null,"K4AAG165WA-BCWE\nK4AAG165WB-MCPB/RC/TD\nK4AAG165WC-BCWE","H5ANAG6NCMR-XNC\nH5ANAG6NCMR-WMC/VKC\nH5ANAG6NDMR-XNC\nH5ANAG6NDMR-WMC/VKC"]
["16Gb","2G x 8","AS4C2G8D4A-62BCN\nMT40A2G8JC-062E\nMT40A2G8JE-062E\nMT40A2G8AG-062E","MT40A2G8AG\nMT40A2G8SA/VA\nMT40A2G8JC/JE",null,"K4AAG085WA-BCWE/TD\nK4AAG085WB-BCWE\nK4AAG085WB-MCPB/RC\nK4AAG085WC-BCWE","H5ANAG8NCMR-XNC\nH5ANAG8NCMR-VKC/WMC\nH5ANAG8NDMR-XNC\nH5ANAG8NDMR-VKC/WMC","IS43QR8K02S2A-083TBL"]
["32Gb","2G x 16","AS4C2G16D4-62BCN","MT40A2G16TBB\nMT40A2G16SKL",null,"K4ABG165WA-MCTD\nK4ABG165WA-MCWE K4ABG165WB-MCWE","H5ANBG6NAMR-XNC\nH5ANBG6NAMR-WNC\nH5ANBG6NAMR-VKC"]
["32Gb","4G x 8","AS4C4G8D4-62BCN","MT40A4G8NEA\nMT40A4G8BAF",null,"K4ABG085WA-MCWE\nK4ABG085WA-MCTD ","H5ANBG8NABR-XNC\nH5ANBG8NABR-WNC\nH5ANBG8NABR-VKC"]

{"sheet":"Mobile LP DRAM-SDRAM","index":12,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
[]
["MOBILE LOW POWER SDRAM"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY","TEMPERATURE OPTIONS","ALLIANCE"]
["128Mb","8M x 16","1.7V ~ 1.95V","54-ball FBGA (8x8mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C8M16MSA-6BIN"]
["256Mb","16M x 16","1.7V ~ 1.95V","54-ball FBGA (8x8mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C16M16MSA-6BIN"]
["256Mb","8M x 32","1.7V ~ 1.95V","90-ball FBGA (8x13mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C8M32MSB-6BIN"]
["512Mb","32M x 16","1.7V ~ 1.95V","54-ball FBGA (8x8mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C32M16MSA-6BIN"]
["512Mb","16M x 32","1.7V ~ 1.95V","90-ball FBGA (8x13mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C16M32MSA-6BIN"]
["MOBILE LP DDR"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE"]
["256Mb","16M x 16","1.8V","60-ball FBGA (8x9mm)","166 MHz","333Mbps","Extended -30°C ~ +85°C","AS4C16M16MD1-6BCN"]
["512Mb","32M x 16","1.8V","60-ball FBGA (8x9mm)","200 MHz","400Mbps","Industrial -40°C ~ +85°C","AS4C32M16MD1B-5BIN"]
["512Mb","16M x 32","1.8V","90-ball FBGA (8x13mm)","200 MHz","400Mbps","Extended -25°C ~ +85°C\nIndustrial -40°C ~ +85°C ","AS4C16M32MD1B-5BIN"]
["2Gb","64M x 32","1.8V","90-ball FBGA (8x13mm)","200 MHz","400Mbps","Extended -25°C ~ +85°C\nIndustrial -40°C ~ +85°C   ","AS4C64M32MD1-5BxN"]
["2Gb","64M x 32","1.8V","90-ball FBGA (8x13mm)","200 MHz","400Mbps","Industrial  -40°C ~ +85°C","AS4C64M32MD1A-5BIN"]
["MOBILE LP DDR2"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY (MHz)","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE"]
["256Mb","8M x 32","1.2V/1.8V","134-ball FBGA","400 MHz","800Mbps","Extended -25°C ~ +85°C","AS4C8M32MD2A-25BCN"]
["256Mb","8M x 32","1.2V/1.8V","168-ball POP FBGA","400 MHz","800Mbps","Extended  -25°C ~ +85°C","AS4C8M32MD2A-25BPCN"]
["1Gb","64M x 16","1.2V/1.8V","134-ball FBGA","400 MHz","800Mbps","Industrial  -40°C ~ +85°C","AS4C64M16MD2A-25BIN"]
["1Gb","32M x 32","1.2V/1.8V","134-ball FBGA","400 MHz","800Mbps","Industrial  -40°C ~ +85°C","AS4C32M32MD2A-25BIN"]
["2Gb","128M x 16","1.2V/1.8V","134-ball FBGA","400MHz","800Mbps","Industrial  -40°C ~ +85°C","AS4C128M16MD2A-25BIN"]
["2Gb","64M x 32","1.2V/1.8V","134-ball FBGA","400 MHz","800Mbps","Industrial  -40°C ~ +85°C","AS4C64M32MD2A-25BIN"]
["4Gb","128M x 32","1.2V/1.8V","134-ball FBGA","533 MHz","1066Mbps","Industrial  -40°C ~ +85°C","AS4C128M32MD2A-18BIN"]
["4Gb","128M x 32","1.2V/1.8V","134-ball FBGA","400 MHz","800Mbps","Industrial  -40°C ~ +85°C","AS4C128M32MD2A-25BIN"]

{"sheet":"Mobile LP DRAM Cross Reference","index":13,"n_rows":26,"n_cols":9,"rows_kept":26,"cut":false,"hidden":false,"merged":[]}
[]
["MOBILE LOW POWER SDRAM Cross Reference"]
["DENSITY","ALLIANCE","MICRON","ISSI","NANYA","WINBOND"]
["128Mb","AS4C8M16MSA-6BIN","MT48H8M16LFB4 (EOL)","IS42VM16800H",null,"W987D6HBGX"]
["256Mb","AS4C16M16MSA-6BIN","MT48H16M16LFBF (EOL)","IS42VM16160K",null,"W988D6FBGX"]
["256Mb","AS4C8M32MSB-6BIN","MT48H8M32LFB5 (EOL)","IS42VM32800K",null,"W988D2FBJX"]
["512Mb","AS4C32M16MSA-6BIN","MT48H32M16LFB4-6 IT (EOL)","IS42VM16320E","NT6SM32M16BG-S1","W989D6DBGX"]
["512Mb","AS4C16M32MSA-6BIN","MT48H16M32LFB5-6 IT (EOL)","IS42VM32160E","NT6SM16M32BK-S1","W989D2DBJX"]
[]
["MOBILE LP DDR1 Cross Reference"]
["DENSITY","ALLIANCE","MICRON","SAMSUNG","ISSI","HYNIX","NANYA","ELITE (ESMT)","WINBOND"]
["256Mb","AS4C16M16MD1-6BCN","MT46H16M16LFBF-6 (EOL)","K4X56163SPN","IS43LR16160","HY5MS5B6/ H5MS2562","NT6DM16M16AD-T1","M53D2561616A-6BG2F","W948D6FBHX"]
["512Mb","AS4C32M16MD1B-5BIN","MT46H32M16LFBF-5","K4X51163PI","IS43R16320B","HY5MS7B6/ H5MS5162","NT6DM32M16A(B)D-T1","M53D5121632A-5BG2T","W949D6DBHX"]
["512Mb","AS4C16M32MD1B-5BIN","MT46H16M32LFB5-5","K4X51323PI","IS43LR32160B","H5MS5132/ H5MS5122","NT6DM16M32A(B)C-T1","M53D5123216A-5BG2S","W949D2DBJX"]
["2Gb","AS4C64M32MD1-5BxN","MT46H64M32LFKQ-5","K4X2G323PC","IS43LR32640A","H5M52G22"]
["2Gb","AS4C64M32MD1A-5BIN","MT46H64M32LFKQ-5","K4X2G323PC","IS43LR32640A","H5M52G22"]
[]
["MOBILE LP DDR2 Cross Reference"]
["DENSITY","ALLIANCE","MICRON","SAMSUNG","ISSI","HYNIX","NANYA","ELITE (ESMT)","WINBOND"]
["256Mb","AS4C8M32MD2A-25B(P)CN",null,null,"IS43LD32800A-25BLx\nIS43LD32800B-25BLx",null,null,null,"W978H2KBVX2E"]
["1Gb","AS4C64M16MD2A-25BIN","MT42L64M16D1HE-25",null,"IS43LD16640C/A",null,"NT6TL64M16BA(I)-G0",null,"W97AH6KBVX2"]
["1Gb","AS4C32M32MD2A-25BIN","MT42L32M32D1HE-25",null,"IS43LD32320C/A",null,"NT6TL32M32BI(A)-G0",null,"W97AH2KBVX2"]
["2Gb","AS4C128M16MD2A-25BIN","MT42L128M16D1TK-25",null,"IS43LD16128B",null,"NT6TL128M16CI(A)-G0",null,"W97BH6KBVX2"]
["2Gb","AS4C64M32MD2A-25BIN","MT42L64M32D1TK-25",null,"IS43LD32640B",null,"NT6TL64M32CI(A)-G0",null,"W97BH2KBVX2"]
["4Gb","AS4C128M32MD2A-18BIN","MT42L128M32D1GU-18",null,"IS43LD32128A",null,"NT6TL128M32BI(A)-G0"]
["4Gb","AS4C128M32MD2A-25BIN","MT42L128M32D1GU-18",null,"IS43LD32128A",null,"NT6TL128M32BI(A)-G0"]

{"sheet":"LPDDR4-LPDDR4X","index":14,"n_rows":28,"n_cols":9,"rows_kept":28,"cut":false,"hidden":false,"merged":[[27,0,27,8]]}
[]
["LPDDR4"]
["DENSITY","ORG","VDD1 / VDD2 / VDDQ","PACKAGES","CLOCK FREQUENCY","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE","REMARKS"]
["2Gb","128M x 16","1.8V / 1.1V / 1.1V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Automotive A2 (-40°C to 105°C)","AS4C128M16MD4-062BAN","With ECC"]
["2Gb","64M x 32","1.8V / 1.1V / 1.1V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Automotive A2 (-40°C to 105°C)","AS4C64M32MD4-062BAN","With ECC"]
["4Gb","128M x 32","1.8V / 1.1V / 1.1V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Automotive A2 (-40°C to 105°C)","AS4C128M32MD4-062BAN","With ECC"]
["4Gb","256M x 16","1.8V / 1.1V / 1.1V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Automotive A2 (-40°C to 105°C)","AS4C256M16MD4-062BAN","With ECC"]
["8Gb","256M x 32","1.8V / 1.1V / 1.1V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Automotive A2 (-40°C to 105°C)","AS4C256M32MD4-062BAN","With ECC"]
["4Gb","128M x 32","1.8V / 1.1V / 1.1V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Industrial (-40C to 85C)","AS4C128M32MD4A-062BIN","With ECC"]
["4Gb","256M x 16","1.8V / 1.1V / 1.1V","200b TFBGA\n(10x14.5mm)","2133 MHz","4266 Mbps","Industrial (-40C to 85C)","AS4C256M16MD4A-046BIN","Without ECC"]
["8Gb","256M x 32","1.8V / 1.1V / 1.1V","200b TFBGA\n(10x14.5mm)","2133 MHz","4266 Mbps","Industrial (-40C to 85C)","AS4C256M32MD4A-046BIN","Without ECC"]
["LPDDR4X"]
["DENSITY","ORG","VDD1 / VDD2 / VDDQ","PACKAGES","CLOCK FREQUENCY","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE","REMARKS"]
["2Gb","128M x 16","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Automotive A2 (-40°C to 105°C)","AS4C128M16MD4V-062BAN","With ECC"]
["4Gb","128M x 32","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Industrial (-40°C to 85°C)","AS4C128M32MD4VA-062BIN","With ECC"]
["4Gb","256M x 16","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Automotive A2 (-40°C to 105°C)","AS4C256M16MD4V-062BAN","With ECC"]
["4Gb","256M x 16","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x14.5mm)","2133 MHz","4266 Mbps","Industrial (-40°C to 85°C)","AS4C256M16MD4VA-046BIN","Without ECC"]
["8Gb","256M x 32","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Automotive A2 (-40°C to 105°C)","AS4C256M32MD4V-062BAN","With ECC"]
["8Gb","256M x 32","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x14.5mm)","2133 MHz","4266 Mbps","Industrial (-40°C to 85°C)","AS4C256M32MD4VA-046BIN","Without ECC"]
["8Gb","512M x 16","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x15mm)","1866 MHz","3733 Mbps","Industrial (-40°C to 95°C)","AS4C512M16MD4V-053BIN","without ECC"]
["8Gb","512M x 16","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x15mm)","2133 MHz","4266 Mbps","Industrial (-40°C to 85°C)","AS4C512M16MD4VA-046BIN","without ECC"]
["16Gb","1G x 16","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x15mm)","2133 MHz","4266 Mbps","Industrial (-40°C to 95°C)","AS4C1G16MD4V-046BIN","without ECC"]
["16Gb","1G x 16","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x15mm)","2133 MHz","4266 Mbps","Industrial (-40°C to 85°C)","AS4C1G16MD4VA-046BIN","without ECC"]
["16Gb","512M x 32","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x15mm)","1866 MHz","3733 Mbps","Industrial (-40°C to 95°C)","AS4C512M32MD4V-053BIN","without ECC"]
["16Gb","512M x 32","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x15mm)","2133 MHz","4266 Mbps","Industrial (-40°C to 95°C)","AS4C512M32MD4V-046BIN","without ECC"]
["16Gb","512M x 32","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x15mm)","2133 MHz","4266 Mbps","Industrial (-40°C to 95°C)","AS4C512M32MD4VA-046BIN*","without ECC"]
["32Gb","1Gb x 32","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x15mm)","2133 MHz","4266 Mbps","Industrial (-40°C to 95°C)","AS4C1G32MD4V-046BIN","without ECC"]
["* New Product coming soon"]

{"sheet":"LPDDR4-LPDDR4X cross Reference","index":15,"n_rows":19,"n_cols":10,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
[]
["LPDDR4 Cross Reference "]
["DENSITY","ORG","ALLIANCE","MICRON","SAMSUNG","HYNIX","NANYA","ISSI","WINBOND","IM"]
["2Gb","128M x 16","AS4C128M16MD4-062BAN","MT53E128M16D1DS",null,"H9HCNNNBKUMLXR/HR","NT6AN128M16AV","IS43/46LQ16128A\nIS43/46LQ16128EA","W66BL6NBU\nW66BP6NBU"]
["2Gb","64M x 32","AS4C64M32MD4-062BAN",null,null,null,null,"IS43/46LQ32640A\nIS43/46LQ32640EA","W66CL2NQU\nW66CP2NQU\nW66CP2NQQ"]
["4Gb","128M x 32","AS4C128M32MD4-062BAN\nAS4C128M32MD4A-062BIN","MT53B128M32D1DS\nMT53E128M32D2DS\nMT53E128M32D2FW","K4F4E3S4HF-GFCJ\nK4F4E3S4HF-GHCJ",null,"NT6AN128T32AV","IS43/46LQ32128A\nIS43/46LQ32128EA","W66CL2NQU\nW66CP2NQU","IME4G32L4HABG"]
["4Gb","256M x 16","AS4C256M16MD4-062BAN\nAS4C256M16MD4A-046BIN","MT53E256M16D1DS\nMT53E256M16D1FW",null,"H9HCNNN4KUMLHR","NT6AN256M16AV","IS43/46LQ16256A\nIS43/46LQ16256EA","W66CP6NBU\nW66CL6NBU"]
["8Gb","256M x 32","AS4C256M32MD4-062BAN\nAS4C256M32MD4A-046BIN","MT53B256M32D1DS\nMT53E256M32D2DS\nMT53E256M32D2FW","K4F8E304HB-MGCJ\nK4F8E3S4HB-MFCJ\nK4F8E3S4HB-MHCJ","H9HCNNN8KUMLHR","NT6AN256T32AV","IS43/46LQ32256A\nIS43/46LQ32256EA","W66DP2NQU\nW66DL2NQU","IME8G32L4HADG"]
["LPDDR4X Cross Reference "]
["DENSITY","ORG","ALLIANCE","MICRON","SAMSUNG","HYNIX","NANYA","ISSI","WINBOND","IM"]
["2Gb","128M x 16","AS4C128M16MD4V-062BAN",null,null,null,null,"IS43/46LQ16128AL\nIS43/46LQ16128EA","W66BQ6NBU"]
["4Gb","256M x 16","AS4C256M16MD4V-062BAN\nAS4C256M16MD4VA-046BIN","MT53E256M16D1DS\nMT53E256M16D1FW","K4U8E3S4AD-GFCL\nK4U8E3S4AD-GHC","H9HCNNN4KMMLHR","NT6AP256M16AV","IS43/46LQ16256AL\nIS43/46LQ16256EA","W66CQ6NQU","IM4G16L4JCBG"]
["4Gb","128M x 32","AS4C128M32MD4VA-062BIN","MT53B128M32D1DS\nMT53E128M32D2DS\nMT53E128M32D2FW","K4U4E3S4x",null,"NT6AP128T32AV","IS43/46LQ32128AL","W66CQ2NQU","IME4G32L4JCBG"]
["8Gb","256M x 32","AS4C256M32MD4V-062BAN\nAS4C256M32MD4VA-046BIN","MT53B256M32D1DS\nMT53E256M32D2DS\nMT53E256M32D2FW","K4U8E3S4Ax",null,"NT6AP256T32AV","IS43/46LQ32256AL\nIS43/46LQ32256EAL","W66DQ2NQU","IM8G32L4JCBG"]
["8Gb","512M x 16","AS4C512M16MD4V-053BIN\nAS4C512M16MD4VA-046BIN","MT53D512M16D1DS\nMT53E512M16D1FW",null,null,"NT6AP512M16AV","IS43LQ16512AL",null,"IM8G16L4JCBG-046"]
["16Gb","1G x 16","AS4C1G16MD4V-046BIN\nAS4C1G16MD4VA-046BIN","MT53E1G16D1ZW-046",null,null,"NT6AT1024M16AV",null,null,"IMAG16L4HBBG"]
["16Gb","512M x 32","AS4C512M32MD4V-053BIN","MT53D512M32D2Dx\nMT53D512M32D1ZW\nMT53D512M32D2FW","K4U6E3S4Ax","H9HCNNNBPUMLHR\n","NT6AP512T32BY",null,null,"IMAG32L4JCBG-046"]
["16Gb","512M x 32","AS4C512M32MD4V-046BIN\nAS4C512M32MD4VA-046BIN","MT53D512M32D2Dx\nMT53E512M32D2FW\nMT53E512M32D1ZW","K4U6E3S4Ax","H9HCNNNBKMMLXR\nH9HCNNNBPUMLHR\n","NT6AP512T32BY",null,null,"IMAG32L4JCBG-046"]
["32Gb","1G x 32","AS4C1G32MD4V-046BIN","MT53D1024M32D4Dx\nMT53E1G32D2FW\nMT53E1G32D2Nx","K4UBE3D4Ax","H9HCNNNCPMMLXR\nH9HCNNNCPMMLXR","NT6AP1024F32B",null,null,"IMBG32L4KBBG\nIMBG32L4KDDG"]

{"sheet":"pSRAM","index":16,"n_rows":11,"n_cols":7,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
[]
["pSRAM"]
["DENSITY","ORG","VCC","PACKAGE","TEMPERATURE","SPEED","ALLIANCE ( EOL )"]
["8Mb","512K x 16","1.8V","48 FPBGA (6x7mm)","Industrial (-30°C ~+85°C)","70ns","AS1C512K16PL-70BIN"]
["8Mb","512K x 16","3V","48 FPBGA (6x7mm)","Industrial (-40°C~ +85°C)","70ns","AS1C512K16P-70BIN"]
["16Mb","1M x 16","1.8V","48 FPBGA (6x7mm)","Industrial (-40°C~ +85°C)","70ns","AS1C1M16PL-70BIN"]
["16Mb","1M x 16","3V","48 FPBGA (6x7mm)","Industrial (-40°C~ +85°C)","70ns","AS1C1M16P-70BIN"]
["32Mb","2M x 16","3V","48 FPBGA (6x7mm)","Industrial (-40°C~ +85°C)","70ns","AS1C2M16P-70BIN"]
["64Mb","4M x 16","1.8V","49 FBGA (4x4mm)","Industrial (-30°C ~+85°C)","70ns","AS1C4M16PL-70BIN***"]
["128Mb\n(*2-stacked die)","8M x 16","1.8V","49 FBGA (4x4mm)","Industrial (-30°C ~+85°C)","70ns","AS1C8M16PL-70BIN***"]
["*** AS1C4M16PL-70BIN /  AS1C8M16PL-70BIN  : EOL'ed, LTS date is 30April2025. "]

{"sheet":"pSRAM Cross Reference","index":17,"n_rows":10,"n_cols":9,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
[]
["pSRAM Cross Reference"]
["ORG","DENSITY","PACKAGE","COMMENTS/ PREV REV","ALLIANCE","JSC/JEJU","ISSI","FIDELIX","AP MEMORY"]
["8Mb","512K x 16","48 FPBGA","page mode & Non-DPD","AS1C512K16PL-70BIN","EM784SP16BPP-70LF","IS66WV51216EALL-70BLI"]
["8Mb","512K x 16","48 FPBGA","Non-page mode & Non-DPD","AS1C512K16P-70BIN","JS784SU16BSP-70LFI","IS66/67WV51216EBLL-70BL","FMP0817CAx"]
["16Mb","1M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C1M16PL-70BIN","EM7164SP16CSP-70LFI","IS66W1M16EALL-70BLI","FMP1617CCx"]
["16Mb","1M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C1M16P-70BIN","JS164SU16BSP-70LFI","IS66/67WV1M16EBLL-70BL","FMP1617CAx"]
["32Mb","2M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C2M16P-70BIN","JS7324SU16BSP-70LFI","IS66WVE2M16EBLL-70B","FMP3217CAx"]
["64Mb","4M X16","49 FBGA","DPD mode","AS1C4M16PL-70BIN","EMC643SP16CKDT-70LF"]
["128Mb\n(*2-stacked die)","8M X16","49 FBGA","DPD mode","AS1C8M16PL-70BIN","JSC283SP16ATDT-70LF",null,null,"APS128XX"]

{"sheet":"Fast Asynchronous SRAM","index":18,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
[]
["5V FAST ASYNCHRONOUS SRAM"]
["DENSITY","ORG","VCC","PACKAGES","TEMPERATURE","SPEED (NS)","ALLIANCE"]
["64Kb","8K x 8","5V","28pin SOJ (300mils),Skinny 28pin PDIP (300mils)","Commercial  0°C ~ +70°C\nIndustrial  -40°C ~ +85°C",15,"AS7C164A"]
["256Kb","32K x 8","5V","28pin SOJ (300mils), 28pin TSOP I (8x13.4mm)","Commercial  0°C ~ +70°C\nIndustrial  -40°C ~ +85°C","10,12,15,20","AS7C256A"]
["256Kb","32K x 8","5V","28pin PDIP (300mils)","Commercial  0°C ~ +70°C",15,"AS7C256C"]
["512Kb","32K x 16","5V","44pin SOJ (400mils), 44pin TSOP II (400mils)","Commercial  0°C ~ +70°C","12,15","AS7C513B"]
["1Mb","128K x 8","5V","32pin TSOP I (8x13.4mm) Corner Vcc & Gnd","Commercial  0°C ~ +70°C\nIndustrial  -40°C ~ +85°C","12,15,20","AS7C1024B"]
["1Mb","128K x 8","5V","32pin SOJ (300mils & 400mils) Corner Vcc & Gnd","Industrial  -40°C ~ +85°C",12,"AS7C1024D"]
["1Mb","128K x 8","5V","32pin SOJ (300mils & 400mils), Center Vcc & Gnd","Commercial  0°C ~ +70°C\nIndustrial  -40°C ~ +85°C","10,12,15","AS7C1025B"]
["1Mb","64K x 16","5V","44pin SOJ (400mils), 44pin TSOP II (400mils)","Commercial  0°C ~ +70°C\nIndustrial  -40°C ~ +85°C","10,12,15,20","AS7C1026B"]
["4Mb","512K x 8","5V","36pin SOJ (400mils), 44pin TSOP II (400mils)","Commercial  0°C ~ +70°C\nIndustrial  -40°C ~ +85°C","10,12,15,20","AS7C4096A"]
["4Mb","256K x 16","5V","44pin SOJ (400mils), 44pin TSOP II (400mils)","Commercial  0°C ~ +70°C\nIndustrial  -40°C ~ +85°C","10,12,15,20","AS7C4098A"]
["3.3V FAST ASYNCHRONOUS SRAM"]
["DENSITY","ORG","VCC","PACKAGES","TEMPERATURE","SPEED (NS)","ALLIANCE"]
["256Kb","32K x 8","3.3V","28pin SOJ (300mils), 28pin TSOP I (8x13.4mm)","Commercial\nIndustrial","10,12,15,20","AS7C3256A"]
["512Kb","32K x 16","3.3V","44pin SOJ (400mils), 44pin TSOP II (400mils)","Commercial","10,12,15,20","AS7C3513B"]
["1Mb","128K x 8","3.3V","32pin SOJ (300 & 400mils), 32pin TSOP I (8x13.4mm), Corner Vcc & Gnd","Commercial","10,12,15,20","AS7C31024B"]
["1Mb","128K x 8","3.3V","32pin SOJ (300 & 400mils), Center Vcc & Gnd","Commercial\nIndustrial","10,12,15,20","AS7C31025B"]
["1Mb","64K x 16","3.3V","44pin SOJ (400mils), 44pin TSOP II (400mils)","Commercial\nIndustrial","10,12,15,20","AS7C31026B"]
["2Mb","128K x 16","3.3V","44pin TSOP II (400mils)","Commercial\nIndustrial","10,12,15,20","AS7C32098A"]
["2Mb","256K x 8","3.3V","44pin TSOP II (400mils)","Commercial\nIndustrial","10,12,15,20","AS7C32096A"]
["4Mb","512K x 8","3.3V","36pin SOJ (400mils), 44pin TSOP II (400mils), 36b TFBGA (6x8mm)","Commercial\nIndustrial","8,10,12,15,20","AS7C34096A , B"]
["4Mb","256K x 16","3.3V","44pin SOJ (400mils), 44pin TSOP II (400mils), 48b TFBGA (6x8mm, 8x10mm)","Commercial\nIndustrial","8,10,12,15,20","AS7C34098A , B"]
["8Mb","1M x 8","3.3V","44pin TSOP II (400mils), 48b TFBGA (6x8mm)","Industrial",10,"AS7C38096A , B"]
["8Mb","512K x 16","3.3V","44pin TSOP II (400mils), 48b TFBGA (6x8mm)","Industrial",10,"AS7C38098A"]
["8Mb","256K x 32","3.3V","90b TFBGA (8x13mm)","Industrial",10,"AS7C325632"]
["16Mb","512K x32","3.3V","90b TFBGA (9x13mm)","Industrial",10,"AS7C351232"]
["16Mb","1M x 16","3.3V","48b TFBGA (6x8mm), 48pin TSOP I (12x20mm), 54pin TSOP II (400mils)","Industrial",10,"AS7C316098A , B"]
["16Mb","2M x 8","3.3V","48b TFBGA (6x8mm), 48pin TSOP I (12x20mm), 44pin TSOP II, 54pin TSOP II","Industrial",10,"AS7C316096A , B , C"]
["32Mb","2M x 16","1.65V ~ 3.6V","48b FBGA (6x8mm)","Industrial",10,"AS7CW2M16-10BIN"]
["1.8V/2.5V/3.3V FAST ASYNCHRONOUS SRAM"]
["DENSITY","ORG","VCC","PACKAGES","TEMPERATURE","SPEED (NS)","ALLIANCE"]
["32Mb","2M x 16","1.65V ~ 3.6V","48b FBGA (6x8mm)","Industrial",10,"AS7CW2M16-10BIN"]

{"sheet":"Fast Asyn SRAM Cross Reference","index":19,"n_rows":78,"n_cols":10,"rows_kept":78,"cut":false,"hidden":false,"merged":[]}
[]
["Fast Asynchronous SRAM Cross Reference"]
["64K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS (EOL)","IDT","ISSI"]
["8K x 8","5V","28pin SOJ (300mil)",15,"AS7C164A-15JxN",null,"CY7C185-xxVI/VC (EOL)","7164SxxYG              \n7164LxxYG","IS61C64AL-xxJLI (EOL)"]
["8K x 8","5V","28pin Skinny PDIP 300mil",15,"AS7C164A-15PxN",null,"CY7C185-xxPC (EOL)","7164S20TPG"]
["256K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS (EOL)","IDT","ISSI"]
["32K x 8","5V","28pin SOJ","10,12,15,20","AS7C256A-xxJCN/JIN","K6E0808C1E-J (EOL)","CY7C199D-10VXI(EOL)   CY7C199CN–xxVXI/VXC(EOL) ","71256LxxYG                 71256SAxxYG","IS61C256AL-xxJL/JLI","    "]
["32K x 8","5V","28pin TSOP I","10,12,15,20","AS7C256A-xxTCN/TIN","K6E0808C1E-T (EOL)","CY7C199D-10ZXI(EOL)   CY7C199CN–xxZXC/ZXI(EOL)  ","71256SAxxPZG","IS61C256AL-xxTL/TLI"]
["32K x 8","3.3V","28pin SOJ","10,12,15,20","AS7C3256A-xxJCN/JIN","K6E0808V1E-J (EOL)","CY7C1399BN-xxVXC(EOL)","71V256SAxxYG","IS61LV256AL-10JL/JLI"]
["32K x 8","3.3V","28pin TSOP I","10,12,15,20","AS7C3256A-xxTCN/TIN","K6E0808V1E-T (EOL)","CY7C1399BN-xxZXI/ZXC(EOL)","71V256SAxxPZG","IS61LV256AL-10TL/TLI"]
["32K x 8","5V","28pin DIP",15,"AS7C256C-xxPCN",null,"CY7C199CN-15/25PXC (EOL)","71256LxxTDB     \n71256SxxTDB  \n71256SAxxTPG"]
["512K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI"]
["32K x 16","5V","44pin SOJ (400mil)",15,"AS7C513B-xxJCN",null,"CY7C1020D-10VXI(EOL)",null,"IS61C3216AL-12KLI "]
["32K x 16","5V","44pin TSOP II (400mil)","12,15","AS7C513B-xxTCN",null,"CY7C1020D-10ZSXI",null,"IS61C3216AL-12TLI"]
["32K x 16","3.3V","44pin TSOP II (400mil)","12,15,20","AS7C3513B-xxTCN",null,"CY7C1020DV33-10ZSXI",null,"IS61WV3216BLL-xxTLI"]
["32K x 16","3.3V","44pin SOJ (400mil)","10,12,15","AS7C3513B-xxJCN",null,"CY7C1020DV33-10VXI"]
["1M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG (EOL)","CYPRESS","IDT","ISSI","GSI"]
["128K x 8","5V","32pin SOJ (400mil)","12,15,20","AS7C1025B-xxJCN/JIN","K6R1008C1D-KI10","CY7C1019D-10VXI(EOL)","71124SxxYG(EOL)"]
["128K x 8","3.3V","32pin SOJ (400mil)","10,12,15,20","AS7C31025B-xxJCN/JIN","K6R1008V1D-KI10","CY7C1019DV33-10VXI","71V124SAxxYG","IS63LV1024-xxK/KI (EOL)"]
["128K x 8","5V","32pin SOJ (300mil)","10,12,15,20","AS7C1025B-xxTJCN"]
["128K x 8","3.3V","32pin SOJ (400mil)",12,"AS7C31025B-xxJIN",null,"CY7C1019DV33-10VXI"]
["128K x 8","3.3V","32pin SOJ (300mil)","10,12,15,20","AS7C31025B-xxTJCN/-12TJIN",null,"CY7C1018DV33-10VXI(EOL)","71V124SAxxTYG","IS63WV1288DBLL-xxJLI             IS63LV1024L-10JLI(EOL)"]
["128K x 8","5V","32pin SOJ (400mil)","12,15,20","AS7C1024D-12JIN",null,"CY7C109D-10VXI","71024SxxYG","IS61C1024AL-12KLI (EOL)"]
["128K x 8","5V","32pin TSOP I","12,15,20","AS7C1024B-xxTCN",null,"CY7C109D-10ZXI",null,"IS61C1024AL-12TLI"]
["128K x 8","5V","32pin SOJ (300mil)","12,15,20","AS7C1024D-12TJIN",null,"CY7C1009D-10VXI(EOL)","71024SxxTYG","IS61C1024AL-12JLI"]
["128K x 8","3.3V","32pin SOJ (400mil)","12,15,20","AS7C31024B-xxJCN"]
["128K x 8","3.3V","32pin TSOP I","10,12,15,20","AS7C31024B-xxTCN"]
["128K x 8","3.3V","32pin SOJ (300mil)","10,12,15,20","AS7C31024B-xxTJCN"]
["64K x 16","5V","44pin SOJ (400mil)","10,12,15,20","AS7C1026B-xxJCN/JIN","K6R1016C1D-KI10","CY7C1021D-10VXI","71016SxxYG","IS61C6416AL-12KLI"]
["64K x 16","5V","44pin TSOP II (400mil)","10,12,15,20","AS7C1026B-xxTCN/TIN","K6R1016C1D-UI10","CY7C1021D-10ZSXI/A(EOL)","71016SxxPHG","IS61C6416AL-12TLI"]
["64K x 16","3.3V","44pin SOJ (400mil)","10,12,15,20","AS7C31026B-xxJCN/TIN","K6R1016V1D-KI10","CY7C1021DV33-10VXI","71V016SAxxYG","IS61WV6416DBLL-xxKLI IS61LV6416-xxKL/KLI"]
["64K x 16","3.3V","44pin TSOP II (400mil)","10,12,15,20","AS7C31026B-xxTCN/TIN","K6R1016V1D-UI10","CY7C1021DV33-10ZSXI    CY7C1021DV33-10ZSXA(EOL)","71V016SAxxPHG","IS61WV6416DBLL-xxTLI IS61WV6416EEBLL-xxTLI IS61LV6416-xxT/TL/TI/TLI","GS71116AGP-xx"]
["2M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["128K x 16","3.3V","44pin TSOP II","10,12,15,20","AS7C32098A-xxTxN",null,"CY7C1011G30-10ZSXA     CY7C1011DV33-10ZSXI",null,"IS61WV12816EDBLL-xxTLI    IS64WV12816EDBLL-10CTLA1 IS61WV12816EFBLL-10TLI IS61WV12816FBLL-10TLI IS61WV12816DBLS-35TLI(EOL) IS61WV12816DBLL-10TL/TLI/TI(EOL) ","GS72116AGP-xx                                  GS72116ATP-xx(EOL)"]
["256K x 8","3.3V","44pin TSOP II","10,12,15,20","AS7C32096A-xxTxN",null,null,null,"IS61WV2568EDBLL-xxTLI IS64WV2568EDBLL-10CTLA1 IS61WV2568EFBLL-10TLI  IS61WV2568FBLL-10TLI ","GS72108AGP-xx                            GS72108ATP-xx(EOL)"]
["4M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["512K x 8","5V","36pin SOJ (400mil)","10,12,15,20","AS7C4096A-xxJxN","K6R4008C1D-KI10","CY7C1049D-10VXI(EOL)\nCY7C1049G-10VXI                   \nCY7C1049GN-10VXI","R1RP0408DGE-2LR(PI/PR)#B1","IS61C5128AL-10KLI"]
["512K x 8","5V","44pin TSOP II (400mil)","10,12,15,20","AS7C4096A-xxTxN","K6R4008C1D-UI10","CY7C1049G-10ZSXI",null,"IS61C5128AL-10TLI"]
["512K x 8","3.3V","36pin SOJ (400mil)","8,10,12,15,20","AS7C34096A-xxJxN","K6R4008V1D-KI10","CY7C1049DV33-10VXI (EOL)\nCY7C1049G30-10VXI                      CY7C1049GN30-10VXI ","71V424LxxYG      \n71V424SxxYG\nR1RW0408DGE-2LR(PI/PR)#B1","IS61WV5128FBLL-10KLI  IS64WV5128EFBLL-10KLA3  IS61WV5128EDBLL-10KLI/KLA1 IS61WV5128BLL-10KLI "]
["512K x 8","3.3V","44pin TSOP II (400mil)","10,12,15,20","AS7C34096A-xxTxN","K6R4008V1D-UI10","CY7C1049DV33-10ZSXI(EOL)\nCY7C1049G30-10ZSXI                      CY7C1049GN30-10ZSXI ","71V424LxxPHG    \n71V424SxxPHG","IS61WV5128FBLL-10TLI  IS64WV5128EFBLL-10CTLA3 IS61WV5128EDBLL-10TLI  IS64WV5128EDBLL-10CTA1/CTLA1 IS61WV5128BLL-10TL/TLI    IS61WV5128BLS-25TLI "]
["512K x 8","2.7 ~ 3.6V","44pin TSOP II",10,"AS7C34096B-10TIN",null,"CY7C1049G30-10ZSXI                      CY7C1049GN30-10ZSXI ","71V424LxxPHG     \n71V424SxxPHG","IS61WV5128FBLL-10TLI  IS64WV5128EFBLL-10CTLA3 IS61WV5128EDBLL-10TLI  IS64WV5128EDBLL-10CTA1/CTLA1 IS61WV5128BLL-10TL/TLI    IS61WV5128BLS-25TLI "]
["512K x 8","2.7 ~ 3.6V","36ball TFBGA",10,"AS7C34096B-10BIN",null,null,null,"IS61WV5128FBLL-10BI/BLI IS64WV5128EFBLL-10BA3/BLA3 IS61WV5128EDBLL-10BI/BLI IS64WV5128EDBLL-10BA1/BLA1  IS61WV5128BLL-10BI/BLI "]
["256K x 16","5V","44pin SOJ (400mil)","10,12,15,20","AS7C4098A-xxJxN","K6R4016C1D-KI10","CY7C1041D-10VXI(EOL)\nCY7C1041G-10VXI","R1RP0416DGE-2LR(PI/PR)#B1","IS61C25616AL-10KLI                  IS61C25616AS-25KLI"]
["256K x 16","5V","44pin TSOP II (400mil)","10,12,15,20","AS7C4098A-xxTxN","K6R4016C1D-UI10","CY7C1041D-10ZSXI(EOL)\nCY7C1041G-10ZSXI                          CY7C1041GN-10ZSXI ","R1RP0416DSB-0PI(PR)#D1     R1RP0416DSB-2LR(PI/PR/SR)#D1  R1RP0416DSB-2LR(PR)#S1","IS61C25616AL-10TL/TLI                 IS61C25616AS-25TLI"]
["256K x 16","3.3V","44pin SOJ (400mil)","10,12,15,20","AS7C34098A-xxJxN","K6R4016V1D-KI10","CY7C1041DV33-10VXI (EOL)\nCY7C1041GN30-10VXI(EOL)\nCY7C1041G30-10VXI","71V416LxxYG   \n71V416SxxYG\nR1RW0416DGE-2LR(PI/PR)#B1","IS61WV25616BLL-xxKLI(EOL)"]
["256K x 16","3.3V","44pin TSOP II (400mil)","8,10,12,15,20","AS7C34098A-xxTxN","K6R4016V1D-UI10","CY7C1041DV33-10ZSXI(EOL)\nCY7C1041G30-10ZSXI/A\n","71V416LxxPHG   \n71V416SxxPHG\nR1RW0416DSB-0PI(PR)#D1  R1RW0416DSB-0PI(PR)#S1  R1RW0416DSB-2LR(PI/PR/SR)#D1 R1RW0416DSB-2PI(PR)#S1","IS61WV25616EDBLL-xxTLI/CTLA1   IS61WV25616EFBLL-10TLI IS61WV25616FBLL-10TL    IS61WV25616BLL-xxTL/TLI(EOL)   IS61WV25616BLS-25TLI(EOL)","GS74116AGP-xx"]
["256K x 16","3.3V","48ball TFBGA",10,"AS7C34098A-xxBIN",null,"CY7C1041DV33-10BVXI(EOL)\nCY7C1041G30-10BVJXI\n","71V416LxxBE  \n71V416SxxBE","IS61WV25616EDBLL-xxBLI/BLA1   IS61WV25616EFBLL-10BLI IS61WV25616FBLL-10BI/BLI   IS61WV25616BLL-xxBLI (EOL)","GS74117AX-xx  GS74117AGX-xx"]
["256K x 16","2.7 ~ 3.6V","44pin TSOP II",10,"AS7C34098B-10TIN",null,"CY7C1041DV33-10ZSXI(EOL)\nCY7C1041G30-10ZSXI/A\n","71V416LxxPHG   \n71V416SxxPHG\nR1RW0416DSB-0PI(PR)#D1  R1RW0416DSB-0PI(PR)#S1  R1RW0416DSB-2LR(PI/PR/SR)#D1 R1RW0416DSB-2PI(PR)#S1","IS61WV25616EDBLL-xxTLI/CTLA1   IS61WV25616EFBLL-10TLI IS61WV25616FBLL-10TL    IS61WV25616BLL-xxTL/TLI(EOL)   IS61WV25616BLS-25TLI(EOL)","GS74116AGP-xx"]
["256K x 16","2.7 ~ 3.6V","48ball TFBGA",10,"AS7C34098B-10BIN",null,"CY7C1041DV33-10BVXI(EOL)\nCY7C1041G30-10BVJXI\n","71V416LxxBE   \n71V416SxxBE","IS61WV25616EDBLL-xxBLI/BLA1   IS61WV25616EFBLL-10BLI IS61WV25616FBLL-10BLI   IS61WV25616BLL-xxBLI (EOL)","GS74117AX-xx  GS74117AGX-xx"]
["8M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI"]
["512K x 16","3.3V","44pin TSOP II",10,"AS7C38098A-10TIN",null,"CY7C1051DV33-10/12ZSXI(EOL)\nCY7C1051H30-10ZSXI",null,"IS61WV51216EEBLL-xxTLI     IS61WV51216EDBLL-xxTLI    IS61WV51216BLL-xxTLI"]
["512K x 16","3.3V","48ball TFBGA",10,"AS7C38098A-10BIN",null,"CY7C1051DV33-10BAXI (EOL)\nCY7C1051H30-10BVXI",null,"IS61WV51216EEBLL-xxBLI   IS61WV51216EDBLL-xxBLI  IS61WV51216BLL-xxMLI"]
["256K x 32","3.3V","90ball TFBGA",10,"AS7C325632-10BIN",null,null,null,"IS61WV25632BLL-10BLI"]
["1M x 8","3.3V","44pin TSOP II",10,"AS7C38096A-10TIN",null,"CY7C1059DV33-10ZSXI(EOL)\nCY7C1059DV33-12ZSXI/Q(EOL)                      CY7C1059H30-10ZSXI",null,"IS61WV10248BLL-xxTLI   IS61WV10248EEBLL-8TLI   IS61WV10248EDBLL-xxTLI"]
["1M x 8","3.3V","48ball TFBGA (different pinout)",10,"AS7C38096A-10BIN"]
["1M x 8","3.3V","48ball TFBGA (different pinout)",10,"AS7C38096B-10BIN",null,null,null,"IS61WV10248BLL-xxMLI  IS61WV10248EEBLL-xxBLI  IS61WV10248EDBLL-xxBLI "]
["16M  FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI"]
["1M x 16","3.3V","48pin TSOP I",10,"AS7C316098A-10TIN",null,"CY7C1061GN30-10ZXI    CY7C1061G30-10ZXI",null,"IS61WV102416BLL-xxTLI(EOL)  IS61WV102416DALL-12TLI  IS62WV102416BLL-25TLI   IS61WV102416EDBLL-10TL/TLI   IS61WV102416FBLL-xxTLI "]
["1M x 16","3.3V","48ball TFBGA",10,"AS7C316098A-10BIN",null,"CY7C1061GN30-10BV1XI (EOL)    CY7C1061G30-10BV1X",null,"IS61WV102416BLL-10MLI(EOL)    IS61WV102416DALL-12BLI    IS61WV102416EDBLL-10BL/BLI  IS61WV102416FBLL-xxBLI"]
["1M x 16","3.3V","54pin TSOP II",10,"AS7C316098B-10TIN",null,"CY7C1061GN30-10ZSXI    CY7C1061G30-10ZSXI CY7C10612G30-10ZSXI ",null,"IS61WV102416FBLL-xxT2LI"]
["1M x 16","3.3V","48ball TFBGA",10,"AS7C316098B-10BIN",null,"CY7C1061GN30-10BVJXI             CY7C1061GN30-10BVXI   CY7C1061G30-10BVJXI",null,"IS62WV102416BLL-25MLI    IS61WV102416FBLL-xxB2LI"]
["2M x 8","3.3V","48pin TSOP I",10,"AS7C316096A-10TIN"]
["2M x 8","3.3V","54pin TSOP II",10,"AS7C316096B-10TIN",null,"CY7C1069DV33-10ZSXI (EOL)\nCY7C1069GN30-10ZSXI\nCY7C1069G30-10ZSXI   ",null,"IS61WV20488FBLL-xxT2LI"]
["2M x 8","3.3V","44pin TSOP II",10,"AS7C316096C-10TIN",null,null,null,"IS61WV20488FBLL-xxTLI  IS61WV20488BLL-xxTLI (EOL)    IS62WV20488BLL-25TLI "]
["2M x 8","3.3V","48ball TFBGA (1CE)",10,"AS7C316096C-10BIN",null,null,null,"IS61WV20488BLL-xxMLI(EOL)  IS61WV20488FBLL-xxBLI"]
["2M x 8","3.3V","48ball TFBGA (2CE)",10,"AS7C316096B-10BIN",null,"CY7C1069GN30-10BVXI   CY7C1069G30-10BVXI     CY7C1069DV33-10BVXI(EOL)"]
["512K x 32","3.3V","90ball TFBGA",10,"A7C351232-10BIN",null,null,null,"IS61WV51232BLL-10BLI "]
["32M  FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI"]
["2M x 16","1.8V/2.5V/3.3V","48b FBGA (6x8mm)",10,"AS7CW2M16-10BIN",null,"CY7C1071DV33-12BAXI (3.3V)",null,"IS61WV204816ALL-10BL/I (1.8V) IS61WV204816BLL-10BL/I (3.3V) "]

{"sheet":"Low Power Asynchronous SRAM","index":20,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
[]
["2.7V- 3.6V LOW POWER SRAMS"]
["DENSITY","ORG","VCC","PACKAGES","SPEED(NS)","ALLIANCE MEMORY PART#"]
["256Kb","32K x 8","2.5 ~ 3.6V","28pin SOP (330mm)",70,"AS62V256A-70SIN"]
["1Mb","64K x16 with ECC","2.7 ~ 3.6V","44pin TSOP II (400mils)",45,"AS6CE1016A-45ZIN"]
["2Mb","256K x 8","2.7 ~ 3.6V","32pin SOP(450mils), 32pin TSOP I (8x20mm), 32pin STSOP (8x13.4mm), 36ball TFBGA (6x8mm)",55,"AS6C2008"]
["4Mb","256K x 16","2.7 ~ 3.6V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm)",45,"AS6C4016B"]
["4Mb","256K x16 with ECC","2.7 ~ 3.6V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm)",45,"AS6CE4016B"]
["8Mb","1M x 8","2.7 ~ 3.6V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm)","45/55","AS6C8008B"]
["8Mb","512K x 16","2.7 ~ 3.6V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm)","45/55","AS6C8016B"]
["16Mb","1M x 16","2.7 ~ 3.6V","48pin TSOP I (12x20mm), 48ball TFBGA (6x8mm) ","45/55","AS6C1616B"]
["16Mb","1M x 16 / 2M x 8","2.7 ~ 3.6V","48pin TSOP I (12x20mm)",45,"AS6C1616C-45TIN"]
["16Mb","2M x 8","2.7 ~ 3.6V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm)",45,"AS6C1608B"]
["32Mb","2M x 16 / 4M x8","2.7 ~ 3.6V","48pin TSOP I (12x20mm) , 48ball TFBGA (8x10mm)",55,"AS6C3216A"]
["64Mb","4M x 16 / 8M x8","2.7 ~ 3.6V","48pin TSOP I (12x20mm),  48ball TFBGA (8x10mm) (dual chip select)",55,"AS6C6416"]
["2.7V - 5.5V LOW POWER SRAMS"]
["DENSITY","ORG","VCC","PACKAGES","SPEED (NS)","ALLIANCE MEMORY PART#"]
["64Kb","8K x 8","2.7 ~ 5.5V","28pin PDIP (600mils), 28pin SOP (330mils), 28pin sTSOP (8x13.4mm)",55,"AS6C6264"]
["256Kb","32K x 8","2.7 ~ 5.5V","28pin PDIP (600mils), 28pin SOP (330mils), 28pin sTSOP (8x13.4mm)",55,"AS6C62256"]
["1Mb","64K x 16","2.7 ~ 5.5V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm)",55,"AS6C1016"]
["1Mb","128K x 8","2.7 ~ 5.5V","32p SOP (450mils), 32p TSOP I (8x20mm), 32p sTSOP (8x13.4mm), 36b TFBGA (6x8mm), 32p PDIP (600mils)",55,"AS6C1008"]
["2Mb","256K x 8","2.7 ~ 5.5V","32p SOP (450mils), 32p TSOP I (8x20mm), 32p sTSOP (8x13.4mm), 36b TFBGA (6x8mm)",55,"AS6C2008A"]
["2Mb","128K x 16","2.7 ~ 5.5V","44pin TSOP II (400mils), 48b TFBGA (6x8mm)",55,"AS6C2016"]
["4Mb","512K x 8","2.7 ~ 5.5V","32p SOP (450mils), 32p TSOP I (8x20mm), 32p sTSOP (8x13.4mm), 36b TFBGA (6x8mm), 32p TSOP II (400mils)",55,"AS6C4008"]
["4Mb","512K x 8","2.7 ~ 5.5V","32p SOP (450mils)",70,"AS6C4008-70SAN"]
["4Mb","256K x 16","2.7 ~ 5.5V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm)",55,"AS6C4016"]
["8Mb","1M x 8","2.7 ~ 5.5V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm)",55,"AS6C8008"]
["8Mb","512K x 16","2.7 ~ 5.5V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm) one chip select pins:B5**",55,"AS6C8016"]
["8Mb","512K x 16","2.7 ~ 3.6V","48pin TSOP I (12x20mm)",55,"AS6C8016-55TIN"]

{"sheet":"Low Power Asyn SRAM Cross Refer","index":21,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[]}
[]
["Low Power Asynchronous SRAM Cross Reference"]
["64K"]
["ORG","VCC","PACKAGE","ALLIANCE","ZMD","CYPRESS (EOL)","HITACHI (EOL)","NEC (EOL)","HYNIX (EOL)"]
["8K x 8","2.7V ~ 5.5V","28pin 600mil DIP","AS6C6264-55PCN / PIN","U6264BDC07LLG1",null,"HM6264BLP",null,"HY6264P"]
["8K x 8","2.7V ~ 5.5V","28pin 330mil SOP","AS6C6264-55SCN / SIN","U6264BS2C07LLG1","CY6264-55SNXC/I(EOL)             CY6264-70SNXC/I(EOL)","HM6264BLFP","uPD4464","HY6264G"]
["8K x 8","2.7V ~ 5.5V","28pin STSOP (8 x 13.4 mm)","AS6C6264-55STCN"]
["256K"]
["ORG","VCC","PACKAGE","ALLIANCE","ZMD","SAMSUNG (EOL)","CYPRESS (EOL)","RENESAS","BRILLIANCE (EOL)","ISSI"]
["32K x 8","2.7V ~ 5.5V","28pin 600mil DIP","AS6C62256-55PCN","U62256ADC07LLG1","K6X0808C1D-DF55","CY62256NLL-70PXC(EOL)",null,"BS62LV256PCP-55"]
["32K x 8","2.7V ~ 5.5V","28pin 330mil SOP","AS6C62256-55SxN","U62256AS2C07LLG1","K6X0808C1D-BF55","CY62256NLL-55SNXI(EOL)  CY62256NLL-70SNXA(EOL)  CY62256NVLL-70SNXI(EOL)","R1LP5256ESP-5SI   \nR1LV5256ESP-5SI","BS62LV256SCP-55","IS62C256AL-xxULI/UL.           IS62LV256AL-45ULI"]
["32K x 8","2.4V ~ 3.6V","28pin 330mil SOP","AS62V256-70SIN",null,null,"CY62256NVLL-70SNXI(EOL)","R1LV5256ESP-5SI","BS62LV256SCP-55","IS62LV256AL-45ULI"]
["32K x 8","2.7V ~ 5.5V","28pin STSOP (8 x 13.4 mm)","AS6C62256-55STxN",null,"K6X0808C1D-LF55","CY62256NLL-70ZRXI(EOL)\nCY62256NLL-55ZXI/A(EOL)  CY62256VNLL-70ZXC/I(EOL) ","R1LP5256ESA-5SI   \nR1LV5256ESA-5SI","BS62LV256STCP-55","IS62LV256AL-xxTL/TLI                 IS62C256AL-45TL/TLI"]
["1M"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","BRILLIANCE (EOL)","NEC (EOL)","ISSI"]
["128K x 8","2 .7V ~ 5.5V","32pin 600mil DIP","AS6C1008-55PCN / PIN","K6X1008C2D-DB55",null,null,"BS62LV1027PCP-55","uPD431000ACZ-70L"]
["128K x 8","2.7V ~ 5.5V","32pin 450mil SOP","AS6C1008-55SIN","K6X1008C2D-GF55(Lead)/BF","CY62128ELL-45SXI/A    CY62128EV30LL-45SXI","M5M51008DFP-55HI\nR1LP0108ESN-5SI      R1LV0108ESN-5SI","BS62LV1027SIP-55","uPD431000AGW-70L","IS62C1024AL-35QLI IS62WV1288FBLL-45QLI    IS62WV1288BLL-45/55QLI (EOL) IS62WV1288DBLL-45QLI(EOL)"]
["128K x 8","2.7V ~ 5.5V","32pin TSOP I (8 x 20 mm)","AS6C1008-55TIN","K6X1008C2D-TF55 or PF","CY62128ELL-45ZXI/A   CY62128EV30LL-45ZXI","M5M51008DVP-55HI\nR1LP0108ESF-5SI   \nR1LV0108ESF-5SI","BS62LV1027TIP-55","uPD431000AGZ-70LL-KKH","IS62C1024AL-35TLI   IS62WV1288FBLL-45TLI  IS62WV1288BLL-45/55TLI(EOL)   IS65WV1288BLL-55TLA1(EOL)    IS62WV1288DBLL-45TLI(EOL)"]
["128K x 8","2.7V ~ 5.5V","32pin STSOP (8 x 13.4 mm)","AS6C1008-55STIN",null,"CY62128EV30LL-45ZAXI     CY62128ELL-45ZAXI(EOL)  ","M5M51008DKV-55HI\nR1LP0108ESA-5SI   \nR1LV0108ESA-5SI","BS62LV1027STIP-55","uPD431000AGU-B10-9JH"," IS62WV1288FBLL-45HLI    IS62WV1288BLL-45/55HLI(EOL)  IS65WV1288BLL-55HLA1(EOL) S62WV1288DBLL-45HLI(EOL)"]
["64K x 16","2.7V ~ 5.5V","48ball TFBGA","AS6C1016-55BIN","K6F1016U4C-EF55"," CY62126EV30LL-45BVXI",null,"BS616LV1010AI-70",null,"IS62WV6416FBLL-45BLI    IS62WV6416DBLL-45BLI(EOL)    IS62WV6416BLL-45/55BLI(EOL)"]
["64K x 16","2.7V ~ 5.5V","44pin TSOP II","AS6C1016-55ZIN",null,"CY62126EV30LL-45ZSXI/A",null,"BS616LV1010EI-70",null,"IS62WV6416FBLL-45TLI      IS62WV6416DBLL-45TLI(EOL)   IS62WV6416BLL-45/55TLI(EOL)"]
["64K x 16","2.7V ~3.6V","44pin TSOP II","AS6CE1016A-45ZIN",null,null,null,null,null,"IS61WV6416EEBLL"]
["2M"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["256K x 8","2.7V ~ 3.6V","32pin 450mil SOP","AS6C2008-55SIN",null,"CY62138FLL-45SXI    CY62138FV30LL-45SXI(EOL)",null,"BS62LV2006SIP-55"]
["256K x 8","2.7V ~ 3.6V","32pin TSOP I (8 x 20 mm)","AS6C2008-55TIN",null,"CY62138FV30LL-45ZXI",null,"BS62LV2006TIP-55","IS62WV2568BLL-45/55TLI  IS62WV2568EBLL-45TLI   IS62WV2568FBLL-45TLI "]
["256K x 8","2.7V ~ 3.6V","32pin STSOP (8 x 13.4 mm)","AS6C2008-55STIN","K6F2008V2E-LF70000","CY62138FV30LL-45ZAXI/A","M5M5V208AKV-55HI\nR1LV0208BSA-5SI","BS62LV2006STIP-55","IS62WV2568BLL-45/55HLI     IS62WV2568EBLL-45HLI   IS62WV2568FBLL-45HLI"]
["256K x 8","2.7V ~ 3.6V","36ball TFBGA (6mm x 8mm)","AS6C2008-55BIN",null,"CY62138FV30LL-45BVXI   ",null,null,"IS62WV2568BLL-45/55BLI     IS62WV2568EBLL-45BLI   IS62WV2568FBLL-45BLI"]
["128K x 16","2.7V ~ 5.5V","44pin TSOP II","AS6C2016-55ZIN",null,"CY62136VLL-70ZSXI(EOL)\nCY62136E/FV30LL-55ZSXI\nCY62136E/FV30LL-45ZSXI\nCY62137FV30LL-45ZSXI","M5M5V216ATP-70HI\nR1LV0216BSB-5SI","BS616LV2016EIP-55","IS62WV12816BLL-45/55TLI IS62WV12816EBLL-45/55TLI  IS62WV12816FBLL-45TLI    IS62WV12816DBLL-35/45/55TLI "]
["128K x 16","2.7V ~ 3.6V","48ball TFBGA","AS6C2016-55BIN","K6F2016U4E-EF55000","CY62136E/FV30LL-45BVXI\nCY62137FV30LL-45BVXI\nCY62137EV30LL-45BVXI(EOL)",null,"BS616LV2019AIG-55","IS62WV12816BLL-45/55BLI  IS62WV12816EBLL-45/55BLI   IS62WV12816FBLL-45BLI    IS62WV12816DBLL-35/45/55BLI"]
["256K x 8","2.7V ~ 5.5V","32pin 450mil SOP","AS6C2008A-55SIN",null,"CY62138FLL-45SXI    CY62138FV30LL-45SXI(EOL)",null,"BS62LV2006SIP-55"]
["256K x 8","2.7V ~ 5.5V","32pin TSOP I (8 x 20mm)","AS6C2008A-55TIN",null,"CY2138FV30LL-45ZXI",null,"BS62LV2006TIP-55","IS62WV2568BLL-45/55TLI  IS62WV2568EBLL-45TLI   IS62WV2568FBLL-45TLI "]
["256K x 8","2.7V ~ 5.5V","36ball TFBGA (6mm x 8mm)","AS6C2008A-55BIN",null,"CY62138FV30LL-45BVXI   ",null,null,"IS62WV2568BLL-45/55BLI     IS62WV2568EBLL-45BLI   IS62WV2568FBLL-45BLI"]
["4M"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["512K x 8","2.7V ~ 5.5V","32pin 600mil DIP","AS6C4008-55PCN","K4X4008C1F-DB55",null,null,"BS62LV4006PCP-55"]
["512K x 8","2.7V ~ 5.5V","32pin 450mil SOP","AS6C4008-55SIN","K6X4008C1F-GF55 or BF","CY62148ELL-55SXI      CY62148EV30LL-55SXI      CY62148G30-45SXI\nCY62148G-45SXI(EOL)             ","R1LP0408DSP-5SI    RMLV0408EGSP-4S2","BS62LV4006SIP-55","IS62C5128EL-45QLI      IS62WV5128DBLL-45QLI    IS62WV5128EBLL-45QLI   IS62WV5128BLL-55QLI "]
["512K x 8","2.7V ~ 5.5V","32pin STSOP (8 x 13.4mm)","AS6C4008-55STIN",null,"CY62148ESL-55ZAXI/A      ","RMLV0408EGSA-4S2","BS62LV4006STIP-55","IS62C5128EL-45HLI     IS62WV5128DBLL-45HLI   IS62WV5128EBLL-45HLI  IS62WV5128EHBLL-45HLI/HL  IS62WV5128BLL-55HLI "]
["512K x 8","2.7V ~ 5.5V","32pin TSOP I (8 x 20mm)","AS6C4008-55TIN",null,null,null,null,"IS62WV5128DBLL-45TLI  IS62WV5128EBLL-45TLI  IS62WV5128EHBLL-45TLI/TL  IS62WV5128BLL-55TLI "]
["512K x 8","2.7V ~ 5.5V","32pin TSOP II","AS6C4008-55ZIN","K6X4008C1F-VF55","CY62148ELL-45ZSXI    \nCY62148EV30LL-45ZSXI    \nCY62148G30-45ZSXI                CY62148G-45ZSXI(EOL)\nCY62148GN-45ZSXIT(EOL)\nCY62148GN30-45ZSXIT(EOL)","R1LP0408DSB-5SI   RMLV0408EGSB-4S2","BS62LV4006ECP55","IS62WV5128DBLL-45T2LI  IS62C5128EL-45TLI   IS62WV5128EBLL-45T2LI   IS62WV5128EHBLL-45T2LI/T2L IS62WV5128BLL-55T2LI"]
["512K x 8","2.7V ~ 5.5V","36pin TFBGA (6mm x 8mm)","AS6C4008-55BIN",null,"CY62148EV30LL-45BVXI     ",null,null,"IS62WV5128EBLL-45BLI  IS62WV5128DBLL-45BLI   IS62WV5128EHBLL-45BLI/BL   IS62WV5128BLL-55BLI "]
["256K x 16","2.7V ~ 5.5V","44pin TSOP II","AS6C4016-55ZIN","K6X4016C3F-TF70000","CY62146ELL-45ZSXI                    CY62146ESL-45ZSXI               CY62146EV30LL-45ZSXI\nCY62147EV30LL-45ZSXI      \nCY62146G-45ZSXI                \nCY62147G-45ZSXI                        CY62147G30-45ZSXI/A     \nCY62147GN30-45ZSXI                         \nCY62146GN-45ZSXI(EOL)\nCY62147GE-45ZSXI(EOL)   ","RMLV0414EGSB-4S2  RMLV0416EGSB-4S2","BS616LV4017EIP-55","IS62WV25616BLL-55TLI   IS62WV25616DBLL-45/55TLI   IS65WV25616DBLL-45CTLA1   IS62WV25616EBLL-45/55TLI   IS65WV25616EBLL-45CTLA1"]
["256K x 16","2.7V ~ 3.6V","44pin TSOP II","AS6C4016B-45ZIN","K6X4016T3F-TF70000","CY62146EV30LL-45ZSXI  \nCY62147EV30LL-45ZSXI     \nCY62147G30-45ZSXI/A    \nCY62147GN30-45ZSXI  \nCY62146GN30-45ZSXI(EOL)","RMLV0414EGSB-4S2  RMLV0416EGSB-4S2","BS616LV4017EIP-55","IS62WV25616BLL-55TLI   IS62WV25616DBLL-45/55TLI   IS65WV25616DBLL-45CTLA1   IS62WV25616EBLL-45/55TLI   IS65WV25616EBLL-45CTLA1"]
["256K x 16","2.7V ~ 3.6V","48ball  TFBGA","AS6C4016B-45BIN","K6F4016U6G-EF70000","CY62146EV30LL-45BVXI  \nCY62147EV30LL-45BVXI  \nCY62147G30-45BVXI                 \nCY62147G30-45BVXA(EOL)\nCY62146GN30-45BVXI (EOL)\nCY62147GN30-45BVXI(EOL)","RMLV0416EGBG-4S2","BS616LV4017AIP-55","IS62WV25616BLL-55BLI   IS62WV25616DBLL-45BLI   IS62WV25616EBLL-45/55BLI  IS65WV25616EBLL-45BLA1"]
["256K x 16","2.7V ~ 3.6V","44pin TSOP II","AS6CE4016B-45ZIN","K6X4016T3F-TF70000","CY62146G30-45ZSXI           \nCY62146G-45ZSXA                  \nCY62147G30-45ZSXA                 CY621472G30-45ZSXI/A         \nCY62147GE30-45ZSXI(EOL)","RMLV0414EGSB-4S2  RMLV0416EGSB-4S2","BS616LV4017EIP-55","IS62WV25616EHBLL-45TL/TLI  IS65WV25616EHBLL- 45CTLA1"]
["256K x 16","2.7V ~ 3.6V","48ball  TFBGA","AS6CE4016B-45BIN","K6F4016U6G-EF70000","CY62146G30-45BVXI  \nCY62147EV30LL-45BVXI\nCY62146GE30-45BVXI(EOL)","RMLV0416EGBG-4S2","BS616LV4017AIP-55","IS62WV25616EHBLL-45BLI"]
["8M"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","BRILLIANCE","ISSI"]
["1M x 8","2.7 ~ 5.5V","44pin TSOP II","AS6C8008-55ZIN","K6X8008(C/T)2B-UF55","CY62158EV30LL-45ZSXI   CY62158G30-45ZSXI  \nCY62158ELL-45ZSXI ","RMLV0808BGSB-4S2\nHM62V8100LTTI-5SL","BS62LV8001ECP-55","IS62C10248AL-55TLI   IS62WV10248EBLL-45/55TLI  IS62WV10248EFBLL-45TLI   IS62WV10248HBLL-45TL/TLI  IS62WV10248DBLL-55TLI"]
["1M x 8","2.7 ~ 5.5V","44pin TSOP II","AS6C8008B-45/55ZIN","K6X8008(C/T)2B-UF55","CY62158EV30LL-45ZSXI     CY62158G30-45ZSXI  \nCY62158ELL-45ZSXI   ","RMLV0808BGSB-4S2\nHM62V8100LTTI-5SL","BS62LV8001ECP-55","IS62C10248AL-55TLI   IS62WV10248EBLL-45/55TLI  IS62WV10248EFBLL-45TLI   IS62WV10248HBLL-45TL/TLI  IS62WV10248DBLL-55TLI"]
["1M x 8","2.7 ~ 5.5V","48ball TFBGA","AS6C8008-55BIN",null,"CY62158EV30LL-45BVXI    CY62158G30-45BVXI   CY62158GE30-45BVXI","HM62V8100LBPI-5SL","BS62LV8001ECP-55","IS62C10248AL-55MLI   IS62WV10248EBLL-45/55BLI  IS62WV10248EFBLL-45BLI     IS62WV10248HBLL-45B2L/B2LI  IS62WV10248DBLL-55MLI   IS62WV10248BLL-55BLI "]
["1M x 8","2.7 ~ 3.6V","48ball TFBGA","AS6C8008B-45BIN",null,"CY62158EV30LL-45BVXI","HM62V8100LBPI-5SL","BS62LV8001FIP-55","IS62WV10248EBLL-45/55BLI  IS62WV10248EFBLL-45BLI     IS62WV10248HBLL-45B2L/B2LI  IS62WV10248DBLL-55MLI   IS62WV10248BLL-55BLI "]
["512K x 16","2.7 ~ 5.5V","48ball TFBGA (6 x 8mm)*","AS6C8016-55BIN*","K6F8016U6G-FF55",null,"M5M5W816WG-55HI","BS616LV8017ECP55","IS62WV51216HBLL-45BL/BLI"]
["512K x 16","2.7 ~3.6V","48ball TFBGA (6 x 8mm)**","AS6C8016B-45/55BIN",null,"CY62157EV30LL-45BVXI/A    CY62157G30-45BVXI  ","RMLV0816BGBG-4S2",null,"IS62WV51216EBLL-45/55BLI   IS62WV51216EFBLL-45/55BLI   IS62WV51216HBLL-45B2L/B2LI"]
["512K x 16","2.7 ~ 5.5V","44pin TSOP II","AS6C8016 -55ZIN","K6X8016(C/T)3B-UF55","CY62157EV30LL-45ZSXI/A CY62157ESL-45ZSXI     CY62157ELL-45ZSXI\nCY62157G30-45ZSXI","RMLV0816BGSB-4S2\nHM62165I14LTT-5SL\nM5M5W816TP-55HI","BS616LV8017FCP70","IS62C51216AL-55TLI    IS62WV51216EBLL-45/55TLI   IS62WV51216EFBLL-45/55TLI   IS62WV51216HBLL-45/55TL "]
["512K x 16","2.7 ~3.6V","44pin TSOP II","AS6C8016B-45/55ZIN",null,"CY62157EV30LL-45ZSXI/A   CY62157ESL-45ZSXI    CY62157EV30LL-45ZSXI    CY62157G30-45ZSXI","RMLV0816BGSB-4S2",null,"IS62WV51216EFBLL-45/55TLI    IS62WV51216HBLL-45TL/TLI"]
["512K x 16","2.7 ~ 5.5V","48pin TSOP I","AS6C8016-55TIN",null,"CY62157EV30LL-45ZXI/A    CY62157G30-45ZXI","RMLV0816BGSA-4S2",null,"IS62WV51216GBLL-45TLI   "]
["* = one chip select pin:B5 ** = two chip select pins: B5 and A6"]
["16M"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["1M x 16","2.7 ~ 3.6V","48pin TSOP I","AS6C1616-55TIN\nAS6C1616B-45/55TIN","CY62167E30LL-45/55ZXI   CY62167EV30LL-45/55ZXI    CY62167DV30LL-55ZXI  CY62167EV30LL-45ZXI/A   CY62167G30-45ZXI/A   CY62167GN30-45ZXI ","RMLV1616AGSA-4/5U2   RMLV1616AGBG-5S2    RMLV1616AGSA-5S2 R1LV1616RSA-5/7/8S(EOL)","BS6216LV1611TCP55","IS62WV102416DBLL-45/55TLI     IS62WV102416GBLL-45TLI"]
["1M x 16","2.7 ~ 3.6V","48pin TSOP I","AS6C1616C-45TIN","CY62167E30LL-45/55ZXI\nCY62167EV30LL-45/55ZXI    CY62167DV30LL-55ZXI  CY62167EV30LL-45ZXI/A    CY62167G30-45ZXI/A     CY62167GN30-45ZXI ","RMLV1616AGSA-4/5U2   RMLV1616AGBG-5S2    RMLV1616AGSA-5S2 R1LV1616RSA-5/7/8S(EOL)","BS6216LV1611TCP55","IS62WV102416DBLL-45/55TLI     IS62WV102416GBLL-45TLI"]
["1M x 16","2.7 ~ 3.6V","48ball TFBGA","AS6C1616B-45/55BIN","CY62167DV30LL-70BVXI(EOL)\nCY62167DV30LL-55BVXI    CY62167EV30LL-45BVXI/A   CY62167G30-45BVX/A    CY62167GN30-45BVXI","R1LV1616HBG-4/5SI(EOL)   RMLV1616AGBG-4/5U2  RMLV1616AGBG-5S2","BS6216LV1611FCP70","IS62WV102416FBLL-45/55BLI   IS62WV102416EBLL-45/55BLI"]
["2M x 8","2.7 ~ 3.6V","44pin TSOP I","AS6C1608B-45TIN",null,null,"BS6216LV1600EIP55"]
["2M x 8","2.7 ~ 3.6V","48ball TFBGA","AS6C1608B-45BIN","CY62168EV30LL-45BVXI   CY62168G30-45BVXI   CY62168GN30-45BVXI",null,null,"IS62WV20488EBLL-45/55BLI     IS62WV20488FBLL-45/55BLI"]
["32M"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS"]
["2M x 16","2.7 ~ 3.6V","48pin TSOP I","AS6C3216A-55TIN*","CY62177EV30LL-55ZXI     CY62177G30-55ZXI","RMLV3216AGSA-5S2    R1LV3216RSA-5/7S(EOL)   "]
["2M x 16","2.7 ~ 3.6V","48ball TFBGA","AS6C3216A-55BIN","CY62177EV30LL-55BAXI   CY62177G30-55BAXI        CY62177G30-55BKXI   ","RMWV3216AGBG-5S2 RMLV3216AGBG-5S2"]
["*48pin TSOP I (please note: dual chip select 2Mx16 or 4Mx8)"]
["64M"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS"]
["4M x 16","2.7V ~ 3.6V","48pin TSOP I","AS6C6416-55TIN",null,"RMWV6416AGSA-5S2     R1WV6416RSA-5/7S(EOL)"]
["4M x 16","2.7V ~ 3.6V","48ball BGA","AS6C6416-55BIN","CY62187EV30LL-55BAXI     CY62187G30-55BAXI","RMWV6416AGBG-5S2     R1WV6416RBG-5/7S(EOL)"]
["*48pin TSOP I (please note: dual chip select 4Mx16 or 8Mx8)"]

{"sheet":"Parallel 5V NOR Flash","index":22,"n_rows":16,"n_cols":8,"rows_kept":16,"cut":false,"hidden":false,"merged":[[16,0,16,8]]}
[]
["Parallel 5V NOR Flash"]
["DENSITY","BUS WIDTH","VCC","PACKAGES","TEMPERATURE RANGE","SPEED (NS)","ALLIANCE PART#","REMARKS"]
["1Mb","x8","5V","PLCC 32","-40°C to 85°C",55,"AS29CF010-55CCIN","Uniform Sector, Industrial Grade"]
["4Mb","x8","5V","PLCC 32","-40°C to 85°C",55,"AS29CF040-55CCIN","Uniform Sector, Industrial Grade"]
["4Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 85°C",55,"M29F400FT5AN6E2","Top Boot, Automotive Grade3"]
["4Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 125°C",55,"M29F400FB55N3E2 \nM29F400FB55N3F2","Bottom Boot, Automotive Grade1"]
["8Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 85°C",55,"AS29CF800T-55TIN","Top Boot, Industrial Grade"]
["8Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 85°C",55,"AS29CF800B-55TIN","Bottom Boot, Industrial Grade"]
["8Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 85°C",55,"M29F800FB5AN6E2 \nM29F800FB5AN6F2","Bottom Boot, Automotive Grade3"]
["8Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 125°C",55,"M29F800FT55N3E2","Top Boot, Automotive Grade1"]
["16Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 85°C",55,"AS29CF160B-55TIN","Bottom Boot, Industrial Grade"]
["16Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 85°C",55,"AS29CF160T-55TIN","Top Boot, Industrial Grade"]
["16Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 85°C",55,"M29F160FB5AN6F2","Bottom Boot, Automotive Grade3"]
["16Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 125°C",55,"M29F160FT55N3E2","Top Boot, Automotive Grade1"]
["For Wafer Sales / KGD, contact Alliance Sale Representative"]

{"sheet":"Parallel 5V NOR Falsh Cross Ref","index":23,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[]
["Parallel 5V NOR Flash Cross Reference"]
["DENSITY","VCC","PACKAGE","SPEED (NS)","ALLIANCE","MICRON","CYPRESS/SPANSION","MACRONIX"]
["1Mb","5V","PLCC 32",55,"AS29CF010-55CCIN",null,"AM29F010B* (EOL)"]
["4Mb","5V","PLCC 32",55,"AS29CF040-55CCIN","M29F040","AM29F040B","MX29F040C"]
["4Mb","5V","TSOP 48pin",55,"M29F400FB55N3E2 \nM29F400FB55N3F2","M29F400F","AM29F400BB* (EOL)","MX29F400CBT"]
["4Mb","5V","TSOP 48pin",55,"M29F400FT5AN6E2","M29F400F","AM29F400BT* (EOL)","MX29F400CTT"]
["8Mb","5V","TSOP 48pin",55,"AS29CF800T-55TIN","M29F800F","AM29F800BT* (EOL)","MX29F800C T/B"]
["8Mb","5V","TSOP 48pin",55,"AS29CF800B-55TIN","M29F800F","AM29F800BB* (EOL)","MX29F800C T/B"]
["8Mb","5V","TSOP 48pin",55,"M29F800FB5AN6E2\nM29F800FB5AN6F2","M29F800F","AM29F800BB* (EOL)","MX29F800CBT"]
["8Mb","5V","TSOP 48pin",55,"M29F800FT55N3E2","M29F800F","AM29F800BT* (EOL)","MX29F800CTT"]
["16Mb","5V","TSOP 48pin",55,"AS29CF160T-55TIN","M29F160F","AM29F160DT* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"AS29CF160B-55TIN","M29F160F","AM29F160DB* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"M29F160FB5AN6F2","M29F160F","AM29F160DB* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"M29F160FT55N3E2","M29F160F","AM29F160DT* (EOL)"]

{"sheet":"SLC Parallel NAND Flash","index":24,"n_rows":11,"n_cols":8,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
[]
["SLC Parallel NAND Flash"]
["DENSITY","BUS WIDTH","VCC","PACKAGES","TEMPERATURE RANGE","SPEED (NS)","ALLIANCE","REMARKS"]
["1Gb","x8","3.3V","63b FBGA\n(9x11mm)","Industrial\n(-40°C to 85°C)","25ns","AS9F31G08SA-25BIN","4bit ECC, 2K page, 64B Spare"]
["2Gb","x8","3.3V","63b FBGA\n(9x11mm)","Industrial\n(-40°C to 85°C)","25ns","AS9F32G08SA-25BIN","4bit ECC, 2K page, 128B Spare"]
["4Gb","x8","3.3V","63b FBGA\n(9x11mm)","Industrial\n(-40°C to 85°C)","25ns","AS9F34G08SA-25BIN","4bit ECC, 2K page, 128B Spare"]
["8Gb","x8","3.3V","63b FBGA\n(9x11mm)","Industrial\n(-40°C to 85°C)","25ns","AS9F38G08SA-25BIN","4bit ECC, 2K page, 128B Spare"]
["4Gb","x8","1.8V","63b FBGA\n(9x11mm)","Industrial\n(-40°C to 85°C)","45ns","AS9F14G08SA-45BIN","4bit ECC, 2K page, 128B Spare"]
["8Gb","x8","1.8V","63b FBGA\n(9x11mm)","Industrial\n(-40°C to 85°C)","45ns","AS9F18G08SA-45BIN","4bit ECC, 2K page, 128B Spare, DDP"]
["4Gb","x8","1.8V","63b FBGA\n(9x11mm)","Automotive Grade2\n(-40°C to 105°C)","45ns","AS9F14G08SA-45BAN","4bit ECC, 2K page, 64B Spare"]
["8Gb","x8","1.8V","63b FBGA\n(9x11mm)","Automotive Grade2\n(-40°C to 105°C)","45ns","AS9F18G08SA-45BAN","4bit ECC, 2K page, 128B Spare, DDP"]

{"sheet":"SLC Parallel NAND Flash.Cross R","index":25,"n_rows":11,"n_cols":15,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
[]
["SLC Parallel NAND Flash Cross Reference"]
["DENSITY","VCC","BUS WIDTH","PACKAGE","TEMPERATURE","ALLIANCE","MICRON","SKY HIGH","CYPRESS","WINBOND","MACRONIX","KIOXIA","ISSI","GIGA DEVICES","ESMT"]
["1Gb","3.3V","x8","63b FBGA","-40°C to 85°C","AS9F31G08SA-25BIN","MT29F1G08ABADAH4\nMT29F1G08ABAEAH4","S34SL01G200BFI\nS34ML01G200BFI\nS34ML01G300BFI","S34ML01G100BFI","W29N01HV\nW29N01GV","MX30LF1G18AC","TC58NVG0S3HBA","IS34ML01G084","GD9FU1G8F3AL","F59L1G81MB"]
["2Gb","3.3V","x8","63b FBGA","-40°C to 85°C","AS9F32G08SA-25BIN","MT29F2G08ABAEAH4\nMT29F2G08ABAGAH4","S34SL02G200BFI\nS34ML02G200BFI\nS34ML02G300BFI","S34ML02G100BFI","W29N02GV\nW29N02KV","MX30LF2G18AC","TC58NVG1S3HBA","IS34ML02G084","GD9FU2G8F2AL","F59L2G81A\nF59L2G81KA"]
["4Gb","3.3V","x8","63b FBGA","-40°C to 85°C","AS9F34G08SA-25BIN","MT29F4G08ABADAH4\nMT29F4G08ABAEAH4\nMT29F4G08ABAFAH4","S34SL04G200BFI\nS34ML04G200BFI","S34ML04G100BFI","W29N04GV","MX30LF4G18AC","TC58NVG2S0HBA","IS34ML04G084","GD9FU4G8F2AL","F59L4G81XB"]
["8Gb","3.3V","x8","63b FBGA","-40°C to 85°C","AS9F38G08SA-25BIN","MT29F8G08ADACAH4","S34ML08G201BFI","S34ML08G101BFI","W29N08GV","MX60LF8G18AC","TH58NVG3S0HBA","IS34ML08G088\nIS34ML08G168","GD9FU8G8E2AL","F59D4G81XB\nF59D4G-81KA"]
["4Gb","1.8V","x8","63b FBGA","-40°C to 85°C","AS9F14G08SA-45BIN","MT29F4G08ABBDAH4\nMT29F4G08ABBEAH4\nMT29F4G08ABBFAH4","S34MS04G200BFI","S34MS04G100BFI","W29N04GZ\nW29N04GW","MX30UF4G18AC","TC58NYG2S0HBA","IS34MW04G164","GD9FS4G8F2AL","F59D8G81XB"]
["8Gb","1.8V","x8","63b FBGA","-40°C to 85°C","AS9F18G08SA-45BIN","MT29F8G08ADBCAH4\nMT29F8G08ADBDAH4\nMT29F8G08ABBCAH4\nMT29F8G08ABBDAH4","S34MS08G201BFI","S34MS08G101BFI","W29N08GW\nW29N08GZ","MX60UF8G18AC","TH58NYG3S0HBA","IS34MW08G088\nIS34MW08G168","GD9FS8G8E2AL"]
["4Gb","1.8V","x8","63b FBGA","-40°C to 105°C","AS9F14G08SA-45BAN","MT29F4G08ABBDAH4-A\nMT29F4G08ABBEAH4-A","S34MS04G200BFI","S34MS04G100BFV","W29N04GZ\nW29N04GW",null,null,"IS35MW04G084","GD9FS4G8F2AL"]
["8Gb","1.8V","x8","63b FBGA","-40°C to 105°C","AS9F18G08SA-45BAN","MT29F8G08ADBDAH4-A","S34MS08G201BFA","S34MS08G101BFA","W29N08GW\nW29N08GZ",null,null,null,"GD9FS8G8E2AL"]

{"sheet":"Serial NOR Flash","index":26,"n_rows":28,"n_cols":8,"rows_kept":28,"cut":false,"hidden":false,"merged":[]}
[]
["Serial NOR Flash"]
["DENSITY","BUS WIDTH","VCC","PACKAGES","TEMPERATURE RANGE","SPEED (MHz)","ALLIANCE","REMARKS"]
["2Mb","x1","3.3V","8pin SOIC (150mils)","-40°C to 85°C",75,"M45PE20-VMN6P","PAGE ERASABLE, 2Mb Serial Flash (256K x 8bits, 1024 pages, 4 Sectors), Industrial Grade"]
["8Mb","x1","3.3V","8pin DFN (6x5mm)","-40°C to 85°C",75,"M45PE80-VMP6TG","PAGE ERASABLE 8Mb Serial Flash (1K x 8bits, 4096 pages, 16 Sectors), Industrial Grade, T&R"]
["16Mb","x1","3.3V","8pin SOIC (208mils)","-40°C to 85°C",75,"M45PE16-VMW6TG","PAGE ERASABLE, 16Mb Serial Flash (2K x 8bits, 8192 pages, 32 Sectors), Industrial Grade"]
["4Mb","x1, x2","3.3V","8pin SOIC (150mils)","-40°C to 85°C",104,"AS25F304MD-10S1IN","4Mb, 3.3V Serial NOR Flash, Dual IO, Industrial Grade, 8pin SOIC (150mils) package"]
["16Mb","x1, x2, x4","3.3V","8pin SOIC (150mils)","-40°C to 85°C",104,"AS25F316MQ-10S1IN","16Mb, 3.3V Serial NOR Flash, Multiple IO, Industrial Grade, 8pin SOIC (150mils) Package"]
["32Mb","x1, x2, x4","3.3V","8pin DFN (4x3mm)","-40°C to 125°C",108,"N25Q032A13EF4A0F","32Mb Serial NOR Flash, Multiple IO, 64 Sectors, 4KB Sector Erase, Automotive Grade T&R"]
["32Mb","x1, x2, x4","3.3V","8pin SOIC (150mils)","-40°C to 85°C",108,"N25Q032A13ESC40G","32Mb Serial NOR Flash, Multiple IO, 64 Sectors, 4KB Sector Erase, Industrial Grade, Tube"]
["32Mb","x1, x2, x4","3.3V","8pin SOIC (150mils)","-40°C to 125°C",108,"N25Q032A13ESCA0F","32Mb Serial NOR Flash, Multiple IO, 64 Sectors, 4KB Sector Erase, Automotive Grade, T&R"]
["32Mb","x1, x2, x4","3.3V","16pin SOIC (300mils)","-40°C to 125°C",108,"N25Q032A13ESFA0F","32Mb Serial NOR Flash, Multiple IO, 64 Sectors, 4KB Sector Erase, Automotive Grade, T&R"]
["64Mb","x1, x2, x4","1.8V","8pin SOIC (208mils)","-40°C to 125°C",108,"N25Q064A11ESEA0F","64Mb Serial NOR Flash, Multiple IO, 128 Sectors, 4KB Sector Erase, Automotive Grade T&R"]
["64Mb","x1, x2, x4","3.3V","8pin DFN (6x5mm)","-40°C to 85°C",108,"N25Q064A13EF640E","64Mb Serial NOR Flash, Multiple IO, 128 Sectors, 4KB Sector Erase, Industrial Grade, Tray"]
["64Mb","x1, x2, x4","3.3V","8pin DFN (8x6mm)","-40°C to 125°C",108,"N25Q064A13EF8A0E","64Mb Serial NOR Flash, Multiple IO, 128 Sectors,  4KB Sector Erase, Automotive Grade Tray"]
["64Mb","x1, x2, x4","3.3V","8pin DFN (8x6mm)","-40°C to 125°C",108,"N25Q064A13EF8A0F","64Mb Serial NOR Flash, Multiple IO, 128 Sectors, 4KB Sector Erase, Automotive Grade T&R"]
["64Mb","x1, x2, x4","3.3V","8pin DFN (8x6mm)","-40°C to 85°C*",108,"N25Q064A13EF8H0E","64Mb Serial NOR Flash, Multiple IO, 128 Sectors, 4KB Sector Erase, Industrial Grade High Reliability, Tray"]
["64Mb","x1, x2, x4","3.3V","16pin SOIC (300mils)","-40°C to 125°C",108,"N25Q064A13ESFA0F","64Mb Serial NOR Flash, Multiple IO, 128 Sectors, 4KB Sector Erase, Automotive Grade T&R"]
["64Mb","x1, x2, x4","3.3V","8pin SOIC (208mils)","-40°C to 85°C",104,"AS25F364MQ-10SIN","64Mb, 3.3V Serial NOR Flash, Multiple IO, Default Feature1, Industrial Grade, 8SOIC Wide Body Package"]
["64Mb","x1, x2, x4","3.3V","8L WSON (6x5mm)","-40°C to 85°C",104,"AS25F364MQ-10WIN","64Mb, 3.3V Serial NOR Flash, Multiple IO, Default Feature1, Industrial Grade, 8WSON Package"]
["128Mb","x1, x2, x4","1.8V","8pin SOIC (208mils)","-40°C to 85°C",133,"AS25F1128MQ-70SIN","128Mb, 1.8V Serial NOR Flash, Multiple IO, Default Feature1, Industrial Grade, 8SOIC Wide Body Package"]
["128Mb","x1, x2, x4","1.8V","8L WSON (6x5mm)","-40°C to 85°C",133,"AS25F1128MQ-70WIN","128Mb, 1.8V Serial NOR Flash, Multiple IO, Default Feature1, Industrial Grade, 8WSON Package"]
["128Mb","x1, x2, x4","3.3V","8pin SOIC (208mils)","-40C to 85C",166,"AS25F3128MQ-6SIN","128Mb, 3.3V Serial NOR Flash, Multiple IO, 166MHz DTR, Industrial Grade, 8pin SOIC Wide Body Package, Tube"]
["128Mb","x1, x2, x4","3.3V","8L WSON (6x5mm)","-40C to 85C",166,"AS25F3128MQ-6WINTR","128Mb, 3.3V Serial NOR Flash, Multiple IO, 166MHz DTR, Industrial Grade, 8pad WSON (6x5mm) Package, T&R"]
["256Mb","x1, x2, x4","3.3V","16pin SOIC (300mils)","-40C to 85C",133,"AS25F3256MQ-7S2INTR","256Mb, 3.3V Serial NOR Flash, Multiple IO, 133MHz STR, Industrial Grade, 16pin SOIC (300mils) Package, T&R"]
["256Mb","x1, x2, x4","3.3V","8L WSON (6x8mm)","-40C to 85C",133,"AS25F3256MQ-7W2INTR","256Mb, 3.3V Serial NOR Flash, Multiple IO, 133MHz STR, Industrial Grade, 8pad WSON(6x8mm) Package, T&R"]
["512Mb","x1, x2, x4","3.3V","16pin SOIC (300mils)","-40C to 85C",133,"AS25F3512MQ-7S2INTR","512Mb, 3.3V Serial NOR Flash, Multiple IO, 133MHz STR, Industrial Grade, 16pin SOIC (300mils) Package, T&R"]
["512Mb","x1, x2, x4","3.3V","8L WSON (6x8mm)","-40C to 85C",133,"AS25F3512MQ-7W2INTR","512Mb, 3.3V Serial NOR Flash, Multiple IO, 133MHz STR, Industrial Grade, 8pad WSON (6x8mm) Package, T&R"]

{"sheet":"Serial NOR Flash Cross Ref","index":27,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
[]
["Serial NOR Flash Cross Reference"]

{"sheet":"Serial NAND Flash","index":28,"n_rows":14,"n_cols":8,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
[]
["Serial NAND Flash"]
["DENSITY","BUS WIDTH","SPEED (NS)","VCC","PACKAGES","TEMPERTURE RANGE","TYPE","ALLIANCE PART#"]
["1Gb","x1, x2, x4","120 Mhz","3.3V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","4bit ECC, (2048 + 64) bytes × 64 pages × 1024 blocks","AS5F31G04SND-08LIN"]
["2Gb","x1, x2, x4","100 Mhz","1.8V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","8bit ECC, (2048 + 128) bytes × 64 pages × 2048 blocks","AS5F12G04SND-10LIN"]
["2Gb","x1, x2, x4","120 Mhz","3.3V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","8bit ECC, (2048 + 128) bytes × 64 pages × 2048 blocks","AS5F32G04SNDA-08LIN"]
["2Gb","x1, x2, x4","120 Mhz","3.3V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","4bit ECC, (2048 + 128) bytes × 64 pages × 2048 blocks","AS5F32G04SNDB-08LIN"]
["4Gb","x1, x2, x4","100 Mhz","1.8V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","8bit ECC, (2048 + 128) bytes × 64 pages × 4096 blocks","AS5F14G04SND-10LIN"]
["4Gb","x1, x2, x4","120 Mhz","3.3V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","8bit ECC, (2048 + 128) bytes × 64 pages × 4096 blocks","AS5F34G04SNDA-08LIN"]
["4Gb","x1, x2, x4","120 Mhz","3.3V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","4bit ECC, (2048 + 128) bytes × 64 pages × 4096 blocks","AS5F34G04SNDB-08LIN"]
["8Gb","x1, x2, x4","100 Mhz","1.8V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","8bit ECC, (4096 + 256) bytes × 64 pages × 4096 blocks, t_Sleep 40ms","AS5F18G04SND-10LIN"]
["8Gb","x1, x2, x4","100 Mhz","1.8V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","8bit ECC, (4096+256) bytes × 64 pages × 4096 blocks, t_Sleep 15ms","AS5F18G04SNDB-10LIN"]
["8Gb","x1, x2, x4","120 Mhz","3.3V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","8bit ECC, (4096 + 256) bytes × 64 pages × 4096 blocks","AS5F38G04SND-08LIN"]
["8Gb","x1, x2, x4","120 Mhz","3.3V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","8bit ECC, (4096 + 256) bytes × 64 pages × 4096 blocks","AS5F38G04SNDA-08LIN"]

{"sheet":"Serial NAND Flash Cross Ref","index":29,"n_rows":10,"n_cols":10,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
[]
["Serial NAND Flash Cross Reference"]
["DENSITY","SPEED (NS)","VCC","ALLIANCE","MICRON","TOSHIBA/KIOXIA","WINBOND","MACRONIX","GIGA DEVICES","ISSI"]
["1Gb","120Mhz","3V","AS5F31G04SND-08LIN","MT29F1G01ABAFDWB-IT","TC58CVG0S3HRAIJ","W25N01GV\nW25N01KV","MX35LF1GE4AB\nMX35LF1G24AD","GD5F1GQ4Ux\nGD5F1GQ5Ux\nGD5F1GM7Ux","IS37SML01G1-LLI\nIS37SML01G8A-JJLI"]
["2Gb","100Mhz","1.8V","AS5F12G04SND-10LIN","MT29F2G01ABBGDWB-IT:G","TC58CYG1S3HRAIJ","W25N02JW\nW25M02GW","MX35UF2G14AC\nMX35UF2G24AD\nMX35UF2GE4AC\nMX35UF2GE4AD","GD5F2GQ4Rx\nGD5F2GQ5Rx\nGD5F2GM7Rx","IS37SMW02G8A-JJLI"]
["2Gb","120Mhz","3V","AS5F32G04SNDA-08LIN AS5F32G04SNDB-08LIN","MT29F2G01ABAGDWB-IT","TC58CVG1S3HRAIJ","W25M02GV","MX35LF2G14AC\nMX35LF2GE4AD\nMX35LF2G24AD","GD5F2GQ4Ux\nGD5F2GQ5Ux\nGD5F2GM7Ux","IS37SML02G8A-JJLI"]
["4Gb","100Mhz","1.8V","AS5F14G04SND-10LIN","MT29F4G01ABBFDWB-IT","TC58CYG2S0HRAIJ","W25N04KW","MX35UF4G24AD\nMX35UF4GE4AD","GD5F4GQ6Rx\nGD5F4GM8Rx","IS37SMW04G8A-JJLI"]
["4Gb","120Mhz","3V","AS5F34G04SNDA-08LIN AS5F34G04SNDB-08LIN","MT29F4G01ABAFDWB","TC58CVG2S0HRAIJ","W25N04KV","MX35LF4G24AD\nMX35LF4GE4AD","GD5F4GQ6Ux\nGD5F4GM8Ux","IS37SML04G8A-JJLI"]
["8Gb","100Mhz","1.8V","AS5F18G04SND-10LIN AS5F18G04SNDB-10LIN",null,"TH58CYG3S0HRAIJ",null,null,null,"IS37SMW08G8A-JJLI"]
["8Gb","120Mhz","3V","AS5F38G04SND-08LIN AS5F38G04SNDA-08LIN",null,"TH58CVG3S0HRAIJ",null,null,null,"IS37SML08G8A-JJLI"]

{"sheet":"eMMC","index":30,"n_rows":12,"n_cols":10,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
[]
["eMMC"]
["DENSITY","VCC","VCCQ","BUS WIDTH","MMC INTERFACE","CLOCK FREQUENCY","PACKAGE","NAND TYPE","TEMPERATURE","ALLIANCE"]
["4GB","2.7V~3.6V","1.8V / 3.3V ","x1 , x4 , x8","v5.1","200 MHz","153b FBGA (11.5x13mm)","MLC","Industrial (-40°C to 85°C)","ASFC4G31MA-51BIN"]
["5GB","2.7V~3.6V","1.8V / 3.3V ","x1 , x4 , x8","v5.1","200 MHz","153b FBGA (11.5x13mm)","pSLC (TLC)","Industrial (-40°C to 85°C)","ASFC5G31P3-51BIN"]
["8GB","2.7V~3.6V","1.8V / 3.3V ","x1 , x4 , x8","v5.1","200 MHz","153b FBGA (11.5x13mm)","MLC","Industrial (-40°C to 85°C)","ASFC8G31MA-51BIN"]
["8GB","2.7V~3.6V","1.8V / 3.3V ","x1 , x4 , x8","v5.1","200 MHz","153b FBGA (11.5x13mm)","MLC","Industrial (-40°C to 85°C)","ASFC8G31MB-51BIN*"]
["10GB","2.7V~3.6V","1.8V / 3.3V ","x1 , x4 , x8","v5.1","200 MHz","153b FBGA (11.5x13mm)","pSLC (TLC)","Industrial (-40°C to 85°C)","ASFC10G31P3-51BIN"]
["16GB","2.7V~3.6V","1.8V / 3.3V ","x1 , x4 , x8","v5.1","200 MHz","153b FBGA (11.5x13mm)","MLC","Ext.Commercial (-25°C to 85°C)","ASFC16G31TA-51BCN"]
["32GB","2.7V~3.6V","1.8V / 3.3V ","x1 , x4 , x8","v5.1","200 MHz","153b FBGA (11.5x13mm)","TLC","Industrial (-40°C to 85°C)","ASFC32G31T3-51BIN"]
["64GB","2.7V~3.6V","1.8V / 3.3V ","x1 , x4 , x8","v5.1","200 MHz","153b FBGA (11.5x13mm)","TLC","Industrial (-40°C to 85°C)","ASFC64G31T5-51BIN"]
["128GB","2.7V~3.6V","1.8V / 3.3V ","x1 , x4 , x8","v5.1","200 MHz","153b FBGA (11.5x13mm)","TLC","Industrial (-40°C to 85°C)","ASFC128G32T5-51BIN"]

{"sheet":"eMMC Cross Reference","index":31,"n_rows":11,"n_cols":14,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
[]
["eMMC Cross Reference"]
["DENSITY","Package Type","Temp Grade","ALLIANCE","MICRON","SAMSUNG","KINGSTON","KIOXIA","ISSI","SANDISK","SK HYNIX","MACRONIX","SKY-HIGH","GREENLIANT"]
["4GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC4G31MA-51BIN ","MTFC4GACAJCN (EOL)\nMTFC4GLGDQ (EOL)\nMTFC4GLWDM (EOL)\nMTFC4GMWDM (EOL)","KLM4G1GXXX (EOL)","EMMC04GMK27\nEMMC04GM627\nEMMC04G-W627","THGBMNG5D1LBA","IS21ES04G-JCLI\nIS21ES04G-BCLI","X","H26M31001HPR","MX52LM04A11X","S40FC004C1B","GLS85VM1004"]
["5GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC5G31P3-51BIN","MTFC4GACAJCN (EOL)\nMTFC4GLGDQ (EOL)\nMTFC4GLWDM (EOL)\nMTFC4GMWDM (EOL)","KLM4G1GXXX (EOL)","EMMC04GMK27\nEMMC04GM627\nEMMC04G-W627","THGBMNG5D1LBA","IS21ES04G-JCLI\nIS21ES04G-BCLI","X","H26M31001HPR","MX52LM04A11X","S40FC004C1B","GLS85VM1004"]
["8GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","\nASFC8G31M-51BIN\nASFC8G31MA-51BIN\nASFC8G31MB-51BIN","MTFC8GACAENS (EOL)\nMTFC8GAKAJCN (EOL)\nMTFC8GAMALBH(EOL)\nMTFC8GAMALGT (EOL)\nMTFC8GLWDM (EOL)","KLM8G1GEUF\nKLM8G1GETF\nKLM8G1GESD (EOL)","EMMC08GML36","THGBMJG6C1LBA","IS21ES08GA-JCLI\nIS21ES08GA-BCLI","SDINBDG4-8G","H26M41208HPR","MX52LM08A11X","S40FC008C3B","GLS85VM1008C-M"]
["10GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC10G31P3-51BIN","MTFC8GACAENS (EOL)\nMTFC8GAKAJCN (EOL)\nMTFC8GAMALBH (EOL)\nMTFC8GAMALGT (EOL)\nMTFC8GLWDM (EOL)","KLM8G1GEUF\nKLM8G1GETF\nKLM8G1GESD (EOL)","EMMC08GML36","THGBMJG6C1LBA","IS21ES08GA-JCLI\nIS21ES08GA-BCLI","SDINBDG4-8G","H26M41208HPR","MX52LM08A11X","S40FC008C3B","GLS85VM1008E-S"]
["16GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC16G31TA-51BCN","MTFC16GAKAECN (EOL)\nMTFC16GAKAEJP (EOL)\nMTFC16GAPALBH (EOL)","KLMAG1JETD\nKLMAG2GEUF\nKLMAG2GESD (EOL)","EMMC16G-TB29\nEMMC16G-IB29","THGBMUG7C1LBA\nTHGAMVG7T13BA","IS21TF16G-JCLI\nIS21TF16G-BCLI","SDINBDA6-16G","H26M51002KPR","X","S40FC016C3B","GLS85VM1016C-M"]
["32GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC32G31T3-51BIN","MTFC32GAKAECN (EOL)\nMTFC32GAKAEJP (EOL)\nMTFC32GAZAQHD(EOL)\nMTFC32GAPALBH (EOL)","KLMBG2JETD\nKLMBG4GESD (EOL)","EMMC32G-TX29\nEMMC32G-IX29","THGBMUG8C2LBA\nTHGAMVG8T13BA\nTHGBMJG88C4LBA","IS21TF32G-JCLI\nIS21TF32G-BCLI","SDINBDA6-32G\nSDINBDG4-32G","H26M62002JPR\nH26M64208EM","X","X","GLS85VM1032C-M"]
["64GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC64G31T5-51BIN","MTFC64GAZAQHD (EOL)\nMTFC64GAPALBH (EOL)","KLMCG2KCTA\nKLMCG2UCTA\nKLMCG4JEUD\nKLMCG2UCTB (EOL)\nKLMCG8GESD (EOL)","EMMC64G-TY29\nEMMC64G-IY29","THGAMVG9T23BA\nTHGBMJG9C8LBA","IS21TF64G-JCLI\nIS21TF64G-BCLI","SDINBDA6-64G\nSDINBDG4-64G","H26M74002HMR\nH26M78208CMR","X","X","GLS85VM1064C-M-I"]
["128GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC128G32T5-51BIN","MTFC128GAPALNS(EOL)\nMTFC128GAZAQJP(EOL)","KLMDG4UCTA\nKLMDG8JEUD\nKLMDG4UCTB(EOL)","EMMC128-TY29\nEMMC128-IY29","THGAMVT0T43BA","IS21TF128G-JCLI\nIS21TF128G-BCLI","SDINBDA6-128G","X","X","X","X"]

{"sheet":"Part Numbering System - SRAM ","index":32,"n_rows":48,"n_cols":2,"rows_kept":48,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Go Back To ","Index"]

{"sheet":"Part Numbering System - DRAM ","index":33,"n_rows":50,"n_cols":2,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Go Back To","Index"]

{"sheet":"Part Numbering System- P.NAND","index":34,"n_rows":50,"n_cols":2,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Go Back To","Index"]

{"sheet":"Part Numbering System - P.NOR","index":35,"n_rows":50,"n_cols":2,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Go Back To","Index"]

{"sheet":"Part Numbering System - S.NAND","index":36,"n_rows":50,"n_cols":2,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Go Back To","Index"]

{"sheet":"Part Numbering System-S.NOR","index":37,"n_rows":50,"n_cols":2,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Go Back To","Index"]

{"sheet":"Part Numbering System-eMMC","index":38,"n_rows":50,"n_cols":2,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Go Back To","Index"]

{"sheet":"Alliance Memory Contact","index":39,"n_rows":31,"n_cols":15,"rows_kept":31,"cut":false,"hidden":false,"merged":[[24,0,24,4],[36,10,36,14],[34,16,34,20],[39,10,39,14],[10,14,10,18],[15,0,15,4],[15,7,15,11],[15,14,15,18],[20,7,20,11],[20,14,20,18],[24,7,24,11],[24,14,24,18],[10,7,10,11]]}
[]
["Contact Information"]
["US HEADQUARTERS",null,null,null,null,null,null,null,null,null,null,null,"TAIWAN OFFICE"]
["Alliance Memory , Inc."]
["12815 NE 124th St, Suite #D,\nKirkland, WA  98034, United States",null,null,null,null,null,null,null,null,null,null,null,"No.22, Xingde Road, Dayuan District, Taoyuan City 337, Taiwan"]
["Phone: +1(425) 898 4456",null,null,null,null,null,null,null,null,null,null,null,"Phone: +886 (3) 461-4646"]
["Fax: +1(425) 896 8628"]
[]
[]
["David Bagby | CEO ",null,null,null,null,null,null,"David Lenton | Sales Country Manager",null,null,null,null,null,null,"Dima Lupilin | Sales Director"]
["Email: david@alliancememory.com",null,null,null,null,null,null,"Responsible for business in the UK, Norway, Finland, Sweden and Denmark",null,null,null,null,null,null,"Responsible for business in the Western U.S., Spain , Portugal , Australia,"]
["Garrett Bagby | Marketing Director",null,null,null,null,null,null,"Email: davidl@alliancememory.com\t\t\t\t",null,null,null,null,null,null,"New Zealand."]
["Email: garrett@alliancememory.com",null,null,null,null,null,null,null,null,null,null,null,null,null,"Email: dima@alliancememory.com"]
[]
["Fiona Yao | EMS and Global Account Manager-China",null,null,null,null,null,null,"Kelly Chien | Sales Country Manager",null,null,null,null,null,null,"Linus Park | Sales Director"]
["Responsible for business in China Global Account, Hong Kong, ",null,null,null,null,null,null,"Responsible for business in Taiwan and Vietnam",null,null,null,null,null,null,"Responsible for business in Korea"]
["Singapore, Malaysia, Thailand, the Philippines, and Indonesia.",null,null,null,null,null,null,"Email: kelly@alliancememory.com",null,null,null,null,null,null,"Email:linus@alliancememory.com"]
["Email: fiona@alliancememory.com"]
[]
["Mars Zhang | Sales Director",null,null,null,null,null,null,"Penelope VanUxen | Sales Country Manager",null,null,null,null,null,null,"Ramesh Varadharajan"]
["Responsible for business in China",null,null,null,null,null,null,"Responsible for business in France, Belgium, Netherland",null,null,null,null,null,null,"Responsible for business in India"]
["Email: mars@alliancememory.com",null,null,null,null,null,null,"Email: penelope@alliancememory.com",null,null,null,null,null,null,"Email:ram@alliancememory.com"]
[]
["Ted Kasahara | Sales Director",null,null,null,null,null,null,"Tom Gargan | Sales Director",null,null,null,null,null,null,"Zvi Barak | Sales Director"]
["Responsible for business in Japan",null,null,null,null,null,null,"Responsible for business in the Eastern U.S., Canada, Brazil, and Ireland.",null,null,null,null,null,null,"Responsible for business in Israel, Turkey and Eastern Europe."]
["Email:ted@alliancememory.com",null,null,null,null,null,null,"Email: tom@alliancememory.com",null,null,null,null,null,null,"Email: zvi@alliancememory.com"]
[]
["Electra Sales Corporation"]
["NORTH AMERICA REP"]
["21 Goodway Drive, Rochester, NY 14623"]
["Phone: +1 (585) 217-6496"]