{"text_format":"1","workbook":"xlsx","n_sheets":34,"sheets":["Alliance Selection Guide Index","Master cross Reference","SDRAM","SDRAM Cross Reference","DDR1  SDRAM","DDR1 SDRAM Cross Reference","DDR2 SDRAM","DDR2_SDRAM_Cross_Reference","DDR3 SDRAM ","DDR3 SDRAM Cross Reference","DDR4 SDRAM","DDR4 SDRAM Cross Reference","Mobile LP DRAM-SDRAM","Mobile LP DRAM Cross Reference","LPDDR4-LPDDR4X","LPDDR4-LPDDR4X cross Reference","pSRAM","pSRAM Cross Reference","Fast Asynchronous SRAM","Fast Asyn SRAM Cross Reference","Low Power Asynchronous SRAM","Low Power Asyn SRAM Cross Refer","Parallel 5V NOR Flash","Parallel 5V NOR Falsh Cross Ref","Serial NOR Flash","Serial NOR Flash Cross Ref","Serial NAND Flash","Serial NAND Flash Cross Ref","eMMC","eMMC Cross Reference","Alliance Packaging Quantities","Part Numbering System - SRAM ","Part Numbering System - DRAM ","Alliance Memory Contact"],"not_rendered":{"charts":0,"images":3,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Alliance Selection Guide Index","index":0,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,0,0,1],[32,0,33,0]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Last Update:",{"$f":"TODAY()","v":"2023-02-09"}]
["Last Update by:","Virgia & Ram"]

{"sheet":"Master cross Reference","index":1,"n_rows":417,"n_cols":11,"rows_kept":417,"cut":false,"hidden":false,"merged":[[66,5,66,6]]}
["Synchronous DRAM 3.3V Cross Reference"]
["DENSITY","ORG","ALLIANCE","SAMSUNG (EOL)","MICRON","SK HYNIX (EOL)","ISSI","WINBOND","NANYA (EOL)","ELITE (ESMT)","ELPIDA (EOL)"]
["16Mb","1M x 16","AS4C1M16S-6/7TxN","K4S161622E","MT48LC1M16A1","HY57V161610","IS42S16100","W9816G6TH","NT56V1616AOT","M12L16161A-xTG2Q","EDS1616AGTA"]
["64Mb","4M x 16","AS4C4M16SA-6/7TxN","K4S641632N-UCxx","MT48LC4M16A2P","HY57V641620","IS42S16400","W9864G6JH","NT56V6620C0T-xxB","M12L64164A-xTG2U","uPD4564163G5-Axx"]
["64Mb","4M x 16","AS4C4M16SA-6/7BxN",null,"MT48LCM16A2B4(F4)","HY5V66D","IS42S16400","W9864G6JT",null,"M12L64154A-xBG2C"]
["64Mb","4M x 16","AS4C4M16SA-7B2CN",null,null,null,"IS42S16400","W9864G6JB-7"]
["64Mb","2M x 32","AS4C2M32S-6/7BxN",null,"MT48LC2M32B2B5-x","HY5V62","IS42S32200","W9864G2IB-x",null,null,"EDS6432AFBH"]
["64Mb","2M x 32","AS4C2M32SA-6/7TxN","K4S643232H-Ucxx","MT48LC2M32B2P-x (EOL)","HY57V643220","IS42S32200","W9864G2J(G,I)H-x",null,"M12L64322A-xTG2U","EDS6432AFTA"]
["128Mb","8M x 16","AS4C8M16SA-6/7TxN","K4S281632K-UCxx","MT48LC8M16A2P","HY57V281620","IS42S16800","W9812G6K(G,I)H","NT5SV8M16AT-xxB","M12L128168A-xTG2N","uPD45128163G5-Axx"]
["128Mb","8M x 16","AS4C8M16SA-6/7BxN","K4S281632D-RL75","MT48LC8M16A2B4(F4)","HY5V26","IS42S16800","W9812G6JB",null,"M12L128168A-xBG2N"]
["128Mb","4M x 32","AS4C4M32S-6/7BxN",null,"MT48LC4M32B2B5-x","HY5V22","IS42S32400","W9812G21(G)B-x",null,"M12L128324-xBG2E","EDS1232AHBH"]
["128Mb","4M x 32","AS4C4M32SA-6/7TxN",null,"MT48LC4M32B2P-x (EOL)","HY57V283220T","IS42S32400","W9812G2GH",null,null,"EDS1232AHTA"]
["256Mb","16M x 16","AS4C16M16SA/B-6/7TxN","K4S561632N-UCxx","MT48LC16M16A2P","H57V2562GTR","IS42S16160","W9825G6K(D,E,J)H","NT5SV16M16AT-xxB","M12L2561616A-xTG2A","EDS2516AP(AF,AC)TA-xx"]
["256Mb","16M x 16","AS4C16M16SA-6/7BxN","K4S561632D-RL75","MT48LC16M16A2B4","HY5V56","IS42S16160","W9825G6JB",null,"M12L2561616A-xBG2A","EDS2516EE(JE)BH"]
["256Mb","8M x 32","AS4C8M32S-6/7BTN",null,"MT48LC8M32B2B5-x (EOL)","HY5V52","IS42S32800","W9825G2J(D)B-x",null,null,"EDS2532EEBH"]
["256Mb","8M x 32","AS4C8M32SA-6/7BxN",null,"MT48LC8M32B2B5-x","HY5V52","IS42S32800","W9825G2J(D)B-x",null,null,"EDS2532EEBH"]
["256Mb","32M X 8","AS4C32M8SA-6/7TxN",null,"MT48LC32M8A2P",null,"IS42S83200J"]
["256Mb","64M x 4","AS4C64M4SA-6/7TxN",null,"MT48LC64M4A2P (EOL)",null,"IS42S32800"]
["512Mb","32M x 16","AS4C32M16SB-7BIN",null,null,null,"IS42S16320"]
["512Mb","32M x 16","AS4C32M16SB-7TxN","K4S511632M-TC75","MT48LC32M16A2 (EOL)",null,"IS42S16320",null,null,null,"EDS5116ABTA"]
["512Mb","32M x 16","AS4C32M16SC-7TIN","K4S511632M-TC75","MT48LC32M16A2 (EOL)",null,"IS42S16320",null,null,null,"EDS5116ABTA"]
["512Mb","16M x 32","AS4C16M32SC-7TIN",null,null,null,"IS42S32160"]
["512Mb","64M x 8","AS4C64M8SC-7TIN",null,"MT48LC64M8A2P-75:C (EOL)",null,"IS42S86400"]
["512Mb","64M x 8","AS4C64M8SD-7TCN",null,"MT48LC64M8A2P-75:C (EOL)",null,"IS42S86400"]
[]
[]
[]
["DDR1       2.5V SDRAM Cross Reference"]
["DENSITY","ALLIANCE","SAMSUNG (EOL)","MICRON","ISSI","HYNIX - ALL EOL","WINBOND","NANYA","ELITE (ESMT)","ELPIDA"]
["64Mb","AS4C4M16D1A-5TxN","K4H641638N","MT46V4M16TG (EOL)","IS43R16400B-5TL",null,"W9464G6K(I,J)H",null,"M13S64164A-5TG2Y","(EOL)"]
["64Mb","AS4C2M32D1A-5BxN"]
["128Mb","AS4C8M16D1-5BXN","K4H281638D",null,"IS43R16800E-5BL",null,"W9412G6JB",null,"M13S128168A-5BG2N","EDD1216A"]
["128Mb","AS4C8M16D1A-5TxN","K4H281638D","MT46V8M16 (EOL)","IS43R16800E-5TL","HY5DU1281622","W9412G6K(I,J)H",null,"M13S128168A-5TG2N","EDD1216A"]
["128Mb","AS4C4M32D1A-5BxN",null,"MT46V4M32FK (EOL)","IS43R32400E-5BL",null,"W9412GIB",null,"M13S128324A-5BG2M","EDD1232A"]
["256Mb","AS4C32M8D1-5TxN","K4H560838N","MT46V32M8P (EOL)","IS43R83200","HY5DU56822",null,"NT5DS32M8ES",null,"EDD2508A"]
["256Mb","AS4C16M16D1-5BxN","K4H561638D","MT46V16M16CY-5B","IS43R16160","HY5DU561622","W9425G6JB",null,"M13S2561616A-xBG2A"]
["256Mb","AS4C16M16D1A-5TxN","KH561638D","MT46V16M16P","IS43R16160","HY5DU561622","W945G6K(D,E,J)H",null,"M13S2561616A-xTG2A","EDD2516A"]
["512Mb","AS4C32M16D1-5BxN","K4H511638J","MT46V32M16CY","IS43R16320","HY5DU121622",null,null,null,"EDD5116"]
["512Mb","AS4C32M16D1A-5TxN","K4H511638J","MT46V32M16P","IS43R16320","HY5DU121622",null,"NT5DS32M16ES","M13S5121632A-5TG2S","EDD5116A"]
["512Mb","AS4C64M8D1-5TxN","K4H510838J","MT46V64M8P","IS43R86400","HY5DU12822",null,"NT5DS64M8ES",null,"EDD5108A"]
["512Mb","AS4C64M8D1-5BxN","K4H510838J","MT46V64M8CY(BN)","IS43R86400","HY5DU12822"]
["1Gb","AS4C64M16D1-6TxN",null,"MT46V64M16P (EOL)"]
["1Gb","AS4C64M16D1A-6TxN",null,"MT46V64M16P (EOL)"]
[]
[]
[]
[]
[]
["DDR2    1.8V SDRAM Cross Reference"]
["DENSITY","ALLIANCE","SAMSUNG (EOL)","MICRON","ISSI","WINBOND","NANYA","ELITE (ESMT)","HYNIX (EOL)"]
["256Mb","AS4C16M16D2-25BxN","K4T56163Q","MT47H16M16BG","IS43DR16160","W9725G6K(J)B","NT5TU16M16BG","M14D2561616A-2.5BG","HY5PS561621"]
["512Mb","AS4C32M16D2A/C-25BxN","K4T51163Q","MT47H32M16HR(NF)-25E","IS43DR16320","W9751G6K(J)B","NT5TU32M16GG","M14D5121632A-2.5BG","HY5PS121621"]
["512Mb","AS4C64M8D2-25BxN","K4T51083Q","MT47H64M8CF(SH)-25E","IS43DR86400","W9751G8K(J)B","NT5TU64M8EE",null,"H5PS5182KFR"]
["1Gb","AS4C64M16D2A-25BxN","K4T1G164Q","MT47H64M16HR(NF)-25E","IS43DR16640","W971GG6JB","NT5TU64M16HG","M14D1G1664A-2.5BG","H5PS1G63"]
["1Gb","AS4C64M16D2B-25BCN","K4T1G164Q","MT47H64M16HR(NF)-25E","IS43DR16640","W971GG6JB","NT5TU64M16HG","M14D1G1664A-2.5BG","H5PS1G63"]
["1Gb","AS4C128M8D2A-25BxN","K4T1G084Q","MT47H128M8SH-25E","IS43DR81280","W971GG8JB","NT5TU128M8HE",null,"H5PS1G83"]
["2Gb","AS4C128M16D2-25BxN",null,"MT47H128M16RT-25E","IS43DR16128","W972GG6JB"]
["2Gb","AS4C128M16D2A-25BxN",null,"MT47H128M16RT-25E","IS43DR16128","W972GG6JB"]
["2Gb","AS4C256M8D2A-25BxN",null,"MT47H256M8EB-25E","IS43DR82560","W972GG8JB"]
[]
[]
[]
[]
["DDR3 SDRAM Cross Reference"]
["DENSITY","ALLIANCE","MICRON","SAMSUNG","ISSI","HYNIX","WINBOND","ELITE (ESMT)","ELPIDA","NANYA"]
["512Mb","AS4C32M16D3-12BxN",null,null,null,null,"W6351G6KB-x",null,"EDJ5316BASE"]
["512Mb","AS4C64M8D3-12BxN",null,null,null,null,null,null,"EDJ5308BASE"]
["512Mb","AS4C32M16D3L-12BxN",null,null,null,null,null,null,"EDJ5316BASE"]
["512Mb","AS4C64M8D3L-12BxN",null,null,null,null,null,null,"EDJ5308BASE"]
["1Gb","AS4C64M16D3B-12BxN","MT41J64M16JT(TW)-125 (EOL)","K4B1G1646E(G)","IS43TR16640","H5TQ1G63D","W631GG6KB-x","M15F1G1664A","EDJ1116DJ(BA) BG","NT5CB64M16F(G)P"]
["1Gb","AS4C64M16D3LB/C-12BxN","MT41K64M16JT(TW)-125","K4B1G1646E(G)","IS43TR16640A(B)L","H5TC1G63EFR (EOL)","W631GU6KB-x","M15T1G1664A-(2C)","EDJ1116EJBG","NT5CC64M16F(G)P-DI"]
["1Gb","AS4C128M8D3B-12BxN","MT41J128M8JP(DA)-125","K4B1G0846E(F,G)","IS43TR81280","H5TQ1G83","W631GG8KB-x",null,"EDJ1108DJ(BA) BG","NT5CB128M8F(G)N-DI"]
["1Gb","AS4C128M8D3LB/C-12BxN","MT41K128M8JP(DA)-125","K4B1G0846G-BY","IS43TR81280A(B)L","H5TC1G83EFR (EOL)","W631GU8KB-x",null,"EDJ1108EJBG","NT5CC128M8F(G)N-DI"]
["2Gb","AS4C128M16D3C-93BCN","MT41J128M16JT(TW)-125","K4B2G1646E-B","IS43TR16128","H5TQ2G63","W632GG6KB-x","M15F2G16128A","EDJ2116DEBG","NT5CB128M16I(F)P-DI"]
["2Gb","AS4C128M16D3LC-12BxN","MT41K128M16JT-125","K4B2G1646Q-B","IS43TR16128A(B,C)L","H5TC2G63","W632GU6KB-x",null,"EDJ2116EEBG","NT5CC128M16I(F)P-DI"]
["2Gb","AS4C256M8D3LC-12BxN","MT41K256M8DA-125","K4B2G0846Q-BCK","IS43TR82560A-xBL","H5TQ2G83FFR-x","W632GG8KB-x",null,"EDJ2108DEBG","NT5CB256M8IN-FL"]
["4Gb","AS4C256M16D3C-93BCN AS4C256M16D3C-10BxN AS4C256M16D3C-12BxN","MT41J256M16HA-107 MT41J256M16HA-125","K4B4G1646B(D)","IS43TR16256A","H5TQ4G63","W634GG6MB/ NB","M15F4G16256A","EDJ4216BFBG (BASE)","NT5CB256M16C(D,E) P-DI"]
["4Gb","AS4C256M16D3LC-10BxN AS4C256M16D3LC-12BxN","MT41K256M16HA-107/125 MT41K256M16TW-107/125","K4B4G1646E(Q)","IS43TR16256AL","H5TC4G63","W634GU6MB/NB",null,"EDJ4216EFBG","NT5CC256M16C(D,E) P-DI"]
["4Gb","AS4C512M8D3LC-12BxN","MT41K512M8DA-125","K4B4G0846B(C,D)","IS43TR85120AL","H5TC4G83","W634GU8MB/NB",null,"EDJ4208EFBG","NT5CC512M8C(D,E) N-DI"]
["8Gb","AS4C512M16D3LA-10BxN","MT41K512M16VRN-107 MT41K512M16VRP-107 MT41K512M16HA-125 (EOL)","K4B8G1646x (EOL)","IS43TR16512","H5TC8G63CMR"]
["8Gb","AS4C512M16D3LB-12BxN","MT41K512M16HA-125 (EOL)","K4B8G1646x (EOL)","IS43TR16512","H5TC8G63CMR"]
["8Gb","AS4C1G8D3LA-10BxN","MT41K1G8SN-107/125:E","K4B8G0846x (EOL)","IS43TR81024","H5TC8G83BMR"]
["8Gb","MT41K512M16HA-125","MT41K512M16HA-125","K4B8G1646x (EOL)","IS43TR16512","H5TC8G63CMR"]
[]
[]
["DDR4 SDRAM Cross Reference"]
[]
["DENSITY","ORG","ALLIANCE","MICRON","NANYA","SAMSUNG","HYNIX","ISSI"]
["4Gb","256M x 16","AS4C256M16D4-83BxN","MT40A256M16GE","NT5AD256M16D4","K4A4G165WE","H5AN4G6NBJR","IS43QR16256A/B"]
["4Gb","512M x 8","AS4C512M8D4-83BxN","MT40A512M8RH","NT5AD512M8D4","K4A4G085WE","H5AN4G8NBJR","IS43QR85120B"]
["4Gb","256M x 16","AS4C256M16D4A-75BxN","MT40A256M16GE","NT5AD256M16D4","K4A4G165WE","H5AN4G6NBJR","IS43QR16256A/B"]
["4Gb","512M x 8","AS4C512M8D4A-75BxN","MT40A512M8RH","NT5AD512M8D4","K4A4G085WE","H5AN4G8NBJR","IS43QR85120B"]
["8Gb","512M x 16","AS4C512M16D4-75BxN","MT40A512M16LY/JY","NT5AD512M16C4","K4A8G165WB/C","H5AN8G6NCJR","IS43QR16512A"]
["8Gb","1G x 8","AS4C1G8D4-75BxN","MT40A1G8SA/WE","NT5AD1024M8C3","K4A8G085WB/C","H5AN8G8NCJR","IS43QR81024A"]
[]
[]
["MOBILE LOW POWER SDRAM Cross Reference"]
["DENSITY","ALLIANCE","MICRON","ISSI","NANYA","WINBOND"]
["128Mb","AS4C8M16MSA-6BIN","NA","IS42VM16800H","NA","W987D6HBGX"]
["128Mb","AS4C4M32MSA-6BIN","NA","IS42VM32400H","NA","W987D2HBJX"]
["256Mb","AS4C16M16MSA-6BIN","MT48H16M16LFBF (EOL)","IS42VM16160K","NA","W988D6FBGX"]
["256Mb","AS4C8M32MSA-6BIN","MT48H8M32LFB5 (EOL)","IS42VM32800K","NA","W988D2FBJX"]
["512Mb","AS4C32M16MSA-6BIN","MT48H32M16LFB4-6 IT","IS42VM16320E","NT6SM32M16BG-S1","W989D6DBGX"]
["512Mb","AS4C16M32MSA-6BIN","MT48H16M32LFB5-6 IT","IS42VM32160E","NT6SM16M32BK-S1","W989D2DBJX"]
[]
["MOBILE LP DDR1 Cross Reference"]
["DENSITY","ALLIANCE","MICRON","SAMSUNG","ISSI","HYNIX","NANYA","ELITE (ESMT)","WINBOND"]
["256Mb","AS4C16M16MD1-6BCN","MT46H16M16LFBF-6","K4X56163SPN","IS43LR16160","HY5MS5B6/ H5MS2562","NT6DM16M16AD-T1","M53D2561616A-6BG2F","W948D6FBHX"]
["512Mb","AS4C32M16MD1A-5BCN","MT46H32M16LFBF-5","K4X51163PI","IS43R16320B","HY5MS7B6/ H5MS5162","NT6DM32M16A(B)D-T1","M53D5121632A-5BG2T","W949D6DBHX"]
["512Mb","AS4C16M32MD1-5BxN","MT46H16M32LFB5-5","K4X51323PI","IS43LR32160B","H5MS5132/ H5MS5122","NT6DM16M32A(B)C-T1","M53D5123216A-5BG2S","W949D2DBJX"]
["1Gb","AS4C64M16MD1A-5BIN","MT46H64M16LFBF","K4X1G163PE","IS43LR16640A","H5MS1G62"]
["1Gb","AS4C32M32MD1A-5BIN","MT46H32M32LFB5-5","K4X1G323PF","IS43LR32320B","H5MS1G22","NT6DM32M32BC-T1","M53D1G3232A","W94AD2KBJX"]
["2Gb","AS4C64M32MD1-5BxN","MT46H64M32LFKQ-5","K4X2G323PC","IS43LR32640A","H5M52G22"]
[]
["MOBILE LP DDR2 Cross Reference"]
["DENSITY","ALLIANCE","MICRON","SAMSUNG","ISSI","HYNIX","NANYA","ELITE (ESMT)","WINBOND"]
["256Mb","AS4C8M32MD2A-25B(2)CN",null,null,"IS43LD32800A-25BL",null,null,null,"W978H2KBVX2E"]
["1Gb","AS4C64M16MD2A-25BIN","MT42L64M16D1HE-25",null,"IS43LD16640C/A",null,"NT6TL64M16BA(I)-G0",null,"W97AH6KBVX2"]
["1Gb","AS4C32M32MD2A-25BIN","MT42L32M32D1HE-25",null,"IS43LD32320C/A",null,"NT6TL32M32BI(A)-G0",null,"W97AH2KBVX2"]
["2Gb","AS4C128M16MD2A-25BIN","MT42L128M16D1TK-25",null,"IS43LD16128B",null,"NT6TL128M16CI(A)-G0",null,"W97BH6KBVX2"]
["2Gb","AS4C64M32MD2A-25BIN","MT42L64M32D1TK-25",null,"IS43LD32640B",null,"NT6TL64M32CI(A)-G0",null,"W97BH2KBVX2"]
["4Gb","AS4C128M32MD2A-18BIN","MT42L128M32D1GU-18",null,"IS43LD32128A",null,"NT6TL128M32BI(A)-G0"]
["4Gb","AS4C128M32MD2A-25BIN","MT42L128M32D1GU-18",null,"IS43LD32128A",null,"NT6TL128M32BI(A)-G0"]
[]
[]
["LPDDR4 / LPDDR4X Cross Reference"]
["DENSITY","ORG","ALLIANCE","MICRON","SAMSUNG","HYNIX","NANYA","ISSI","WINBOND"]
["2Gb","128M x 16","AS4C128M16MD4-062BAN",null,null,null,"NT6AN128M16AV","IS43/46LQ16128A","W66BP6NB"]
["4Gb","128M x 32","AS4C128M32MD4-062BAN","MT53B128M32D1DS","K4F4E3S4H",null,"NT6AN128T32AV","IS43/46LQ32128A","W66CP2NQ"]
["4Gb","256M x 16","AS4C256M16MD4-062BAN",null,null,"H9HCNNN4KUMLHR","NT6AN256M16AV","IS43/46LQ16256A","W66CP6NB"]
["8Gb","256M x 32","AS4C256M32MD4-062BAN","MT53B256M32D1DS","K4F8E3S4H",null,"NT6AN256T32AV","IS43/46LQ32256A"]
["8Gb","256M x 32","AS4C256M32MD4V-062BAN","MT53E256M32D2DS","K4U8E3S4AD-GFCL\nK4U8E3S4AD-GHCL",null,"NT6AP256T32AV","IS43/46LQ32256AL\nIS43/46LQ32256EAL","W66DQ2NQU"]
[]
[]
[]
[]
[]
[]
["Fast Asynchronous SRAM Cross Reference"]
[]
["64K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS (EOL)","IDT","ISSI"]
["8K x 8","5V","28pin SOJ (300mil)",15,"AS7C164A-15JxN",null,"CY7C185-15VI (EOL)","IDT7164SXXYG","IS61C64AL-XXJLI"]
["8K x 8","5V","28pin Skinny PDIP 300mil",15,"AS7C164A-15PxN",null,"CY7C185-20PXC (EOL)"]
[]
[]
["256K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS (EOL)","IDT","ISSI"]
["32K x 8","5V","28pin SOJ","10,12,15,20","AS7C256A-xxJCN/JIN","K6E0808C (EOL)","CY7C199D-XXVXI","IDT71256SAXXYG","IS61C256AL-XXJL"]
["32K x 8","5V","28pin TSOP I","10,12,15,20","AS7C256A-xxTCN/TIN",null,"CY7C199D-XXZXI","IDT71256SAXXPZG","IS61C256AL-XXTL"]
["32K x 8","3.3V","28pin SOJ","10,12,15,20","AS7C3256A-xxJCN/JIN","K6E0808V","CY7C1399BN-12VXC","IDT71V256SAXXYG","IS61LV256AL-10JL"]
["32K x 8","3.3V","28pin TSOP I","10,12,15,20","AS7C3256A-xxTCN/TIN",null,"CY7C1399BN-XXZXI","IDT71V256SAXXPZG","IS61LV256AL-10TL"]
["32K x 8","5V","28pin DIP",15,"AS7C256B-xxPIN","(EOL)","CY7C199CN-15PXC (EOL)","IDT71256SAXXTPG"]
[]
[]
["512K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI"]
["32K x 16","5V","44pin SOJ (400MIL)",15,"AS7C513B-xxJCN",null,"CY7C1020D-10VXI",null,"IS61C321AL-12KLI"]
["32K x 16","5V","44pin TSOP II (400MIL)","12,15","AS7C513B-xxTCN",null,"CY7C1020D-10ZSXI",null,"IS61C3216AL-12TLI"]
["32K x 16","3.3V","44pin TSOP II (400MIL)","12,15,20","AS7C3513B-xxTCN",null,"CY7C1020DV33-10ZSXI",null,"IS61WV3216BLL-12TLI"]
["32K x 16","3.3V","44pin SOJ (400MIL)","10,12,15","AS7C3513B-xxJCN",null,"CY7C1020DV33-10VXI"]
[]
["1M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG (EOL)","CYPRESS","IDT","ISSI","GSI (EOL)"]
["128K x 8","5V","32pin SOJ (400MIL)","12,15,20","AS7C1025B-xxJCN/JIN","K6R1008C1D-KI10",null,"IDT71124SXXYG"]
["128K x 8","3.3V","32pin SOJ (400MIL)","10,12,15,20","AS7C31025B-xxJCN/JIN","K6R1008V1D-KI10","CY7C1019DV33-10VXI","IDT71V124SAXXYG","IS63WV1024L-10KLI"]
["128K x 8","3.3V","32pin TSOP II",12,"AS7C31025C-12TIN","K6R1008V1D-UIXX","CY7C1019DV33-XXZSXI","IDT71V124SAXXPHG","IS63WV1288DBLLXXTLI"]
["128K x 8","5V","32pin SOJ (300MIL)","10,12,15,20","AS7C1025B-xxTJCN",null,"CY7C1019D-10VXI"]
["128K x 8","5V","32pin SOJ (400MIL)",15,"AS7C1025C-15JIN"]
["128K x 8","3.3V","32pin SOJ (400MIL)",12,"AS7C31025C-12JIN"]
["128K x 8","3.3V","32pin SOJ (300MIL)","10,12,15,20","AS7C31025B-xxTJCN",null,"CY7C1018DV33-10VXI","IDT71V124SAXXTYG","IS63WV1288DBLL-10JLI"]
["128K x 8","5V","32pin SOJ (400MIL)","12,15,20","AS7C1024B-xxJCN/JIN",null,"CY7C109D-10VXI","IDT71024SXXYG","IS61C1024AL-12KLI"]
["128K x 8","5V","32pin TSOP I","12,15,20","AS7C1024B-xxTCN",null,"CY7C109D-10ZXI",null,"IS61C1024AL-12TLI"]
["128K x 8","5V","32pin SOJ (300MIL)","12,15,20","AS7C1024B-xxTJCN",null,"CY7C1009D-10VXI","IDT71024SXXTYG","IS61C1024AL-12JLI"]
["128K x 8","5V","32pinSOJ(300MIL/400MIL)",12,"AS7C1024C-12JIN",null,"CY7C1019D-10VXI",null,"IS61C1024AL-12KLI"]
["128K x 8","3.3V","32pin SOJ (400MIL)","12,15,20","AS7C31024B-xxJCN",null,"CY1019DV33-10VXI",null,"IS63WV1288DBLL-10KLI"]
["128K x 8","3.3V","32pin TSOP I","10,12,15,20","AS7C31024B-xxTCN",null,null,null,"IS63WV1288DBLL-10HLI"]
["128K x 8","3.3V","32pin SOJ (300MIL)","10,12,15,20","AS7C31024B-xxTJCN",null,"CY7C1018DV33-10VXI",null,"IS63WV1288DBLL-10JLI"]
["64K x 16","5V","44pin SOJ (400MIL)","10,12,15,20","AS7C1026B/C-xxJCN/JIN","K6R1016C1D-KI10","CY7C1021D-XXVXC","IDT71016SXXYG","IS61C6416AL-12KLI"]
["64K x 16","5V","44pin TSOP II (400MIL)","10,12,15,20","AS7C1026B/C-xxTCN/TIN","K6R1016C1D-UI10","CY7C1021D-XXZSXI","IDT71016SXXPHG","IS61C6416AL-12TLI"]
["64K x 16","3.3V","44pin SOJ (400MIL)","10,12,15,20","AS7C31026B/C-xxJCN/TIN","K6R1016V1D-KI10","CY7C1021DV33-XXVXI","IDT71V016SAXXYG","IS61WV6416DBLL-10KLI"]
["64K x 16","3.3V","44pin TSOP II (400MIL)","10,12,15,20","AS7C31026B/C-xxTCN/TIN","K6R1016V1D-UI10","CY7C1021DV33-XXZSXI","IDT71V016SAXXPHG","IS61WV6416DBLL-10TLI","GS71116AGP-XX"]
["64K x 16","3.3V","48 ball BGA",12,"AS7C31026C-12BIN"]
[]
["2M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["128K x 16","3.3V","44pin TSOP II","10,12,15,20","AS7C32098A-xxTxN",null,"CY7C1011DV33-10ZSXI",null,"IS61WV12816DBLL-10TL","GS72116AGP-XX"]
["256K x 8","3.3V","44pin TSOP II","10,12,15,20","AS7C32096A-xxTxN",null,"CY7C1010DV33-10ZSXI",null,"IS61WV256EDBLL-10TLI","GS72108AGP-XX"]
[]
["4M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["512K x 8","5V","36pin SOJ (400MIL)","12,15,20","AS7C4096A-xxJxN","K6R4008C1D-KI10","CY7C1049D-10VXI",null,"IS61C5128AL-10KLI"]
["512K x 8","5V","44pin TSOP II (400MIL)","12,15,20","AS7C4096A-xxTxN","K6R4008C1D-UI10",null,null,"IS61C5128AL-10TLI"]
["512K x 8","3.3V","36pin SOJ (400MIL)","8,10,12,15,20","AS7C34096A-xxJxN","K6R4008V1D-KI10","CY7C1049DV33-10VXI","IDT71V424SXXYG","IS61WV5128EDBLL-10KLI"]
["512K x 8","3.3V","44pin TSOP II (400MIL)","10,12,15,20","AS7C34096A-xxTxN","K6R4008V1D-UI10","CY7C1049DV33-10ZSI","IDT71V424SXXPHG","IS61WV5128EDBLL-10TLI","GS74108AGP-XX"]
["512K x 8","2.7 ~ 3.6V","44pin TSOP II",10,"AS7C34096B-10TIN"]
["512K x 8","2.7 ~ 3.6V","36ball TFBGA",10,"AS7C34096B-10BIN"]
["256K x 16","5V","44pin SOJ (400MIL)","12,15,20","AS7C4098A-xxJxN","K6R4016C1D-KI10","CY7C1041D-10VXI",null,"IS61C25616AL-10KLI"]
["256K x 16","5V","44pin TSOP II (400MIL)","12,15,20","AS7C4098A-xxTxN","K6R4016C1D-UI10","CY7C1041D-10ZSXI",null,"IS61C25616AL-10TL"]
["256K x 16","3.3V","44pin SOJ (400MIL)","10,12,15,20","AS7C34098A-xxJxN","K6R4016V1D-KI10","CY7C1041DV33-10VXI","IDT71V416SXXYG","NA"]
["256K x 16","3.3V","44pin TSOP II (400MIL)","8,10,12,15,20","AS7C34098A-xxTxN","K6R4016V1D-UI10","CY7C1041DV33-10ZSXI","IDT71V416SXXPHG","IS61WV25616EDBLL-10TLI","GS74116AGP-XX"]
["256K x 16","3.3V","48ball TFBGA",10,"AS7C34098A-xxBIN",null,"CY7C1041DV33-10BVXI","IDT71V416SXXBE","IS61WV25616EDBLL-10BLI","GS75116AGX-XX"]
["256K x 16","2.7 ~ 3.6V","44pin TSOP II",10,"AS7C34098B-10TIN"]
["256K x 16","2.7 ~ 3.6V","48ball TFBGA",10,"AS7C34098B-10BIN"]
[]
["8M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["512K x 16","3.3V","44pin TSOP II",10,"AS7C38098A-10TIN",null,"CY7C1051DV33-10ZSXI",null,"IS61WV51216BLL-XXTLI"]
["512K x 16","3.3V","48ball TFBGA",10,"AS7C38098A-10BIN",null,"CY7C1051DV33-10BAXI",null,"IS61WV51216BLL-10MLI"]
["256K x 32","3.3V","90ball TFBGA",10,"AS7C325632-10BIN",null,null,null,"IS61WV25632BLL-10BLI"]
["1M x 8","3.3V","44pin TSOP II",10,"AS7C38096A-10TIN",null,"CY7C1059DV33-10ZSXI",null,"IS61WV10248BLL-10TLI"]
["1M x 8","3.3V","48ball TFBGA (different pinout)",10,"AS7C38096A-10BIN"]
["1M x 8","3.3V","48ball TFBGA (different pinout)",10,"AS7C38096B-10BIN",null,null,null,"IS61WV10248BLL-10MLI"]
[]
["16M  FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["1M x 16","3.3V","48pin TSOP I",10,"AS7C316098A-10TIN",null,"CY7C1061GN30-10ZXI",null,"IS61WV102416FBLL-10TLI"]
["1M x 16","3.3V","48ball TFBGA",10,"AS7C316098A-10BIN",null,"CY7C1061GN30-10BV1XI",null,"IS61WV102416FBLL-10BLI"]
["1M x 16","3.3V","54pin TSOP II",10,"AS7C316098B-10TIN",null,"CY7C1061GN30-10ZSXI",null,"IS61WV102416FBLL-10T2LI"]
["1M x 16","3.3V","48ball TFBGA",10,"AS7C316098B-10BIN"]
["2M x 8","3.3V","48pin TSOP I",10,"AS7C316096A-10TIN",null,"CY7C1069GN30-10ZSXI",null,"IS61WV20488FBLL-10T2LI"]
["2M x 8","3.3V","54pin TSOP II",10,"AS7C316096B-10TIN",null,"CY7C1069DV33-10ZSXI"]
["2M x 8","3.3V","44pin TSOP II",10,"AS7C316096C-10TIN",null,null,null,"IS61WV20488FBLL-10TLI"]
["2M x 8","3.3V","48ball TFBGA (1CE)",10,"AS7C316096C-10BIN",null,null,null,"IS61WV20488FBLL-10BLI"]
["2M x 8","3.3V","48ball TFBGA (2CE)",10,"AS7C316096B-10BIN",null,"CY7C1069GN30-10BVXI"]
["512K x 32","3.3V","90ball TFBGA",10,"A7C351232-10BIN",null,null,null,"IS61WV51232BLL-10BLI"]
[]
[]
[]
["64K LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","ZMD","CYPRESS (EOL)","HITACHI (EOL)","NEC (EOL)","HYNIX (EOL)"]
["8K x 8","2.7V ~ 5.5V","28pin 600mil DIP","AS6C6264-55PCN","U6264BDC07LLG1",null,"HM6264BLP",null,"HY6264P"]
["8K x 8","2.7V ~ 5.5V","28pin 330mil SOP","AS6C6264-55SCN","U6264BS2C07LLG1","CY6264-55SNXI","HM6264BLFP","uPD4464","HY6264G"]
["8K x 8","2.7V ~ 5.5V","28pin STSOP (8 x 13.4 mm)","AS6C6264-55STCN"]
[]
["256K LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","ZMD","SAMSUNG (EOL)","CYPRESS (EOL)","RENESAS","BRILLIANCE (EOL)","ISSI"]
["32K x 8","2.7V ~ 5.5V","28pin 600mil DIP","AS6C62256-55PCN","U62256ADC07LLG1","K6X0808C1D-DF55","CY62256NLL-70PXC",null,"BS62LV256PCP-55"]
["32K x 8","2.7V ~ 5.5V","28pin 330mil SOP","AS6C62256-55SxN","U62256AS2C07LLG1","K6X0808C1D-BF55","CY62256NLL-55SNXI","R1LP5256ESP-5S","BS62LV256SCP-55","IS62C256AL-45ULI"]
["32K x 8","2.4V ~ 3.6V","28pin 330mil SOP","AS62V256-70SIN",null,null,"CY62256NVLL-70SNXI","R1LV5256ESP-5S","BS62LV256SCP-55","IS62LV256AL-45ULI"]
["32K x 8","2.7V ~ 5.5V","28pin STSOP (8 x 13.4 mm)","AS6C62256-55STxN",null,"K6X0808C1D-LF55","CY62256NLL-55ZRXI","R1LP5256ESA-5S","BS62LV256STCP-55","IS62LV256AL-45TLI"]
[]
[]
["1M LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","RENESAS","BRILLIANCE (EOL)","NEC (EOL)","ISSI"]
["128K x 8","2 .7V ~ 5.5V","32pin 600mil DIP","AS6C1008-55PCN","K6X1008C2D-DB55",null,null,null,"BS62LV1027PCP-55","uPD431000ACZ-70L"]
["128K x 8","2.7V ~ 5.5V","32pin 450mil SOP","AS6C1008-55SIN","K6X1008C2D-GF55(Lead)/BF","CY62128ELL-45SXI","M5M51008DFP-55HI","R1LP0108ESP-5SI","BS62LV1027SIP-55","uPD431000AGW-70L","IS62C1024AL-35QLI"]
["128K x 8","2.7V ~ 5.5V","32pin TSOP I (8 x 20 mm)","AS6C1008-55TIN","K6X1008C2D-TF55 or PF","CY62128ELL-45ZXI","M5M51008DVP-55HI","R1LP0108ESF-5SI","BS62LV1027TIP-55","uPD431000AGZ-70LL-KKH","IS62C1024AL-35TLI"]
["128K x 8","2.7V ~ 5.5V","32pin STSOP (8 x 13.4 mm)","AS6C1008-55STIN",null,"CY62128ELL-45ZAXI","M5M51008DKV-55HI","R1LP0108ESA-5SI","BS62LV1027STIP-55","uPD431000AGU-B10-9JH","IS62C1024AL-45HLI"]
["64K x 16","2.7V ~ 5.5V","48ball TFBGA","AS6C1016-55BIN","K6F1016U4C-EF55","CY62127DV30LL-55BVXI",null,null,"BS616LV1010AI-70",null,"IS62WV6416DBLL-45BLI"]
["64K x 16","2.7V ~ 5.5V","44pin TSOP II","AS6C1016-55ZIN",null,"CY62126EV30LL-45SXIT",null,null,"BS616LV1010EI-70",null,"IS62WV6416DBLL-45TLI"]
[]
["2M LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["256K x 8","3.3V","32pin 450mil SOP","AS6C2008-55SIN",null,"CY62138FV30LL-45SXI",null,null,"BS62LV2006SIP-55"]
["256K x 8","3.3V","32pin TSOP I (8 x 20 mm)","AS6C2008-55TIN",null,"CY62138FV30LL-45ZXI",null,null,"BS62LV2006TIP-55","IS62WV2568BLL-55TLI"]
["256K x 8","3.3V","32pin STSOP (8 x 13.4 mm)","AS6C2008-55STIN","K6F2008V2E-LF70000","CY62138FV30LL-45ZAXI","M5M5V208AKV-55HI","R1LV0208BSA-5SI","BS62LV2006STIP-55","IS62WV2568BLL-55HLI"]
["256K x 8","3.3V","36ball TFBGA (6mm x 8mm)","AS6C2008-55BIN",null,"CY62138FV30LL-45BVXI",null,null,null,"IS62WV2568BLL-55B2LI"]
["128K x 16","2.7V ~ 5.5V","44pin TSOP II","AS6C2016-55ZIN",null,"CY62136FVLL-70ZSXI","M5M5V216ATP-70HI","R1LV0216-BSB-5SI","BS616LV2016EIP-55","IS62WV12816BLL-55TLI"]
["128K x 16","3.3V","48ball TFBGA","AS6C2016-55BIN","K6F2016U4E-EF55000","CY62136FVLL-70BVXI",null,null,"BS616LV2019AIG-55","IS62WV12816BLL-55B2LI"]
["256K x 8","2.7V ~ 5.5V","32pin 450mil SOP","AS6C2008A-55SIN",null,"CY2138FV30LL-45SXI",null,null,"BS62LV2006SIP-55"]
["256K x 8","2.7V ~ 5.5V","32pin TSOP I (8 x 20mm)","AS6C2008A-55TIN",null,"CY2138FV30LL-45ZXI",null,null,"BS62LV2006TIP-55","IS62WV256BLL-55TLI"]
["256K x 8","2.7V ~ 5.5V","36ball TFBGA (6mm x 8mm)","AS6C2008A-55BIN",null,"CY62138FV30LL-45BVXI",null,null,null,"IS62WV256BLL-55B2LI"]
[]
["4M LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["512K x 8","2.7 ~ 5.5V","32pin 600mil DIP","AS6C4008-55PCN","K4X4008C1F-DB55",null,null,"BS62LV4006PCP-55"]
["512K x 8","2.7 ~ 5.5V","32pin 450mil SOP","AS6C4008-55SIN","K6X4008C1F-GF55 or BF","CY62148ELL-55SXI","R1LV0408CSP-5SI","BS62LV4006SIP-55","IS62C5128BLL-45QLI"]
["512K x 8","3.3V","32pin 450mil SOP","AS6C4008A-55SIN","K6X4008T1F-GF55 or BF","CY62148EV30LL-55SXI","R1LV0408CSP-5SI","BS62LV4006SIP-55","IS62WV5128DBLL-45QLI"]
["512K x 8","2.7 ~ 5.5V","32pin TSOP I (8 x 20mm)","AS6C4008A-55TIN",null,null,null,"BS62LV4006ECP-55","IS62WV5128EBLL-45QLI"]
["512K x 8","2.7 ~ 5.5V","32pin STSOP (8 x 13.4mm)","AS6C4008-55STIN",null,"CY62148ELL-55ZAXI","R1LV0408DSA-5SI","BS62LV4006STIP-55","IS62C512BL-45HLI"]
["512K x 8","3.3V","32pin STSOP (8 x 13.4mm)","AS6C4008A-55STIN","K6X4008T1F-YF55 or LF","CY62148EV30LL-55ZAXI","R1LV0408DSA-5SI","BS62LV4006STIP-55","IS62WV5128DBLL-45HLI"]
["512K x 8","2.7 ~ 5.5V","32pin TSOP II","AS6C4008-55ZIN","K6X4008C1F-VF55","CY62148ELL-45ZSXI","R1LV0408DSB-5SI","BS62LV4006ECP55","IS62WV5128DBLL-45T2LI"]
["512K x 8","3.3V","32pin TSOP II","AS6C4008A-55ZIN",null,"CY62148DV30",null,null,"IS62WV5128DBLL-55T2L1"]
["512K x 8","2.7 ~ 5.5V","36pin TFBGA (6mm x 8mm)","AS6C4008-55BIN",null,"CY62148EV30LL-55BVXI","RILV0408DBG-5SI",null,"IS62WV5128EBLL-45BLI"]
["512K x 8","3.3V","36pin TFBGA (6mm x 8mm)","AS6C4008A-55BIN",null,"CY62148DV30-55BVXI","R1LV0408DBG-5SI","BS62LV4006HIG-55","IS62WV5128EBLL-45BLI"]
["256K x 16","2.7 ~ 5.5V","44pin TSOP II","AS6C4016-55ZIN","K6X4016C3F-TF70000","CY62146ELL-45ZSXI",null,"BS616LV4017EIP-55","IS62WV5128BLL-55TLI"]
["256K x 16","3.3V","44pin TSOP II","AS6C4016A-55ZIN","K6X4016T3F-TF70000","CY62147EV30LL-45ZSXI","R1LV0414DSB-5SI","BS616LV4017EIP-55","IS62C25616BL-45T2LI"]
["256K x 16","3.3V","48ball  TFBGA","AS6C4016A-55BIN","K6F4016U6G-EF70000","CY62147EV30LL-45BVXI","RMLV0416EGBG-4S2","BS616LV4017AIP-55","IS62WV25616DBLL-45BLI"]
[]
[]
[]
["8M LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","RENESAS","RENESAS","BRILLIANCE","ISSI"]
["1M x 8","2.7 ~ 5.5V","44pin TSOP II","AS6C8008-55ZIN","K6X8008(C/T)2B-UF55","CY62158EV30LL-45ZSXI",null,"R1LV0808ASB-5SI","HM62V8100LTTI-5SL","BS62LV8001ECP-55","IS62WV1024BLL-55TLI"]
["1M x 8","2.7 ~ 5.5V","44pin TSOP II","AS6C8008A-45ZIN","K6X8008(C/T)2B-UF55","CY62158EV30LL-45ZSXI",null,"R1LV0808ASB-5SI","HM62V8100LTTI-5SL","BS62LV8001ECP-55","IS62WV1024BLL-55TLI"]
["1M x 8","2.7 ~ 5.5V","48ball TFBGA","AS6C8008-55BIN",null,"CY62158EV30LL-45BVXI","EOL",null,"HM62V8100LBPI-5SL","BS62LV8001ECP-55","IS62WV1024BLL-55MLI"]
["1M x 8","2.7 ~ 3.6V","48ball TFBGA","AS6C8008A-45BIN",null,"CY62158EV30LL-45BVXI","EOL",null,"HM62V8100LBPI-5SL","BS62LV8001FIP-55","IS62WV1024BLL-55MLI"]
["512K x 16","2.7 ~ 5.5V","48ball TFBGA (6 x 8mm)*","AS6C8016-55BIN*","K6F8016U6G-FF55","CY62157EV30LL-55BVXI","M5M5W816WG-55HI","R1LV0816ABG-5SI",null,"BS616LV8017ECP55","IS62WV51216BLL-55BLI"]
["512K x 16","2.7 ~3.6V","48ball TFBGA (8 x 10mm)**","AS6C8016A-55BIN**",null,"CY2157EV30LL-45BVXIT"]
["512K x 16","2.7 ~ 5.5V","44pin TSOP II","AS6C8016 -55ZIN","K6X8016(C/T)3B-UF55","CY62157EV30LL-55ZSXI","M5M5W816TP-55HI","R1LV0816ASA-5SI","HM62165I14LTT-5SL","BS616LV8017FCP70","IS62WV51216BLL-55T2LI"]
["512K x 16","3.3V","44pin TSOP II","AS6C8016A-55ZIN",null,"CY62157EV30LL-45ZSXIT",null,null,null,null,"IS62WV51216BLL-55T2LI"]
["512K x 16","2.7 ~ 5.5V","48pin TSOP I","AS6C8016-55TIN",null,"CY62157EV30LL-45ZXIT",null,null,null,null,"IS62WV51216GBLL-45TLI"]
[]
["* = one chip select pin:B5 ** = two chip select pins: B5 and A6"]
[]
[]
[]
["16M LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["1M x 16","2.7 ~ 3.6V","48ball TFBGA","AS6C1616-55BIN",null,null,null,"IS62WV102416EBLL-55BLI"]
["1M x 16","2.7 ~ 3.6V","48ball TFBGA","AS6C1616-70BIN","CY62167EV30LL-70BVI","R1LV1616RBG-7SI","BS6216LV1611FCP70","IS62WV102416EBLL-55BLI"]
["1M x 16","2.7 ~ 3.6V","48pin TSOP I","AS6C1616-55TIN","CY62167E30LL-55ZXI","R1LV1616RSA-5SI","BS6216LV1611TCP55"]
["1M x 16","2.7 ~ 3.6V","48ball TFBGA","AS6C1616A-55BIN","CY62167DV30LL-55BVXIT","R1LV1616HBG-4SI",null,"IS62WV102416EBLL-55BLI"]
["2M x 8","2.7 ~ 3.6V","44pin TSOP I","AS6C1608-55TIN","CY62168EV30LL-55ZXI",null,"BS6216LV1600EIP55","IS62WV20488EBLL-55BLI"]
["2M x 8","2.7 ~ 3.6V","48ball TFBGA","AS6C1608-55BIN","CY62168DV30LL-55BVI"]
[]
["32M LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS"]
["2M x 16","2.7 ~ 3.6V","48pin TSOP I","AS6C3216A-55TIN*","CY62177EV30LL-55ZXI","R1LV3216RSA-5SI"]
["2M x 16","2.7 ~ 3.6V","48ball TFBGA","AS6C3216-55BIN AS6C3216A-55BIN","CY62177EV30LL-55BAXI","R1LV3216CSA-5SI"]
["*48pin TSOP I (please note: dual chip select 2Mx16 or 4Mx8)"]
[]
[]
["64M LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS"]
["4M x 16","2.7V ~ 3.6V","48pin TSOP I","AS6C6416-55TIN",null,"R1WV6416RSA-5S"]
["4M x 16","2.7V ~ 3.6V","48ball BGA","AS6C6416-55BIN","CY62187EV30LL-55BAXI","R1WV6416RBG-5S"]
["*48pin TSOP I (please note: dual chip select 4Mx16 or 8Mx8)"]
[]
[]
["Sync SRAM Cross Reference"]
["ORG","DENSITY","PACKAGE","MODE","ALLIANCE","IDT","SAMSUNG","CYPRESS","GSI","ISSI"]
["4M","128K x 36","100TQFP","SPB","AS8C403600-QC150N","71V3576SxxxPFG","K7A403600B-QCxx","CY7C1347G-xxxAX","GS84036AGT-xxx","IS61LPS12836A-xxxTQ"]
["4M","256K x 16","100TQFP",null,"AS8C401800-QC150N","71V3578SxxxPFG","K7A401800B-QCxx","CY7C1327G-xxxAX","GS84018AGT-xxx","IS61LPS25618A-xxxTQ"]
["4M","128K x 36","100TQFP","SB","AS8C403625-QC75N","71V3577SxxPFG","K7B403625B-QCxx","CY7C1345G-xxxAX","GS84036AGT-xxx","IS61LF12836A-xxxTQ"]
["4M","256K x 18","100TQFP",null,"AS8C401825-QC75N","71V3579SxxPFG","K7B401825B-QCxx","CY7C1325G-xxxAX","GS84018AGT-xxx","IS61LF25618A-xxxTQ"]
["4M","128K x 36","100TQFP","ZBT/SPB","AS8C403601-QC166N","71V3556SxxxPFG","K7N403601B-QCxx","CY7C1350G-xxxAX","GS840Z36AGT-xxx","IS61NLP12836A-xxxTQ"]
["4M","256K x 18","100TQFP",null,"AS8C401801-QC166N","71V3558SxxxPFG","K7N401801B-QCxx","CY7C1352G-xxxAX","GS840Z18AGT-xxx","IS61NLP25618A-xxxTQ"]
["9M","256K x 36","100TQFP","SPB","AS8C803600-QC150N","71V67603SxxxPFG","K7A803600B-QCxx","CY7C1360C-xxxAJX","GS88036CT-xxx","IS61LPS25636A-xxxTQ"]
["9M","512K x 18","100TQFP",null,"AS8C801800-QC150N","71V67803SxxxPFG","K7A801800B-QCxx","CY7C1362C-xxxAJX","GS88018CT-xxx","IS61LPS51218A-xxxTQ"]
["9M","256K x 36","100TQFP","SB","AS8C803625-QC75N","71V67703SxxPFG","K7B803625B-QCxx","CY7C1361C-xxxAJX","GS88036CT-xxx","IS61LPS25636A-xxxTQ"]
["9M","256K x 36","100TQFP",null,"AS8C801825-QC75N","71V67903SxxPFG","K7B801825B-QCxx","CY7C1363C-xxxAJX","GS88018CT-xxx","IS61LPS51218A-xxxTQ"]
["9M","512K x 18","100TQFP","ZBT/SPB","AS8C803601-QC150N","71V65603SxxxPFG","K7N803601B-QCxx","CY7C1354C-xxxAJX","GS880Z36CT-xxx","IS61NLP25636A-xxxTQ"]
["9M","512K x 18","100TQFP",null,"AS8C801801-QC150N","71V65803SxxxPFG","K7N801801B-QCxx","CY7C1356C-xxxAJX","GS880Z18CT-xxx","IS61NLP51218A-xxxTQ"]
["9M","256K x 36","100TQFP","ZBT/SB","AS8C803625A-QC75N","71V65703SxxPFG","K7M803625B-QCxx","CY7C1351C-xxxAJX","GS880Z36CT-xxx","N/A"]
["9M","512K x 18","100TQFP",null,"AS8C801825A-QC75N","71V65903SxxPFG","K7M801825B-QCxx","CY7C1353C-xxxAJX","GS880Z18CT-xxx","N/A"]
["18M","512K x 36","100TQFP","ZBT/SPB","AS8C163631-QC166N","71T75602SxxxPFG","K7N163631B-QCxx","CY7C1370D-xxxAX","GS880Z36CT-xxx","IS61LPS12836A-xxxTQ"]
["18M","1M x 18","100TQFP",null,"AS8C161831-QC166N","71T75802SxxxPFG","K7N161831B-QCxx","CY7C1372D-xxxAX","GS880Z18CT-xxx","IS61LPS102418A-xxxTQ"]
[]
[]
[]
["pSRAM Cross Reference"]
[]
["ORG","DENSITY","PACKAGE","COMMENTS/ PREV REV","ALLIANCE","JSC/JEJU","ISSI","FIDELIX","AP MEMORY"]
["8M","512K x 16","48 FPBGA","page mode & Non-DPD","AS1C512K16PL-70BIN","EM784SP16BPP-70LF","IS66WV51216EALL-70BLI"]
["8M","512K x 16","48 FPBGA","Non-page mode & Non-DPD","AS1C512K16P-70BIN","JS784SU16BSP-70LFI","IS66/67WV51216EBLL-70BL","FMP0817CAx"]
["16M","1M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C1M16PL-70BIN","EM7164SP16CSP-70LFI","IS66W1M16EALL-70BLI","FMP1617CCx"]
["16M","1M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C1M16P-70BIN","JS164SU16BSP-70LFI","IS66/67WV1M16EBLL-70BL","FMP1617CAx"]
["32M","2M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C2M16P-70BIN","JS7324SU16BSP-70LFI","IS66WVE2M16EBLL-70B","FMP3217CAx"]
["64M","4M X16","449FBGA","DPD mode","AS1C4M16PL-70BIN","EMC643SP16CKDT-70LF"]
["128M\n(*2-stacked die)","8M X16","49FBGA","DPD mode","AS1C8M16PL-70BIN","JSC283SP16ATDT-70LF",null,null,"APS128XX"]
[]
[]
[]
["Parallel 5V NOR Flash Cross Reference"]
[]
["DENSITY","VCC","PACKAGE","SPEED (NS)","ALLIANCE","Micron","Cypress / Spansion","Macronix"]
["1Mb","5V","PLCC 32",55,"AS29CF010-55CCIN",null,"AM29F010B* (EOL)"]
["2Mb","5V","SOP 44pin",55,"M29F200FB55M3F2","M29F200F","AM29F200BB* (EOL)","MX29F200CBM* (EOL)"]
["4Mb","5V","PLCC 32",55,"AS29CF040-55CCIN","M29F040","AM29F040B","MX29F040C"]
["4Mb","5V","SOP 44pin",55,"M29F400FB55M3F2","M29F400F","AM29F400BB* (EOL)","MX29F400CBM* (EOL)"]
["4Mb","5V","TSOP 48pin",55,"M29F400FB55N3E2 \nM29F400FB55N3F2","M29F400F","AM29F400BB* (EOL)","MX29F400CBT"]
["4Mb","5V","TSOP 48pin",55,"M29F400FT5AN6E2","M29F400F","AM29F400BT* (EOL)","MX29F400CTT"]
["8Mb","5V","TSOP 48pin",55,"AS29CF800T-55TIN","M29F800F","AM29F800BT* (EOL)","MX29F800C T/B"]
["8Mb","5V","TSOP 48pin",55,"AS29CF800B-55TIN","M29F800F","AM29F800BB* (EOL)","MX29F800C T/B"]
["8Mb","5V","TSOP 48pin",55,"M29F800FB5AN6E2\nM29F800FB5AN6F2","M29F800F","AM29F800BB* (EOL)","MX29F800CBT"]
["8Mb","5V","TSOP 48pin",55,"M29F800FT55N3E2","M29F800F","AM29F800BT* (EOL)","MX29F800CTT"]
["8Mb","5V","SOP 44pin",55,"M29F800FB55M3F2","M29F800F","AM29F800BB* (EOL)","MX29F800CBM* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"AS29CF160T-55TIN","M29F160F","AM29F160DT* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"AS29CF160B-55TIN","M29F160F","AM29F160DB* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"M29F160FB5AN6F2","M29F160F","AM29F160DB* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"M29F160FT55N3E2","M29F160F","AM29F160DT* (EOL)"]
[]
[]
[]
["Serial NOR Flash Cross Reference"]
[]
["DENSITY","VCC","PACKAGES","ALLIANCE","MICRON","WINBOND","ADESTO","SPANSION","MACRONIX","ISSI","GigaDevices"]
["2Mb","3V","8pin SOIC Narrow body","M45PE20-VMN6P",null,null,"AT45DB021E"]
["8Mb","3V","8pin DFN (6mm x 5mm)","M45PE80-VMP6TG",null,null,"AT45DB081E"]
["16Mb","3V","8pin SOIC Wide body","M45PE16-VMW6TG",null,null,"AT45DB161E"]
["32Mb","3V","8pin DFN (4mm x 3mm)","N25Q032A13EF4A0F",null,"W25Q32","AT25DF32/AT25SF32","S25FL032A/P","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3V","8pin SOIC Narrow body","N25Q032A13ESC40F",null,"W25Q32","AT25DF32/AT25SF32","S25FL032A/P","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3V","8pin SOIC Narrow body","N25Q032A13ESC40G",null,"W25Q32","AT25DF32/AT25SF32","S25FL032A/P","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3V","8pin SOIC Narrow body","N25Q032A13ESCA0F",null,"W25Q32","AT25DF32/AT25SF32","S25FL032A/P","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3V","16pin SOIC Wide body","N25Q032A13ESFA0F",null,"W25Q32","AT25DF32/AT25SF32","S25FL032A/P","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["64Mb","1.8V","8pin SOIC Wide body","N25Q064A11ESEA0F",null,"W25Q64","AT25SL64/AT25QL64",null,"MX25U64","IS25WP064","GD25LQ64"]
["64Mb","3V","8pin DFN (6mm x 5mm)","N25Q064A13EF640E",null,"W25Q64","AT25SF64/AT25QF64","S25FL064A/P","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3V","8pin DFN (8mm x 6mm)","N25Q064A13EF8A0E",null,"W25Q64","AT25SF64/AT25QF64","S25FL064A/P","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3V","8pin DFN (8mm x 6mm)","N25Q064A13EF8A0F",null,"W25Q64","AT25SF64/AT25QF64","S25FL064A/P","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3V","8pin DFN (8mm x 6mm)","N25Q064A13EF8H0E",null,"W25Q64","AT25SF64/AT25QF64","S25FL064A/P","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3V","16pin SOIC Wide body","N25Q064A13ESFA0F",null,"W25Q64","AT25SF64/AT25QF64","S25FL064A/P","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3V","8pin SOP Wide Body (209mils)","AS25F364MQ-10SIN","N25Q064A13ESE","W25Q64","AT25QF64","S25FL064","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3V","8L WSON (6x5mm)","AS25F364MQ-10WIN","N25Q064A13EF6","W25Q64","AT25QF64","S25FL064","MX25L64","IS25L064","GD25Q64"]
[]
[]
[]
["Serial NAND Flash Cross Reference"]
[]
["DENSITY","SPEED (NS)","ALLIANCE","Toshiba/KIOXIA","Micron","Winbond","Macronix","GigeDevices"]
["1Gb","120Mhz","AS5F31G04SND-08LIN","TC58CVG0S3HRAIJ","MT29F1G01ABAFDWB-IT","W25N01GV","MX35LF1GE4AB","GD5F1GQ4UB/C/E/Fxxx"]
["2Gb","100Mhz","AS5F12G04SND-10LIN","TC58CYG1S3HRAIJ","MT29F2G01ABBGDWB-IT:G","W25N02JW","MX35UF2G14AC","GD5F2GQ4Rx"]
["2Gb","120Mhz","AS5F32G04SND-08LIN","TC58CVG1S3HRAIJ","MT29F2G01ABAGDWB-IT","W25M02GV","MX35LF2G14AC","GD5F2GQ4Ux"]
["4Gb","100Mhz","AS5F14G04SND-10LIN","TC58CYG2S0HRAIJ","MT29F4G01ABBFDWB-IT",null,null,"GD5F4GQ6Rx"]
["4Gb","120Mhz","AS5F34G04SND-08LIN","TC58CVG2S0HRAIJ","MT29F4G01ABAFDWB","W25N04KV","MX35LF4G24AD","GD5F4GQ6Ux"]
["8Gb","100Mhz","AS5F18G04SND-10LIN","TH58CYG3S0HRAIJ"]
["8Gb","120Mhz","AS5F38G04SND-08LIN","TH58CVG3S0HRAIJ"]
[]
[]
[]
["eMMC Cross Reference"]
[]
["DENSITY","ALLIANCE","MICRON","SAMSUNG","HYNIX","Macronix","Kingston","KIOXIA","Sky-High","ISSI"]
["4GB","ASFC4G31M-51BIN","MTFC4Gxxx","KLM4G1Gxxx ","H26M31001HPR","MX52LM04xxx","EMMC04Gxxx","THGBMNG5Dxxx","S40FC004Cxxx","IS21ES04Gxxx"]
["8GB","ASFC8G31M-51BIN","MTFC8Gxxx","KLM8G1Gxxx","H26M41208HPR","MX52LM08xxx","EMMC08Gxxx","THGBMJG6C1xxx","S40FC008Cxxx","IS21ES08Gxxx\nIS21TF08Gxxx"]
["16GB","ASFC16G31M-51BIN","MTFC16Gxxx","KLMAG2Gxxx","H26M51002xxx",null,"EMMC16Gxxx","THGBMUG7C1xxx","S40FC016xxx","IS21TF16Gxxx"]

{"sheet":"SDRAM","index":2,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
["Synchronous DRAM 3.3V  x8,  x16  and  x32"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY (MHz)","TEMPERATURE","ALLIANCE"]
["16Mb","1M x 16","3.3V","50pin TSOP II","143/166 MHz","Commercial, Industrial","AS4C1M16S-6/7 TxN"]
["64Mb","4M x 16","3.3V","54pin TSOP II","143/166/200 MHz","Commercial, Industrial, Automotive","AS4C4M16SA-5/6/7 TxN"]
["64Mb","4M x 16","3.3V","54pin TSOP II","166 MHz","Industrial","AS4C4M16SB-6TIN"]
["64Mb","4M x 16","3.3V","54-ball FBGA / 60-ball FBGA","143/166 MHz","Commercial, Industrial, Automotive","AS4C4M16SA-6/7 BxN, B2xN"]
["64Mb","2M x 32","3.3V","90-ball TFBGA","143/166 MHz","Commercial, Industrial","AS4C2M32S-6/7 BxN"]
["64Mb","2M x 32","3.3V","86pin TSOP II","143/166 MHz","Commercial, Industrial","AS4C2M32SA-6/7 TxN"]
["128Mb","8M x 16","3.3V","54pin TSOP II/54-ball FBGA","143/166 MHz","Commercial, Industrial, Automotive","AS4C8M16SA-6/7 TxN/BxN"]
["128Mb","8M x 16","3.3V","54pin TSOP II","166 MHz","Inudstrial","AS4C8M16SB-6TIN"]
["128Mb","4M x 32","3.3V","90-ball TFBGA","143/166 MHz","Commercial, Industrial","AS4C4M32S-6/7 BxN"]
["128Mb","4M x 32","3.3V","86pin TSOP II","143/166 MHz","Commercial, Industrial","AS4C4M32SA-6/7 TxN"]
["256Mb","16M x 16","3.3V","54pin TSOP II/54-ball FBGA","143/166 MHz","Commercial, Industrial","AS4C16M16SA-6/7 TxN/BxN"]
["256Mb","16M x 16","3.3V","54pin TSOP II/54-ball FBGA","143/166 MHz","Commercial, Industrial","AS4C16M16SB-6/7 TxN/BxN"]
["256Mb","8M x 32","3.3V","86pin TSOP II","143/166 MHz","Commercial, Industrial","AS4C8M32S-6/7 TxN"]
["256Mb","8M x 32","3.3V","90-ball TFBGA","143/166 MHz","Commercial, Industrial","AS4C8M32SA-6/7 BxN"]
["256Mb","32M x 8","3.3V","54pin TSOP II","143/166 MHz","Commercial, Industrial","AS4C32M8SA-6/7 TxN"]
["256Mb","64M x 4","3.3V","54pin TSOP II","143/166 MHz","Commercial, Industrial","AS4C64M4SA-6/7 TxN"]
["512Mb","32M x 16","3.3V","54-ball FBGA","143 MHz","Industrial","AS4C32M16SB-7BIN"]
["512Mb","32M x 16","3.3V","54pin TSOP II","143 MHz/166 MHz","Commercial, Industrial","AS4C32M16SB-6/7 TxN"]
["512Mb","32M x 16","3.3V","54pin TSOP II","143 MHz","Industrial","AS4C32M16SC-7TIN"]
["512Mb","16M x 32","3.3V","86pin TSOP II","143 MHz","Industrial","AS4C16M32SC-7TIN"]
["512Mb","64M x 8","3.3V","54pin TSOP II","143 MHz","Industrial","AS4C64M8SC-7TIN"]
["512Mb","64M x 8","3.3V","54pin TSOP II","133 MHz","Commercial","AS4C64M8SD-7TCN"]
[]
[]
["x = Temperature Range"]
["C = 0°C ~ +70°C"]
["I = -40°C ~ 85°C"]
["A =  -40°C ~ +105°C"]

{"sheet":"SDRAM Cross Reference","index":3,"n_rows":30,"n_cols":11,"rows_kept":30,"cut":false,"hidden":false,"merged":[[32,0,32,2],[35,0,35,2]]}
[]
[]
[]
[]
[]
["SDRAM    Cross Reference"]
[]
["DENSITY","ORG","ALLIANCE","SAMSUNG (EOL)","MICRON","SK HYNIX (EOL)","ISSI","WINBOND","NANYA (EOL)","ELITE (ESMT)","ELPIDA (EOL)"]
["16Mb","1M x 16","AS4C1M16S-6/7TxN","K4S161622E","MT48LC1M16A1","HY57V161610","IS42S16100","W9816G6TH","NT56V1616AOT","M12L16161A-xTG2Q","EDS1616AGTA"]
["64Mb","4M x 16","AS4C4M16SA-6/7TxN\nAS4C4M16SB-6TIN","K4S641632N-UCxx","MT48LC4M16A2P","HY57V641620","IS42S16400","W9864G6JH","NT56V6620C0T-xxB","M12L64164A-xTG2U","uPD4564163G5-Axx"]
["64Mb","4M x 16","AS4C4M16SA-6/7BxN",null,"MT48LC4M16A2P","HY5V66D","IS42S16400","W9864G6JT",null,"M12L64154A-xBG2C"]
["64Mb","4M x 16","AS4C4M16SA-7B2CN",null,null,null,"IS42S16400","W9864G6JB-7"]
["64Mb","2M x 32","AS4C2M32S-6/7BxN",null,"MT48LC2M32B2B5-x","HY5V62","IS42S32200","W9864G2IB-x",null,null,"EDS6432AFBH"]
["64Mb","2M x 32","AS4C2M32SA-6/7TxN","K4S643232H-Ucxx","MT48LC2M32B2P-x (EOL)","HY57V643220","IS42S32200","W9864G2J(G,I)H-x",null,"M12L64322A-xTG2U","EDS6432AFTA"]
["128Mb","8M x 16","AS4C8M16SA-6/7TxN\nAS4C8M16SB-6TIN","K4S281632K-UCxx","MT48LC8M16A2P","HY57V281620","IS42S16800","W9812G6K(G,I)H","NT5SV8M16AT-xxB","M12L128168A-xTG2N","uPD45128163G5-Axx"]
["128Mb","8M x 16","AS4C8M16SA-6/7BxN","K4S281632D-RL75","MT48LC8M16A2B4","HY5V26","IS42S16800","W9812G6JB",null,"M12L128168A-xBG2N"]
["128Mb","4M x 32","AS4C4M32S-6/7BxN",null,"MT48LC4M32B2B5-x","HY5V22","IS42S32400","W9812G21(G)B-x",null,"M12L128324-xBG2E","EDS1232AHBH"]
["128Mb","4M x 32","AS4C4M32SA-6/7TxN",null,"MT48LC4M32B2P-x (EOL)","HY57V283220T","IS42S32400","W9812G2GH",null,null,"EDS1232AHTA"]
["256Mb","16M x 16","AS4C16M16SA/B-6/7TxN","K4S561632N-UCxx","MT48LC16M16A2P","H57V2562GTR","IS42S16160","W9825G6K(D,E,J)H","NT5SV16M16AT-xxB","M12L2561616A-xTG2A","EDS2516AP(AF,AC)TA-xx"]
["256Mb","16M x 16","AS4C16M16SA-6/7BxN","K4S561632D-RL75","MT48LC16M16A2B4","HY5V56","IS42S16160","W9825G6JB",null,"M12L2561616A-xBG2A","EDS2516EE(JE)BH"]
["256Mb","8M x 32","AS4C8M32S-6/7BTN",null,"MT48LC8M32B2B5-x (EOL)","HY5V52","IS42S32800","W9825G2J(D)B-x",null,null,"EDS2532EEBH"]
["256Mb","8M x 32","AS4C8M32SA-6/7BxN",null,"MT48LC8M32B2B5-x","HY5V52","IS42S32800","W9825G2J(D)B-x",null,null,"EDS2532EEBH"]
["256Mb","32M X 8","AS4C32M8SA-6/7TxN",null,"MT48LC32M8A2P(EOL)",null,"IS42S83200J"]
["256Mb","64M x 4","AS4C64M4SA-6/7TxN",null,"MT48LC64M4A2P (EOL)",null,"IS42S32800"]
["512Mb","32M x 16","AS4C32M16SB-7BIN",null,null,null,"IS42S16320"]
["512Mb","32M x 16","AS4C32M16SB-7TxN","K4S511632M-TC75","MT48LC32M16A2 (EOL)",null,"IS42S16320",null,null,null,"EDS5116ABTA"]
["512Mb","32M x 16","AS4C32M16SC-7TIN","K4S511632M-TC75","MT48LC32M16A2 (EOL)",null,"IS42S16320",null,null,null,"EDS5116ABTA"]
["512Mb","16M x 32","AS4C16M32SC-7TIN",null,null,null,"IS42S32160"]
["512Mb","64M x 8","AS4C64M8SC-7TIN",null,"MT48LC64M8A2P-75:C (EOL)",null,"IS42S86400"]
["512Mb","64M x 8","AS4C64M8SD-7TCN",null,"MT48LC64M8A2P-75:C (EOL)",null,"IS42S86400"]

{"sheet":"DDR1  SDRAM","index":4,"n_rows":28,"n_cols":8,"rows_kept":28,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
["DDR1 2.5V SDRAM"]
[]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY (MHz)","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE"]
["64Mb","4M x 16","2.5V","66pin TSOP II","200 MHz","400Mbps/pin","Commercial, Industrial,Automotive","AS4C4M16D1A-5TxN"]
["64Mb","2M x 32","2.5V","144-ball FBGA","200 MHz","400Mbps/pin","Commercial, Industrial","AS4C2M32D1A-5BxN"]
["128Mb","8M x 16","2.5V","66pin TSOP II","200 MHz","400Mbps/pin","Commercial, Industrial","AS4C8M16D1A-5TxN"]
["128Mb","8M x 16","2.5V","60-ball FBGA","200 MHz","400Mbps/pin","Commercial, Industrial","AS4C8M16D1-5BxN"]
["128Mb","4M x 32","2.5V","144-ball FBGA","200 MHz","400Mbps/pin","Commercial, Industrial","AS4C4M32D1A-5BxN"]
["256Mb","16M x 16","2.5V","66pin TSOP II","200 MHz","400Mbps/pin","Commercial","MT46V16M16P5BM"]
["256Mb","16M x 16","2.5V","60-ball FBGA","200 MHz","400Mbps/pin","Commercial, Industrial","AS4C16M16D1-5BxN"]
["256Mb","16M x 16","2.5V","66pin TSOP II","200 MHz","400Mbps/pin","Commercial, Industrial","AS4C32M8D1-5TxN"]
["512Mb","32M x 16","2.5V","66pin TSOP II","200 MHz","400Mbps/pin","Commercial, Industrial,Automotive","AS4C32M16D1A-5TxN"]
["512Mb","32M x 16","2.5V","60-ball FBGA","200 MHz","400Mbps/pin","Commercial, Industrial,Automotive","AS4C32M16D1-5BxN"]
["512Mb","64M x 8","2.5V","66pin TSOP II, 60-ball\nFBGA","200 MHz","400Mbps/pin","Commercial, Industrial","AS4C64M8D1-5TxN/5BxN"]
["1Gb","64M x 16","2.5V","66pin TSOP II, 60-ball\nFBGA","166 MHz","333Mbps/pin","Commercial, Industrial","AS4C64M16D1-6TxN \nAS4C64M16D1A-6TxN/6BxN"]
[]
[]
[]
["x = Temperature Range"]
["C = 0°C ~ +70°C"]
["I =-40 ~ 95°C"]
["A =  -40°C ~ +105°C"]

{"sheet":"DDR1 SDRAM Cross Reference","index":5,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
["DDR1       2.5V SDRAM Cross Reference"]
[]
[]
["DENSITY","ALLIANCE","SAMSUNG (EOL)","MICRON","ISSI","HYNIX - ALL EOL","WINBOND","NANYA","ELITE (ESMT)","ELPIDA"]
["64Mb","AS4C4M16D1A-5TxN","K4H641638N","MT46V4M16TG (EOL)","IS43R16400B-5TL",null,"W9464G6K(I,J)H",null,"M13S64164A-5TG2Y","(EOL)"]
["64Mb","AS4C2M32D1A-5BxN"]
["128Mb","AS4C8M16D1-5BXN","K4H281638D",null,"IS43R16800E-5BL",null,"W9412G6JB",null,"M13S128168A-5BG2N","EDD1216A"]
["128Mb","AS4C8M16D1A-5TxN","K4H281638D","MT46V8M16 (EOL)","IS43R16800E-5TL","HY5DU1281622","W9412G6K(I,J)H",null,"M13S128168A-5TG2N","EDD1216A"]
["128Mb","AS4C4M32D1A-5BxN",null,"MT46V4M32FK (EOL)","IS43R32400E-5BL",null,"W9412GIB",null,"M13S128324A-5BG2M","EDD1232A"]
["256Mb","AS4C16M16D1-5BxN","K4H561638D","MT46V16M16CY-5B","IS43R16160","HY5DU561622","W9425G6JB",null,"M13S2561616A-xBG2A"]
["256Mb","AS4C16M16D1A-5TxN","KH561638D","MT46V16M16P","IS43R16160","HY5DU561622","W945G6K(D,E,J)H",null,"M13S2561616A-xTG2A","EDD2516A"]
["512Mb","AS4C32M16D1-5BxN","K4H511638J","MT46V32M16CY","IS43R16320","HY5DU121622",null,null,null,"EDD5116"]
["512Mb","AS4C32M16D1A-5TxN","K4H511638J","MT46V32M16P","IS43R16320","HY5DU121622",null,"NT5DS32M16ES","M13S5121632A-5TG2S","EDD5116A"]
["512Mb","AS4C64M8D1-5TxN","K4H510838J","MT46V64M8P","IS43R86400","HY5DU12822",null,"NT5DS64M8ES",null,"EDD5108A"]
["512Mb","AS4C64M8D1-5BxN","K4H510838J","MT46V64M8CY(BN)","IS43R86400","HY5DU12822"]
["1Gb","AS4C64M16D1-6TxN",null,"MT46V64M16P (EOL)"]
["1Gb","AS4C64M16D1A-6TxN",null,"MT46V64M16P (EOL)"]

{"sheet":"DDR2 SDRAM","index":6,"n_rows":24,"n_cols":8,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
["DDR2   1.8V SDRAM"]
[]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY (MHz)","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE"]
["256Mb","16M x 16","1.8V","84-ball FBGA","400 MHz","800 Mbps/pin","Commercial, Industrial","AS4C16M16D2-25BxN"]
["512Mb","32M x 16","1.8V","84-ball FBGA","400 MHz","800Mbps/pin","Commercial, Industrial,Automotive","AS4C32M16D2A/C-25BxN"]
["512Mb","64M x 8","1.8V","60-ball FBGA","400 MHz","800Mbps/pin","Commercial, Industrial,Automotive","AS4C64M8D2-25BxN"]
["1Gb","64M x 16","1.8V","84-ball FBGA","400 MHz","800Mbps/pin","Commercial, Industrial,Automotive","AS4C64M16D2A-25BxN"]
["1Gb","64M x 16","1.8V","84-ball FBGA","400 MHz","800Mbps/pin","Commercial","AS4C64M16D2B-25BCN"]
["1Gb","128M x 8","1.8V","60-ball FBGA","400 MHz","800Mbps/pin","Commercial, Industrial","AS4C128M8D2A-25BxN"]
["2Gb","128M x 16","1.8V","84-ball FBGA","400 MHz","800Mbps/pin","Commercial, Industrial","AS4C128M16D2-25BxN"]
["2Gb","128M x 16","1.8V","84-ball FBGA","400 MHz","800Mbps/pin","Commercial, Industrial","AS4C128M16D2A-25BxN"]
["2Gb","256M x 8","1.8V","60-ball FBGA","400 MHz","800Mbps/pin","Commercial","AS4C256M8D2A-25BCN"]
[]
[]
[]
["x = Temperature Range"]
["C = 0°C ~ +95°C"]
["I =  -40°C ~ +95°C"]
["A =  -40°C ~ +105°C"]

{"sheet":"DDR2_SDRAM_Cross_Reference","index":7,"n_rows":18,"n_cols":9,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
["DDR2    1.8V SDRAM Cross Reference"]
[]
[]
["DENSITY","ALLIANCE","SAMSUNG (EOL)","MICRON","ISSI","WINBOND","NANYA","ELITE (ESMT)","HYNIX (EOL)"]
["256Mb","AS4C16M16D2-25BxN","K4T56163Q","MT47H16M16BG","IS43DR16160","W9725G6K(J)B","NT5TU16M16BG","M14D2561616A-2.5BG","HY5PS561621"]
["512Mb","AS4C32M16D2A/C-25BxN","K4T51163Q","MT47H32M16HR(NF)-25E","IS43DR16320","W9751G6K(J)B","NT5TU32M16GG","M14D5121632A-2.5BG","HY5PS121621"]
["512Mb","AS4C64M8D2-25BxN","K4T51083Q","MT47H64M8CF(SH)-25E","IS43DR86400","W9751G8K(J)B","NT5TU64M8EE",null,"H5PS5182KFR"]
["1Gb","AS4C64M16D2A-25BxN","K4T1G164Q","MT47H64M16HR(NF)-25E","IS43DR16640","W971GG6JB","NT5TU64M16HG","M14D1G1664A-2.5BG","H5PS1G63"]
["1Gb","AS4C64M16D2B-25BCN","K4T1G164Q","MT47H64M16HR(NF)-25E","IS43DR16640","W971GG6JB","NT5TU64M16HG","M14D1G1664A-2.5BG","H5PS1G63"]
["1Gb","AS4C128M8D2A-25BxN","K4T1G084Q","MT47H128M8SH-25E","IS43DR81280","W971GG8JB","NT5TU128M8HE",null,"H5PS1G83"]
["2Gb","AS4C128M16D2-25BxN",null,"MT47H128M16RT-25E","IS43DR16128","W972GG6JB"]
["2Gb","AS4C128M16D2A-25BxN",null,"MT47H128M16RT-25E","IS43DR16128","W972GG6JB"]
["2Gb","AS4C256M8D2A-25BxN",null,"MT47H256M8EB-25E","IS43DR82560","W972GG8JB"]

{"sheet":"DDR3 SDRAM ","index":8,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[[5,0,5,1],[16,0,16,1]]}
[]
[]
[]
[]
[]
["DDR3 1.5V SDRAM"]
[]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY","DATA RATE","TEMPERATURE  OPTIONS","ALLIANCE"]
["512Mb","32M x 16","1.5V","96-ball FBGA","800 MHz","1600 Mbps/pin","Commercial, Industrial","AS4C32M16D3-12BxN"]
["512Mb","64M x 8","1.5V","78-ball FBGA","800 MHz","1600 Mbps/pin","Commercial, Industrial","AS4C64M8D3-12BxN"]
["1Gb","64M x 16","1.5V","96-ball FBGA","800 MHz","1600 Mbps/pin","Commercial, Industrial, Automotive","AS4C64M16D3B-12BxN"]
["1Gb","128M x 8","1.5V","78-ball FBGA","800 MHz","1600 Mbps/pin","Commercial, Industrial, Automotive","AS4C128M8D3B-12BxN"]
["2Gb","128M x 16","1.5V","96-ball FBGA","1066 MHz","2133 Mbps/pin","Commercial","AS4C128M16D3C-93BCN"]
["4Gb","256M x 16","1.5V","96-ball FBGA","800 MHz\n933 MHz\n1066 MHz","1600 Mbps/pin\n1866 Mbps/pin\n2133 Mbps/pin","Commercial, Industrial","AS4C256M16D3C-xxBxN"]
[]
[]
["DDR3L 1.35V SDRAM"]
[]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE"]
["512Mb","32M x 16","1.35V","96-ball FBGA","800 MHz","1600 Mbps/pin","Commercial, Industrial","AS4C32M16D3L-12BxN"]
["512Mb","64M x 8","1.35V","78-ball FBGA","800 MHz","1600 Mbps/pin","Commercial, Industrial","AS4C64M8D3L-12BxN"]
["1Gb","64M x 16","1.35V","96-ball FBGA","800 MHz","1600 Mbps/pin","Commercial, Industrial, Automotive","AS4C64M16D3LB/C-12BxN"]
["1Gb","128M x 8","1.35V","78-ball FBGA","800 MHz","1600 Mbps/pin","Commercial, Industrial, Automotive","AS4C128M8D3LB/C-12BxN"]
["2Gb","128M x 16","1.35V","96-ball FBGA","800 MHz","1600 Mbps/pin","Commercial, Industrial, Automotive","AS4C128M16D3LC-12BxN"]
["2Gb","256M x 8","1.35V","78-ball FBGA","800 MHz","1600 Mbps/pin","Commercial, Industrial, Automotive","AS4C256M8D3LC-12BxN"]
["4Gb","256M x 16","1.35V","96-ball FBGA","800 MHz\n933 MHz","1600 Mbps/pin\n1833 Mbps/pin","Commercial, Industrial, Automotive","AS4C256M16D3LC-xxBxN"]
["4Gb","512M x 8","1.35V","78-ball FBGA","800 MHz","1600 Mbps/pin","Commercial, Industrial, Automotive","AS4C512M8D3LC-12BxN"]
["8Gb","512M x 16","1.35V","96-ball FBGA","933 MHz","1866 Mbps/pin","Commercial, Industrial, Automotive","AS4C512M16D3LA-10BxN"]
["8Gb","512M x 16","1.35V","96-ball FBGA","800 / 933 MHz","1600 / 1866 Mbps/pin","Commercial, Industrial","AS4C512M16D3LB/C-10/12BxN"]
["8Gb","1G x 8","1.35V","78-ball FBGA","933 MHz","1866 Mbps/pin","Commercial, Industrial, Automotive","AS4C1G8D3LA-10BxN"]
[]
["x = Temperature Range"]
["C = 0°C ~ +95°C (Extended) "]
["I =  -40°C ~ +95°C"]
["A =  -40°C ~ +105°C"]

{"sheet":"DDR3 SDRAM Cross Reference","index":9,"n_rows":27,"n_cols":10,"rows_kept":27,"cut":false,"hidden":false,"merged":[[10,5,10,6]]}
[]
[]
[]
[]
[]
[]
["DDR3 SDRAM Cross Reference"]
[]
["DENSITY","ALLIANCE","MICRON","SAMSUNG","ISSI","HYNIX","WINBOND","ELITE (ESMT)","ELPIDA","NANYA"]
["512Mb","AS4C32M16D3-12BxN",null,null,null,null,"W6351G6KB-x","M15F5121632A","EDJ5316BASE"]
["512Mb","AS4C64M8D3-12BxN",null,null,null,null,null,null,"EDJ5308BASE"]
["512Mb","AS4C32M16D3L-12BxN",null,null,null,null,null,"M15T5121632A","EDJ5316BASE"]
["512Mb","AS4C64M8D3L-12BxN",null,null,null,null,null,null,"EDJ5308BASE"]
["1Gb","AS4C64M16D3B-12BxN","MT41J64M16JT(TW)-125 (EOL)","K4B1G1646E(G)","IS43TR16640","H5TQ1G63D","W631GG6KB-x","M15F1G1664A","EDJ1116DJ(BA) BG","NT5CB64M16F(G)P"]
["1Gb","AS4C64M16D3LB/C-12BxN","MT41K64M16JT(TW)-125","K4B1G1646E(G)","IS43TR16640A(B)L","H5TC1G63EFR (EOL)","W631GU6KB-x","M15T1G1664A-(2C)","EDJ1116EJBG","NT5CC64M16F(G)P-DI"]
["1Gb","AS4C128M8D3B-12BxN","MT41J128M8JP(DA)-125","K4B1G0846E(F,G)","IS43TR81280","H5TQ1G83","W631GG8KB-x",null,"EDJ1108DJ(BA) BG","NT5CB128M8F(G)N-DI"]
["1Gb","AS4C128M8D3LB/C-12BxN","MT41K128M8JP(DA)-125","K4B1G0846G-BY","IS43TR81280A(B)L","H5TC1G83EFR (EOL)","W631GU8KB-x",null,"EDJ1108EJBG","NT5CC128M8F(G)N-DI"]
["2Gb","AS4C128M16D3C-93BCN","MT41J128M16JT(TW)-125","K4B2G1646E-B","IS43TR16128","H5TQ2G63","W632GG6KB-x","M15F2G16128A","EDJ2116DEBG","NT5CB128M16I(F)P-DI"]
["2Gb","AS4C128M16D3LC-12BxN","MT41K128M16JT-125","K4B2G1646Q-B","IS43TR16128A(B,C)L","H5TC2G63","W632GU6KB-x",null,"EDJ2116EEBG","NT5CC128M16I(F)P-DI"]
["2Gb","AS4C256M8D3LC-12BxN","MT41K256M8DA-125","K4B2G0846Q-BCK","IS43TR82560A-xBL","H5TQ2G83FFR-x","W632GG8KB-x",null,"EDJ2108DEBG","NT5CB256M8IN-FL"]
["4Gb","AS4C256M16D3C-93BCN AS4C256M16D3C-10BxN AS4C256M16D3C-12BxN","MT41J256M16HA-107 MT41J256M16HA-125","K4B4G1646B(D)","IS43TR16256A","H5TQ4G63","W634GG6MB/ NB","M15F4G16256A","EDJ4216BFBG (BASE)","NT5CB256M16C(D,E) P-DI"]
["4Gb","AS4C256M16D3LC-10BxN AS4C256M16D3LC-12BxN","MT41K256M16HA-107/125 MT41K256M16TW-107/125","K4B4G1646E(Q)","IS43TR16256AL","H5TC4G63","W634GU6MB/NB",null,"EDJ4216EFBG","NT5CC256M16C(D,E) P-DI"]
["4Gb","AS4C512M8D3LC-12BxN","MT41K512M8DA-125","K4B4G0846B(C,D)","IS43TR85120AL","H5TC4G83","W634GU8MB/NB",null,"EDJ4208EFBG","NT5CC512M8C(D,E) N-DI"]
["8Gb","AS4C512M16D3LA-10BxN\nAS4C512M16D3LC-10BxN","MT41K512M16VRN-107 MT41K512M16VRP-107 MT41K512M16HA-125 (EOL)","K4B8G1646x (EOL)","IS43TR16512","H5TC8G63CMR",null,"M15T8G16512A"]
["8Gb","AS4C512M16D3LB-12BxN\nAS4C512M16D3LC-12BxN","MT41K512M16HA-125 (EOL)","K4B8G1646x (EOL)","IS43TR16512","H5TC8G63CMR",null,"M15T8G16512A"]
["8Gb","AS4C1G8D3LA-10BxN","MT41K1G8SN-107/125:E","K4B8G0846x (EOL)","IS43TR81024","H5TC8G83BMR"]
["8Gb","MT41K512M16HA-125","MT41K512M16HA-125","K4B8G1646x (EOL)","IS43TR16512","H5TC8G63CMR",null,"M15T8G16512A"]

{"sheet":"DDR4 SDRAM","index":10,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
["DDR4 SDRAM"]
[]
["DENSITY","ORG","VCC","PACKAGES","CLOCK FREQUENCY","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE"]
["4Gb","256M x 16","1.2V","96-ball FBGA","1200 MHz\n1333 MHz","2400 Mbps/pin\n2600 Mbps/pin","Commercial, Industrial","AS4C256M16D4-75/83BxN"]
["4Gb","512M x 8","1.2V","78-ball FBGA","1200 MHz\n1333 MHz","2400 Mbps/pin","Commercial, Industrial","AS4C512M8D4-75/83BxN"]
["4Gb","256M x 16","1.2V","96-ball FBGA","1333 MHz\n1600 MHz","2666 Mbps/pin\n3200 Mbps/pin","Commercial, Industrial","AS4C256M16D4A-62/75BxN"]
["4Gb","512M x 8","1.2V","78-ball FBGA","1333 MHz","2666 Mbps/pin","Commercial, Industrial","AS4C512M8D4A-75BxN"]
["8Gb","512M x 16","1.2V","96-ball FBGA","1333 MHz","2666 Mbps/pin","Commercial, Industrial","AS4C512M16D4-75BxN"]
["8Gb","1G x 8","1.2V","78-ball FBGA","1333 MHz","2666 Mbps/pin","Commercial, Industrial","AS4C1G8D4-75BxN"]
["16Gb","1G x 16","1.2V","96-ball FBGA","1600 MHz","3200 Mbps/pin","Commercial","MT40A1G16KH-062E"]
["16Gb","1G x 16","1.2V","96-ball FBGA","1600 MHz","3200 Mbps/pin","Commercial","AS4C1G16D4-062BCN"]

{"sheet":"DDR4 SDRAM Cross Reference","index":11,"n_rows":13,"n_cols":8,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["DDR4 SDRAM Cross Reference"]
[]
["DENSITY","ORG","ALLIANCE","MICRON","NANYA","SAMSUNG","HYNIX","ISSI"]
["4Gb","256M x 16","AS4C256M16D4-75/83BxN","MT40A256M16GE","NT5AD256M16D4","K4A4G165WE","H5AN4G6NBJR","IS43QR16256A/B"]
["4Gb","512M x 8","AS4C512M8D4-75/83BxN","MT40A512M8RH","NT5AD512M8D4","K4A4G085WE","H5AN4G8NBJR","IS43QR85120B"]
["4Gb","256M x 16","AS4C256M16D4A-62/75BxN","MT40A256M16GE","NT5AD256M16D4","K4A4G165WE","H5AN4G6NBJR","IS43QR16256A/B"]
["4Gb","512M x 8","AS4C512M8D4A-75BxN","MT40A512M8RH","NT5AD512M8D4","K4A4G085WE","H5AN4G8NBJR","IS43QR85120B"]
["8Gb","512M x 16","AS4C512M16D4-75BxN","MT40A512M16LY/JY","NT5AD512M16C4","K4A8G165WB/C","H5AN8G6NCJR","IS43QR16512A"]
["8Gb","1G x 8","AS4C1G8D4-75BxN","MT40A1G8SA/WE","NT5AD1024M8C3","K4A8G085WB/C","H5AN8G8NCJR","IS43QR81024A"]
["16Gb","1G x 16","MT40A1G16KH-062E\nAS4C1G16D4-062BCN","MT40A1G16KH/KNR",null,"K4AAG165WA-BCWE","H5ANAG6NCMR-XNC\nH5ANAG6NDMR-XNC"]

{"sheet":"Mobile LP DRAM-SDRAM","index":12,"n_rows":36,"n_cols":8,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
["MOBILE LOW POWER SDRAM"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY","TEMPERATURE OPTIONS","ALLIANCE"]
["128Mb","8M x 16","1.7V ~ 1.95V","54-ball FBGA (8 x 8mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C8M16MSA-6BIN"]
["128Mb","4M x 32","1.7V ~ 1.95V","90-ball FBGA (8 x 13mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C4M32MSA-6BIN"]
["256Mb","16M x 16","1.7V ~ 1.95V","54-ball FBGA (8 x 8mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C16M16MSA-6BIN"]
["256Mb","8M x 32","1.7V ~ 1.95V","90-ball FBGA (8 x 13mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C8M32MSA-6BIN"]
["256Mb","8M x 32","1.7V ~ 1.95V","90-ball FBGA (8 x 13mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C8M32MSB-6BIN"]
["512Mb","32M x 16","1.7V ~ 1.95V","54-ball FBGA (8 x 9mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C32M16MSA-6BIN"]
["512Mb","16M x 32","1.7V ~ 1.95V","90-ball FBGA (8 x 13mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C16M32MSA-6BIN"]
["512Mb","16M x 32","1.7V ~ 1.95V","90-ball FBGA (8 x 13mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C16M32MSB-6BIN"]
[]
[]
["MOBILE LP DDR"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE"]
["256Mb","16M x 16","1.8V","60-ball FBGA","166 MHz","333Mbps/pin","Extended -30°C ~ +85°C","AS4C16M16MD1-6BCN"]
["512Mb","32M x 16","1.8V","60-ball FPBGA","200 MHz","400Mbps/pin","Extended -30°C ~ +85°C","AS4C32M16MD1A-5BCN"]
["512Mb","16M x 32","1.8V","90-ball FPBGA","200 MHz","400Mbps/pin","Extended -25°C ~ +85°C   ","AS4C16M32MD1-5BCN"]
["1Gb","64M x 16","1.8V","60-ball FPBGA","200 MHz","400Mbps/pin","Industrial  -40°C ~ +85°C","AS4C64M16MD1A-5BIN"]
["1Gb","32M x 32","1.8V","90-ball FPBGA","200 MHz","400Mbps/pin","Industrial  -40°C ~ +85°C","AS4C32M32MD1A-5BIN"]
["2Gb","64M x 32","1.8V","90-ball FPBGA","200 MHz","400Mbps/pin","Extended -25°C ~ +85°C ","AS4C64M32MD1-5BCN"]
["2Gb","64M x 32","1.8V","90-ball FPBGA","200 MHz","400Mbps/pin","Industrial  -40°C ~ +85°C","AS4C64M32MD1A-5BIN"]
["MOBILE LP DDR2"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY (MHz)","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE"]
["256Mb","8M x 32","1.2V/1.8V","134-ball FBGA","400 MHz","800Mbps/pin","Extended -25°C ~ +85°C","AS4C8M32MD2A-25BCN"]
["256Mb","8M x 32","1.2V/1.8V","168-ball FBGA","400 MHz","800Mbps/pin","Extended  -25°C ~ +85°C","AS4C8M32MD2A-25BPCN"]
["1Gb","64M x 16","1.2V/1.8V","134-ball FBGA","400 MHz","800Mbps/pin","Industrial  -40°C ~ +85°C","AS4C64M16MD2A-25BIN"]
["1Gb","32M x 32","1.2V/1.8V","134-ball FBGA","400 MHz","800Mbps/pin","Industrial  -40°C ~ +85°C","AS4C32M32MD2A-25BIN"]
["2Gb","128M x 16","1.2V/1.8V","134-ball FBGA","400MHz","800Mbps/pin","Industrial  -40°C ~ +85°C","AS4C128M16MD2A-25BIN"]
["2Gb","64M x 32","1.2V/1.8V","134-ball FBGA","400 MHz","800Mbps/pin","Industrial  -40°C ~ +85°C","AS4C64M32MD2A-25BIN"]
["4Gb","128M x 32","1.2V/1.8V","134-ball FBGA","533 MHz","1066Mbps/pin","Industrial  -40°C ~ +85°C","AS4C128M32MD2A-18BIN"]
["4Gb","128M x 32","1.2V/1.8V","134-ball FBGA","400 MHz","800Mbps/pin","Industrial  -40°C ~ +85°C","AS4C128M32MD2A-25BIN"]

{"sheet":"Mobile LP DRAM Cross Reference","index":13,"n_rows":34,"n_cols":9,"rows_kept":34,"cut":false,"hidden":false,"merged":[[9,5,10,5],[9,1,10,1],[9,0,10,0],[9,2,10,2],[9,3,10,3],[9,4,10,4]]}
[]
[]
[]
[]
["MOBILE LOW POWER SDRAM Cross Reference"]
["DENSITY","ALLIANCE","MICRON","ISSI","NANYA","WINBOND"]
["128Mb","AS4C8M16MSA-6BIN","NA","IS42VM16800H","NA","W987D6HBGX"]
["128Mb","AS4C4M32MSA-6BIN","NA","IS42VM32400H","NA","W987D2HBJX"]
["256Mb","AS4C16M16MSA-6BIN","MT48H16M16LFBF (EOL)","IS42VM16160K","NA","W988D6FBGX"]
["256Mb","AS4C8M32MSA-6BIN\nAS4C8M32MSB-6BIN","MT48H8M32LFB5 (EOL)","IS42VM32800K","NA","W988D2FBJX"]
[]
["512Mb","AS4C32M16MSA-6BIN","MT48H32M16LFB4-6 IT","IS42VM16320E","NT6SM32M16BG-S1","W989D6DBGX"]
["512Mb","AS4C16M32MSA-6BIN","MT48H16M32LFB5-6 IT","IS42VM32160E","NT6SM16M32BK-S1","W989D2DBJX"]
["512Mb","AS4C16M32MSB-6BIN","MT48H16M32LFB5-6 IT","IS42VM32160E","NT6SM16M32BK-S1","W989D2DBJX"]
[]
["MOBILE LP DDR1 Cross Reference"]
["DENSITY","ALLIANCE","MICRON","SAMSUNG","ISSI","HYNIX","NANYA","ELITE (ESMT)","WINBOND"]
["256Mb","AS4C16M16MD1-6BCN","MT46H16M16LFBF-6","K4X56163SPN","IS43LR16160","HY5MS5B6/ H5MS2562","NT6DM16M16AD-T1","M53D2561616A-6BG2F","W948D6FBHX"]
["512Mb","AS4C32M16MD1A-5BCN","MT46H32M16LFBF-5","K4X51163PI","IS43R16320B","HY5MS7B6/ H5MS5162","NT6DM32M16A(B)D-T1","M53D5121632A-5BG2T","W949D6DBHX"]
["512Mb","AS4C16M32MD1-5BxN","MT46H16M32LFB5-5","K4X51323PI","IS43LR32160B","H5MS5132/ H5MS5122","NT6DM16M32A(B)C-T1","M53D5123216A-5BG2S","W949D2DBJX"]
["1Gb","AS4C64M16MD1A-5BIN","MT46H64M16LFBF","K4X1G163PE","IS43LR16640A","H5MS1G62"]
["1Gb","AS4C32M32MD1A-5BIN","MT46H32M32LFB5-5","K4X1G323PF","IS43LR32320B","H5MS1G22","NT6DM32M32BC-T1","M53D1G3232A","W94AD2KBJX"]
["2Gb","AS4C64M32MD1-5BCN","MT46H64M32LFKQ-5","K4X2G323PC","IS43LR32640A","H5M52G22"]
["2Gb","AS4C64M32MD1A-5BIN","MT46H64M32LFKQ-5","K4X2G323PC","IS43LR32640A","H5M52G22"]
[]
["MOBILE LP DDR2 Cross Reference"]
["DENSITY","ALLIANCE","MICRON","SAMSUNG","ISSI","HYNIX","NANYA","ELITE (ESMT)","WINBOND"]
["256Mb","AS4C8M32MD2A-25BPCN",null,null,"IS43LD32800A-25BL",null,null,null,"W978H2KBVX2E"]
["1Gb","AS4C64M16MD2A-25BIN","MT42L64M16D1HE-25",null,"IS43LD16640C/A",null,"NT6TL64M16BA(I)-G0",null,"W97AH6KBVX2"]
["1Gb","AS4C32M32MD2A-25BIN","MT42L32M32D1HE-25",null,"IS43LD32320C/A",null,"NT6TL32M32BI(A)-G0",null,"W97AH2KBVX2"]
["2Gb","AS4C128M16MD2A-25BIN","MT42L128M16D1TK-25",null,"IS43LD16128B",null,"NT6TL128M16CI(A)-G0",null,"W97BH6KBVX2"]
["2Gb","AS4C64M32MD2A-25BIN","MT42L64M32D1TK-25",null,"IS43LD32640B",null,"NT6TL64M32CI(A)-G0",null,"W97BH2KBVX2"]
["4Gb","AS4C128M32MD2A-18BIN","MT42L128M32D1GU-18 (EOL)",null,"IS43LD32128A",null,"NT6TL128M32BI(A)-G0"]
["4Gb","AS4C128M32MD2A-25BIN","MT42L128M32D1GU-18 (EOL)",null,"IS43LD32128A",null,"NT6TL128M32BI(A)-G0"]

{"sheet":"LPDDR4-LPDDR4X","index":14,"n_rows":17,"n_cols":7,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["LPDDR4"]
["DENSITY","ORG","PACKAGES","CLOCK FREQUENCY","DATA RATE","TEMPERATURE OPTIONS","Alliance Memory"]
["2Gb","128M x 16","200b FBGA","1600 MHz","3200 Mbps","Automotive A2 (-40°C to 105°C)","AS4C128M16MD4-062BAN"]
["4Gb","128M x 32","200b FBGA","1600 MHz","3200 Mbps","Automotive A2 (-40°C to 105°C)","AS4C128M32MD4-062BAN"]
["4Gb","256M x 16","200b FBGA","1600 MHz","3200 Mbps","Automotive A2 (-40°C to 105°C)","AS4C256M16MD4-062BAN"]
["8Gb","256M x 32","200b FBGA","1600 MHz","3200 Mbps","Automotive A2 (-40°C to 105°C)","AS4C256M32MD4-062BAN"]
[]
[]
[]
[]
[]
["LPDDR4X"]
["DENSITY","ORG","PACKAGES","CLOCK FREQUENCY","DATA RATE","TEMPERATURE OPTIONS","Alliance Memory"]
["8Gb","256M x 32","200b FBGA","1600 MHz","3200 Mbps","Automotive A2 (-40°C to 105°C)","AS4C256M32MD4V-062BAN"]

{"sheet":"LPDDR4-LPDDR4X cross Reference","index":15,"n_rows":12,"n_cols":9,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
["LPDDR4 / LPDDR4X Cross Reference "]
[]
["DENSITY","ORG","ALLIANCE","MICRON","SAMSUNG","HYNIX","NANYA","ISSI","WINBOND"]
["2Gb","128M x 16","AS4C128M16MD4-062BAN",null,null,null,"NT6AN128M16AV","IS43/46LQ16128A","W66BP6NB"]
["4Gb","128M x 32","AS4C128M32MD4-062BAN","MT53B128M32D1DS","K4F4E3S4H",null,"NT6AN128T32AV","IS43/46LQ32128A","W66CP2NQ"]
["4Gb","256M x 16","AS4C256M16MD4-062BAN","MT53E256M16D1DS",null,"H9HCNNN4KUMLHR","NT6AN256M16AV","IS43/46LQ16256A","W66CP6NB"]
["8Gb","256M x 32","AS4C256M32MD4-062BAN","MT53B256M32D1DS","K4F8E3S4H",null,"NT6AN256T32AV","IS43/46LQ32256A"]
["8Gb","256M x 32","AS4C256M32MD4V-062BAN","MT53E256M32D2DS","K4U8E3S4AD-GFCL\nK4U8E3S4AD-GHCL",null,"NT6AP256T32AV","IS43/46LQ32256AL\nIS43/46LQ32256EAL","W66DQ2NQU"]

{"sheet":"pSRAM","index":16,"n_rows":14,"n_cols":6,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
["pSRAM"]
["DENSITY","ORG","VCC","PACKAGE","Temperature","ALLIANCE"]
["8Mb","512K x 16","1.7v ~1.95v (1.8v)","6.0x7.0x1.0mm 48 FPBGA","Industrial (-30°C ~+85°C)","AS1C512K16PL-70BIN"]
["8Mb","512K x 16","2.6v to 3.3v (3V)","6.0x7.0x1.0mm 48 FPBGA","Industrial (-40°C~ +85°C)","AS1C512K16P-70BIN"]
["16Mb","1M x 16","1.7v to 1.95v(1.8v)","6.0x7.0x1.0mm 48 FPBGA","Industrial (-40°C~ +85°C)","AS1C1M16PL-70BIN"]
["16Mb","1M x 16","2.6v to 3.3v (3V)","6.0x7.0x1.0mm 48 FPBGA","Industrial (-40°C~ +85°C)","AS1C1M16P-70BIN"]
["32Mb","2M x 16","2.6v to 3.3v (3V)","6.0x7.0x1.0mm 48 FPBGA","Industrial (-40°C~ +85°C)","AS1C2M16P-70BIN"]
["64Mb","4M x 16","1.7v to 1.95v(1.8v)","4.0x4.0x0.8mm 49FBGA","Industrial (-30°C ~+85°C)","AS1C4M16PL-70BIN"]
["128Mb\n(*2-stacked die)","8M x 16","1.7v to 1.95v(1.8v)","4.0x4.0x1.0mm 49FBGA","Industrial (-30°C ~+85°C)","AS1C8M16PL-70BIN"]

{"sheet":"pSRAM Cross Reference","index":17,"n_rows":16,"n_cols":9,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
["pSRAM Cross Reference"]
[]
["ORG","DENSITY","PACKAGE","COMMENTS/ PREV REV","ALLIANCE","JSC/JEJU","ISSI","FIDELIX","AP MEMORY"]
["8Mb","512K x 16","48 FPBGA","page mode & Non-DPD","AS1C512K16PL-70BIN","EM784SP16BPP-70LF","IS66WV51216EALL-70BLI"]
["8Mb","512K x 16","48 FPBGA","Non-page mode & Non-DPD","AS1C512K16P-70BIN","JS784SU16BSP-70LFI","IS66/67WV51216EBLL-70BL","FMP0817CAx"]
["16Mb","1M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C1M16PL-70BIN","EM7164SP16CSP-70LFI","IS66W1M16EALL-70BLI","FMP1617CCx"]
["16Mb","1M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C1M16P-70BIN","JS164SU16BSP-70LFI","IS66/67WV1M16EBLL-70BL","FMP1617CAx"]
["32Mb","2M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C2M16P-70BIN","JS7324SU16BSP-70LFI","IS66WVE2M16EBLL-70B","FMP3217CAx"]
["64Mb","4M X16","49 FBGA","DPD mode","AS1C4M16PL-70BIN","EMC643SP16CKDT-70LF"]
["128Mb\n(*2-stacked die)","8M X16","49 FBGA","DPD mode","AS1C8M16PL-70BIN","JSC283SP16ATDT-70LF",null,null,"APS128XX"]

{"sheet":"Fast Asynchronous SRAM","index":18,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
["5V FAST ASYNCHRONOUS SRAM"]
["DENSITY","ORG","VCC","PACKAGES","SPEED (NS)","ALLIANCE"]
["64Kb","8K x 8","5V","SOJ (28pin),Skinny PDIP (28pin-300mil)",15,"AS7C164A"]
["256Kb","32K x 8","5V","SOJ (28pin), TSOP I (28pin)","10/12/15/20","AS7C256A"]
["256Kb","32K x 8","5V","PDIP (28pin)",15,"AS7C256B"]
["512Kb","32K x 16","5V","SOJ (44), TSOP II (44)","12/15","AS7C513B"]
["1Mb","128K x 8","5V","SOJ (32.3 & 32.4), TSOP I (32)","2020-12-15","AS7C1024B"]
["1Mb","128K x 8","5V","SOJ (32.3 & 32.4)","2015-10-12","AS7C1025B"]
["1Mb","64K x 16","5V","SOJ (44), TSOP II (44)","10/12/15/20","AS7C1026B"]
["4Mb","512K x 8","5V","SOJ (36), TSOP II (44)","2020-12-15","AS7C4096A"]
["4Mb","256K x 16","5V","SOJ (44), TSOP II (44)","2020-12-15","AS7C4098A"]
[]
[]
[]
["3.3V FAST ASYNCHRONOUS SRAM"]
["DENSITY","ORG","VCC","PACKAGES","SPEED (NS)","ALLIANCE"]
["256Kb","32K x 8","3.3V","SOJ (28), TSOP I (28)","10/12/15/20","AS7C3256A"]
["512Kb","32K x 16","3.3V","SOJ (44), TSOP II (44)","10/12/15/20","AS7C3513B"]
["1Mb","128K x 8","3.3V","SOJ (32.3 & 32.4), TSOP I (32)","10/12/15/20","AS7C31024B"]
["1Mb","128K x 8","3.3V","SOJ (32.3 & 32.4)","10/12/15/20","AS7C31025B"]
["1Mb","64K x 16","3.3V","SOJ (44), TSOP II (44)","10/12/15/20","AS7C31026B"]
["2Mb","128K x 16","3.3V","TSOP II (44)","10/12/15/20","AS7C32098A"]
["2Mb","256K x 8","3.3V","TSOP II (44)","10/12/15/20","AS7C32096A"]
["4Mb","512K x 8","3.3V","SOJ (36), TSOP II (44), TFBGA (36)","8/10/12/15/20","AS7C34096A / B"]
["4Mb","256K x 16","3.3V","SOJ (44), TSOP II (44), TFBGA (48)","8/10/12/15/20","AS7C34098A / B"]
["8Mb","1024K x 8","3.3V","TFBGA (48), TSOP II (44)",10,"AS7C38096A / B"]
["8Mb","512K x 16","3.3V","TFBGA (48), TSOP II (44)",10,"AS7C38098A"]
["8Mb","256K x 32","3.3V","TFBGA (90)",10,"AS7C325632"]
["16Mb","512K x32","3.3V","TFBGA (90)",10,"AS7C351232"]
["16Mb","1M x 16","3.3V","TFBGA (48), TSOP I (48), TSOP II (54)",10,"AS7C316098A / B"]
["16Mb","2M x 8","3.3V","TFBGA (48), TSOP I (48), TSOP II (54), TSOP II (44)",10,"AS7C316096A / B / C"]

{"sheet":"Fast Asyn SRAM Cross Reference","index":19,"n_rows":94,"n_cols":10,"rows_kept":94,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
["Fast Asynchronous SRAM Cross Reference"]
[]
["64K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS (EOL)","IDT","ISSI"]
["8K x 8","5V","28pin SOJ (300mil)",15,"AS7C164A-15JxN",null,"CY7C185-15VI (EOL)","IDT7164SXXYG","IS61C64AL-XXJLI"]
["8K x 8","5V","28pin Skinny PDIP 300mil",15,"AS7C164A-15PxN",null,"CY7C185-20PXC (EOL)"]
[]
[]
["256K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS (EOL)","IDT","ISSI"]
["32K x 8","5V","28pin SOJ","10,12,15,20","AS7C256A-xxJCN/JIN","K6E0808C (EOL)","CY7C199D-XXVXI","IDT71256SAXXYG","IS61C256AL-XXJL"]
["32K x 8","5V","28pin TSOP I","10,12,15,20","AS7C256A-xxTCN/TIN",null,"CY7C199D-XXZXI","IDT71256SAXXPZG","IS61C256AL-XXTL"]
["32K x 8","3.3V","28pin SOJ","10,12,15,20","AS7C3256A-xxJCN/JIN","K6E0808V","CY7C1399BN-12VXC","IDT71V256SAXXYG","IS61LV256AL-10JL"]
["32K x 8","3.3V","28pin TSOP I","10,12,15,20","AS7C3256A-xxTCN/TIN",null,"CY7C1399BN-XXZXI","IDT71V256SAXXPZG","IS61LV256AL-10TL"]
["32K x 8","5V","28pin DIP",15,"AS7C256B-xxPIN","(EOL)","CY7C199CN-15PXC (EOL)","IDT71256SAXXTPG"]
[]
[]
["512K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI"]
["32K x 16","5V","44pin SOJ (400MIL)",15,"AS7C513B-xxJCN",null,"CY7C1020D-10VXI",null,"IS61C321AL-12KLI"]
["32K x 16","5V","44pin TSOP II (400MIL)","12,15","AS7C513B-xxTCN",null,"CY7C1020D-10ZSXI",null,"IS61C3216AL-12TLI"]
["32K x 16","3.3V","44pin TSOP II (400MIL)","12,15,20","AS7C3513B-xxTCN",null,"CY7C1020DV33-10ZSXI",null,"IS61WV3216BLL-12TLI"]
["32K x 16","3.3V","44pin SOJ (400MIL)","10,12,15","AS7C3513B-xxJCN",null,"CY7C1020DV33-10VXI"]
[]
["1M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG (EOL)","CYPRESS","IDT","ISSI","GSI (EOL)"]
["128K x 8","5V","32pin SOJ (400MIL)","12,15,20","AS7C1025B-xxJCN/JIN","K6R1008C1D-KI10",null,"IDT71124SXXYG"]
["128K x 8","3.3V","32pin SOJ (400MIL)","10,12,15,20","AS7C31025B-xxJCN/JIN","K6R1008V1D-KI10","CY7C1019DV33-10VXI","IDT71V124SAXXYG","IS63WV1024L-10KLI"]
["128K x 8","3.3V","32pin TSOP II",12,"AS7C31025C-12TIN","K6R1008V1D-UIXX","CY7C1019DV33-XXZSXI","IDT71V124SAXXPHG","IS63WV1288DBLLXXTLI"]
["128K x 8","5V","32pin SOJ (300MIL)","10,12,15,20","AS7C1025B-xxTJCN",null,"CY7C1019D-10VXI"]
["128K x 8","5V","32pin SOJ (400MIL)",15,"AS7C1025B-15JIN"]
["128K x 8","3.3V","32pin SOJ (400MIL)",12,"AS7C31025B-12JIN"]
["128K x 8","3.3V","32pin SOJ (300MIL)","10,12,15,20","AS7C31025B-xxTJCN",null,"CY7C1018DV33-10VXI","IDT71V124SAXXTYG","IS63WV1288DBLL-10JLI"]
["128K x 8","5V","32pin SOJ (400MIL)","12,15,20","AS7C1024B-xxJCN/JIN",null,"CY7C109D-10VXI","IDT71024SXXYG","IS61C1024AL-12KLI"]
["128K x 8","5V","32pin TSOP I","12,15,20","AS7C1024B-xxTCN",null,"CY7C109D-10ZXI",null,"IS61C1024AL-12TLI"]
["128K x 8","5V","32pin SOJ (300MIL)","12,15,20","AS7C1024B-xxTJCN",null,"CY7C1009D-10VXI","IDT71024SXXTYG","IS61C1024AL-12JLI"]
["128K x 8","5V","32pinSOJ(300MIL/400MIL)",12,"AS7C1024B-12JIN",null,"CY7C1019D-10VXI",null,"IS61C1024AL-12KLI"]
["128K x 8","3.3V","32pin SOJ (400MIL)","12,15,20","AS7C31024B-xxJCN",null,"CY1019DV33-10VXI",null,"IS63WV1288DBLL-10KLI"]
["128K x 8","3.3V","32pin TSOP I","10,12,15,20","AS7C31024B-xxTCN",null,null,null,"IS63WV1288DBLL-10HLI"]
["128K x 8","3.3V","32pin SOJ (300MIL)","10,12,15,20","AS7C31024B-xxTJCN",null,"CY7C1018DV33-10VXI",null,"IS63WV1288DBLL-10JLI"]
["64K x 16","5V","44pin SOJ (400MIL)","10,12,15,20","AS7C1026B-xxJCN/JIN","K6R1016C1D-KI10","CY7C1021D-XXVXC","IDT71016SXXYG","IS61C6416AL-12KLI"]
["64K x 16","5V","44pin TSOP II (400MIL)","10,12,15,20","AS7C1026B-xxTCN/TIN","K6R1016C1D-UI10","CY7C1021D-XXZSXI","IDT71016SXXPHG","IS61C6416AL-12TLI"]
["64K x 16","3.3V","44pin SOJ (400MIL)","10,12,15,20","AS7C31026B-xxJCN/TIN","K6R1016V1D-KI10","CY7C1021DV33-XXVXI","IDT71V016SAXXYG","IS61WV6416DBLL-10KLI"]
["64K x 16","3.3V","44pin TSOP II (400MIL)","10,12,15,20","AS7C31026B-xxTCN/TIN","K6R1016V1D-UI10","CY7C1021DV33-XXZSXI","IDT71V016SAXXPHG","IS61WV6416DBLL-10TLI","GS71116AGP-XX"]
[]
[]
["2M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["128K x 16","3.3V","44pin TSOP II","10,12,15,20","AS7C32098A-xxTxN",null,"CY7C1011DV33-10ZSXI",null,"IS61WV12816DBLL-10TL","GS72116AGP-XX"]
["256K x 8","3.3V","44pin TSOP II","10,12,15,20","AS7C32096A-xxTxN",null,"CY7C1010DV33-10ZSXI",null,"IS61WV256EDBLL-10TLI","GS72108AGP-XX"]
[]
["4M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["512K x 8","5V","36pin SOJ (400MIL)","12,15,20","AS7C4096A-xxJxN","K6R4008C1D-KI10","CY7C1049D-10VXI",null,"IS61C5128AL-10KLI"]
["512K x 8","5V","44pin TSOP II (400MIL)","12,15,20","AS7C4096A-xxTxN","K6R4008C1D-UI10",null,null,"IS61C5128AL-10TLI"]
["512K x 8","3.3V","36pin SOJ (400MIL)","8,10,12,15,20","AS7C34096A-xxJxN","K6R4008V1D-KI10","CY7C1049DV33-10VXI","IDT71V424SXXYG","IS61WV5128EDBLL-10KLI"]
["512K x 8","3.3V","44pin TSOP II (400MIL)","10,12,15,20","AS7C34096A-xxTxN","K6R4008V1D-UI10","CY7C1049DV33-10ZSI","IDT71V424SXXPHG","IS61WV5128EDBLL-10TLI","GS74108AGP-XX"]
["512K x 8","2.7 ~ 3.6V","44pin TSOP II",10,"AS7C34096B-10TIN"]
["512K x 8","2.7 ~ 3.6V","36ball TFBGA",10,"AS7C34096B-10BIN"]
["256K x 16","5V","44pin SOJ (400MIL)","12,15,20","AS7C4098A-xxJxN","K6R4016C1D-KI10","CY7C1041D-10VXI",null,"IS61C25616AL-10KLI"]
["256K x 16","5V","44pin TSOP II (400MIL)","12,15,20","AS7C4098A-xxTxN","K6R4016C1D-UI10","CY7C1041D-10ZSXI",null,"IS61C25616AL-10TL"]
["256K x 16","3.3V","44pin SOJ (400MIL)","10,12,15,20","AS7C34098A-xxJxN","K6R4016V1D-KI10","CY7C1041DV33-10VXI","IDT71V416SXXYG","NA"]
["256K x 16","3.3V","44pin TSOP II (400MIL)","8,10,12,15,20","AS7C34098A-xxTxN","K6R4016V1D-UI10","CY7C1041DV33-10ZSXI","IDT71V416SXXPHG","IS61WV25616EDBLL-10TLI","GS74116AGP-XX"]
["256K x 16","3.3V","48ball TFBGA",10,"AS7C34098A-xxBIN",null,"CY7C1041DV33-10BVXI","IDT71V416SXXBE","IS61WV25616EDBLL-10BLI","GS75116AGX-XX"]
["256K x 16","2.7 ~ 3.6V","44pin TSOP II",10,"AS7C34098B-10TIN"]
["256K x 16","2.7 ~ 3.6V","48ball TFBGA",10,"AS7C34098B-10BIN"]
[]
["8M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["512K x 16","3.3V","44pin TSOP II",10,"AS7C38098A-10TIN",null,"CY7C1051DV33-10ZSXI",null,"IS61WV51216BLL-XXTLI"]
["512K x 16","3.3V","48ball TFBGA",10,"AS7C38098A-10BIN",null,"CY7C1051DV33-10BAXI",null,"IS61WV51216BLL-10MLI"]
["256K x 32","3.3V","90ball TFBGA",10,"AS7C325632-10BIN",null,null,null,"IS61WV25632BLL-10BLI"]
["1M x 8","3.3V","44pin TSOP II",10,"AS7C38096A-10TIN",null,"CY7C1059DV33-10ZSXI",null,"IS61WV10248BLL-10TLI"]
["1M x 8","3.3V","48ball TFBGA (different pinout)",10,"AS7C38096A-10BIN"]
["1M x 8","3.3V","48ball TFBGA (different pinout)",10,"AS7C38096B-10BIN",null,null,null,"IS61WV10248BLL-10MLI"]
[]
["16M  FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["1M x 16","3.3V","48pin TSOP I",10,"AS7C316098A-10TIN",null,"CY7C1061GN30-10ZXI",null,"IS61WV102416FBLL-10TLI"]
["1M x 16","3.3V","48ball TFBGA",10,"AS7C316098A-10BIN",null,"CY7C1061GN30-10BV1XI",null,"IS61WV102416FBLL-10BLI"]
["1M x 16","3.3V","54pin TSOP II",10,"AS7C316098B-10TIN",null,"CY7C1061GN30-10ZSXI",null,"IS61WV102416FBLL-10T2LI"]
["1M x 16","3.3V","48ball TFBGA",10,"AS7C316098B-10BIN"]
["2M x 8","3.3V","48pin TSOP I",10,"AS7C316096A-10TIN"]
["2M x 8","3.3V","54pin TSOP II",10,"AS7C316096B-10TIN",null,"CY7C1069GN30-10ZSXI/\nCY7C1069DV33-10ZSXI",null,"IS61WV20488FBLL-10T2LI"]
["2M x 8","3.3V","44pin TSOP II",10,"AS7C316096C-10TIN",null,null,null,"IS61WV20488FBLL-10TLI"]
["2M x 8","3.3V","48ball TFBGA (1CE)",10,"AS7C316096C-10BIN",null,null,null,"IS61WV20488FBLL-10BLI"]
["2M x 8","3.3V","48ball TFBGA (2CE)",10,"AS7C316096B-10BIN",null,"CY7C1069GN30-10BVXI"]
["512K x 32","3.3V","90ball TFBGA",10,"A7C351232-10BIN",null,null,null,"IS61WV51232BLL-10BLI"]

{"sheet":"Low Power Asynchronous SRAM","index":20,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
["2.7V- 3.6V LOW POWER SRAMS"]
["DENSITY","ORG","VCC","PACKAGES","SPEED\n(NS)","ALLIANCE"]
["256Kb","32K x 8","2.5 ~ 3.6V","28pin SOP (330mm)",70,"AS62V256A"]
["1Mb","64Kx16 with ECC","2.7 ~ 3.6V","44pin TSOP II",45,"AS6CE1016A"]
["2Mb","256K x 8","2.7 ~ 3.6V","32pin 450 mil SOP, 32pin TSOP I (8 x 20mm), 32pin STSOP (8 x 13.4mm), 36ball TFBGA (6 x 8mm)",55,"AS6C2008"]
["4Mb","256Kx16 with ECC","2.7 ~ 3.6V","44pin TSOP II, 48ball TFBGA",45,"AS6CE4016B"]
["8Mb","1M x 8","2.7 ~ 3.6V","48ball TFBGA (8 x 10mm)","45/55","AS6C8008A"]
["8Mb","1M x 8","2.7 ~ 3.6V","44pin TSOP II","45/55","AS6C8008B"]
["8Mb","512K x 16","2.7 ~ 3.6V","44pin TSOP II / 48pin TSOP I,48ball TFBGA (8 x 10mm*)**","45/55","AS6C8016B"]
["16Mb","1M x 16","2.7 ~ 3.6V","48ball TFBGA (6 x 8mm), 48pin TSOP I (12 x 20mm)","45/55","AS6C1616/ AS6C1616B"]
["16Mb","2M x 8","2.7 ~ 3.6V","44pin TSOP II, 48ball TFBGA",45,"AS6C1608B"]
["32Mb","2M x 16","2.7 ~ 3.6V","48pin TSOP I (12 x 20mm) , 48ball FBGA (6x8mm)",55,"AS6C3216A"]
["64Mb","4M x 16 /\n8M x 8","2.7 ~ 3.6V","48pin TSOP,  48ball FBGA(6x8mm)  (dual chip select 4M x 16 or 8M x 8)",55,"AS6C6416"]
[]
[]
[]
[]
["2.7V - 5.5V LOW POWER SRAMS"]
["DENSITY","ORG","VCC","PACKAGES","SPEED (NS)","ALLIANCE"]
["64Kb","8K x 8","2.7 ~ 5.5V","28pin 600 mil PDIP, 28pin 330 mil SOP, 28pin sTSOP (8x13.4mm)",55,"AS6C6264"]
["256Kb","32K x 8","2.7 ~ 5.5V","28pin 600 mil PDIP, 28pin 330 mil SOP, 28pin sTSOP (8x13.4mm)",55,"AS6C62256"]
["1Mb","64K x 16","2.7 ~ 5.5V","44pin 400 mil TSOP II TFBGA (48)",55,"AS6C1016"]
["1Mb","128K x 8","2.7 ~ 5.5V","32pin 450 mil SOP, 32pin TSOP I (8 x 20mm), 32pin sTSOP (8 x 13.4mm), TFBGA (36), 32pin PDIP",55,"AS6C1008"]
["2Mb","256K x 8","2.7 ~ 5.5V","32pin 450 mil SOP, 32pin TSOP I (8 x 20mm) 32pin sTSOP (8 x 13.4mm), TFBGA (36)",55,"AS6C2008A"]
["2Mb","128K x 16","2.7 ~ 5.5V","44pin 400 mil TSOP II, TFBGA (48)",55,"AS6C2016"]
["4Mb","512K x 8","2.7 ~ 5.5V","32pin 450 mil SOP, 32pin TSOP I (8 x 20mm), 32pin sTSOP (8 x 13.4mm), TFBGA (48), 32pin 600 mil PDIP, 32pin TSOP II",55,"AS6C4008"]
["4Mb","256K x 16","2.7 ~ 5.5V","44pin TSOP II, TFBGA (48)",55,"AS6C4016"]
["8Mb","1024K x 8","2.7 ~ 5.5V","44pin TSOP II, TFBGA (48)",55,"AS6C8008"]
["8Mb","512K x 16","2.7 ~ 5.5V","44pin TSOP II, 48ball TFBGA (6 x 8mm*) one chip select pins:B5**",55,"AS6C8016"]

{"sheet":"Low Power Asyn SRAM Cross Refer","index":21,"n_rows":94,"n_cols":11,"rows_kept":94,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
["Low Power Asynchronous SRAM Cross Reference"]
[]
["64K LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","ZMD","CYPRESS (EOL)","HITACHI (EOL)","NEC (EOL)","HYNIX (EOL)"]
["8K x 8","2.7V ~ 5.5V","28pin 600mil DIP","AS6C6264-55PCN","U6264BDC07LLG1",null,"HM6264BLP",null,"HY6264P"]
["8K x 8","2.7V ~ 5.5V","28pin 330mil SOP","AS6C6264-55SCN","U6264BS2C07LLG1","CY6264-55SNXI","HM6264BLFP","uPD4464","HY6264G"]
["8K x 8","2.7V ~ 5.5V","28pin STSOP (8 x 13.4 mm)","AS6C6264-55STCN"]
[]
["256K LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","ZMD","SAMSUNG (EOL)","CYPRESS (EOL)","RENESAS","BRILLIANCE (EOL)","ISSI"]
["32K x 8","2.7V ~ 5.5V","28pin 600mil DIP","AS6C62256-55PCN","U62256ADC07LLG1","K6X0808C1D-DF55","CY62256NLL-70PXC",null,"BS62LV256PCP-55"]
["32K x 8","2.7V ~ 5.5V","28pin 330mil SOP","AS6C62256-55SxN","U62256AS2C07LLG1","K6X0808C1D-BF55","CY62256NLL-55SNXI","R1LP5256ESP-5S","BS62LV256SCP-55","IS62C256AL-45ULI"]
["32K x 8","2.5V ~ 3.6V","28pin 330mil SOP","AS62V256-70SIN",null,null,"CY62256NVLL-70SNXI","R1LV5256ESP-5S","BS62LV256SCP-55","IS62LV256AL-45ULI"]
["32K x 8","2.7V ~ 5.5V","28pin STSOP (8 x 13.4 mm)","AS6C62256-55STxN",null,"K6X0808C1D-LF55","CY62256NLL-55ZRXI","R1LP5256ESA-5S","BS62LV256STCP-55","IS62LV256AL-45TLI"]
[]
[]
["1M LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","RENESAS","BRILLIANCE (EOL)","NEC (EOL)","ISSI"]
["128K x 8","2 .7V ~ 5.5V","32pin 600mil DIP","AS6C1008-55PCN","K6X1008C2D-DB55",null,null,null,"BS62LV1027PCP-55","uPD431000ACZ-70L"]
["128K x 8","2.7V ~ 5.5V","32pin 450mil SOP","AS6C1008-55SIN","K6X1008C2D-GF55(Lead)/BF","CY62128ELL-45SXI","M5M51008DFP-55HI","R1LP0108ESP-5SI","BS62LV1027SIP-55","uPD431000AGW-70L","IS62C1024AL-35QLI"]
["128K x 8","2.7V ~ 5.5V","32pin TSOP I (8 x 20 mm)","AS6C1008-55TIN","K6X1008C2D-TF55 or PF","CY62128ELL-45ZXI","M5M51008DVP-55HI","R1LP0108ESF-5SI","BS62LV1027TIP-55","uPD431000AGZ-70LL-KKH","IS62C1024AL-35TLI"]
["128K x 8","2.7V ~ 5.5V","32pin STSOP (8 x 13.4 mm)","AS6C1008-55STIN",null,"CY62128ELL-45ZAXI","M5M51008DKV-55HI","R1LP0108ESA-5SI","BS62LV1027STIP-55","uPD431000AGU-B10-9JH","IS62C1024AL-45HLI"]
["64K x 16","2.7V ~ 5.5V","48ball TFBGA","AS6C1016-55BIN","K6F1016U4C-EF55","CY62127DV30LL-55BVXI",null,null,"BS616LV1010AI-70",null,"IS62WV6416DBLL-45BLI"]
["64K x 16","2.7V ~ 5.5V","44pin TSOP II","AS6C1016-55ZIN",null,"CY62126EV30LL-45SXIT",null,null,"BS616LV1010EI-70",null,"IS62WV6416DBLL-45TLI"]
["64K x 16","2.7V ~ 3.6V","44pin TSOP II","AS6CE1016A-45ZIN",null,"CY62126EV30LL-45SXIT",null,null,"BS616LV1010EI-70",null,"IS62WV6416DBLL-45TLI"]
[]
["2M LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["256K x 8","3.3V","32pin 450mil SOP","AS6C2008-55SIN",null,"CY62138FV30LL-45SXI",null,null,"BS62LV2006SIP-55"]
["256K x 8","3.3V","32pin TSOP I (8 x 20 mm)","AS6C2008-55TIN",null,"CY62138FV30LL-45ZXI",null,null,"BS62LV2006TIP-55","IS62WV2568BLL-55TLI"]
["256K x 8","3.3V","32pin STSOP (8 x 13.4 mm)","AS6C2008-55STIN","K6F2008V2E-LF70000","CY62138FV30LL-45ZAXI","M5M5V208AKV-55HI","R1LV0208BSA-5SI","BS62LV2006STIP-55","IS62WV2568BLL-55HLI"]
["256K x 8","3.3V","36ball TFBGA (6mm x 8mm)","AS6C2008-55BIN",null,"CY62138FV30LL-45BVXI",null,null,null,"IS62WV2568BLL-55B2LI"]
["128K x 16","2.7V ~ 5.5V","44pin TSOP II","AS6C2016-55ZIN",null,"CY62136FVLL-70ZSXI","M5M5V216ATP-70HI","R1LV0216-BSB-5SI","BS616LV2016EIP-55","IS62WV12816BLL-55TLI"]
["128K x 16","3.3V","48ball TFBGA","AS6C2016-55BIN","K6F2016U4E-EF55000","CY62136FVLL-70BVXI",null,null,"BS616LV2019AIG-55","IS62WV12816BLL-55B2LI"]
["256K x 8","2.7V ~ 5.5V","32pin 450mil SOP","AS6C2008A-55SIN",null,"CY2138FV30LL-45SXI",null,null,"BS62LV2006SIP-55"]
["256K x 8","2.7V ~ 5.5V","32pin TSOP I (8 x 20mm)","AS6C2008A-55TIN",null,"CY2138FV30LL-45ZXI",null,null,"BS62LV2006TIP-55","IS62WV256BLL-55TLI"]
["256K x 8","2.7V ~ 5.5V","36ball TFBGA (6mm x 8mm)","AS6C2008A-55BIN",null,"CY62138FV30LL-45BVXI",null,null,null,"IS62WV256BLL-55B2LI"]
[]
["4M LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["512K x 8","2.7 ~ 5.5V","32pin 600mil DIP","AS6C4008-55PCN","K4X4008C1F-DB55",null,null,"BS62LV4006PCP-55"]
["512K x 8","2.7 ~ 5.5V","32pin 450mil SOP","AS6C4008-55SIN","K6X4008C1F-GF55 or BF","CY62148ELL-55SXI","R1LV0408CSP-5SI","BS62LV4006SIP-55","IS62C5128BLL-45QLI"]
["512K x 8","2.7 ~ 5.5V","32pin TSOP I (8 x 20mm)","AS6C4008-55TIN",null,null,null,"BS62LV4006ECP-55","IS62WV5128EBLL-45QLI"]
["512K x 8","2.7 ~ 5.5V","32pin STSOP (8 x 13.4mm)","AS6C4008-55STIN","K6X4008T1F-YF55 or LF","CY62148ELL-55ZAXI\nCY62148EV30LL-55ZAXI","R1LV0408DSA-5SI","BS62LV4006STIP-55","IS62C512BL-45HLI\nIS62WV5128DBLL-45HLI"]
["512K x 8","2.7 ~ 5.5V","32pin TSOP II","AS6C4008-55ZIN","K6X4008C1F-VF55","CY62148ELL-45ZSXI","R1LV0408DSB-5SI","BS62LV4006ECP55","IS62WV5128DBLL-45T2LI"]
["512K x 8","2.7 ~ 5.5V","36pin TFBGA (6mm x 8mm)","AS6C4008-55BIN",null,"CY62148EV30LL-55BVXI","RILV0408DBG-5SI",null,"IS62WV5128EBLL-45BLI"]
["256K x 16","2.7 ~ 5.5V","44pin TSOP II","AS6C4016-55ZIN","K6X4016C3F-TF70000","CY62146ELL-45ZSXI",null,"BS616LV4017EIP-55","IS62WV5128BLL-55TLI"]
["256K x 16","2.7 ~3.6V","44pin TSOP II","AS6CE4016B-45ZIN","K6X4016T3F-TF70000","CY62147EV30LL-45ZSXI","R1LV0414DSB-5SI","BS616LV4017EIP-55","IS62C25616BL-45T2LI"]
["256K x 16","2.7 ~3.6V","48ball  TFBGA","AS6CE4016B-45BIN","K6F4016U6G-EF70000","CY62147EV30LL-45BVXI","RMLV0416EGBG-4S2","BS616LV4017AIP-55","IS62WV25616DBLL-45BLI"]
[]
[]
[]
["8M LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","RENESAS","RENESAS","BRILLIANCE","ISSI"]
["1M x 8","2.7 ~ 5.5V","44pin TSOP II","AS6C8008-55ZIN","K6X8008(C/T)2B-UF55","CY62158EV30LL-45ZSXI",null,"R1LV0808ASB-5SI","HM62V8100LTTI-5SL","BS62LV8001ECP-55","IS62WV1024BLL-55TLI"]
["1M x 8","2.7 ~ 3.6V","44pin TSOP II","AS6C8008B-45ZIN","K6X8008(C/T)2B-UF55","CY62158EV30LL-45ZSXI",null,"R1LV0808ASB-5SI","HM62V8100LTTI-5SL","BS62LV8001ECP-55","IS62WV1024BLL-55TLI"]
["1M x 8","2.7 ~ 5.5V","48ball TFBGA","AS6C8008-55BIN",null,"CY62158EV30LL-45BVXI","EOL",null,"HM62V8100LBPI-5SL","BS62LV8001ECP-55","IS62WV1024BLL-55MLI"]
["1M x 8","2.7 ~ 3.6V","48ball TFBGA","AS6C8008A-45BIN",null,"CY62158EV30LL-45BVXI","EOL",null,"HM62V8100LBPI-5SL","BS62LV8001FIP-55","IS62WV1024BLL-55MLI"]
["512K x 16","2.7 ~ 5.5V","48ball TFBGA (6 x 8mm)*","AS6C8016-55BIN*","K6F8016U6G-FF55","CY62157EV30LL-55BVXI","M5M5W816WG-55HI","R1LV0816ABG-5SI",null,"BS616LV8017ECP55","IS62WV51216BLL-55BLI"]
["512K x 16","2.7 ~3.6V","48ball TFBGA (8 x 10mm)**","AS6C8016B-45BIN**",null,"CY2157EV30LL-45BVXIT"]
["512K x 16","2.7 ~ 5.5V","44pin TSOP II","AS6C8016 -55ZIN","K6X8016(C/T)3B-UF55","CY62157EV30LL-55ZSXI","M5M5W816TP-55HI","R1LV0816ASA-5SI","HM62165I14LTT-5SL","BS616LV8017FCP70","IS62WV51216BLL-55T2LI"]
["512K x 16","2.7 ~3.6V","44pin TSOP II","AS6C8016B-45ZIN",null,"CY62157EV30LL-45ZSXIT",null,null,null,null,"IS62WV51216BLL-55T2LI"]
["512K x 16","2.7 ~ 5.5V","48pin TSOP I","AS6C8016-55TIN",null,"CY62157EV30LL-45ZXIT",null,null,null,null,"IS62WV51216GBLL-45TLI"]
[]
["* = one chip select pin:B5 ** = two chip select pins: B5 and A6"]
[]
[]
[]
["16M LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["1M x 16","2.7 ~ 3.6V","48pin TSOP I","AS6C1616B-45TIN","CY62167E30LL-55ZXI","R1LV1616RSA-5SI","BS6216LV1611TCP55"]
["1M x 16","2.7 ~ 3.6V","48pin TSOP I","AS6C1616-55TIN","CY62167E30LL-55ZXI","R1LV1616RSA-5SI","BS6216LV1611TCP55"]
["1M x 16","2.7 ~ 3.6V","48ball TFBGA","AS6C1616B-45BIN","CY62167DV30LL-55BVXIT","R1LV1616HBG-4SI",null,"IS62WV102416EBLL-55BLI"]
["2M x 8","2.7 ~ 3.6V","44pin TSOP I","AS6C1608B-45TIN","CY62168EV30LL-55ZXI",null,"BS6216LV1600EIP55","IS62WV20488EBLL-55BLI"]
["2M x 8","2.7 ~ 3.6V","48ball TFBGA","AS6C1608B-45BIN","CY62168DV30LL-55BVI"]
[]
["32M LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS"]
["2M x 16","2.7 ~ 3.6V","48pin TSOP I","AS6C3216A-55TIN*","CY62177EV30LL-55ZXI","R1LV3216RSA-5SI"]
["2M x 16","2.7 ~ 3.6V","48ball TFBGA","AS6C3216-55BIN AS6C3216A-55BIN","CY62177EV30LL-55BAXI","R1LV3216CSA-5SI"]
["*48pin TSOP I (please note: dual chip select 2Mx16 or 4Mx8)"]
[]
[]
["64M LOW POWER"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS"]
["4M x 16","2.7V ~ 3.6V","48pin TSOP I","AS6C6416-55TIN",null,"R1WV6416RSA-5S"]
["4M x 16","2.7V ~ 3.6V","48ball BGA","AS6C6416-55BIN","CY62187EV30LL-55BAXI","R1WV6416RBG-5S"]
["*48pin TSOP I (please note: dual chip select 4Mx16 or 8Mx8)"]

{"sheet":"Parallel 5V NOR Flash","index":22,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
["Parallel 5V NOR Flash"]
[]
["DENSITY","BUS WIDTH","VCC","PACKAGES","TEMPERATURE RANGE","SPEED (NS)","ALLIANCE","REMARKS"]
["1Mb","x8","5V","PLCC 32","-40C to 85C",55,"AS29CF010-55CCIN","Uniform Sector, Industrial Grade"]
["2Mb","x8 , x16","5V","SOP 44pin","-40C to 125C",55,"M29F200FB55M3F2","Bottom Boot, Automotive Grade3"]
["4Mb","x8","5V","PLCC 32","-40C to 85C",55,"AS29CF040-55CCIN","Uniform Sector, Industrial Grade"]
["4Mb","x8 , x16","5V","SOP 44pin","-40C to 125C",55,"M29F400FB55M3F2","Bottom Boot, Automotive Grade3"]
["4Mb","x8 , x16","5V","TSOP I 48pin","-40C to 85C",55,"M29F400FT5AN6E2","Top Boot, Automotive Grade6"]
["4Mb","x8 , x16","5V","TSOP I 48pin","-40C to 125C",55,"M29F400FB55N3E2 \nM29F400FB55N3F2","Bottom Boot, Automotive Grade3"]
["8Mb","x8 , x16","5V","TSOP I 48pin","-40C to 85C",55,"AS29CF800T-55TIN","Top Boot, Industrial Grade"]
["8Mb","x8 , x16","5V","TSOP I 48pin","-40C to 85C",55,"AS29CF800B-55TIN","Bottom Boot, Industrial Grade"]
["8Mb","x8 , x16","5V","TSOP I 48pin","-40C to 85C",55,"M29F800FB5AN6E2 \nM29F800FB5AN6F2","Bottom Boot, Automotive Grade6"]
["8Mb","x8 , x16","5V","TSOP.I 48pin","-40C to 125C",55,"M29F800FT55N3E2","Top Boot, Automotive Grade3"]
["8Mb","x8 , x16","5V","SOP 44pin","-40C to 125C",55,"M29F800FB55M3F2","Bottom Boot, Automotive Grade3"]
["16Mb","x8 , x16","5V","TSOP.I 48pin","-40C to 85C",55,"AS29CF160B-55TIN","Bottom Boot, Industrial Grade"]
["16Mb","x8 , x16","5V","TSOP.I 48pin","-40C to 85C",55,"AS29CF160T-55TIN","Top Boot, Industrial Grade"]
["16Mb","x8 , x16","5V","TSOP.I 48pin","-40C to 85C",55,"M29F160FB5AN6F2","Bottom Boot, Automotive Grade6"]
["16Mb","x8 , x16","5V","TSOP.I 48pin","-40C to 125C",55,"M29F160FT55N3E2","Top Boot, Automotive Grade3"]

{"sheet":"Parallel 5V NOR Falsh Cross Ref","index":23,"n_rows":22,"n_cols":8,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
["Parallel 5V NOR Flash Cross Reference"]
[]
["DENSITY","VCC","PACKAGE","SPEED (NS)","ALLIANCE","Micron","Cypress / Spansion","Macronix"]
["1Mb","5V","PLCC 32",55,"AS29CF010-55CCIN",null,"AM29F010B* (EOL)"]
["2Mb","5V","SOP 44pin",55,"M29F200FB55M3F2","M29F200F","AM29F200BB* (EOL)","MX29F200CBM* (EOL)"]
["4Mb","5V","PLCC 32",55,"AS29CF040-55CCIN","M29F040","AM29F040B","MX29F040C"]
["4Mb","5V","SOP 44pin",55,"M29F400FB55M3F2","M29F400F","AM29F400BB* (EOL)","MX29F400CBM* (EOL)"]
["4Mb","5V","TSOP 48pin",55,"M29F400FB55N3E2 \nM29F400FB55N3F2","M29F400F","AM29F400BB* (EOL)","MX29F400CBT"]
["4Mb","5V","TSOP 48pin",55,"M29F400FT5AN6E2","M29F400F","AM29F400BT* (EOL)","MX29F400CTT"]
["8Mb","5V","TSOP 48pin",55,"AS29CF800T-55TIN","M29F800F","AM29F800BT* (EOL)","MX29F800C T/B"]
["8Mb","5V","TSOP 48pin",55,"AS29CF800B-55TIN","M29F800F","AM29F800BB* (EOL)","MX29F800C T/B"]
["8Mb","5V","TSOP 48pin",55,"M29F800FB5AN6E2\nM29F800FB5AN6F2","M29F800F","AM29F800BB* (EOL)","MX29F800CBT"]
["8Mb","5V","TSOP 48pin",55,"M29F800FT55N3E2","M29F800F","AM29F800BT* (EOL)","MX29F800CTT"]
["8Mb","5V","SOP 44pin",55,"M29F800FB55M3F2","M29F800F","AM29F800BB* (EOL)","MX29F800CBM* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"AS29CF160T-55TIN","M29F160F","AM29F160DT* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"AS29CF160B-55TIN","M29F160F","AM29F160DB* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"M29F160FB5AN6F2","M29F160F","AM29F160DB* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"M29F160FT55N3E2","M29F160F","AM29F160DT* (EOL)"]

{"sheet":"Serial NOR Flash","index":24,"n_rows":26,"n_cols":8,"rows_kept":26,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
["Serial NOR Flash"]
[]
["DENSITY","BUS WIDTH","VCC","PACKAGES","TEMPERATURE RANGE","SPEED (MHz)","ALLIANCE","REMARKS"]
["2Mb","x1","3V","8pin SOICNarrow body","-40C to 85C",75,"M45PE20-VMN6P","PAGE ERASABLE, 2Mb Serial Flash (256K x 8bits, 1024 pages, 4 Sectors), Industrial Grade"]
["8Mb","x1","3V","8pin DFN (6mm x 5mm)","-40C to 85C",75,"M45PE80-VMP6TG","PAGE ERASABLE 8Mb Serial Flash (1K x 8bits, 4096 pages, 16 Sectors), Industrial Grade, T&R"]
["16Mb","x1","3V","8pin SOIC Wide body","-40C to 85C",75,"M45PE16-VMW6TG","PAGE ERASABLE, 16MB Serial Flash (2K x 8bits, 8192 pages, 32 Sectors), Industrial Grade"]
["32Mb","x1/x2/x4","3V","8pin DFN (4 x 3mm)","-40C to 125C",108,"N25Q032A13EF4A0F","32Mb Serial NOR Flash, Multiple IO, 64 Sectors, 4KB Sector Erase, Automotive Grade T&R"]
["32Mb","x1/x2/x4","3V","8pin SOIC Narrow body","-40C to 85C",108,"N25Q032A13ESC40F","32Mb Serial NOR Flash, Multiple IO, 64 Sectors, 4KB Sector Erase, Industrial Grade, T&R"]
["32Mb","x1/x2/x4","3V","8pin SOIC Narrow body","-40C to 85C",108,"N25Q032A13ESC40G","32Mb Serial NOR Flash, Multiple IO, 64 Sectors, 4KB Sector Erase, Industrial Grade, Tube"]
["32Mb","x1/x2/x4","3V","8pin SOIC Narrow body","-40C to 125C",108,"N25Q032A13ESCA0F","32Mb Serial NOR Flash, Multiple IO, 64 Sectors, 4KB Sector Erase, Automotive Grade, T&R"]
["32Mb","x1/x2/x4","3V","16pin SOIC Wide body","-40C to 125C",108,"N25Q032A13ESFA0F","32Mb Serial NOR Flash, Multiple IO, 64 Sectors, 4KB Sector Erase, Automotive Grade, T&R"]
["64Mb","x1/x2/x4","1.8V","8pin SOIC Wide body","-40C to 125C",108,"N25Q064A11ESEA0F","64Mb Serial NOR Flash, Multiple IO, 128 Sectors, 4KB Sector Erase, Automotive Grade T&R"]
["64Mb","x1/x2/x4","3V","8pin DFN (6mm x 5mm)","-40C to 85C",108,"N25Q064A13EF640E","64Mb Serial NOR Flash, Multiple IO, 128 Sectors, 4KB Sector Erase, Industrial Grade, Tray"]
["64Mb","x1/x2/x4","3V","8pin DFN (8mm x 6mm)","-40C to 125C",108,"N25Q064A13EF8A0E","64Mb Serial NOR Flash, Multiple IO, 128 Sectors,  4KB Sector Erase, Automotive Grade Tray"]
["64Mb","x1/x2/x4","3V","8pin DFN (8mm x 6mm)","-40C to 125C",108,"N25Q064A13EF8A0F","64Mb Serial NOR Flash, Multiple IO, 128 Sectors, 4KB Sector Erase, Automotive Grade T&R"]
["64Mb","x1/x2/x4","3V","8pin DFN (8mm x 6mm)","-40C to 85C*",108,"N25Q064A13EF8H0E","64Mb Serial NOR Flash, Multiple IO, 128 Sectors, 4KB Sector Erase, Industrial Grade High Reliability, Tray"]
["64Mb","x1/x2/x4","3V","16pin SOIC Wide body","-40C to 125C",108,"N25Q064A13ESFA0F","64Mb Serial NOR Flash, Multiple IO, 128 Sectors, 4KB Sector Erase, Automotive Grade T&R"]
["64Mb","x1/x2/x4","3V","8pin SOIC (209mils)","-40C to 85C",104,"AS25F364MQ-10SIN","64Mb, 3V Serial NOR Flash, Multiple IO, Default Feature1, Industrial Grade, 8SOIC Wide Body Package"]
["64Mb","x1/x2/x4","3V","8L WSON (6x5mm)","-40C to 85C",104,"AS25F364MQ-10WIN","64Mb, 3V Serial NOR Flash, Multiple IO, Default Feature1, Industrial Grade, 8WSON Package"]
["128Mb","x1/x2/x4","1.8V","8pin SOIC (209mils)","-40C to 85C",133,"AS25F128MQ-70SIN","128Mb, 1.8V Serial NOR Flash, Multiple IO, Default Feature1, Industrial Grade, 8SOIC Wide Body Package"]
["128Mb","x1/x2/x4","1.8V","8L WSON (6x5mm)","-40C to 85C",133,"AS25F128MQ-70WIN","128Mb, 1.8V Serial NOR Flash, Multiple IO, Default Feature1, Industrial Grade, 8WSON Package"]

{"sheet":"Serial NOR Flash Cross Ref","index":25,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
["Serial NOR Flash Cross Reference"]
[]
["DENSITY","VCC","PACKAGES","ALLIANCE","MICRON","WINBOND","ADESTO","SPANSION","MACRONIX","ISSI","GigaDevices"]
["2Mb","3V","8pin SOIC Narrow body","M45PE20-VMN6P",null,null,"AT45DB021E"]
["8Mb","3V","8pin DFN (6mm x 5mm)","M45PE80-VMP6TG",null,null,"AT45DB081E"]
["16Mb","3V","8pin SOIC Wide body","M45PE16-VMW6TG",null,null,"AT45DB161E"]
["32Mb","3V","8pin DFN (4mm x 3mm)","N25Q032A13EF4A0F",null,"W25Q32","AT25DF32/AT25SF32","S25FL032A/P","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3V","8pin SOIC Narrow body","N25Q032A13ESC40F",null,"W25Q32","AT25DF32/AT25SF32","S25FL032A/P","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3V","8pin SOIC Narrow body","N25Q032A13ESC40G",null,"W25Q32","AT25DF32/AT25SF32","S25FL032A/P","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3V","8pin SOIC Narrow body","N25Q032A13ESCA0F",null,"W25Q32","AT25DF32/AT25SF32","S25FL032A/P","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3V","16pin SOIC Wide body","N25Q032A13ESFA0F",null,"W25Q32","AT25DF32/AT25SF32","S25FL032A/P","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["64Mb","1.8V","8pin SOIC Wide body","N25Q064A11ESEA0F",null,"W25Q64","AT25SL64/AT25QL64",null,"MX25U64","IS25WP064","GD25LQ64"]
["64Mb","3V","8pin DFN (6mm x 5mm)","N25Q064A13EF640E",null,"W25Q64","AT25SF64/AT25QF64","S25FL064A/P","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3V","8pin DFN (8mm x 6mm)","N25Q064A13EF8A0E",null,"W25Q64","AT25SF64/AT25QF64","S25FL064A/P","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3V","8pin DFN (8mm x 6mm)","N25Q064A13EF8A0F",null,"W25Q64","AT25SF64/AT25QF64","S25FL064A/P","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3V","8pin DFN (8mm x 6mm)","N25Q064A13EF8H0E",null,"W25Q64","AT25SF64/AT25QF64","S25FL064A/P","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3V","16pin SOIC Wide body","N25Q064A13ESFA0F",null,"W25Q64","AT25SF64/AT25QF64","S25FL064A/P","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3V","8pin SOP (209mils)","AS25F364MQ-10SIN","N25Q064A13ESE","W25Q64","AT25QF64","S25FL064","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3V","8L WSON (6x5mm)","AS25F364MQ-10WIN","N25Q064A13EF6","W25Q64","AT25QF64","S25FL064","MX25L64","IS25L064","GD25Q64"]
["128Mb","1.8V","8pin SOP (209mils)","AS25F1128MQ-70SIN","MT25QU128ABA1ESE","W25Q128JWSIM","AT25SL128A-SUE","S25FS128SDSMFI","MX25U12832FM2I","IS25WP128-JBLE","GD25LB128ESIG"]
["128Mb","1.8V","8L WSON (6x5mm)","AS25F1128MQ-70WIN","MT25QU128ABA1EW7","W25Q128JWPIM","AT25SL128A-MHE","S25FS128SDSNFI","MX25U12832FZNI","IS25WP128-JKLE","GD25LB128EWIG"]

{"sheet":"Serial NAND Flash","index":26,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
["Serial NAND Flash"]
[]
["DENSITY","BUS WIDTH","SPEED (NS)","VCC","PACKAGES","TEMPERTURE RANGE","TYPE","ALLIANCE"]
["1Gb","x1, x2, x4","120 Mhz","3V","LGA 8pin","Industrial (-40°C to 85°C)","4bit ECC, (2048 + 64) bytes × 64 pages × 1024 blocks","AS5F31G04SND-08LIN"]
["2Gb","x1, x2, x4","100 Mhz","1.8V","LGA 8pin","Industrial (-40°C to 85°C)","8bit ECC, (2048 + 128) bytes × 64 pages × 2048 blocks","AS5F12G04SND-10LIN"]
["2Gb","x1, x2, x4","120 Mhz","3V","LGA 8pin","Industrial (-40°C to 85°C)","8bit ECC, (2048 + 128) bytes × 64 pages × 2048 blocks","AS5F32G04SNDA-08LIN"]
["4Gb","x1, x2, x4","100 Mhz","1.8V","LGA 8pin","Industrial (-40°C to 85°C)","8bit ECC, (2048 + 128) bytes × 64 pages × 4096 blocks","AS5F14G04SND-10LIN"]
["4Gb","x1, x2, x4","120 Mhz","3V","LGA 8pin","Industrial (-40°C to 85°C)","8bit ECC, (2048 + 128) bytes × 64 pages × 4096 blocks","AS5F34G04SNDA-08LIN"]
["8Gb","x1, x2, x4","100 Mhz","1.8V","LGA 8pin","Industrial (-40°C to 85°C)","8bit ECC, (4096 + 256) bytes × 64 pages × 4096 blocks","AS5F18G04SND-10LIN"]
["8Gb","x1, x2, x4","120 Mhz","3V","LGA 8pin","Industrial (-40°C to 85°C)","8bit ECC, (4096 + 256) bytes × 64 pages × 4096 blocks","AS5F38G04SND-08LIN"]

{"sheet":"Serial NAND Flash Cross Ref","index":27,"n_rows":16,"n_cols":8,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
["Serial NAND Flash Cross Reference"]
[]
["DENSITY","SPEED (NS)","ALLIANCE","Toshiba/KIOXIA","Micron","Winbond","Macronix","GigeDevices"]
["1Gb","120Mhz","AS5F31G04SND-08LIN","TC58CVG0S3HRAIJ","MT29F1G01ABAFDWB-IT","W25N01GV","MX35LF1GE4AB","GD5F1GQ4UB/C/E/Fxxx"]
["2Gb","100Mhz","AS5F12G04SND-10LIN","TC58CYG1S3HRAIJ","MT29F2G01ABBGDWB-IT:G","W25N02JW","MX35UF2G14AC","GD5F2GQ4Rx"]
["2Gb","120Mhz","AS5F32G04SNDA-08LIN","TC58CVG1S3HRAIJ","MT29F2G01ABAGDWB-IT","W25M02GV","MX35LF2G14AC","GD5F2GQ4Ux"]
["4Gb","100Mhz","AS5F14G04SND-10LIN","TC58CYG2S0HRAIJ","MT29F4G01ABBFDWB-IT","W25N04KW","MX35UF4Gx4AD","GD5F4GQ6Rx"]
["4Gb","120Mhz","AS5F34G04SNDA-08LIN","TC58CVG2S0HRAIJ","MT29F4G01ABAFDWB","W25N04KV","MX35LF4G24AD","GD5F4GQ6Ux"]
["8Gb","100Mhz","AS5F18G04SND-10LIN","TH58CYG3S0HRAIJ"]
["8Gb","120Mhz","AS5F38G04SND-08LIN","TH58CVG3S0HRAIJ"]

{"sheet":"eMMC","index":28,"n_rows":10,"n_cols":8,"rows_kept":10,"cut":false,"hidden":false,"merged":[[6,7,6,9],[7,7,7,9],[8,7,8,9],[9,7,9,9]]}
[]
[]
[]
[]
["eMMC"]
[]
["DENSITY","VCC","VCCQ","CLOCK FREQUENCY","Package","NAND Type","TEMPERATURE","Alliance Memory"]
["4GB","2.7V~3.6V","1.8V / 3.3V ","200 MHz","153b FBGA","MLC","Industrial(-40°C to 85°C)","ASFC4G31M-51BIN"]
["8GB","2.7V~3.6V","1.8V / 3.3V ","200 MHz","153b FBGA","MLC","Industrial(-40°C to 85°C)","ASFC8G31M-51BIN"]
["16GB","2.7V~3.6V","1.8V / 3.3V ","200 MHz","153b FBGA","MLC","Industrial(-40°C to 85°C)","ASFC16G31M-51BIN"]

{"sheet":"eMMC Cross Reference","index":29,"n_rows":10,"n_cols":10,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
["eMMC Cross Reference"]
[]
["DENSITY","ALLIANCE","MICRON","SAMSUNG","SK HYNIX","MACRONIX","KINGSTON","KIOXIA","SKY-HIGH","ISSI"]
["4GB","ASFC4G31M-51BIN","MTFC4Gxxx","KLM4G1Gxxx ","H26M31001HPR","MX52LM04xxx","EMMC04Gxxx","THGBMNG5Dxxx","S40FC004Cxxx","IS21ES04Gxxx"]
["8GB","ASFC8G31M-51BIN","MTFC8Gxxx","KLM8G1Gxxx","H26M41208HPR","MX52LM08xxx","EMMC08Gxxx","THGBMJG6C1xxx","S40FC008Cxxx","IS21ES08Gxxx\nIS21TF08Gxxx"]
["16GB","ASFC16G31M-51BIN","MTFC16Gxxx","KLMAG2Gxxx","H26M51002xxx",null,"EMMC16Gxxx","THGBMUG7C1xxx","S40FC016xxx","IS21TF16Gxxx"]

{"sheet":"Alliance Packaging Quantities","index":30,"n_rows":118,"n_cols":8,"rows_kept":118,"cut":false,"hidden":false,"merged":[[68,0,68,4],[72,0,72,4],[78,0,78,4]]}
["FAST SRAM ORDER QTY"]
["Part #","Package","Package","Box Qty","Quantity Per Tray/Tube","Reel size","Tape Width (mm)","Tape Pitch (mm)"]
["164A, 256A, 3256A","JxN","28 SOJ - 300mil",2500,"25/Tube",1000,24,12]
["256B","JIN","28 SOJ - 300mil",1080,"27/Tube",1000,24,12]
["3256B","JIN","28 SOJ - 300mil",1352,"26/Tube",1000,24,12]
["256A, 3256A","TxN","28 TSOP I (8x13.4)",2340,"234/Tray",1000,24,12]
["1025B, 31025B, 1024B, 31024B","TJCN","32.3 SOJ - 300mil",2200,"22/Tube",1000,32,12]
["1024C","TJIN","32.3 SOJ - 300mil",920,"23/Tube",1000,32,12]
["31025C","TJIN","32.3 SOJ - 300mil",805,"23/Tube",1000,32,12]
["1025B, 31025B, 1024B, 31024B","JCN","32.4 SOJ - 400mil",2100,"21/Tube",1000,32,16]
["1024C, 1025C, 31025C","JIN","32.4 SOJ - 400mil",805,"23/Tube",1000,32,16]
["513B, 3513B, 1026B, 31026B","JCN","44 SOJ - 400mil - 1 Meg",1600,"16/Tube",500,44,16]
["1026C, 31026C","JIN","44 SOJ - 400mil - 1 Meg",560,"16/Tube",500,44,16]
["1024B, 31024B","TCN","32 TSOP I (8x20)",1560,"156/Tray",1000,32,12]
["31025C","TIN","32 TSOP I (8x20)",805,"23/Tube",1000,32,12]
["513B, 3513B, 1026B, 31026B","TCN","44 TSOP II - 400mil - 1 Meg",1350,"135/Tray",1000,32,16]
["1026C, 31026C","TIN","44 TSOP II - 400mil - 1 Meg",1352,"26/Tube",1500,32,16]
["31026C","BIN","48ball FBGA",3600,"360/Tray",2000,44,16]
["4096A, 34096A, 4098A, 34098A","TxN","44 TSOP II - 400mil - 4 Meg",1350,"135/Tray",1000,32,16]
["4096A, 34096A","JxN","36 SOJ - 400mil",1900,"19/Tube",500,44,16]
["4098A, 34098A","JxN","44 SOJ - 400mil - 4 Meg",1600,"16/Tube",500,44,16]
["34098A","B","48ball BGA",2200,"480/Tray"]
["38096A, 38098A","TIN","44 TSOP II",1350,"135/Tray",1000,44,16]
["38096A, 38098A","B","48ball BGA",4800,"480/Tray",2000,44,16]
["316096A, 316098A","TIN","48 TSOP I",1350,"135/Tray",1000,44,16]
["316098A","B","48ball BGA",4800,"480/Tray",2000,16,16]
["325632,351232","BIN","90ball TFBGA",2400,"240/Tray",2000]
[]
[]
[]
["LOW POWER SRAM ORDER QTY"]
["Part #","Package Suffix","Package","Box Qty","Quantity Per Tray/Tube","Reel size","Tape Width (mm)","Tape Pitch (mm)"]
["6264/62256","S","28pin 330mil SOP",2500,"25/Tube",1000,24,16]
["6264/62256","P","28pin 600mil DIP",600,"15S/Tube","NA","NA","NA"]
["6264/62256","ST","28pin STSOP (8x13.4)",2340,"234/Tray",1500,24,12]
["1008/2008/4008","P","32pin 600mil DIP",520,"13S/Tube","NA","NA","NA"]
["1008/2008/4008","S","32pin 450mil SOP",2200,"22/Tube",1000,32,16]
["1008/2008/4008","T","32pin TSOP I (8x20)",1560,"156/Tray",1500,32,12]
["1008/2008/4008","ST","32pin STSOP (8x13.4)",2340,"234/Tray",1500,24,12]
["1016/2016/4016/8008/8016","Z","44pin TSOP II 400mil",1350,"135/Tray",1000,32,12]
["1616/6416","T","48pin TSOP I",960,"96/Tray",1500]
["1008/2008/4008/8008/1016/\n1616/2016/4016/8016/1616/3216","B","36B/48B TFBGA (6x8)","4800 or 3000","480/Tray Or 300/Tray",2000,16,12]
[4008,"Z","32pin TSOP II",1170,"117/Tray",1000,32,16]
[]
[]
[]
["DRAM ORDER QTY"]
["Part# ","Package ","Box Qty ","Quantity Tray ","Reel size "]
["SDRAM "]
["AS4C1M16S","50pin TSOP II",1170,"117/Tray",1000]
["AS4C4M16S/AS4C4M16SA","54pin TSOP II",1080,"108/Tray",1000]
["AS4C4M16S/AS4C4M16SA","54ball BGA",3480,"348/Tray",2500]
["AS4C4M16SA-7B2CN","60ball FBGA",2860,"286/Tray",2000]
["AS4C2M32SA/AS4C4M32SA","86pin TSOP II",1080,"108/Tray",1000]
["AS4C2M32S/AS4C4M32S","90ball BGA",1900,"190/Tray",2000]
["AS4C8M16S/AS4C8M16SA","54pin TSOP II",1080,"108/Tray",1000]
["AS4C8M16S/AS4C8M16SA","54ball TFBGA",3480,"348/Tray",2500]
["AS4C16M16S/AS4C16M16SA","54pin TSOP II",1080,"108/Tray",1000]
["AS4C16M16S/AS4C16M16SA","54ball FBGA",3480,"348/Tray",2500]
["AS4C8M32S","90 ball LFBGA",1900,"190/Tray",2000]
["AS4C32M16SA","54pin TSOP II",1080,"108/Tray",1000]
["AS4C32M16SA","54ball FBGA",3480,"348/Tray",1000]
["MT48LC32M16A2P-75*","54pin TSOP II",1000,"108/Tray",1000]
["MT48LC64M8A2P-75*","54pin TSOP II",1000,"108/Tray",1000]
["*Alliance Memory has collaborated with Micron for exclusive rights to continue to provide these Micron marked parts"]
[]
[]
["Part #","Package","Box Qty","Quantity Tray/Reel","Reel size"]
["DDR1"]
["AS4C4M16D1A/AS4C8M16D1/AS4C8M16D1A/AS4C16M16D1/AS4C16M16D1A/ AS4C32M8D1/AS4C32M16D1/AS4C32M16D1A/AS4C64M8D1/ AS4C64M16D1/AS4C64M16D1A","66pin TSOP II",1080,"108/Tray",1000]
["AS4C8M16D1/AS4C16M16D1/AS4C32M16D1/AS4C64M8D1","60ball BGA",2400,"240/Tray",2500]
["AS4C2M32D1A/AS4C4M32D1A","144ball FBGA",1890,"189/Tray",1500]
["DDR2"]
["AS4C16M16D2/AS4C32M16D2/AS4C32M16D2A/AS4C64M16D2","84ball FBGA",2090,"209/Tray",2500]
["AS4C64M8D2","60ball FBGA",2090,"209/Tray",2500]
["AS4C128M8D2","60ball FBGA",3000,"300/Tray",2500]
["AS4C128M16D2/AS4C128M16D2A","84ball FBGA",2090,"209/Tray",2500]
["AS4C256M8D2","60ball FBGA",1360,"136/Tray",2500]
["DDR3"]
["AS4C32M16D3-12BxN/AS4C32M16D3L-12BxN","96ball FBGA",2090,"209/Tray",1500]
["AS4C64M8D3-12BxN/AS4C64M8D3L-12BxN","78ball FBGA",2420,"242/Tray",2500]
["AS4C128M8D3/AS4C128M8D3L","78ball FBGA",2420,"242/Tray",1000]
["AS4C64M16D3A","96ball FBGA",2090,"209/Tray",2000]
["AS4C64M16D3LA","96ball FBGA",1900,"190/Tray",2000]
["AS4C128M16D3A/AS4C128M16D3B","96ball FBGA",2090,"209/Tray",1500]
["AS4C128M16D3LA/ AS4C128M16D3LB","96ball FBGA",1900,"190/Tray",2000]
["AS4C256M8D3A/AS4C256M8D3LA","78ball FBGA",2420,"242/Tray",1000]
["AS4C256M16D3A/AS4C256M16D3LA","96ball FBGA",1900,"190/Tray",1000]
["AS4C256M16D3B/AS4C256M16D3LB","96ball FBGA",1800,"180/Tray",2000]
["AS4C512M8D3B/AS4C512M8D3LB","78ball FBGA",2200,"220/Tray",1000]
["AS4C256M32D3/AS4C256M32D3L","136-ball FBGA",2200,"220/Tray",1000]
["AS4C512M16D3L/AS4C1G8MD3L","96ball FBGA",1020,"170/Tray",1000]
[]
[]
[]
[]
["Part#","Package","Box Qty","Quantity Tray","Reel size"]
["MOBILE SDRAM"]
["AS4C8M16MSA/AS4C16M16MSA/AS4C32M16MSA","54-ball FBGA",3190,"319/Tray",1000]
["AS4C4M32MSA/AS4C8M32MSA/AS4C16M32MSA","90-ball FBGA",1900,"190/Tray",1000]
[]
["MOBILE DDR1"]
["AS4C16M16MD1","60-ball FPBGA",1600,"160/Tray",1000]
["AS4C32M16MD1/ AS4C32M16MD1A","60-ball FPBGA",1600,"160/Tray",1000]
["AS4C16M32MD1","90-ball FPBGA",2400,"240/Tray",1000]
["AS4C64M16MD1A","60-ball FPBGA",1600,"160/Tray",1000]
["AS4C32M32MD1A","90-ball FPBGA",2400,"240/Tray",1000]
["AS4C64M32MD1","90-ball FPBGA",2400,"240/Tray",1000]
[]
["MOBILE DDR2"]
["AS4C64M16MD2-25BCN/AS4C32M32MD2-25BCN","134ball FBGA (10 x 11.5 x 1.0)",1280,"128/Tray",1000]
["AS4C128M16MD2-25BCN/AS4C64M32MD2-25BCN","134ball FBGA (10 x 11.5 x 1.0)",1280,"128/Tray",1000]
["AS4C128M32MD2-18BxN","134ball FBGA (11.5 x 11.5 x 1.0)",1680,"168/Tray",1000]
["AS4C256M32MD2--18BxN","134ball FBGA (11.5 x 11.5 x 1.0)",1680,"168/Tray",1000]
[]
[]
[]
["Back to Index"]

{"sheet":"Part Numbering System - SRAM ","index":31,"n_rows":48,"n_cols":2,"rows_kept":48,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Go Back To ","Index"]

{"sheet":"Part Numbering System - DRAM ","index":32,"n_rows":50,"n_cols":2,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Go Back To","Index"]

{"sheet":"Alliance Memory Contact","index":33,"n_rows":30,"n_cols":15,"rows_kept":30,"cut":false,"hidden":false,"merged":[]}
[]
["Contact Information"]
[]
[]
["US Headquarter",null,null,null,null,null,null,"ASIA Headquarter",null,null,null,null,null,null,"INDIA Sales Office"]
["Alliance Memory , Inc.",null,null,null,null,null,null,"Alliance Memory, Inc.",null,null,null,null,null,null,"Bangalore – INDIA"]
["12815 NE 124th St, Suite #D,\nKirkland, WA  98034",null,null,null,null,null,null,"NO.22, Xingde Road,Dayuan DIST,",null,null,null,null,null,null,"Ramesh Varadharajan"]
["- Phone: +1(425) 898 4456",null,null,null,null,null,null,"Taoyuan City 337002, Taiwan",null,null,null,null,null,null,"- Phone: +91 96065 00288"]
["- Fax: +1(425) 896 8628",null,null,null,null,null,null,"- Phone: +886 3461 4646",null,null,null,null,null,null,"- Email: ram@alliancememory.com"]
[null,null,null,null,null,null,null,"- Fax:+886 3461 0697"]
[null,null,null,null,null,null,null,"- Email: judy@alliancememory.com"]
[]
[]
[]
["CANADA Sales Office",null,null,null,null,null,null,"CHINA Sales Office",null,null,null,null,null,null,"Romania Sales Office"]
["Tom Gargan",null,null,null,null,null,null,"Excellence Century Center",null,null,null,null,null,null,"Viorel Toadere"]
["- Phone:+1(514) 442-0677",null,null,null,null,null,null,"Fuhua 3 Road, Futian District 518000",null,null,null,null,null,null,"- Phone: +40(722) 435 465"]
["- Email: tom@alliancememory.com",null,null,null,null,null,null,"Shenzhen, Guangdong,China",null,null,null,null,null,null,"- Email: viorel@alliancememory.com"]
[null,null,null,null,null,null,null,"- Phone: +86(189) 2600 6867"]
[null,null,null,null,null,null,null,"- Email: mars@alliancememory.com"]
[]
[]
[]
[]
["EMEA Headquarter",null,null,null,null,null,null,"JAPAN Sales Office",null,null,null,null,null,null,"NORTH AMERICA REP"]
["Alliance Memory, Inc.",null,null,null,null,null,null,"3-7-10, Sakurajyousui, Setagaya-Ku",null,null,null,null,null,null,"Eclipse Technologies"]
["7 Pauls Field",null,null,null,null,null,null," Tokyo, Japan 156-0045",null,null,null,null,null,null,"WI-IL Region covered"]
["Eversley, Hampshire, RG27, ONE, United Kingdom",null,null,null,null,null,null,"- Phone: +81(90) 3963 0869"]
["- Phone: +44(0) 787-634-4055",null,null,null,null,null,null,"- Email: ted@alliancememory.com"]
["- Email: sue@alliancememory.com"]