{"text_format":"1","workbook":"xlsx","n_sheets":40,"sheets":["Alliance Selection Guide Index","Master cross Reference","SDRAM","SDRAM Cross Reference","DDR1  SDRAM","DDR1 SDRAM Cross Reference","DDR2 SDRAM","DDR2 SDRAM Cross Reference","DDR3 SDRAM ","DDR3 SDRAM Cross Reference","DDR4 SDRAM","DDR4 SDRAM Cross Reference","Mobile LP DRAM-SDRAM","Mobile LP DRAM Cross Reference","LPDDR4-LPDDR4X","LPDDR4-LPDDR4X cross Reference","pSRAM","pSRAM Cross Reference","Fast Asynchronous SRAM","Fast Asyn SRAM Cross Reference","Low Power Asynchronous SRAM","Low Power Asyn SRAM Cross Refer","Parallel 5V NOR Flash","Parallel 5V NOR Falsh Cross Ref","SLC Parallel NAND Flash","SLC Parallel NAND Flash.Cross R","Serial NOR Flash","Serial NOR Flash Cross Ref","Serial NAND Flash","Serial NAND Flash Cross Ref","eMMC","eMMC Cross Reference","Alliance Packaging Quantities","Part Numbering System - SRAM ","Part Numbering System - DRAM ","Part Numbering System - Paralle","Part Numbering System - S.NAND","Part Numbering System-Serial SL","Part Numbering System-eMMC","Alliance Memory Contact"],"not_rendered":{"charts":0,"images":8,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Alliance Selection Guide Index","index":0,"n_rows":12,"n_cols":2,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,0,0,1],[33,0,34,0]]}
[" "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Last Update:",{"$f":"TODAY()","v":"2024-04-24"}]
["Last Update by:","VB-RV-GH"]

{"sheet":"Master cross Reference","index":1,"n_rows":383,"n_cols":12,"rows_kept":383,"cut":false,"hidden":false,"merged":[[94,5,95,5],[96,0,97,0],[96,2,97,2],[96,3,97,3],[96,4,97,4],[96,5,97,5],[94,0,95,0],[94,2,95,2],[94,3,95,3],[94,4,95,4],[91,0,92,0],[91,2,92,2],[91,3,92,3],[91,4,92,4],[91,5,92,5],[58,5,58,6],[89,0,90,0],[89,2,90,2],[89,3,90,3],[89,4,90,4],[89,5,90,5]]}
["Synchronous DRAM 3.3V Cross Reference"]
["DENSITY","ORG","ALLIANCE","SAMSUNG (EOL)","MICRON","SK HYNIX (EOL)","ISSI","WINBOND","NANYA (EOL)","ELITE (ESMT)","ELPIDA (EOL)"]
["16Mb","1M x 16","AS4C1M16S-6/7TxN","K4S161622E","MT48LC1M16A1","HY57V161610","IS42S16100","W9816G6TH","NT56V1616AOT","M12L16161A-xTG2Q","EDS1616AGTA"]
["64Mb","4M x 16","AS4C4M16SA-5/6/7TxN\nAS4C4M16SB-6TIN","K4S641632N-UCxx","MT48LC4M16A2P","HY57V641620","IS42S16400\nIS45S16400","W9864G6JH","NT56V6620C0T-xxB","M12L64164A-xTG2U","uPD4564163G5-Axx"]
["64Mb","4M x 16","AS4C4M16SA-6/7BxN",null,"MT48LCM16A2B4(F4)","HY5V66D","IS42S16400\nIS45S16400","W9864G6JT",null,"M12L64154A-xBG2C"]
["64Mb","4M x 16","AS4C4M16SA-7B2CN",null,null,null,"IS42S16400","W9864G6JB-7"]
["64Mb","2M x 32","AS4C2M32S-6/7BxN",null,"MT48LC2M32B2B5-x","HY5V62","IS42S32200","W9864G2IB-x",null,null,"EDS6432AFBH"]
["64Mb","2M x 32","AS4C2M32SA-6/7TxN","K4S643232H-Ucxx","MT48LC2M32B2P-x (EOL)","HY57V643220","IS42S32200","W9864G2J(G,I)H-x",null,"M12L64322A-xTG2U","EDS6432AFTA"]
["128Mb","8M x 16","AS4C8M16SA-6/7TxN\nAS4C8M16SB-6TIN","K4S281632K-UCxx","MT48LC8M16A2P","HY57V281620","IS42S16800\nIS45S16800","W9812G6K(G,I)H","NT5SV8M16AT-xxB","M12L128168A-xTG2N","uPD45128163G5-Axx"]
["128Mb","8M x 16","AS4C8M16SA-6/7BxN","K4S281632D-RL75","MT48LC8M16A2B4(F4)","HY5V26","IS42S16800\nIS45S16800","W9812G6JB",null,"M12L128168A-xBG2N"]
["128Mb","4M x 32","AS4C4M32S-6/7BxN",null,"MT48LC4M32B2B5-x","HY5V22","IS42S32400","W9812G21(G)B-x",null,"M12L128324-xBG2E","EDS1232AHBH"]
["128Mb","4M x 32","AS4C4M32SA-6/7TxN",null,"MT48LC4M32B2P-x (EOL)","HY57V283220T","IS42S32400","W9812G2GH",null,null,"EDS1232AHTA"]
["256Mb","16M x 16","AS4C16M16SA/B-6/7TxN","K4S561632N-UCxx","MT48LC16M16A2P","H57V2562GTR","IS42S16160\nIS45S16160","W9825G6K(D,E,J)H","NT5SV16M16AT-xxB","M12L2561616A-xTG2A","EDS2516AP(AF,AC)TA-xx"]
["256Mb","16M x 16","AS4C16M16SA/B-6/7BxN","K4S561632D-RL75","MT48LC16M16A2B4","HY5V56","IS42S16160\nIS45S16160","W9825G6JB",null,"M12L2561616A-xBG2A","EDS2516EE(JE)BH"]
["256Mb","8M x 32","AS4C8M32S-6/7TxN",null,"MT48LC8M32B2B5-x (EOL)","HY5V52","IS42S32800","W9825G2J(D)B-x",null,null,"EDS2532EEBH"]
["256Mb","8M x 32","AS4C8M32SA-6/7BxN",null,"MT48LC8M32B2B5-x","HY5V52","IS42S32800","W9825G2J(D)B-x",null,null,"EDS2532EEBH"]
["256Mb","32M X 8","AS4C32M8SA-6/7TxN",null,"MT48LC32M8A2P",null,"IS42S83200J"]
["256Mb","64M x 4","AS4C64M4SA-6/7TxN",null,"MT48LC64M4A2P (EOL)",null,"IS42S32800"]
["512Mb","32M x 16","AS4C32M16SB-7BIN",null,null,null,"IS42S16320",null,null,"M12L5121632A"]
["512Mb","32M x 16","AS4C32M16SB-6/7TxN","K4S511632M-TC75","MT48LC32M16A2 (EOL)",null,"IS42S16320",null,null,"M12L5121632A","EDS5116ABTA"]
["512Mb","32M x 16","AS4C32M16SC-7TIN","K4S511632M-TC75","MT48LC32M16A2 (EOL)",null,"IS42S16320",null,null,"M12L5121632A","EDS5116ABTA"]
["512Mb","16M x 32","AS4C16M32SB-6BxN",null,"MT48LC16M32S2 (EOL)",null,"IS42S32160"]
["512Mb","16M x 32","AS4C16M32SC-7TIN",null,null,null,"IS42S32160"]
["512Mb","64M x 8","AS4C64M8SC-7TIN",null,"MT48LC64M8A2P-75:C (EOL)",null,"IS42S86400"]
["512Mb","64M x 8","AS4C64M8SD-7TCN",null,"MT48LC64M8A2P-75:C (EOL)",null,"IS42S86400"]
[]
["DDR1       2.5V SDRAM Cross Reference"]
["DENSITY","ALLIANCE","SAMSUNG (EOL)","MICRON","ISSI","HYNIX - ALL EOL","WINBOND","NANYA","ELITE (ESMT)","ELPIDA"]
["64Mb","AS4C4M16D1A-5TxN","K4H641638N","MT46V4M16TG (EOL)","IS43R16400B",null,"W9464G6K(I,J)H",null,"M13S64164A-5TG2Y","(EOL)"]
["64Mb","AS4C2M32D1A-5BxN"]
["128Mb","AS4C8M16D1-5BXN","K4H281638D",null,"IS43R16800E-5BL",null,"W9412G6JB",null,"M13S128168A-5BG2N","EDD1216A"]
["128Mb","AS4C8M16D1A-5TxN","K4H281638D","MT46V8M16 (EOL)","IS43R16800E-5TL","HY5DU1281622","W9412G6K(I,J)H",null,"M13S128168A-5TG2N","EDD1216A"]
["128Mb","AS4C4M32D1A-5BxN",null,"MT46V4M32FK (EOL)","IS43R32400E-5BL",null,"W9412GIB",null,"M13S128324A-5BG2M","EDD1232A"]
["256Mb","AS4C32M8D1-5TxN","K4H560838N","MT46V32M8P (EOL)","IS43R83200","HY5DU56822",null,"NT5DS32M8ES",null,"EDD2508A"]
["256Mb","AS4C16M16D1-5BxN","K4H561638D","MT46V16M16CY-5B","IS43R16160\nIS46R16160","HY5DU561622","W9425G6JB",null,"M13S2561616A-xBG2A"]
["256Mb","AS4C16M16D1A-5TxN","KH561638D","MT46V16M16P","IS43R16160","HY5DU561622","W945G6K(D,E,J)H",null,"M13S2561616A-xTG2A","EDD2516A"]
["512Mb","AS4C32M16D1-5BxN","K4H511638J","MT46V32M16CY","IS43R16320\nIS46R16320","HY5DU121622",null,null,null,"EDD5116"]
["512Mb","AS4C32M16D1A-5TxN","K4H511638J","MT46V32M16P","IS43R16320\nIS46R16320","HY5DU121622",null,"NT5DS32M16ES","M13S5121632A-5TG2S","EDD5116A"]
["512Mb","AS4C64M8D1-5TxN","K4H510838J","MT46V64M8P","IS43R86400","HY5DU12822",null,"NT5DS64M8ES",null,"EDD5108A"]
["512Mb","AS4C64M8D1-5BxN","K4H510838J","MT46V64M8CY(BN)","IS43R86400","HY5DU12822"]
["1Gb","AS4C64M16D1-6TxN",null,"MT46V64M16P (EOL)"]
["1Gb","AS4C64M16D1A-6BIN"]
[]
["DDR2    1.8V SDRAM Cross Reference"]
["DENSITY","ALLIANCE","SAMSUNG (EOL)","MICRON","ISSI","WINBOND","NANYA","ELITE (ESMT)","HYNIX (EOL)"]
["256Mb","AS4C16M16D2-25BxN","K4T56163Q","MT47H16M16BG","IS43DR16160","W9725G6K(J)B","NT5TU16M16BG","M14D2561616A-2.5BG","HY5PS561621"]
["512Mb","AS4C32M16D2A/C-25BxN","K4T51163Q","MT47H32M16HR(NF)-25E","IS43DR16320\nIS46DR16320","W9751G6K(J)B","NT5TU32M16GG","M14D5121632A-2.5BG","HY5PS121621"]
["512Mb","AS4C64M8D2-25BxN","K4T51083Q","MT47H64M8CF(SH)-25E","IS43DR86400\nIS46DR86400","W9751G8K(J)B","NT5TU64M8EE",null,"H5PS5182KFR"]
["1Gb","AS4C64M16D2A-25BxN","K4T1G164Q","MT47H64M16HR(NF)-25E","IS43DR16640\nIS46DR16640","W971GG6JB","NT5TU64M16HG","M14D1G1664A-2.5BG","H5PS1G63"]
["1Gb","AS4C64M16D2B-25BCN","K4T1G164Q","MT47H64M16HR(NF)-25E","IS43DR16640","W971GG6JB","NT5TU64M16HG","M14D1G1664A-2.5BG","H5PS1G63"]
["1Gb","AS4C128M8D2A-25BxN","K4T1G084Q","MT47H128M8SH-25E","IS43DR81280","W971GG8JB","NT5TU128M8HE","M14D1G8128A","H5PS1G83"]
["2Gb","AS4C128M16D2-25BxN",null,"MT47H128M16RT-25E","IS43DR16128","W972GG6JB"]
["2Gb","AS4C128M16D2A-25BxN",null,"MT47H128M16RT-25E","IS43DR16128\nIS46DR16128","W972GG6JB"]
["2Gb","AS4C256M8D2A-25BCN",null,"MT47H256M8EB-25E","IS43DR82560","W972GG8JB"]
[]
["DDR3 SDRAM Cross Reference"]
["DENSITY","ALLIANCE","MICRON","SAMSUNG(EOL)","ISSI","HYNIX","WINBOND","ELITE (ESMT)","ELPIDA","NANYA"]
["512Mb","AS4C32M16D3-12BxN",null,null,null,null,"W6351G6KB-x","M15T5121632A","EDJ5316BASE"]
["512Mb","AS4C64M8D3-12BxN",null,null,null,null,null,null,"EDJ5308BASE"]
["512Mb","AS4C32M16D3L-12BxN",null,null,null,null,null,"M15T5121632A","EDJ5316BASE"]
["512Mb","AS4C64M8D3L-12BxN",null,null,null,null,null,null,"EDJ5308BASE"]
["1Gb","AS4C64M16D3B-12BxN","MT41J64M16JT(TW)-125 (EOL)","K4B1G1646x","IS43TR16640\nIS46TR16640","H5TQ1G63D","W631GG6KB-x","M15F1G1664A","EDJ1116DJ(BA) BG","NT5CB64M16F(G)P"]
["1Gb","AS4C64M16D3LB/C-12BxN","MT41K64M16JT(TW)-125","K4B1G1646x","IS43TR16640xL\nIS46TR16640xL","H5TC1G63EFR (EOL)","W631GU6KB-x","M15T1G1664A-(2C)","EDJ1116EJBG","NT5CC64M16F(G)P-DI"]
["1Gb","AS4C128M8D3B-12BxN","MT41J128M8JP(DA)-125","K4B1G0846x","IS43TR81280\nIS46TR81280","H5TQ1G83","W631GG8KB-x","M15T1G8128A","EDJ1108DJ(BA) BG","NT5CB128M8F(G)N-DI"]
["1Gb","AS4C128M8D3LB/C-12BxN","MT41K128M8JP(DA)-125","K4B1G0846x","IS43TR81280xL\nIS46TR81280xL","H5TC1G83EFR (EOL)","W631GU8KB-x","M15T1G8128A","EDJ1108EJBG","NT5CC128M8F(G)N-DI"]
["2Gb","AS4C128M16D3C-93BCN","MT41J128M16JT(TW)-125","K4B2G1646x","IS43TR16128","H5TQ2G63","W632GG6KB-x","M15F2G16128A","EDJ2116DEBG","NT5CB128M16I(F)P-DI"]
["2Gb","AS4C128M16D3LC-12BxN","MT41K128M16JT-125","K4B2G1646x","IS43TR16128xL\nIS46TR16128xL","H5TC2G63","W632GU6KB-x","M15F2G16128A","EDJ2116EEBG","NT5CC128M16I(F)P-DI"]
["2Gb","AS4C256M8D3LC-12BxN","MT41K256M8DA-125","K4B2G0846x","IS43TR82560xL\nIS46TR82560xL","H5TQ2G83FFR-x","W632GG8KB-x","M15T2G8256A","EDJ2108DEBG","NT5CB256M8IN-FL"]
["4Gb","AS4C256M16D3C-93BCN AS4C256M16D3C-10BxN AS4C256M16D3C-12BxN","MT41J256M16HA-107 MT41J256M16HA-125","K4B4G1646x","IS43TR16256","H5TQ4G63","W634GG6MB/ NB","M15F4G16256A","EDJ4216BFBG (BASE)","NT5CB256M16C(D,E) P-DI"]
["4Gb","AS4C256M16D3LC-10BxN AS4C256M16D3LC-12BxN","MT41K256M16HA-107/125 MT41K256M16TW-107/125","K4B4G1646x","IS43TR16256xL\nIS46TR16256xL","H5TC4G63","W634GU6MB/NB","M15T4G16256A","EDJ4216EFBG","NT5CC256M16C(D,E) P-DI"]
["4Gb","AS4C512M8D3LC-10BAN\nAS4C512M8D3LC-12BxN","MT41K512M8DA-125","K4B4G0846x","IS43TR85120xL\nIS46TR85120xL","H5TC4G83","W634GU8MB/NB","M15T4G8512A","EDJ4208EFBG","NT5CC512M8C(D,E) N-DI"]
["8Gb","AS4C512M16D3LA-10BxN","MT41K512M16VRN-107 MT41K512M16VRP-107 MT41K512M16HA-125 (EOL)","K4B8G1646x","IS43TR16512","H5TC8G63CMR","W638GU6QB","M15T8G16512A–DE",null,"NT5CC512T16EH-DI/A/H\nNT5CC512T16EH-EK/A/H"]
["8Gb","AS4C512M16D3LB-12BxN","MT41K512M16HA-125 (EOL)","K4B8G1646x","IS43TR16512","H5TC8G63CMR","W638GU6QB","M15T8G16512A–BD",null,"NT5CC512T16EH-DI/A/H"]
["8Gb","AS4C512M16D3LC-10BxN\nAS4C512M16D3LC-12BxN","MT41K512M16VRN-107 MT41K512M16VRP-107 MT41K512M16HA-125 (EOL)","K4B8G1646x","IS43TR16512","H5TC8G63CMR","W638GU6QB","M15T8G16512A–BD\nM15T8G16512A–DE",null,"NT5CC512T16EH-DI/A/H\nNT5CC512T16EH-EK/A/H"]
["8Gb","AS4C1G8D3LA-10BxN","MT41K1G8SN-107/125:E","K4B8G0846x","IS43TR81024","H5TC8G83BMR"]
["8Gb","MT41K512M16HA-125","MT41K512M16HA-125","K4B8G1646x","IS43TR16512","H5TC8G63CMR","W638GU6QB","M15T8G16512A–BD",null,"NT5CC512T16EH-DI/A/H"]
[]
["DDR4 SDRAM Cross Reference"]
["DENSITY","ORG","ALLIANCE","MICRON","NANYA","SAMSUNG","HYNIX","ISSI"]
["4Gb","256M x 16","AS4C256M16D4-83BxN\nAS4C256M16D4-75BxN","MT40A256M16GE","NT5AD256M16D4","K4A4G165Wx","H5AN4G6NBJR","IS43QR16256"]
["4Gb","512M x 8","AS4C512M8D4-83BxN\nAS4C512M8D4-75BxN","MT40A512M8RH","NT5AD512M8D4","K4A4G085Wx","H5AN4G8NBJR","IS43QR85120"]
["4Gb","256M x 16","AS4C256M16D4A-62BxN\nAS4C256M16D4A-75BxN","MT40A256M16GE","NT5AD256M16D4","K4A4G165Wx","H5AN4G6NBJR","IS43QR16256"]
["4Gb","512M x 8","AS4C512M8D4A-75BxN","MT40A512M8RH","NT5AD512M8D4","K4A4G085Wx","H5AN4G8NBJR","IS43QR85120"]
["8Gb","512M x 16","AS4C512M16D4-75BxN\nAS4C512M16D4A-62BxN","MT40A512M16LY/JY","NT5AD512M16C4","K4A8G165Wx","H5AN8G6NCJR","IS43QR16512A\nIS46QR16512A"]
["8Gb","1G x 8","AS4C1G8D4-75BxN\nAS4C1G8D4A-62BxN","MT40A1G8SA/WE","NT5AD1024M8C3","K4A8G085Wx","H5AN8G8NCJR","IS43QR81024A"]
["16Gb","1G x 16","MT40A1G16KH-062E\nAS4C1G16D4-062BCN","MT40A1G16KH/KNR",null,"K4AAG165Wx","H5ANAG6NCMR-XNC\nH5ANAG6NDMR-XNC"]
[]
["MOBILE LOW POWER SDRAM Cross Reference"]
["DENSITY","ALLIANCE","MICRON","ISSI","NANYA","WINBOND"]
["128Mb","AS4C8M16MSA-6BIN",null,"IS42VM16800H",null,"W987D6HBGX"]
[null,"AS4C8M16MSB-6BIN"]
["256Mb","AS4C16M16MSA-6BIN","MT48H16M16LFBF (EOL)","IS42VM16160K",null,"W988D6FBGX"]
[null,"AS4C16M16MSB-6BIN"]
["256Mb","AS4C8M32MSB-6BIN","MT48H8M32LFB5 (EOL)","IS42VM32800K",null,"W988D2FBJX"]
["512Mb","AS4C32M16MSA-6BIN","MT48H32M16LFB4-6 IT","IS42VM16320E","NT6SM32M16BG-S1","W989D6DBGX"]
[null,"AS4C32M16MSB-6BIN"]
["512Mb","AS4C16M32MSA-6BIN","MT48H16M32LFB5-6 IT","IS42VM32160E","NT6SM16M32BK-S1","W989D2DBJX"]
[null,"AS4C16M32MSB-6BIN"]
[]
["MOBILE LP DDR1 Cross Reference"]
["DENSITY","ALLIANCE","MICRON","SAMSUNG","ISSI","HYNIX","NANYA","ELITE (ESMT)","WINBOND"]
["256Mb","AS4C16M16MD1-6BCN","MT46H16M16LFBF-6","K4X56163SPN","IS43LR16160","HY5MS5B6/ H5MS2562","NT6DM16M16AD-T1","M53D2561616A-6BG2F","W948D6FBHX"]
["512Mb","AS4C32M16MD1A-5BCN","MT46H32M16LFBF-5","K4X51163PI","IS43R16320B","HY5MS7B6/ H5MS5162","NT6DM32M16A(B)D-T1","M53D5121632A-5BG2T","W949D6DBHX"]
["512Mb","AS4C16M32MD1-5BxN","MT46H16M32LFB5-5","K4X51323PI","IS43LR32160B","H5MS5132/ H5MS5122","NT6DM16M32A(B)C-T1","M53D5123216A-5BG2S","W949D2DBJX"]
["1Gb","AS4C64M16MD1A-5BIN","MT46H64M16LFBF","K4X1G163PE","IS43LR16640A","H5MS1G62"]
["1Gb","AS4C32M32MD1A-5BIN","MT46H32M32LFB5-5","K4X1G323PF","IS43LR32320B","H5MS1G22","NT6DM32M32BC-T1","M53D1G3232A","W94AD2KBJX"]
["2Gb","AS4C64M32MD1-5BxN","MT46H64M32LFKQ-5","K4X2G323PC","IS43LR32640A","H5M52G22"]
["2Gb","AS4C64M32MD1A-5BIN","MT46H64M32LFKQ-5","K4X2G323PC","IS43LR32640A","H5M52G22"]
[]
["MOBILE LP DDR2 Cross Reference"]
["DENSITY","ALLIANCE","MICRON","SAMSUNG","ISSI","HYNIX","NANYA","ELITE (ESMT)","WINBOND"]
["256Mb","AS4C8M32MD2A-25B(P)CN",null,null,"IS43LD32800A-25BLx\nIS43LD32800B-25BLx",null,null,null,"W978H2KBVX2E"]
["1Gb","AS4C64M16MD2A-25BIN","MT42L64M16D1HE-25",null,"IS43LD16640C/A",null,"NT6TL64M16BA(I)-G0",null,"W97AH6KBVX2"]
["1Gb","AS4C32M32MD2A-25BIN","MT42L32M32D1HE-25",null,"IS43LD32320C/A",null,"NT6TL32M32BI(A)-G0",null,"W97AH2KBVX2"]
["2Gb","AS4C128M16MD2A-25BIN","MT42L128M16D1TK-25",null,"IS43LD16128B",null,"NT6TL128M16CI(A)-G0",null,"W97BH6KBVX2"]
["2Gb","AS4C64M32MD2A-25BIN","MT42L64M32D1TK-25",null,"IS43LD32640B",null,"NT6TL64M32CI(A)-G0",null,"W97BH2KBVX2"]
["4Gb","AS4C128M32MD2A-18BIN","MT42L128M32D1GU-18",null,"IS43LD32128A",null,"NT6TL128M32BI(A)-G0"]
["4Gb","AS4C128M32MD2A-25BIN","MT42L128M32D1GU-18",null,"IS43LD32128A",null,"NT6TL128M32BI(A)-G0"]
[]
["LPDDR4 Cross Reference "]
["DENSITY","ORG","ALLIANCE","MICRON","SAMSUNG","HYNIX","NANYA","ISSI","WINBOND","IM"]
["2Gb","128M x 16","AS4C128M16MD4-062BAN","MT53E128M16D1DS",null,"H9HCNNNBKUMLXR/HR","NT6AN128M16AV","IS43/46LQ16128A\nIS43/46LQ16128EA","W66BL6NBU\nW66BP6NBU"]
["2Gb","64M x 32","AS4C64M32MD4-062BAN",null,null,null,null,"IS43/46LQ32640A\nIS43/46LQ32640EA","W66CL2NQU\nW66CP2NQU\nW66CP2NQQ"]
["4Gb","128M x 32","AS4C128M32MD4-062BAN","MT53B128M32D1DS\nMT53E128M32D2DS\nMT53E128M32D2FW","K4F4E3S4HF-GFCJ\nK4F4E3S4HF-GHCJ",null,"NT6AN128T32AV","IS43/46LQ32128A\nIS43/46LQ32128EA","W66CL2NQU\nW66CP2NQU","IME4G32L4HABG"]
["4Gb","256M x 16","AS4C256M16MD4-062BAN","MT53E256M16D1DS\nMT53E256M16D1FW",null,"H9HCNNN4KUMLHR","NT6AN256M16AV","IS43/46LQ16256A\nIS43/46LQ16256EA","W66CP6NBU\nW66CL6NBU"]
["8Gb","256M x 32","AS4C256M32MD4-062BAN","MT53B256M32D1DS\nMT53E256M32D2DS\nMT53E256M32D2FW","K4F8E304HB-MGCJ\nK4F8E3S4HB-MFCJ\nK4F8E3S4HB-MHCJ","H9HCNNN8KUMLHR","NT6AN256T32AV","IS43/46LQ32256A\nIS43/46LQ32256EA","W66DP2NQU\nW66DL2NQU","IME8G32L4HADG"]
[]
["LPDDR4X Cross Reference "]
["DENSITY","ORG","ALLIANCE","MICRON","SAMSUNG","HYNIX","NANYA","ISSI","WINBOND","IM"]
["2Gb","128M x 16","AS4C128M16MD4V-062BAN",null,null,null,null,"IS43/46LQ16128AL\nIS43/46LQ16128EA","W66BQ6NBU"]
["4Gb","256M x 16","AS4C256M16MD4V-062BAN","MT53E256M16D1DS\nMT53E256M16D1FW","K4U8E3S4AD-GFCL\nK4U8E3S4AD-GHC","H9HCNNN4KMMLHR","NT6AP256M16AV","IS43/46LQ16256AL\nIS43/46LQ16256EA","W66CQ6NQU","IM4G16L4JCBG"]
["8Gb","256M x 32","AS4C256M32MD4V-062BAN","MT53B256M32D1DS\nMT53E256M32D2DS\nMT53E256M32D2FW","K4U8E3S4Ax",null,"NT6AP256T32AV","IS43/46LQ32256AL\nIS43/46LQ32256EAL","W66DQ2NQU","IM8G32L4JCBG"]
["8Gb","512M x 16","AS4C512M16MD4V-053BIN","MT53D512M16D1DS\nMT53E512M16D1FW",null,null,"NT6AP512M16AV","IS43LQ16512AL",null,"IM8G16L4JCBG-046"]
["16Gb","512M x 32","AS4C512M32MD4V-053BIN","MT53D512M32D2Dx\nMT53D512M32D1ZW\nMT53D512M32D2FW","K4U6E3S4Ax","H9HCNNNBPUMLHR\n","NT6AP512T32BY",null,null,"IMAG32L4JCBG-046"]
["16Gb","512M x 32","AS4C512M32MD4V-046BIN","MT53D512M32D2Dx\nMT53E512M32D2FW\nMT53E512M32D1ZW","K4U6E3S4Ax","H9HCNNNBKMMLXR\nH9HCNNNBPUMLHR","NT6AP512T32BY",null,null,"IMAG32L4JCBG-046"]
["32Gb","1G x 32","AS4C1G32MD4V-046BIN","MT53D1024M32D4Dx\nMT53E1G32D2FW\nMT53E1G32D2Nx","K4UBE3D4Ax","H9HCNNNCPMMLXR\nH9HCNNNCPMMLXR","NT6AP1024F32B"]
["Fast Asynchronous SRAM Cross Reference"]
["64K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS (EOL)","IDT","ISSI"]
["8K x 8","5V","28pin SOJ (300mil)",15,"AS7C164A-15JxN",null,"CY7C185-15VI (EOL)","IDT7164SXXYG","IS61C64AL-10JLI (EOL)"]
["8K x 8","5V","28pin Skinny PDIP 300mil",15,"AS7C164A-15PxN",null,"CY7C185-20PXC (EOL)"]
["256K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS (EOL)","IDT","ISSI"]
["32K x 8","5V","28pin SOJ","10,12,15,20","AS7C256A-xxJCN/JIN","K6E0808C (EOL)","CY7C199D-XXVXI","IDT71256SAXXYG","IS61C256AL-XXJL (EOL)"]
["32K x 8","5V","28pin TSOP I","10,12,15,20","AS7C256A-xxTCN/TIN",null,"CY7C199D-XXZXI","IDT71256SAXXPZG","IS61C256AL-XXTL"]
["32K x 8","3.3V","28pin SOJ","10,12,15,20","AS7C3256A-xxJCN/JIN","K6E0808V","CY7C1399BN-12VXC","IDT71V256SAXXYG","IS61LV256AL-10JL (EOL)"]
["32K x 8","3.3V","28pin TSOP I","10,12,15,20","AS7C3256A-xxTCN/TIN",null,"CY7C1399BN-XXZXI","IDT71V256SAXXPZG","IS61LV256AL-10TL"]
["32K x 8","5V","28pin DIP",15,"AS7C256B-xxPIN","(EOL)","CY7C199CN-15PXC (EOL)","IDT71256SAXXTPG"]
["512K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI"]
["32K x 16","5V","44pin SOJ (400mil)",15,"AS7C513B-xxJCN",null,"CY7C1020D-10VXI",null,"IS61C321AL-12KLI (EOL)"]
["32K x 16","5V","44pin TSOP II (400mil)","12,15","AS7C513B-xxTCN",null,"CY7C1020D-10ZSXI",null,"IS61C3216AL-12TLI"]
["32K x 16","3.3V","44pin TSOP II (400mil)","12,15,20","AS7C3513B-xxTCN",null,"CY7C1020DV33-10ZSXI",null,"IS61WV3216BLL-12TLI"]
["32K x 16","3.3V","44pin SOJ (400mil)","10,12,15","AS7C3513B-xxJCN",null,"CY7C1020DV33-10VXI"]
["1M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG (EOL)","CYPRESS","IDT","ISSI"]
["128K x 8","5V","32pin SOJ (400mil)","12,15,20","AS7C1025B-xxJCN/JIN","K6R1008C1D-KI10",null,"IDT71124SXXYG"]
["128K x 8","3.3V","32pin SOJ (400mil)","10,12,15,20","AS7C31025B-xxJCN/JIN","K6R1008V1D-KI10","CY7C1019DV33-10VXI","IDT71V124SAXXYG","IS63WV1024L-10KLI (EOL)"]
["128K x 8","5V","32pin SOJ (300mil)","10,12,15,20","AS7C1025B-xxTJCN",null,"CY7C1019D-10VXI"]
["128K x 8","3.3V","32pin SOJ (400mil)",12,"AS7C31025C-12JIN"]
["128K x 8","3.3V","32pin SOJ (300mil)","10,12,15,20","AS7C31025B-xxTJCN",null,"CY7C1018DV33-10VXI","IDT71V124SAXXTYG","IS63WV1288DBLL-10JLI (EOL)"]
["128K x 8","5V","32pin SOJ (400mil)","12,15,20","AS7C1024B-xxJCN/JIN",null,"CY7C109D-10VXI","IDT71024SXXYG","IS61C1024AL-12KLI (EOL)"]
["128K x 8","5V","32pin TSOP I","12,15,20","AS7C1024B-xxTCN",null,"CY7C109D-10ZXI",null,"IS61C1024AL-12TLI"]
["128K x 8","5V","32pin SOJ (300mil)","12,15,20","AS7C1024B-xxTJCN",null,"CY7C1009D-10VXI","IDT71024SXXTYG","IS61C1024AL-12JLI (EOL)"]
["128K x 8","3.3V","32pin SOJ (400mil)","12,15,20","AS7C31024B-xxJCN",null,"CY1019DV33-10VXI",null,"IS63WV1288DBLL-10KLI (EOL)"]
["128K x 8","3.3V","32pin TSOP I","10,12,15,20","AS7C31024B-xxTCN",null,null,null,"IS63WV1288DBLL-10HLI"]
["128K x 8","3.3V","32pin SOJ (300mil)","10,12,15,20","AS7C31024B-xxTJCN",null,"CY7C1018DV33-10VXI",null,"IS63WV1288DBLL-10JLI"]
["64K x 16","5V","44pin SOJ (400mil)","10,12,15,20","AS7C1026B-xxJCN/JIN","K6R1016C1D-KI10","CY7C1021D-XXVXC","IDT71016SXXYG","IS61C6416AL-12KLI (EOL)"]
["64K x 16","5V","44pin TSOP II (400mil)","10,12,15,20","AS7C1026B-xxTCN/TIN","K6R1016C1D-UI10","CY7C1021D-XXZSXI","IDT71016SXXPHG","IS61C6416AL-12TLI"]
["64K x 16","3.3V","44pin SOJ (400mil)","10,12,15,20","AS7C31026B-xxJCN/TIN","K6R1016V1D-KI10","CY7C1021DV33-XXVXI","IDT71V016SAXXYG","IS61WV6416DBLL-10KLI (EOL)"]
["64K x 16","3.3V","44pin TSOP II (400mil)","10,12,15,20","AS7C31026B-xxTCN/TIN","K6R1016V1D-UI10","CY7C1021DV33-XXZSXI","IDT71V016SAXXPHG","IS61WV6416DBLL-10TLI"]
["2M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["128K x 16","3.3V","44pin TSOP II","10,12,15,20","AS7C32098A-xxTxN",null,"CY7C1011DV33-10ZSXI",null,"IS61WV12816DBLL-10TL","GS72116AGP-XX"]
["256K x 8","3.3V","44pin TSOP II","10,12,15,20","AS7C32096A-xxTxN",null,"CY7C1010DV33-10ZSXI",null,"IS61WV256EDBLL-10TLI","GS72108AGP-XX"]
["4M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI"]
["512K x 8","5V","36pin SOJ (400mil)","10,12,15,20","AS7C4096A-xxJxN","K6R4008C1D-KI10","CY7C1049D-10VXI",null,"IS61C5128AL-10KLI (EOL)"]
["512K x 8","5V","44pin TSOP II (400mil)","10,12,15,20","AS7C4096A-xxTxN","K6R4008C1D-UI10",null,null,"IS61C5128AL-10TLI"]
["512K x 8","3.3V","36pin SOJ (400mil)","8,10,12,15,20","AS7C34096A-xxJxN","K6R4008V1D-KI10","CY7C1049DV33-10VXI","IDT71V424SXXYG","IS61WV5128EDBLL-10KLI (EOL)"]
["512K x 8","3.3V","44pin TSOP II (400mil)","10,12,15,20","AS7C34096A-xxTxN","K6R4008V1D-UI10","CY7C1049DV33-10ZSI","IDT71V424SXXPHG","IS61WV5128EDBLL-10TLI"]
["512K x 8","2.7 ~ 3.6V","44pin TSOP II",10,"AS7C34096B-10TIN"]
["512K x 8","2.7 ~ 3.6V","36ball TFBGA",10,"AS7C34096B-10BIN"]
["256K x 16","5V","44pin SOJ (400mil)","10,12,15,20","AS7C4098A-xxJxN","K6R4016C1D-KI10","CY7C1041D-10VXI",null,"IS61C25616AL-10KLI (EOL)"]
["256K x 16","5V","44pin TSOP II (400mil)","10,12,15,20","AS7C4098A-xxTxN","K6R4016C1D-UI10","CY7C1041D-10ZSXI",null,"IS61C25616AL-10TL"]
["256K x 16","3.3V","44pin SOJ (400mil)","10,12,15,20","AS7C34098A-xxJxN","K6R4016V1D-KI10","CY7C1041DV33-10VXI","IDT71V416SXXYG"]
["256K x 16","3.3V","44pin TSOP II (400mil)","8,10,12,15,20","AS7C34098A-xxTxN","K6R4016V1D-UI10","CY7C1041DV33-10ZSXI","IDT71V416SXXPHG","IS61WV25616EDBLL-10TLI"]
["256K x 16","3.3V","48ball TFBGA",10,"AS7C34098A-xxBIN",null,"CY7C1041DV33-10BVXI","IDT71V416SXXBE","IS61WV25616EDBLL-10BLI"]
["256K x 16","2.7 ~ 3.6V","44pin TSOP II",10,"AS7C34098B-10TIN"]
["256K x 16","2.7 ~ 3.6V","48ball TFBGA",10,"AS7C34098B-10BIN"]
["8M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["512K x 16","3.3V","44pin TSOP II",10,"AS7C38098A-10TIN",null,"CY7C1051DV33-10ZSXI",null,"IS61WV51216BLL-XXTLI"]
["512K x 16","3.3V","48ball TFBGA",10,"AS7C38098A-10BIN",null,"CY7C1051DV33-10BAXI",null,"IS61WV51216BLL-10MLI"]
["256K x 32","3.3V","90ball TFBGA",10,"AS7C325632-10BIN",null,null,null,"IS61WV25632BLL-10BLI"]
["1M x 8","3.3V","44pin TSOP II",10,"AS7C38096A-10TIN",null,"CY7C1059DV33-10ZSXI",null,"IS61WV10248BLL-10TLI"]
["1M x 8","3.3V","48ball TFBGA (different pinout)",10,"AS7C38096A-10BIN"]
["1M x 8","3.3V","48ball TFBGA (different pinout)",10,"AS7C38096B-10BIN",null,null,null,"IS61WV10248BLL-10MLI"]
["16M  FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["1M x 16","3.3V","48pin TSOP I",10,"AS7C316098A-10TIN",null,"CY7C1061GN30-10ZXI",null,"IS61WV102416FBLL-10TLI"]
["1M x 16","3.3V","48ball TFBGA",10,"AS7C316098A-10BIN",null,"CY7C1061GN30-10BV1XI",null,"IS61WV102416FBLL-10BLI"]
["1M x 16","3.3V","54pin TSOP II",10,"AS7C316098B-10TIN",null,"CY7C1061GN30-10ZSXI",null,"IS61WV102416FBLL-10T2LI"]
["1M x 16","3.3V","48ball TFBGA",10,"AS7C316098B-10BIN"]
["2M x 8","3.3V","48pin TSOP I",10,"AS7C316096A-10TIN",null,"CY7C1069GN30-10ZSXI",null,"IS61WV20488FBLL-10T2LI"]
["2M x 8","3.3V","54pin TSOP II",10,"AS7C316096B-10TIN",null,"CY7C1069DV33-10ZSXI"]
["2M x 8","3.3V","44pin TSOP II",10,"AS7C316096C-10TIN",null,null,null,"IS61WV20488FBLL-10TLI"]
["2M x 8","3.3V","48ball TFBGA (1CE)",10,"AS7C316096C-10BIN",null,null,null,"IS61WV20488FBLL-10BLI"]
["2M x 8","3.3V","48ball TFBGA (2CE)",10,"AS7C316096B-10BIN",null,"CY7C1069GN30-10BVXI"]
["512K x 32","3.3V","90ball TFBGA",10,"A7C351232-10BIN",null,null,null,"IS61WV51232BLL-10BLI"]
[]
["Low Power Asynchronous SRAM Cross Reference"]
["64K"]
["ORG","VCC","PACKAGE","ALLIANCE","ZMD","CYPRESS (EOL)","HITACHI (EOL)","NEC (EOL)","HYNIX (EOL)"]
["8K x 8","2.7V ~ 5.5V","28pin 600mil DIP","AS6C6264-55PCN / PIN","U6264BDC07LLG1",null,"HM6264BLP",null,"HY6264P"]
["8K x 8","2.7V ~ 5.5V","28pin 330mil SOP","AS6C6264-55SCN / SIN","U6264BS2C07LLG1","CY6264-55SNXI","HM6264BLFP","uPD4464","HY6264G"]
["8K x 8","2.7V ~ 5.5V","28pin STSOP (8 x 13.4 mm)","AS6C6264-55STCN"]
["256K"]
["ORG","VCC","PACKAGE","ALLIANCE","ZMD","SAMSUNG (EOL)","CYPRESS (EOL)","RENESAS","BRILLIANCE (EOL)","ISSI"]
["32K x 8","2.7V ~ 5.5V","28pin 600mil DIP","AS6C62256-55PCN","U62256ADC07LLG1","K6X0808C1D-DF55","CY62256NLL-70PXC",null,"BS62LV256PCP-55"]
["32K x 8","2.7V ~ 5.5V","28pin 330mil SOP","AS6C62256-55SxN","U62256AS2C07LLG1","K6X0808C1D-BF55","CY62256NLL-55SNXI","R1LP5256ESP-5S","BS62LV256SCP-55","IS62C256AL-45ULI"]
["32K x 8","2.4V ~ 3.6V","28pin 330mil SOP","AS62V256-70SIN",null,null,"CY62256NVLL-70SNXI","R1LV5256ESP-5S","BS62LV256SCP-55","IS62LV256AL-45ULI"]
["32K x 8","2.7V ~ 5.5V","28pin STSOP (8 x 13.4 mm)","AS6C62256-55STxN",null,"K6X0808C1D-LF55","CY62256NLL-55ZRXI","R1LP5256ESA-5S","BS62LV256STCP-55","IS62LV256AL-45TLI"]
["1M"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","RENESAS","BRILLIANCE (EOL)","NEC (EOL)","ISSI"]
["128K x 8","2 .7V ~ 5.5V","32pin 600mil DIP","AS6C1008-55PCN / PIN","K6X1008C2D-DB55",null,null,null,"BS62LV1027PCP-55","uPD431000ACZ-70L"]
["128K x 8","2.7V ~ 5.5V","32pin 450mil SOP","AS6C1008-55SIN","K6X1008C2D-GF55(Lead)/BF","CY62128ELL-45SXI","M5M51008DFP-55HI","R1LP0108ESP-5SI","BS62LV1027SIP-55","uPD431000AGW-70L","IS62C1024AL-35QLI"]
["128K x 8","2.7V ~ 5.5V","32pin TSOP I (8 x 20 mm)","AS6C1008-55TIN","K6X1008C2D-TF55 or PF","CY62128ELL-45ZXI","M5M51008DVP-55HI","R1LP0108ESF-5SI","BS62LV1027TIP-55","uPD431000AGZ-70LL-KKH","IS62C1024AL-35TLI"]
["128K x 8","2.7V ~ 5.5V","32pin STSOP (8 x 13.4 mm)","AS6C1008-55STIN",null,"CY62128ELL-45ZAXI","M5M51008DKV-55HI","R1LP0108ESA-5SI","BS62LV1027STIP-55","uPD431000AGU-B10-9JH","IS62C1024AL-45HLI"]
["64K x 16","2.7V ~ 5.5V","48ball TFBGA","AS6C1016-55BIN","K6F1016U4C-EF55","CY62127DV30LL-55BVXI",null,null,"BS616LV1010AI-70",null,"IS62WV6416DBLL-45BLI"]
["64K x 16","2.7V ~ 5.5V","44pin TSOP II","AS6C1016-55ZIN",null,"CY62126EV30LL-45SXIT",null,null,"BS616LV1010EI-70",null,"IS62WV6416DBLL-45TLI"]
["64K x 16","2.7V ~3.6V","44pin TSOP II","AS6CE1016A-45ZIN",null,"CY62126EV30LL-45ZSXI",null,null,null,null,"IS61WV6416EEBLL"]
["2M"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["256K x 8","2.7V ~ 3.6V","32pin 450mil SOP","AS6C2008-55SIN",null,"CY62138FV30LL-45SXI",null,null,"BS62LV2006SIP-55"]
["256K x 8","2.7V ~ 3.6V","32pin TSOP I (8 x 20 mm)","AS6C2008-55TIN",null,"CY62138FV30LL-45ZXI",null,null,"BS62LV2006TIP-55","IS62WV2568BLL-55TLI"]
["256K x 8","2.7V ~ 3.6V","32pin STSOP (8 x 13.4 mm)","AS6C2008-55STIN","K6F2008V2E-LF70000","CY62138FV30LL-45ZAXI","M5M5V208AKV-55HI","R1LV0208BSA-5SI","BS62LV2006STIP-55","IS62WV2568BLL-55HLI"]
["256K x 8","2.7V ~ 3.6V","36ball TFBGA (6mm x 8mm)","AS6C2008-55BIN",null,"CY62138FV30LL-45BVXI",null,null,null,"IS62WV2568BLL-55B2LI"]
["128K x 16","2.7V ~ 5.5V","44pin TSOP II","AS6C2016-55ZIN",null,"CY62136FVLL-70ZSXI","M5M5V216ATP-70HI","R1LV0216-BSB-5SI","BS616LV2016EIP-55","IS62WV12816BLL-55TLI"]
["128K x 16","2.7V ~ 3.6V","48ball TFBGA","AS6C2016-55BIN","K6F2016U4E-EF55000","CY62136FVLL-70BVXI",null,null,"BS616LV2019AIG-55","IS62WV12816BLL-55B2LI"]
["256K x 8","2.7V ~ 5.5V","32pin 450mil SOP","AS6C2008A-55SIN",null,"CY2138FV30LL-45SXI",null,null,"BS62LV2006SIP-55"]
["256K x 8","2.7V ~ 5.5V","32pin TSOP I (8 x 20mm)","AS6C2008A-55TIN",null,"CY2138FV30LL-45ZXI",null,null,"BS62LV2006TIP-55","IS62WV256BLL-55TLI"]
["256K x 8","2.7V ~ 5.5V","36ball TFBGA (6mm x 8mm)","AS6C2008A-55BIN",null,"CY62138FV30LL-45BVXI",null,null,null,"IS62WV256BLL-55B2LI"]
["4M"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["512K x 8","2.7V ~ 5.5V","32pin 600mil DIP","AS6C4008-55PCN","K4X4008C1F-DB55",null,null,"BS62LV4006PCP-55"]
["512K x 8","2.7V ~ 5.5V","32pin 450mil SOP","AS6C4008-55SIN","K6X4008C1F-GF55 or BF","CY62148ELL-55SXI","R1LV0408CSP-5SI","BS62LV4006SIP-55","IS62C5128BLL-45QLI"]
["512K x 8","2.7V ~ 5.5V","32pin STSOP (8 x 13.4mm)","AS6C4008-55STIN",null,"CY62148ELL-55ZAXI","R1LV0408DSA-5SI","BS62LV4006STIP-55","IS62C512BL-45HLI"]
["512K x 8","2.7V ~ 5.5V","32pin TSOP II","AS6C4008-55ZIN","K6X4008C1F-VF55","CY62148ELL-45ZSXI","R1LV0408DSB-5SI","BS62LV4006ECP55","IS62WV5128DBLL-45T2LI"]
["512K x 8","2.7V ~ 5.5V","36pin TFBGA (6mm x 8mm)","AS6C4008-55BIN",null,"CY62148EV30LL-55BVXI","RILV0408DBG-5SI",null,"IS62WV5128EBLL-45BLI"]
["256K x 16","2.7V ~ 5.5V","44pin TSOP II","AS6C4016-55ZIN","K6X4016C3F-TF70000","CY62146ELL-45ZSXI",null,"BS616LV4017EIP-55","IS62WV5128BLL-55TLI"]
["256K x 16","2.7V ~ 3.6V","44pin TSOP II","AS6C4016B-45ZIN","K6X4016T3F-TF70000","CY62147EV30LL-45ZSXI","R1LV0414DSB-5SI","BS616LV4017EIP-55","IS62C25616BL-45T2LI"]
["256K x 16","2.7V ~ 3.6V","48ball  TFBGA","AS6C4016B-45BIN","K6F4016U6G-EF70000","CY62147EV30LL-45BVXI","RMLV0416EGBG-4S2","BS616LV4017AIP-55","IS62WV25616DBLL-45BLI"]
["256K x 16","2.7V ~ 3.6V","44pin TSOP II","AS6CE4016B-45ZIN","K6X4016T3F-TF70000","CY62147EV30LL-45ZSXI","R1LV0414DSB-5SI","BS616LV4017EIP-55","IS62C25616EDBLL"]
["256K x 16","2.7V ~ 3.6V","48ball  TFBGA","AS6CE4016B-45BIN","K6F4016U6G-EF70000","CY62147EV30LL-45BVXI","RMLV0416EGBG-4S2","BS616LV4017AIP-55","IS62C25616EDFA/BLL"]
["8M"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","RENESAS","RENESAS","BRILLIANCE","ISSI"]
["1M x 8","2.7 ~ 5.5V","44pin TSOP II","AS6C8008-55ZIN","K6X8008(C/T)2B-UF55","CY62158EV30LL-45ZSXI",null,"R1LV0808ASB-5SI","HM62V8100LTTI-5SL","BS62LV8001ECP-55","IS62WV1024BLL-55TLI"]
["1M x 8","2.7 ~ 5.5V","44pin TSOP II","AS6C8008B-45/55ZIN","K6X8008(C/T)2B-UF55","CY62158EV30LL-45ZSXI",null,"R1LV0808ASB-5SI","HM62V8100LTTI-5SL","BS62LV8001ECP-55","IS62WV1024BLL-55TLI"]
["1M x 8","2.7 ~ 5.5V","48ball TFBGA","AS6C8008-55BIN",null,"CY62158EV30LL-45BVXI","EOL",null,"HM62V8100LBPI-5SL","BS62LV8001ECP-55","IS62WV1024BLL-55MLI"]
["1M x 8","2.7 ~ 3.6V","48ball TFBGA","AS6C8008B-45BIN",null,"CY62158EV30LL-45BVXI","EOL",null,"HM62V8100LBPI-5SL","BS62LV8001FIP-55","IS62WV1024BLL-55MLI"]
["512K x 16","2.7 ~ 5.5V","48ball TFBGA (6 x 8mm)*","AS6C8016-55BIN*","K6F8016U6G-FF55","CY62157EV30LL-55BVXI","M5M5W816WG-55HI","R1LV0816ABG-5SI",null,"BS616LV8017ECP55","IS62WV51216BLL-55BLI"]
["512K x 16","2.7 ~3.6V","48ball TFBGA (6 x 8mm)**","AS6C8016B-45/55BIN",null,"CY2157EV30LL-45BVXIT"]
["512K x 16","2.7 ~ 5.5V","44pin TSOP II","AS6C8016 -55ZIN","K6X8016(C/T)3B-UF55","CY62157EV30LL-55ZSXI","M5M5W816TP-55HI","R1LV0816ASA-5SI","HM62165I14LTT-5SL","BS616LV8017FCP70","IS62WV51216BLL-55T2LI"]
["512K x 16","2.7 ~3.6V","44pin TSOP II","AS6C8016B-45/55ZIN",null,"CY62157EV30LL-45ZSXIT",null,null,null,null,"IS62WV51216BLL-55T2LI"]
["512K x 16","2.7 ~ 5.5V","48pin TSOP I","AS6C8016-55TIN",null,"CY62157EV30LL-45ZXIT",null,null,null,null,"IS62WV51216GBLL-45TLI"]
["* = one chip select pin:B5 ** = two chip select pins: B5 and A6"]
["16M"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["1M x 16","2.7 ~ 3.6V","48pin TSOP I","AS6C1616-55TIN\nAS6C1616B-45/55TIN","CY62167E30LL-45/55ZXI","R1LV1616RSA-5SI","BS6216LV1611TCP55","IS62WV102416xxLL"]
["1M x 16","2.7 ~ 3.6V","48pin TSOP I","AS6C1616C-45TIN","CY62167E30LL-45/55ZXI","R1LV1616RSA-5SI","BS6216LV1611TCP55","IS62WV102416xxLL"]
["1M x 16","2.7 ~ 3.6V","48ball TFBGA","AS6C1616B-45/55BIN","CY62167DV30LL-xxBVXIT","R1LV1616HBG-4SI","BS6216LV1611FCP70","IS62WV102416xxLL-xxBLI"]
["2M x 8","2.7 ~ 3.6V","44pin TSOP I","AS6C1608B-45TIN","CY62168EV30LL-xxZXI",null,"BS6216LV1600EIP55","IS62WV20488xxLL-xxTLI"]
["2M x 8","2.7 ~ 3.6V","48ball TFBGA","AS6C1608B-45BIN","CY62168DV30LL-xxBVI",null,null,"IS62WV20488xxLL-xxBLI"]
["32M"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS"]
["2M x 16","2.7 ~ 3.6V","48pin TSOP I","AS6C3216A-55TIN*","CY62177EV30LL-55ZXI","R1LV3216RSA-5SI"]
["2M x 16","2.7 ~ 3.6V","48ball TFBGA","AS6C3216A-55BIN","CY62177EV30LL-55BAXI","R1LV3216CSA-5SI"]
["*48pin TSOP I (please note: dual chip select 2Mx16 or 4Mx8)"]
["64M"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS"]
["4M x 16","2.7V ~ 3.6V","48pin TSOP I","AS6C6416-55TIN",null,"R1WV6416RSA-5S"]
["4M x 16","2.7V ~ 3.6V","48ball BGA","AS6C6416-55BIN","CY62187EV30LL-55BAXI","R1WV6416RBG-5S"]
["*48pin TSOP I (please note: dual chip select 4Mx16 or 8Mx8)"]
["Sync SRAM Cross Reference"]
["ORG","DENSITY","PACKAGE","MODE","ALLIANCE","IDT","SAMSUNG","CYPRESS","GSI","ISSI"]
["4M","128K x 36","100TQFP","SPB","AS8C403600-QC150N","71V3576SxxxPFG","K7A403600B-QCxx","CY7C1347G-xxxAX","GS84036AGT-xxx","IS61LPS12836A-xxxTQ"]
["4M","256K x 16","100TQFP",null,"AS8C401800-QC150N","71V3578SxxxPFG","K7A401800B-QCxx","CY7C1327G-xxxAX","GS84018AGT-xxx","IS61LPS25618A-xxxTQ"]
["4M","128K x 36","100TQFP","SB","AS8C403625-QC75N","71V3577SxxPFG","K7B403625B-QCxx","CY7C1345G-xxxAX","GS84036AGT-xxx","IS61LF12836A-xxxTQ"]
["4M","256K x 18","100TQFP",null,"AS8C401825-QC75N","71V3579SxxPFG","K7B401825B-QCxx","CY7C1325G-xxxAX","GS84018AGT-xxx","IS61LF25618A-xxxTQ"]
["4M","128K x 36","100TQFP","ZBT/SPB","AS8C403601-QC166N","71V3556SxxxPFG","K7N403601B-QCxx","CY7C1350G-xxxAX","GS840Z36AGT-xxx","IS61NLP12836A-xxxTQ"]
["4M","256K x 18","100TQFP",null,"AS8C401801-QC166N","71V3558SxxxPFG","K7N401801B-QCxx","CY7C1352G-xxxAX","GS840Z18AGT-xxx","IS61NLP25618A-xxxTQ"]
["9M","256K x 36","100TQFP","SPB","AS8C803600-QC150N","71V67603SxxxPFG","K7A803600B-QCxx","CY7C1360C-xxxAJX","GS88036CT-xxx","IS61LPS25636A-xxxTQ"]
["9M","512K x 18","100TQFP",null,"AS8C801800-QC150N","71V67803SxxxPFG","K7A801800B-QCxx","CY7C1362C-xxxAJX","GS88018CT-xxx","IS61LPS51218A-xxxTQ"]
["9M","256K x 36","100TQFP","SB","AS8C803625-QC75N","71V67703SxxPFG","K7B803625B-QCxx","CY7C1361C-xxxAJX","GS88036CT-xxx","IS61LPS25636A-xxxTQ"]
["9M","256K x 36","100TQFP",null,"AS8C801825-QC75N","71V67903SxxPFG","K7B801825B-QCxx","CY7C1363C-xxxAJX","GS88018CT-xxx","IS61LPS51218A-xxxTQ"]
["9M","512K x 18","100TQFP","ZBT/SPB","AS8C803601-QC150N","71V65603SxxxPFG","K7N803601B-QCxx","CY7C1354C-xxxAJX","GS880Z36CT-xxx","IS61NLP25636A-xxxTQ"]
["9M","512K x 18","100TQFP",null,"AS8C801801-QC150N","71V65803SxxxPFG","K7N801801B-QCxx","CY7C1356C-xxxAJX","GS880Z18CT-xxx","IS61NLP51218A-xxxTQ"]
["9M","256K x 36","100TQFP","ZBT/SB","AS8C803625A-QC75N","71V65703SxxPFG","K7M803625B-QCxx","CY7C1351C-xxxAJX","GS880Z36CT-xxx","N/A"]
["9M","512K x 18","100TQFP",null,"AS8C801825A-QC75N","71V65903SxxPFG","K7M801825B-QCxx","CY7C1353C-xxxAJX","GS880Z18CT-xxx","N/A"]
["18M","512K x 36","100TQFP","ZBT/SPB","AS8C163631-QC166N","71T75602SxxxPFG","K7N163631B-QCxx","CY7C1370D-xxxAX","GS880Z36CT-xxx","IS61LPS12836A-xxxTQ"]
["18M","1M x 18","100TQFP",null,"AS8C161831-QC166N","71T75802SxxxPFG","K7N161831B-QCxx","CY7C1372D-xxxAX","GS880Z18CT-xxx","IS61LPS102418A-xxxTQ"]
[]
["pSRAM Cross Reference"]
["ORG","DENSITY","PACKAGE","COMMENTS/ PREV REV","ALLIANCE","JSC/JEJU","ISSI","FIDELIX","AP MEMORY"]
["8Mb","512K x 16","48 FPBGA","page mode & Non-DPD","AS1C512K16PL-70BIN","EM784SP16BPP-70LF","IS66WV51216EALL-70BLI"]
["8Mb","512K x 16","48 FPBGA","Non-page mode & Non-DPD","AS1C512K16P-70BIN","JS784SU16BSP-70LFI","IS66/67WV51216EBLL-70BL","FMP0817CAx"]
["16Mb","1M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C1M16PL-70BIN","EM7164SP16CSP-70LFI","IS66W1M16EALL-70BLI","FMP1617CCx"]
["16Mb","1M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C1M16P-70BIN","JS164SU16BSP-70LFI","IS66/67WV1M16EBLL-70BL","FMP1617CAx"]
["32Mb","2M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C2M16P-70BIN","JS7324SU16BSP-70LFI","IS66WVE2M16EBLL-70B","FMP3217CAx"]
["64Mb","4M X16","49 FBGA","DPD mode","AS1C4M16PL-70BIN","EMC643SP16CKDT-70LF"]
["128Mb\n(*2-stacked die)","8M X16","49 FBGA","DPD mode","AS1C8M16PL-70BIN","JSC283SP16ATDT-70LF",null,null,"APS128XX"]
[]
["Parallel 5V NOR Flash Cross Reference"]
["DENSITY","VCC","PACKAGE","SPEED (NS)","ALLIANCE","MICRON","CYPRESS/SPANSION","MACRONIX"]
["1Mb","5V","PLCC 32",55,"AS29CF010-55CCIN",null,"AM29F010B* (EOL)"]
["4Mb","5V","PLCC 32",55,"AS29CF040-55CCIN","M29F040","AM29F040B","MX29F040C"]
["4Mb","5V","TSOP 48pin",55,"M29F400FB55N3E2 \nM29F400FB55N3F2","M29F400F","AM29F400BB* (EOL)","MX29F400CBT"]
["4Mb","5V","TSOP 48pin",55,"M29F400FT5AN6E2","M29F400F","AM29F400BT* (EOL)","MX29F400CTT"]
["8Mb","5V","TSOP 48pin",55,"AS29CF800T-55TIN","M29F800F","AM29F800BT* (EOL)","MX29F800C T/B"]
["8Mb","5V","TSOP 48pin",55,"AS29CF800B-55TIN","M29F800F","AM29F800BB* (EOL)","MX29F800C T/B"]
["8Mb","5V","TSOP 48pin",55,"M29F800FB5AN6E2\nM29F800FB5AN6F2","M29F800F","AM29F800BB* (EOL)","MX29F800CBT"]
["8Mb","5V","TSOP 48pin",55,"M29F800FT55N3E2","M29F800F","AM29F800BT* (EOL)","MX29F800CTT"]
["16Mb","5V","TSOP 48pin",55,"AS29CF160T-55TIN","M29F160F","AM29F160DT* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"AS29CF160B-55TIN","M29F160F","AM29F160DB* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"M29F160FB5AN6F2","M29F160F","AM29F160DB* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"M29F160FT55N3E2","M29F160F","AM29F160DT* (EOL)"]
[]
["SLC Parallel NAND Flash Cross Reference"]
["DENSITY","VCC","BUS WIDTH","PACKAGE","TEMPERATURE","ALLIANCE","MICRON","SKY HIGH","CYPRESS","WINBOND","MACRONIX","KIOXIA"]
["1Gb","3.3V","x8","63b FBGA","-40°C to 85°C","AS9F31G08SA-25BIN","MT29F1G08ABADAH4\nMT29F1G08ABAEAH4","S34SL01G200BFI\nS34ML01G200BFI\nS34ML01G300BFI","S34ML01G100BFI","W29N01HV\nW29N01GV","MX30LF1G18AC","TC58NVG0S3HBA"]
["2Gb","3.3V","x8","63b FBGA","-40°C to 85°C","AS9F32G08SA-25BIN","MT29F2G08ABAEAH4\nMT29F2G08ABAGAH4","S34SL02G200BFI\nS34ML02G200BFI\nS34ML02G300BFI","S34ML02G100BFI","W29N02GV\nW29N02KV","MX30LF2G18AC","TC58NVG1S3HBA"]
["4Gb","3.3V","x8","63b FBGA","-40°C to 85°C","AS9F34G08SA-25BIN","MT29F4G08ABADAH4\nMT29F4G08ABAEAH4\nMT29F4G08ABAFAH4","S34SL04G200BFI\nS34ML04G200BFI","S34ML04G100BFI","W29N04GV","MX30LF4G18AC","TC58NVG2S0HBA"]
["8Gb","3.3V","x8","63b FBGA","-40°C to 85°C","AS9F38G08SA-25BIN","MT29F8G08ADACAH4","S34ML08G201BFI","S34ML08G101BFI","W29N08GV","MX60LF8G18AC","TH58NVG3S0HBA"]
["4Gb","1.8V","x8","63b FBGA","-40°C to 85°C","AS9F14G08SA-45BIN","MT29F4G08ABBDAH4\nMT29F4G08ABBEAH4\nMT29F4G08ABBFAH4","S34MS04G200BFI","S34MS04G100BFI","W29N04GZ\nW29N04GW","MX30UF4G18AC","TC58NYG2S0HBA"]
["8Gb","1.8V","x8","63b FBGA","-40°C to 85°C","AS9F18G08SA-45BIN","MT29F8G08ADBCAH4\nMT29F8G08ADBDAH4\nMT29F8G08ABBCAH4\nMT29F8G08ABBDAH4","S34MS08G201BFI","S34MS08G101BFI","W29N08GW\nW29N08GZ","MX60UF8G18AC","TH58NYG3S0HBA"]
["4Gb","1.8V","x8","63b FBGA","-40°C to 105°C","AS9F14G08SA-45BAN","MT29F4G08ABBDAH4-A\nMT29F4G08ABBEAH4-A","S34MS04G200BFI","S34MS04G100BFV","W29N04GZ\nW29N04GW"]
["8Gb","1.8V","x8","63b FBGA","-40°C to 105°C","AS9F18G08SA-45BAN","MT29F8G08ADBDAH4-A","S34MS08G201BFA","S34MS08G101BFA","W29N08GW\nW29N08GZ"]
[]
["Serial NOR Flash Cross Reference"]
["DENSITY","VCC","PACKAGES","ALLIANCE","MICRON","ADESTO","SPANSION","WINBOND","MACRONIX","ISSI","GIGA DEVICES"]
["2Mb","3.3V","8pin SOIC (150mils)","M45PE20-VMN6P","M45PE20-VMN6","AT45DB021E"]
["8Mb","3.3V","8pin DFN (6x5mm)","M45PE80-VMP6G","M45PE80-VMP6","AT45DB081E"]
["8Mb","3.3V","8pin DFN (6x5mm)","M45PE80-VMP6TG","M45PE80-VMP6","AT45DB081E"]
["16Mb","3.3V","8pin SOIC (208mils)","M45PE16-VMW6TG","M45PE16-VMW6","AT45DB161E"]
["4Mb","3.3V","8pin SOIC (150mils)","AS25F34MD-10S1IN","M25P40-AVMN6","AT25SF041","S25FL040","W25Q40","MX25L40\nMX25V40","IS25LP040\nIS25LQ040","GD25Q40\nGD25B40\nGD25D40"]
["16Mb","3.3V","8pin SOIC (150mils)","AS25F316MQ-10S1IN","M25P16-AVMN6\nM25PX16","AT25SF161\nAT25FF161","S25FL016","W25Q16","MX25L16\nMX25V16","IS25LP016\nIS25LQ016","GD25Q16\nGD25B16"]
["32Mb","3.3V","8pin DFN (4x3mm)","N25Q032A13EF440F","N25Q032A13EF4","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3.3V","8pin DFN (4x3mm)","N25Q032A13EF4A0F","N25Q032A13EF4","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3.3V","8pin DFN (6x5mm)","N25Q032A13EF640F","N25Q032A13EF6","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3.3V","8pin SOIC (150mils)","N25Q032A13ESC40F","N25Q032A13ESC","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3.3V","8pin SOIC (150mils)","N25Q032A13ESC40G","N25Q032A13ESC","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3.3V","8pin SOIC (150mils)","N25Q032A13ESCA0F","N25Q032A13ESC","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3.3V","16pin SOIC (300mils)","N25Q032A13ESFA0F","N25Q032A13ESF","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["64Mb","1.8V","8pin SOIC (208mils)","N25Q064A11ESEA0F","N25Q064A11ESE","AT25SL64/AT25QL64",null,"W25Q64","MX25U64","IS25WP064","GD25LQ64"]
["64Mb","3.3V","8pin DFN (6x5mm)","N25Q064A13EF640E","N25Q064A13EF6","AT25SF64/AT25QF64","S25FL064A/P","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","8pin DFN (8x6mm)","N25Q064A13EF8A0E","N25Q064A13EF8","AT25SF64/AT25QF64","S25FL064A/P","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","8pin DFN (8x6mm)","N25Q064A13EF8A0F","N25Q064A13EF8","AT25SF64/AT25QF64","S25FL064A/P","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","8pin DFN (8x6mm)","N25Q064A13EF8H0E","N25Q064A13EF8","AT25SF64/AT25QF64","S25FL064A/P","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","16pin SOIC (300mils)","N25Q064A13ESFA0F","N25Q064A13ESF","AT25SF64/AT25QF64","S25FL064A/P","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","8pin SOIC (208mils)","AS25F364MQ-10SIN","N25Q064A13ESE","AT25QF64","S25FL064","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","8L WSON (6x5mm)","AS25F364MQ-10WIN","N25Q064A13EF6","AT25QF64","S25FL064","W25Q64","MX25L64","IS25L064","GD25Q64"]
["128Mb","1.8V","8pin SOIC (208mils)","AS25F1128MQ-70SIN","MT25QU128ABA1ESE","AT25SL128A-SUE","S25FS128SDSMFI","W25Q128JWSIM","MX25U12832FM2I","IS25WP128-JBLE","GD25LB128ESIG"]
["128Mb","1.8V","8L WSON (6x5mm)","AS25F1128MQ-70WIN","MT25QU128ABA1EW7","AT25SL128A-MHE","S25FS128SDSNFI","W25Q128JWPIM","MX25U12832FZNI","IS25WP128-JKLE","GD25LB128EWIG"]
[]
["Serial NAND Flash Cross Reference"]
["DENSITY","SPEED (NS)","VCC","ALLIANCE","MICRON","TOSHIBA/KIOXIA","WINBOND","MACRONIX","GIGA DEVICES","ISSI"]
["1Gb","120Mhz","3V","AS5F31G04SND-08LIN","MT29F1G01ABAFDWB-IT","TC58CVG0S3HRAIJ","W25N01GV\nW25N01KV","MX35LF1GE4AB\nMX35LF1G24AD","GD5F1GQ4Ux\nGD5F1GQ5Ux\nGD5F1GM7Ux","IS37SML01G1-LLI\nIS37SML01G8A-JJLI"]
["2Gb","100Mhz","1.8V","AS5F12G04SND-10LIN","MT29F2G01ABBGDWB-IT:G","TC58CYG1S3HRAIJ","W25N02JW\nW25M02GW","MX35UF2G14AC\nMX35UF2G24AD\nMX35UF2GE4AC\nMX35UF2GE4AD","GD5F2GQ4Rx\nGD5F2GQ5Rx\nGD5F2GM7Rx","IS37SMW02G8A-JJLI"]
["2Gb","120Mhz","3V","AS5F32G04SNDA-08LIN AS5F32G04SNDB-08LIN","MT29F2G01ABAGDWB-IT","TC58CVG1S3HRAIJ","W25M02GV","MX35LF2G14AC\nMX35LF2GE4AD\nMX35LF2G24AD","GD5F2GQ4Ux\nGD5F2GQ5Ux\nGD5F2GM7Ux","IS37SML02G8A-JJLI"]
["4Gb","100Mhz","1.8V","AS5F14G04SND-10LIN","MT29F4G01ABBFDWB-IT","TC58CYG2S0HRAIJ","W25N04KW","MX35UF4G24AD\nMX35UF4GE4AD","GD5F4GQ6Rx\nGD5F4GM8Rx","IS37SMW04G8A-JJLI"]
["4Gb","120Mhz","3V","AS5F34G04SNDA-08LIN AS5F34G04SNDB-08LIN","MT29F4G01ABAFDWB","TC58CVG2S0HRAIJ","W25N04KV","MX35LF4G24AD\nMX35LF4GE4AD","GD5F4GQ6Ux\nGD5F4GM8Ux","IS37SML04G8A-JJLI"]
["8Gb","100Mhz","1.8V","AS5F18G04SND-10LIN",null,"TH58CYG3S0HRAIJ",null,null,null,"IS37SMW08G8A-JJLI"]
["8Gb","120Mhz","3V","AS5F38G04SND-08LIN",null,"TH58CVG3S0HRAIJ",null,null,null,"IS37SML08G8A-JJLI"]
[]
["eMMC Cross Reference"]
["DENSITY","PACKAGETYPE","TEMP GRADE","ALLIANCE","MICRON","SAMSUNG","KINGSTON","KIOXIA","ISSI","SANDISK","SK HYNIX","MACRONIX"]
["4GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC4G31M-51BIN","MTFC4GACAJCN\nMTFC4GMWDM","KLM4G1GXXX","EMMC04GMK27\nEMMC04GM627\nEMMC04G-W627","THGBMNG5D1LBA","IS21ES04G-JCLI\nIS21ES04G-BCLI","X","H26M31001HPR","MX52LM04A11X"]
["8GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC8G31M-51BIN","MTFC8GACAENS\nMTFC8GAKAJCN\nMTFC8GAMALBH\nMTFC8GAMALGT\nMTFC8GLWDM","KLM8G1GEUF\nKLM8G1GESD\nKLM8G1GETF","EMMC08GML36","THGBMJG6C1LBA","IS21ES08GA-JCLI\nIS21ES08GA-BCLI","SDINBDG4-8G","H26M41208HPR","MX52LM08A11X"]
["16GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC16G31M-51BIN","MTFC16GAKAECN\nMTFC16GAKAEJP\nMTFC16GAPALBH","KLMAG1JETD\nKLMAG2GESD\nKLMAG2GEUF","EMMC16G-TB29\nEMMC16G-IB29","THGBMUG7C1LBA\nTHGAMVG7T13BA","IS21TF16G-JCLI\nIS21TF16G-BCLI","SDINBDA6-16G","H26M51002KPR","X"]
["32GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC32G31T3-51BIN","MTFC32GAKAECN\nMTFC32GAKAEJP\nMTFC32GAZAQHD\nMTFC32GAPALBH","KLMBG2JETD\nKLMBG4GESD","EMMC32G-TX29\nEMMC32G-IX29","THGBMUG8C2LBA\nTHGAMVG8T13BA\nTHGBMJG88C4LBA","IS21TF32G-JCLI\nIS21TF32G-BCLI","SDINBDA6-32G\nSDINBDG4-32G","H26M62002JPR\nH26M64208EM","X"]
["64GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC64G32T5-51BIN","MTFC64GAZAQHD\nMTFC64GAPALBH","KLMCG2KCTA\nKLMCG2UCTA\nKLMCG2UCTB\nKLMCG4JEUD\nKLMCG8GESD","EMMC64G-TY29\nEMMC64G-IY29","THGAMVG9T23BA\nTHGBMJG9C8LBA","IS21TF64G-JCLI\nIS21TF64G-BCLI","SDINBDA6-64G\nSDINBDG4-64G","H26M74002HMR\nH26M78208CMR","X"]
["128GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC128G32T5-51BIN","MTFC128GAPALNS\nMTFC128GAZAQJP","KLMDG4UCTA\nKLMDG4UCTB\nKLMDG8JEUD","EMMC128-TY29\nEMMC128-IY29","THGAMVT0T43BA","IS21TF128G-JCLI\nIS21TF128G-BCLI","SDINBDA6-128G","X","X"]

{"sheet":"SDRAM","index":2,"n_rows":27,"n_cols":7,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
[]
["Synchronous DRAM 3.3V  x8,  x16  and  x32"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY (MHz)","TEMPERATURE","ALLIANCE"]
["64Mb","4M x 16","3.3V","54-ball FBGA / 60-ball FBGA","143/166 MHz","Commercial, Industrial, Automotive","AS4C4M16SA-6/7 BxN, B2xN"]
["64Mb","2M x 32","3.3V","90-ball TFBGA","143/166 MHz","Commercial, Industrial","AS4C2M32S-6/7 BxN"]
["64Mb","2M x 32","3.3V","86pin TSOP II","143/166 MHz","Commercial, Industrial","AS4C2M32SA-6/7 TxN"]
["128Mb","8M x 16","3.3V","54pin TSOP II/54-ball FBGA","143/166 MHz","Commercial, Industrial, Automotive","AS4C8M16SA-6/7 TxN/BxN"]
["128Mb","8M x 16","3.3V","54pin TSOP II","166 MHz","Inudstrial","AS4C8M16SB-6TIN"]
["128Mb","4M x 32","3.3V","90-ball TFBGA","143/166 MHz","Commercial, Industrial","AS4C4M32S-6/7 BxN"]
["128Mb","4M x 32","3.3V","86pin TSOP II","143/166 MHz","Commercial, Industrial","AS4C4M32SA-6/7 TxN"]
["256Mb","16M x 16","3.3V","54pin TSOP II/54-ball FBGA","143/166 MHz","Commercial, Industrial","AS4C16M16SA-6/7 TxN/BxN"]
["256Mb","16M x 16","3.3V","54pin TSOP II/54-ball FBGA","143/166 MHz","Commercial, Industrial","AS4C16M16SB-6/7 TxN/BxN"]
["256Mb","8M x 32","3.3V","86pin TSOP II","143/166 MHz","Commercial, Industrial","AS4C8M32S-6/7 TxN"]
["256Mb","8M x 32","3.3V","90-ball TFBGA","143/166 MHz","Commercial, Industrial","AS4C8M32SA-6/7 BxN"]
["256Mb","32M x 8","3.3V","54pin TSOP II","143/166 MHz","Commercial, Industrial","AS4C32M8SA-6/7 TxN"]
["256Mb","64M x 4","3.3V","54pin TSOP II","143/166 MHz","Commercial, Industrial","AS4C64M4SA-6/7 TxN"]
["512Mb","32M x 16","3.3V","54-ball FBGA","143 MHz","Industrial","AS4C32M16SB-7BIN"]
["512Mb","32M x 16","3.3V","54pin TSOP II","143 MHz/166 MHz","Commercial, Industrial","AS4C32M16SB-6/7 TxN"]
["512Mb","32M x 16","3.3V","54pin TSOP II","143 MHz","Industrial","AS4C32M16SC-7TIN"]
["512Mb","16M x 32","3.3V","86pin TSOP II","143 MHz","Industrial","AS4C16M32SC-7TIN"]
["512Mb","16M x 32","3.3V","90ball TFBGA","166MHz","Commercial, Industrial","AS4C16M32SB-6BxN"]
["512Mb","64M x 8","3.3V","54pin TSOP II","143 MHz","Industrial","AS4C64M8SC-7TIN"]
["512Mb","64M x 8","3.3V","54pin TSOP II","133 MHz","Commercial","AS4C64M8SD-7TCN"]
["512Mb","16M x 32","3.3V","90ball TFBGA","166MHz","Commercial, Industrial","AS4C16M32SB-6BxN"]
["512Mb","64M x 8","3.3V","54pin TSOP II","143 MHz","Industrial","AS4C64M8SC-7TIN"]
["512Mb","64M x 8","3.3V","54pin TSOP II","133 MHz","Commercial","AS4C64M8SD-7TCN"]
["* X= TEMPERATURE GRADE; C = COMMERCIAL ; I = INDUSTRIAL; A = AUTOMOTIVE"]

{"sheet":"SDRAM Cross Reference","index":3,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[[28,0,28,2],[31,0,31,2],[1,0,1,2]]}
[]
["Synchronous DRAM 3.3V Cross Reference"]
["DENSITY","ORG","ALLIANCE","SAMSUNG (EOL)","MICRON","SK HYNIX (EOL)","ISSI","WINBOND","NANYA (EOL)","ELITE (ESMT)","ELPIDA (EOL)"]
["16Mb","1M x 16","AS4C1M16S-6/7TxN","K4S161622E","MT48LC1M16A1","HY57V161610","IS42S16100","W9816G6TH","NT56V1616AOT","M12L16161A-xTG2Q","EDS1616AGTA"]
["64Mb","4M x 16","AS4C4M16SA-5/6/7TxN\nAS4C4M16SB-6TIN","K4S641632N-UCxx","MT48LC4M16A2P","HY57V641620","IS42S16400\nIS45S16400","W9864G6JH","NT56V6620C0T-xxB","M12L64164A-xTG2U","uPD4564163G5-Axx"]
["64Mb","4M x 16","AS4C4M16SA-6/7BxN",null,"MT48LCM16A2B4(F4)","HY5V66D","IS42S16400\nIS45S16400","W9864G6JT",null,"M12L64154A-xBG2C"]
["64Mb","4M x 16","AS4C4M16SA-7B2CN",null,null,null,"IS42S16400","W9864G6JB-7"]
["64Mb","2M x 32","AS4C2M32S-6/7BxN",null,"MT48LC2M32B2B5-x","HY5V62","IS42S32200","W9864G2IB-x",null,null,"EDS6432AFBH"]
["64Mb","2M x 32","AS4C2M32SA-6/7TxN","K4S643232H-Ucxx","MT48LC2M32B2P-x (EOL)","HY57V643220","IS42S32200","W9864G2J(G,I)H-x",null,"M12L64322A-xTG2U","EDS6432AFTA"]
["128Mb","8M x 16","AS4C8M16SA-6/7TxN\nAS4C8M16SB-6TIN","K4S281632K-UCxx","MT48LC8M16A2P","HY57V281620","IS42S16800\nIS45S16800","W9812G6K(G,I)H","NT5SV8M16AT-xxB","M12L128168A-xTG2N","uPD45128163G5-Axx"]
["128Mb","8M x 16","AS4C8M16SA-6/7BxN","K4S281632D-RL75","MT48LC8M16A2B4(F4)","HY5V26","IS42S16800\nIS45S16800","W9812G6JB",null,"M12L128168A-xBG2N"]
["128Mb","4M x 32","AS4C4M32S-6/7BxN",null,"MT48LC4M32B2B5-x","HY5V22","IS42S32400","W9812G21(G)B-x",null,"M12L128324-xBG2E","EDS1232AHBH"]
["128Mb","4M x 32","AS4C4M32SA-6/7TxN",null,"MT48LC4M32B2P-x (EOL)","HY57V283220T","IS42S32400","W9812G2GH",null,null,"EDS1232AHTA"]
["256Mb","16M x 16","AS4C16M16SA/B-6/7TxN","K4S561632N-UCxx","MT48LC16M16A2P","H57V2562GTR","IS42S16160\nIS45S16160","W9825G6K(D,E,J)H","NT5SV16M16AT-xxB","M12L2561616A-xTG2A","EDS2516AP(AF,AC)TA-xx"]
["256Mb","16M x 16","AS4C16M16SA/B-6/7BxN","K4S561632D-RL75","MT48LC16M16A2B4","HY5V56","IS42S16160\nIS45S16160","W9825G6JB",null,"M12L2561616A-xBG2A","EDS2516EE(JE)BH"]
["256Mb","8M x 32","AS4C8M32S-6/7TxN",null,"MT48LC8M32B2B5-x (EOL)","HY5V52","IS42S32800","W9825G2J(D)B-x",null,null,"EDS2532EEBH"]
["256Mb","8M x 32","AS4C8M32SA-6/7BxN",null,"MT48LC8M32B2B5-x","HY5V52","IS42S32800","W9825G2J(D)B-x",null,null,"EDS2532EEBH"]
["256Mb","32M X 8","AS4C32M8SA-6/7TxN",null,"MT48LC32M8A2P",null,"IS42S83200J"]
["256Mb","64M x 4","AS4C64M4SA-6/7TxN",null,"MT48LC64M4A2P (EOL)",null,"IS42S32800"]
["512Mb","32M x 16","AS4C32M16SB-7BIN",null,null,null,"IS42S16320",null,null,"M12L5121632A"]
["512Mb","32M x 16","AS4C32M16SB-6/7TxN","K4S511632M-TC75","MT48LC32M16A2 (EOL)",null,"IS42S16320",null,null,"M12L5121632A","EDS5116ABTA"]
["512Mb","32M x 16","AS4C32M16SC-7TIN","K4S511632M-TC75","MT48LC32M16A2 (EOL)",null,"IS42S16320",null,null,"M12L5121632A","EDS5116ABTA"]
["512Mb","16M x 32","AS4C16M32SB-6BxN",null,"MT48LC16M32S2 (EOL)",null,"IS42S32160"]
["512Mb","16M x 32","AS4C16M32SC-7TIN",null,null,null,"IS42S32160"]
["512Mb","64M x 8","AS4C64M8SC-7TIN",null,"MT48LC64M8A2P-75:C (EOL)",null,"IS42S86400"]
["512Mb","64M x 8","AS4C64M8SD-7TCN",null,"MT48LC64M8A2P-75:C (EOL)",null,"IS42S86400"]

{"sheet":"DDR1  SDRAM","index":4,"n_rows":17,"n_cols":8,"rows_kept":17,"cut":false,"hidden":false,"merged":[[11,0,12,0],[11,1,12,1],[11,2,12,2]]}
[]
["DDR1 2.5V SDRAM"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY (MHz)","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE"]
["64Mb","4M x 16","2.5V","66pin TSOP II","200 MHz","400 Mbps","Commercial, Industrial, Automotive","AS4C4M16D1A-5TxN"]
["64Mb","2M x 32","2.5V","144-ball FBGA","200 MHz","400 Mbps","Commercial, Industrial","AS4C2M32D1A-5BxN"]
["128Mb","8M x 16","2.5V","66pin TSOP II","200 MHz","400 Mbps","Commercial, Industrial","AS4C8M16D1A-5TxN"]
["128Mb","8M x 16","2.5V","60-ball FBGA","200 MHz","400 Mbps","Commercial, Industrial","AS4C8M16D1-5BxN"]
["128Mb","4M x 32","2.5V","144-ball FBGA","200 MHz","400 Mbps","Commercial, Industrial","AS4C4M32D1A-5BxN"]
["256Mb","16M x 16","2.5V","60-ball FBGA","200 MHz","400 Mbps","Commercial, Industrial, Automotive","AS4C16M16D1-5BxN"]
["256Mb","16M x 16","2.5V","66pin TSOP II","200 MHz","400 Mbps","Commercial, Industrial","AS4C16M16D1A-5TxN"]
["512Mb","32M x 16","2.5V","66pin TSOP II","200 MHz","400 Mbps","Commercial, Industrial, Automotive","AS4C32M16D1A-5TxN"]
["512Mb","32M x 16","2.5V","60-ball FBGA","200 MHz","400 Mbps","Commercial, Industrial, Automotive","AS4C32M16D1-5BxN"]
[null,null,null,"66pin TSOP II","200 MHz","400 Mbps","Commercial, Industrial","AS4C32M16D1-5TxN"]
["512Mb","64M x 8","2.5V","66pin TSOP II\n60-ball FBGA","200 MHz","400 Mbps","Commercial, Industrial","AS4C64M8D1-5TxN\nAS4C64M8D1-5BxN"]
["1Gb","64M x 16","2.5V","66pin TSOP II","166 MHz","333Mbps","Commercial, Industrial","AS4C64M16D1-6TxN"]
["1Gb","64M x 16","2.5V","60-ball FBGA","166 MHz","333Mbps","Industrial","AS4C64M16D1A-6BIN"]
["* X= TEMPERATURE GRADE; C = COMMERCIAL ; I = INDUSTRIAL; A = AUTOMOTIVE"]

{"sheet":"DDR1 SDRAM Cross Reference","index":5,"n_rows":17,"n_cols":10,"rows_kept":17,"cut":false,"hidden":false,"merged":[[1,0,1,2]]}
[]
["DDR1       2.5V SDRAM Cross Reference"]
["DENSITY","ALLIANCE","SAMSUNG (EOL)","MICRON","ISSI","HYNIX - ALL EOL","WINBOND","NANYA","ELITE (ESMT)","ELPIDA"]
["64Mb","AS4C4M16D1A-5TxN","K4H641638N","MT46V4M16TG (EOL)","IS43R16400B",null,"W9464G6K(I,J)H",null,"M13S64164A-5TG2Y","(EOL)"]
["64Mb","AS4C2M32D1A-5BxN"]
["128Mb","AS4C8M16D1-5BXN","K4H281638D",null,"IS43R16800E-5BL",null,"W9412G6JB",null,"M13S128168A-5BG2N","EDD1216A"]
["128Mb","AS4C8M16D1A-5TxN","K4H281638D","MT46V8M16 (EOL)","IS43R16800E-5TL","HY5DU1281622","W9412G6K(I,J)H",null,"M13S128168A-5TG2N","EDD1216A"]
["128Mb","AS4C4M32D1A-5BxN",null,"MT46V4M32FK (EOL)","IS43R32400E-5BL",null,"W9412GIB",null,"M13S128324A-5BG2M","EDD1232A"]
["256Mb","AS4C32M8D1-5TxN","K4H560838N","MT46V32M8P (EOL)","IS43R83200","HY5DU56822",null,"NT5DS32M8ES",null,"EDD2508A"]
["256Mb","AS4C16M16D1-5BxN","K4H561638D","MT46V16M16CY-5B","IS43R16160\nIS46R16160","HY5DU561622","W9425G6JB",null,"M13S2561616A-xBG2A"]
["256Mb","AS4C16M16D1A-5TxN","KH561638D","MT46V16M16P","IS43R16160","HY5DU561622","W945G6K(D,E,J)H",null,"M13S2561616A-xTG2A","EDD2516A"]
["512Mb","AS4C32M16D1-5BxN","K4H511638J","MT46V32M16CY","IS43R16320\nIS46R16320","HY5DU121622",null,null,null,"EDD5116"]
["512Mb","AS4C32M16D1A-5TxN","K4H511638J","MT46V32M16P","IS43R16320\nIS46R16320","HY5DU121622",null,"NT5DS32M16ES","M13S5121632A-5TG2S","EDD5116A"]
["512Mb","AS4C64M8D1-5TxN","K4H510838J","MT46V64M8P","IS43R86400","HY5DU12822",null,"NT5DS64M8ES",null,"EDD5108A"]
["512Mb","AS4C64M8D1-5BxN","K4H510838J","MT46V64M8CY(BN)","IS43R86400","HY5DU12822"]
["1Gb","AS4C64M16D1-6TxN",null,"MT46V64M16P (EOL)"]
["1Gb","AS4C64M16D1A-6BIN"]

{"sheet":"DDR2 SDRAM","index":6,"n_rows":14,"n_cols":8,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
[]
["DDR2   1.8V SDRAM"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY (MHz)","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE"]
["256Mb","16M x 16","1.8V","84-ball FBGA","400 MHz","800 Mbps","Commercial, Industrial","AS4C16M16D2-25BxN"]
["512Mb","32M x 16","1.8V","84-ball FBGA","400 MHz","800Mbps","Commercial, Industrial, Automotive","AS4C32M16D2A/C-25BxN"]
["512Mb","64M x 8","1.8V","60-ball FBGA","400 MHz","800 Mbps","Commercial, Industrial, Automotive","AS4C64M8D2-25BxN"]
["1Gb","64M x 16","1.8V","84-ball FBGA","400 MHz","800Mbps","Commercial, Industrial, Automotive","AS4C64M16D2A-25BxN"]
["1Gb","64M x 16","1.8V","84-ball FBGA","400 MHz","800 Mbps","Commercial","AS4C64M16D2B-25BCN"]
["1Gb","128M x 8","1.8V","60-ball FBGA","400 MHz","800Mbps","Commercial, Industrial","AS4C128M8D2A-25BxN"]
["2Gb","128M x 16","1.8V","84-ball FBGA","400 MHz","800 Mbps","Commercial, Industrial","AS4C128M16D2-25BxN"]
["2Gb","128M x 16","1.8V","84-ball FBGA","400 MHz","800Mbps","Commercial, Industrial","AS4C128M16D2A-25BxN"]
["2Gb","256M x 8","1.8V","60-ball FBGA","400 MHz","800 Mbps","Commercial","AS4C256M8D2A-25BCN"]
[]
["* X= TEMPERATURE GRADE; C = COMMERCIAL ; I = INDUSTRIAL; A = AUTOMOTIVE"]

{"sheet":"DDR2 SDRAM Cross Reference","index":7,"n_rows":12,"n_cols":9,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
[]
["DDR2    1.8V SDRAM Cross Reference"]
["DENSITY","ALLIANCE","SAMSUNG (EOL)","MICRON","ISSI","WINBOND","NANYA","ELITE (ESMT)","HYNIX (EOL)"]
["256Mb","AS4C16M16D2-25BxN","K4T56163Q","MT47H16M16BG","IS43DR16160","W9725G6K(J)B","NT5TU16M16BG","M14D2561616A-2.5BG","HY5PS561621"]
["512Mb","AS4C32M16D2A/C-25BxN","K4T51163Q","MT47H32M16HR(NF)-25E","IS43DR16320\nIS46DR16320","W9751G6K(J)B","NT5TU32M16GG","M14D5121632A-2.5BG","HY5PS121621"]
["512Mb","AS4C64M8D2-25BxN","K4T51083Q","MT47H64M8CF(SH)-25E","IS43DR86400\nIS46DR86400","W9751G8K(J)B","NT5TU64M8EE",null,"H5PS5182KFR"]
["1Gb","AS4C64M16D2A-25BxN","K4T1G164Q","MT47H64M16HR(NF)-25E","IS43DR16640\nIS46DR16640","W971GG6JB","NT5TU64M16HG","M14D1G1664A-2.5BG","H5PS1G63"]
["1Gb","AS4C64M16D2B-25BCN","K4T1G164Q","MT47H64M16HR(NF)-25E","IS43DR16640","W971GG6JB","NT5TU64M16HG","M14D1G1664A-2.5BG","H5PS1G63"]
["1Gb","AS4C128M8D2A-25BxN","K4T1G084Q","MT47H128M8SH-25E","IS43DR81280","W971GG8JB","NT5TU128M8HE","M14D1G8128A","H5PS1G83"]
["2Gb","AS4C128M16D2-25BxN",null,"MT47H128M16RT-25E","IS43DR16128","W972GG6JB"]
["2Gb","AS4C128M16D2A-25BxN",null,"MT47H128M16RT-25E","IS43DR16128\nIS46DR16128","W972GG6JB"]
["2Gb","AS4C256M8D2A-25BCN",null,"MT47H256M8EB-25E","IS43DR82560","W972GG8JB"]

{"sheet":"DDR3 SDRAM ","index":8,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[[1,0,1,1],[10,0,10,1]]}
[]
["DDR3 1.5V SDRAM"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY (MHz)","DATA RATE","TEMPERATURE  OPTIONS","ALLIANCE"]
["512Mb","32M x 16","1.5V","96-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial","AS4C32M16D3-12BxN"]
["512Mb","64M x 8","1.5V","78-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial","AS4C64M8D3-12BxN"]
["1Gb","64M x 16","1.5V","96-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial, Automotive","AS4C64M16D3B-12BxN"]
["1Gb","128M x 8","1.5V","78-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial, Automotive","AS4C128M8D3B-12BxN"]
["2Gb","128M x 16","1.5V","96-ball FBGA","1066 MHz","2133 Mbps","Commercial","AS4C128M16D3C-93BCN"]
["4Gb","256M x 16","1.5V","96-ball FBGA","800 MHz\n933 MHz\n1066 MHz","1600 Mbps\n1866 Mbps\n2133 Mbps","Commercial, Industrial","AS4C256M16D3C-12BxN \nAS4C256M16D3C-10BxN\nAS4C256M16D3C-93BxN"]
["* X= TEMPERATURE GRADE; C = COMMERCIAL ; I = INDUSTRIAL; A = AUTOMOTIVE"]
["DDR3L 1.35V SDRAM"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY (MHz)","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE"]
["512Mb","32M x 16","1.35V","96-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial","AS4C32M16D3L-12BxN"]
["512Mb","64M x 8","1.35V","78-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial","AS4C64M8D3L-12BxN"]
["1Gb","64M x 16","1.35V","96-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial, Automotive","AS4C64M16D3LB-12BxN\nAS4C64M16D3LC-12BxN"]
["1Gb","128M x 8","1.35V","78-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial, Automotive","AS4C128M8D3LB-12BxN\nAS4C128M8D3LC-12BxN"]
["2Gb","128M x 16","1.35V","96-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial, Automotive","AS4C128M16D3LC-12BxN"]
["2Gb","256M x 8","1.35V","78-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial, Automotive","AS4C256M8D3LC-12BxN"]
["4Gb","256M x 16","1.35V","96-ball FBGA","800 MHz\n933 MHz","1600 Mbps\n1866 Mbps","Commercial, Industrial, Automotive","AS4C256M16D3LC-12BxN AS4C256M16D3LC-10BxN"]
["4Gb","512M x 8","1.35V","78-ball FBGA","800 MHz\n933 MHz","1600 Mbps\n1866 Mbps","Commercial, Industrial, Automotive","AS4C512M8D3LC-12BxN AS4C512M8D3LC-10BAN"]
["8Gb","512M x 16","1.35V","96-ball FBGA","933 MHz","1866 Mbps","Commercial, Industrial, Automotive","AS4C512M16D3LA-10BxN"]
["8Gb","512M x 16","1.35V","96-ball FBGA","800 MHz","1600 Mbps","Commercial, Industrial","AS4C512M16D3LB-12BxN"]
["8Gb","512M x 16","1.35V","96-ball FBGA","800 MHz\n933 MHz","1600 Mbps\n1866 Mbps","Commercial, Industrial","AS4C512M16D3LC-10BxN\nAS4C512M16D3LC-12BxN"]
["8Gb","1G x 8","1.35V","78-ball FBGA","933 MHz","1866 Mbps","Commercial, Industrial, Automotive","AS4C1G8D3LA-10BxN"]
["* X= TEMPERATURE GRADE; C = COMMERCIAL ; I = INDUSTRIAL; A = AUTOMOTIVE"]

{"sheet":"DDR3 SDRAM Cross Reference","index":9,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
[]
["DDR3 SDRAM Cross Reference"]
["DENSITY","ALLIANCE","MICRON","SAMSUNG(EOL)","ISSI","HYNIX","WINBOND","ELITE (ESMT)","ELPIDA","NANYA"]
["512Mb","AS4C32M16D3-12BxN",null,null,null,null,"W6351G6KB-x","M15T5121632A","EDJ5316BASE"]
["512Mb","AS4C64M8D3-12BxN",null,null,null,null,null,null,"EDJ5308BASE"]
["512Mb","AS4C32M16D3L-12BxN",null,null,null,null,null,"M15T5121632A","EDJ5316BASE"]
["512Mb","AS4C64M8D3L-12BxN",null,null,null,null,null,null,"EDJ5308BASE"]
["1Gb","AS4C64M16D3B-12BxN","MT41J64M16JT(TW)-125 (EOL)","K4B1G1646x","IS43TR16640\nIS46TR16640","H5TQ1G63D","W631GG6KB-x","M15F1G1664A","EDJ1116DJ(BA) BG","NT5CB64M16F(G)P"]
["1Gb","AS4C64M16D3LB/C-12BxN","MT41K64M16JT(TW)-125","K4B1G1646x","IS43TR16640xL\nIS46TR16640xL","H5TC1G63EFR (EOL)","W631GU6KB-x","M15T1G1664A-(2C)","EDJ1116EJBG","NT5CC64M16F(G)P-DI"]
["1Gb","AS4C128M8D3B-12BxN","MT41J128M8JP(DA)-125","K4B1G0846x","IS43TR81280\nIS46TR81280","H5TQ1G83","W631GG8KB-x","M15T1G8128A","EDJ1108DJ(BA) BG","NT5CB128M8F(G)N-DI"]
["1Gb","AS4C128M8D3LB/C-12BxN","MT41K128M8JP(DA)-125","K4B1G0846x","IS43TR81280xL\nIS46TR81280xL","H5TC1G83EFR (EOL)","W631GU8KB-x","M15T1G8128A","EDJ1108EJBG","NT5CC128M8F(G)N-DI"]
["2Gb","AS4C128M16D3C-93BCN","MT41J128M16JT(TW)-125","K4B2G1646x","IS43TR16128","H5TQ2G63","W632GG6KB-x","M15F2G16128A","EDJ2116DEBG","NT5CB128M16I(F)P-DI"]
["2Gb","AS4C128M16D3LC-12BxN","MT41K128M16JT-125","K4B2G1646x","IS43TR16128xL\nIS46TR16128xL","H5TC2G63","W632GU6KB-x","M15F2G16128A","EDJ2116EEBG","NT5CC128M16I(F)P-DI"]
["2Gb","AS4C256M8D3LC-12BxN","MT41K256M8DA-125","K4B2G0846x","IS43TR82560xL\nIS46TR82560xL","H5TQ2G83FFR-x","W632GG8KB-x","M15T2G8256A","EDJ2108DEBG","NT5CB256M8IN-FL"]
["4Gb","AS4C256M16D3C-93BCN AS4C256M16D3C-10BxN AS4C256M16D3C-12BxN","MT41J256M16HA-107 MT41J256M16HA-125","K4B4G1646x","IS43TR16256","H5TQ4G63","W634GG6MB/ NB","M15F4G16256A","EDJ4216BFBG (BASE)","NT5CB256M16C(D,E) P-DI"]
["4Gb","AS4C256M16D3LC-10BxN AS4C256M16D3LC-12BxN","MT41K256M16HA-107/125 MT41K256M16TW-107/125","K4B4G1646x","IS43TR16256xL\nIS46TR16256xL","H5TC4G63","W634GU6MB/NB","M15T4G16256A","EDJ4216EFBG","NT5CC256M16C(D,E) P-DI"]
["4Gb","AS4C512M8D3LC-10BAN\nAS4C512M8D3LC-12BxN","MT41K512M8DA-125","K4B4G0846x","IS43TR85120xL\nIS46TR85120xL","H5TC4G83","W634GU8MB/NB","M15T4G8512A","EDJ4208EFBG","NT5CC512M8C(D,E) N-DI"]
["8Gb","AS4C512M16D3LA-10BxN","MT41K512M16VRN-107 MT41K512M16VRP-107 MT41K512M16HA-125 (EOL)","K4B8G1646x","IS43TR16512","H5TC8G63CMR","W638GU6QB","M15T8G16512A–DE",null,"NT5CC512T16EH-DI/A/H\nNT5CC512T16EH-EK/A/H"]
["8Gb","AS4C512M16D3LB-12BxN","MT41K512M16HA-125 (EOL)","K4B8G1646x","IS43TR16512","H5TC8G63CMR","W638GU6QB","M15T8G16512A–BD",null,"NT5CC512T16EH-DI/A/H"]
["8Gb","AS4C512M16D3LC-10BxN\nAS4C512M16D3LC-12BxN","MT41K512M16VRN-107 MT41K512M16VRP-107 MT41K512M16HA-125 (EOL)","K4B8G1646x","IS43TR16512","H5TC8G63CMR","W638GU6QB","M15T8G16512A–BD\nM15T8G16512A–DE",null,"NT5CC512T16EH-DI/A/H\nNT5CC512T16EH-EK/A/H"]
["8Gb","AS4C1G8D3LA-10BxN","MT41K1G8SN-107/125:E","K4B8G0846x","IS43TR81024","H5TC8G83BMR"]
["8Gb","MT41K512M16HA-125","MT41K512M16HA-125","K4B8G1646x","IS43TR16512","H5TC8G63CMR","W638GU6QB","M15T8G16512A–BD",null,"NT5CC512T16EH-DI/A/H"]

{"sheet":"DDR4 SDRAM","index":10,"n_rows":14,"n_cols":8,"rows_kept":14,"cut":false,"hidden":false,"merged":[[1,0,1,1]]}
[]
["DDR4 SDRAM"]
["DENSITY","ORG","VCC","PACKAGES","CLOCK FREQUENCY","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE PART#"]
["4Gb","256M x 16","1.2V","96-ball FBGA (7.5x13.5mm)","1333 MHz\n1200 MHz","2666 Mbps\n2400 Mbps","Commercial, Industrial","AS4C256M16D4-75BxN\nAS4C256M16D4-83BxN"]
["4Gb","512M x 8","1.2V","78-ball FBGA\n(7.5x10.6mm)","1333 MHz\n1200 MHz","2666 Mbps\n2400 Mbps","Commercial, Industrial","AS4C512M8D4-75BxN\nAS4C512M8D4-83BxN"]
["4Gb","256M x 16","1.2V","96-ball FBGA (7.5x13mm)","1600 MHz\n1333 MHz","3200 Mbps\n2666 Mbps","Commercial, Industrial","AS4C256M16D4A-62BxN\nAS4C256M16D4A-75BxN"]
["4Gb","512M x 8","1.2V","78-ball FBGA\n(7.5x11mm)","1333 MHz","2666 Mbps","Commercial, Industrial","AS4C512M8D4A-75BxN"]
["8Gb","512M x 16","1.2V","96-ball FBGA\n(7.5x13mm)","1333 MHz","2666 Mbps","Commercial, Industrial","AS4C512M16D4-75BxN"]
["8Gb","512M x 16","1.2V","96-ball FBGA\n(7.5x13mm)","1600 MHz","3200 Mbps","Commercial, Industrial","AS4C512M16D4A-62BxN"]
["8Gb","512M x 16","1.2V","96-ball FBGA\n(7.5x13mm)","1600 MHz","3200 Mbps","Automotive Temperature\n-40°C to 105°C","AS4C512M16D4A-62BAN"]
["8Gb","1G x 8","1.2V","78-ball FBGA\n(7.5x12mm)","1333 MHz","2666 Mbps","Commercial, Industrial","AS4C1G8D4-75BxN"]
["8Gb","1G x 8","1.2V","78-ball FBGA\n(7.5x12mm)","1600 MHz","3200 Mbps","Commercial, Industrial","AS4C1G8D4A-62BxN"]
["16Gb","1G x 16","1.2V","96-ball FBGA\n(9x13mm)","1600 MHz","3200 Mbps","Commercial","MT40A1G16KH-062E"]
["16Gb","1G x 16","1.2V","96-ball FBGA\n(9x13mm)","1600 MHz","3200 Mbps","Commercial","AS4C1G16D4-062BCN"]

{"sheet":"DDR4 SDRAM Cross Reference","index":11,"n_rows":10,"n_cols":8,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
[]
["DDR4 SDRAM Cross Reference"]
["DENSITY","ORG","ALLIANCE","MICRON","NANYA","SAMSUNG","HYNIX","ISSI"]
["4Gb","256M x 16","AS4C256M16D4-83BxN\nAS4C256M16D4-75BxN","MT40A256M16GE","NT5AD256M16D4","K4A4G165Wx","H5AN4G6NBJR","IS43QR16256"]
["4Gb","512M x 8","AS4C512M8D4-83BxN\nAS4C512M8D4-75BxN","MT40A512M8RH","NT5AD512M8D4","K4A4G085Wx","H5AN4G8NBJR","IS43QR85120"]
["4Gb","256M x 16","AS4C256M16D4A-62BxN\nAS4C256M16D4A-75BxN","MT40A256M16GE","NT5AD256M16D4","K4A4G165Wx","H5AN4G6NBJR","IS43QR16256"]
["4Gb","512M x 8","AS4C512M8D4A-75BxN","MT40A512M8RH","NT5AD512M8D4","K4A4G085Wx","H5AN4G8NBJR","IS43QR85120"]
["8Gb","512M x 16","AS4C512M16D4-75BxN\nAS4C512M16D4A-62BxN","MT40A512M16LY/JY","NT5AD512M16C4","K4A8G165Wx","H5AN8G6NCJR","IS43QR16512A\nIS46QR16512A"]
["8Gb","1G x 8","AS4C1G8D4-75BxN\nAS4C1G8D4A-62BxN","MT40A1G8SA/WE","NT5AD1024M8C3","K4A8G085Wx","H5AN8G8NCJR","IS43QR81024A"]
["16Gb","1G x 16","MT40A1G16KH-062E\nAS4C1G16D4-062BCN","MT40A1G16KH/KNR",null,"K4AAG165Wx","H5ANAG6NCMR-XNC\nH5ANAG6NDMR-XNC"]

{"sheet":"Mobile LP DRAM-SDRAM","index":12,"n_rows":31,"n_cols":8,"rows_kept":31,"cut":false,"hidden":false,"merged":[[5,4,6,4],[5,5,6,5],[8,0,9,0],[8,1,9,1],[8,2,9,2],[8,3,9,3],[8,4,9,4],[8,5,9,5],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[3,5,4,5],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,4,3],[3,4,4,4],[10,5,11,5],[10,0,11,0],[10,1,11,1],[10,2,11,2],[10,3,11,3],[10,4,11,4]]}
[]
["MOBILE LOW POWER SDRAM"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY","TEMPERATURE OPTIONS","ALLIANCE"]
["128Mb","8M x 16","1.7V ~ 1.95V","54-ball FBGA (8x8mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C8M16MSA-6BIN"]
[null,null,null,null,null,null,"AS4C8M16MSB-6BIN"]
["256Mb","16M x 16","1.7V ~ 1.95V","54-ball FBGA (8x8mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C16M16MSA-6BIN"]
[null,null,null,null,null,null,"AS4C16M16MSB-6BIN"]
["256Mb","8M x 32","1.7V ~ 1.95V","90-ball FBGA (8x13mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C8M32MSB-6BIN"]
["512Mb","32M x 16","1.7V ~ 1.95V","54-ball FBGA (8x8mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C32M16MSA-6BIN"]
[null,null,null,null,null,null,"AS4C32M16MSB-6BIN"]
["512Mb","16M x 32","1.7V ~ 1.95V","90-ball FBGA (8x13mm)","166 MHz","Industrial -40°C ~ +85°C","AS4C16M32MSA-6BIN"]
[null,null,null,null,null,null,"AS4C16M32MSB-6BIN"]
["MOBILE LP DDR"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE"]
["256Mb","16M x 16","1.8V","60-ball FBGA (8x9mm)","166 MHz","333Mbps","Extended -30°C ~ +85°C","AS4C16M16MD1-6BCN"]
["512Mb","32M x 16","1.8V","60-ball FBGA (8x9mm)","200 MHz","400Mbps","Extended -30°C ~ +85°C","AS4C32M16MD1A-5BCN"]
["512Mb","16M x 32","1.8V","90-ball FBGA (8x13mm)","200 MHz","400Mbps","Extended -25°C ~ +85°C\nIndustrial -40°C ~ +85°C   ","AS4C16M32MD1-5BxN"]
["1Gb","64M x 16","1.8V","60-ball FPBGA (8x9mm)","200 MHz","400Mbps","Industrial  -40°C ~ +85°C","AS4C64M16MD1A-5BIN"]
["1Gb","32M x 32","1.8V","90-ball FBGA (8x13mm)","200 MHz","400Mbps","Industrial  -40°C ~ +85°C","AS4C32M32MD1A-5BIN"]
["2Gb","64M x 32","1.8V","90-ball FBGA (8x13mm)","200 MHz","400Mbps","Extended -25°C ~ +85°C\nIndustrial -40°C ~ +85°C   ","AS4C64M32MD1-5BxN"]
["2Gb","64M x 32","1.8V","90-ball FBGA (8x13mm)","200 MHz","400Mbps","Industrial  -40°C ~ +85°C","AS4C64M32MD1A-5BIN"]
["MOBILE LP DDR2"]
["DENSITY","ORG","VCC","PACKAGE","CLOCK FREQUENCY (MHz)","DATA RATE","TEMPERATURE OPTIONS","ALLIANCE"]
["256Mb","8M x 32","1.2V/1.8V","134-ball FBGA","400 MHz","800Mbps","Extended -25°C ~ +85°C","AS4C8M32MD2A-25BCN"]
["256Mb","8M x 32","1.2V/1.8V","168-ball POP FBGA","400 MHz","800Mbps","Extended  -25°C ~ +85°C","AS4C8M32MD2A-25BPCN"]
["1Gb","64M x 16","1.2V/1.8V","134-ball FBGA","400 MHz","800Mbps","Industrial  -40°C ~ +85°C","AS4C64M16MD2A-25BIN"]
["1Gb","32M x 32","1.2V/1.8V","134-ball FBGA","400 MHz","800Mbps","Industrial  -40°C ~ +85°C","AS4C32M32MD2A-25BIN"]
["2Gb","128M x 16","1.2V/1.8V","134-ball FBGA","400MHz","800Mbps","Industrial  -40°C ~ +85°C","AS4C128M16MD2A-25BIN"]
["2Gb","64M x 32","1.2V/1.8V","134-ball FBGA","400 MHz","800Mbps","Industrial  -40°C ~ +85°C","AS4C64M32MD2A-25BIN"]
["4Gb","128M x 32","1.2V/1.8V","134-ball FBGA","533 MHz","1066Mbps","Industrial  -40°C ~ +85°C","AS4C128M32MD2A-18BIN"]
["4Gb","128M x 32","1.2V/1.8V","134-ball FBGA","400 MHz","800Mbps","Industrial  -40°C ~ +85°C","AS4C128M32MD2A-25BIN"]

{"sheet":"Mobile LP DRAM Cross Reference","index":13,"n_rows":32,"n_cols":9,"rows_kept":32,"cut":false,"hidden":false,"merged":[[8,5,9,5],[8,0,9,0],[8,2,9,2],[8,3,9,3],[8,4,9,4],[3,0,4,0],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[5,0,6,0],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,5],[10,0,11,0],[10,2,11,2],[10,3,11,3],[10,5,11,5],[10,4,11,4]]}
[]
["MOBILE LOW POWER SDRAM Cross Reference"]
["DENSITY","ALLIANCE","MICRON","ISSI","NANYA","WINBOND"]
["128Mb","AS4C8M16MSA-6BIN",null,"IS42VM16800H",null,"W987D6HBGX"]
[null,"AS4C8M16MSB-6BIN"]
["256Mb","AS4C16M16MSA-6BIN","MT48H16M16LFBF (EOL)","IS42VM16160K",null,"W988D6FBGX"]
[null,"AS4C16M16MSB-6BIN"]
["256Mb","AS4C8M32MSB-6BIN","MT48H8M32LFB5 (EOL)","IS42VM32800K",null,"W988D2FBJX"]
["512Mb","AS4C32M16MSA-6BIN","MT48H32M16LFB4-6 IT","IS42VM16320E","NT6SM32M16BG-S1","W989D6DBGX"]
[null,"AS4C32M16MSB-6BIN"]
["512Mb","AS4C16M32MSA-6BIN","MT48H16M32LFB5-6 IT","IS42VM32160E","NT6SM16M32BK-S1","W989D2DBJX"]
[null,"AS4C16M32MSB-6BIN"]
[]
["MOBILE LP DDR1 Cross Reference"]
["DENSITY","ALLIANCE","MICRON","SAMSUNG","ISSI","HYNIX","NANYA","ELITE (ESMT)","WINBOND"]
["256Mb","AS4C16M16MD1-6BCN","MT46H16M16LFBF-6","K4X56163SPN","IS43LR16160","HY5MS5B6/ H5MS2562","NT6DM16M16AD-T1","M53D2561616A-6BG2F","W948D6FBHX"]
["512Mb","AS4C32M16MD1A-5BCN","MT46H32M16LFBF-5","K4X51163PI","IS43R16320B","HY5MS7B6/ H5MS5162","NT6DM32M16A(B)D-T1","M53D5121632A-5BG2T","W949D6DBHX"]
["512Mb","AS4C16M32MD1-5BxN","MT46H16M32LFB5-5","K4X51323PI","IS43LR32160B","H5MS5132/ H5MS5122","NT6DM16M32A(B)C-T1","M53D5123216A-5BG2S","W949D2DBJX"]
["1Gb","AS4C64M16MD1A-5BIN","MT46H64M16LFBF","K4X1G163PE","IS43LR16640A","H5MS1G62"]
["1Gb","AS4C32M32MD1A-5BIN","MT46H32M32LFB5-5","K4X1G323PF","IS43LR32320B","H5MS1G22","NT6DM32M32BC-T1","M53D1G3232A","W94AD2KBJX"]
["2Gb","AS4C64M32MD1-5BxN","MT46H64M32LFKQ-5","K4X2G323PC","IS43LR32640A","H5M52G22"]
["2Gb","AS4C64M32MD1A-5BIN","MT46H64M32LFKQ-5","K4X2G323PC","IS43LR32640A","H5M52G22"]
[]
["MOBILE LP DDR2 Cross Reference"]
["DENSITY","ALLIANCE","MICRON","SAMSUNG","ISSI","HYNIX","NANYA","ELITE (ESMT)","WINBOND"]
["256Mb","AS4C8M32MD2A-25B(P)CN",null,null,"IS43LD32800A-25BLx\nIS43LD32800B-25BLx",null,null,null,"W978H2KBVX2E"]
["1Gb","AS4C64M16MD2A-25BIN","MT42L64M16D1HE-25",null,"IS43LD16640C/A",null,"NT6TL64M16BA(I)-G0",null,"W97AH6KBVX2"]
["1Gb","AS4C32M32MD2A-25BIN","MT42L32M32D1HE-25",null,"IS43LD32320C/A",null,"NT6TL32M32BI(A)-G0",null,"W97AH2KBVX2"]
["2Gb","AS4C128M16MD2A-25BIN","MT42L128M16D1TK-25",null,"IS43LD16128B",null,"NT6TL128M16CI(A)-G0",null,"W97BH6KBVX2"]
["2Gb","AS4C64M32MD2A-25BIN","MT42L64M32D1TK-25",null,"IS43LD32640B",null,"NT6TL64M32CI(A)-G0",null,"W97BH2KBVX2"]
["4Gb","AS4C128M32MD2A-18BIN","MT42L128M32D1GU-18",null,"IS43LD32128A",null,"NT6TL128M32BI(A)-G0"]
["4Gb","AS4C128M32MD2A-25BIN","MT42L128M32D1GU-18",null,"IS43LD32128A",null,"NT6TL128M32BI(A)-G0"]

{"sheet":"LPDDR4-LPDDR4X","index":14,"n_rows":17,"n_cols":9,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
[]
["LPDDR4"]
["DENSITY","ORG","VDD1 / VDD2 / VDDQ","PACKAGES","CLOCK FREQUENCY","DATA RATE","TEMPERATURE OPTIONS","ALLIIANCE","REMARKS"]
["2Gb","128M x 16","1.8V / 1.1V / 1.1V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Automotive A2 \n(-40°C to 105°C)","AS4C128M16MD4-062BAN","With ECC"]
["2Gb","64M x 32","1.8V / 1.1V / 1.1V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Automotive A2 \n(-40°C to 105°C)","AS4C64M32MD4-062BAN","With ECC"]
["4Gb","128M x 32","1.8V / 1.1V / 1.1V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Automotive A2 \n(-40°C to 105°C)","AS4C128M32MD4-062BAN","With ECC"]
["4Gb","256M x 16","1.8V / 1.1V / 1.1V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Automotive A2 \n(-40°C to 105°C)","AS4C256M16MD4-062BAN","With ECC"]
["8Gb","256M x 32","1.8V / 1.1V / 1.1V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Automotive A2 \n(-40°C to 105°C)","AS4C256M32MD4-062BAN","With ECC"]
["LPDDR4X"]
["DENSITY","ORG","VDD1 / VDD2 / VDDQ","PACKAGES","CLOCK FREQUENCY","DATA RATE","TEMPERATURE OPTIONS","ALLIIANCE","REMARKS"]
["2Gb","128M x 16","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Automotive A2 \n(-40°C to 105°C)","AS4C128M16MD4V-062BAN","With ECC"]
["4Gb","256M x 16","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Automotive A2 \n(-40°C to 105°C)","AS4C256M16MD4V-062BAN","With ECC"]
["8Gb","256M x 32","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x14.5mm)","1600 MHz","3200 Mbps","Automotive A2 \n(-40°C to 105°C)","AS4C256M32MD4V-062BAN","With ECC"]
["8Gb","512M x 16","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x15mm)","1866 MHz","3733 Mbps","Industrial (-40C to 85C)","AS4C512M16MD4V-053BIN","without ECC"]
["16Gb","512M x 32","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x15mm)","1866 MHz","3733 Mbps","Industrial (-40C to 85C)","AS4C512M32MD4V-053BIN","without ECC"]
["16Gb","512M x 32","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x15mm)","2133 MHz","4266 Mbps","Industrial (-40C to 95C)","AS4C512M32MD4V-046BIN","without ECC"]
["32Gb","1Gb x 32","1.8V / 1.1V / 0.6V","200b TFBGA\n(10x15mm)","2133 MHz","4266 Mbps","Industrial (-40C to 95C)","AS4C1G32MD4V-046BIN","without ECC"]

{"sheet":"LPDDR4-LPDDR4X cross Reference","index":15,"n_rows":17,"n_cols":10,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
[]
["LPDDR4 Cross Reference "]
["DENSITY","ORG","ALLIANCE","MICRON","SAMSUNG","HYNIX","NANYA","ISSI","WINBOND","IM"]
["2Gb","128M x 16","AS4C128M16MD4-062BAN","MT53E128M16D1DS",null,"H9HCNNNBKUMLXR/HR","NT6AN128M16AV","IS43/46LQ16128A\nIS43/46LQ16128EA","W66BL6NBU\nW66BP6NBU"]
["2Gb","64M x 32","AS4C64M32MD4-062BAN",null,null,null,null,"IS43/46LQ32640A\nIS43/46LQ32640EA","W66CL2NQU\nW66CP2NQU\nW66CP2NQQ"]
["4Gb","128M x 32","AS4C128M32MD4-062BAN","MT53B128M32D1DS\nMT53E128M32D2DS\nMT53E128M32D2FW","K4F4E3S4HF-GFCJ\nK4F4E3S4HF-GHCJ",null,"NT6AN128T32AV","IS43/46LQ32128A\nIS43/46LQ32128EA","W66CL2NQU\nW66CP2NQU","IME4G32L4HABG"]
["4Gb","256M x 16","AS4C256M16MD4-062BAN","MT53E256M16D1DS\nMT53E256M16D1FW",null,"H9HCNNN4KUMLHR","NT6AN256M16AV","IS43/46LQ16256A\nIS43/46LQ16256EA","W66CP6NBU\nW66CL6NBU"]
["8Gb","256M x 32","AS4C256M32MD4-062BAN","MT53B256M32D1DS\nMT53E256M32D2DS\nMT53E256M32D2FW","K4F8E304HB-MGCJ\nK4F8E3S4HB-MFCJ\nK4F8E3S4HB-MHCJ","H9HCNNN8KUMLHR","NT6AN256T32AV","IS43/46LQ32256A\nIS43/46LQ32256EA","W66DP2NQU\nW66DL2NQU","IME8G32L4HADG"]
["LPDDR4X Cross Reference "]
["DENSITY","ORG","ALLIANCE","MICRON","SAMSUNG","HYNIX","NANYA","ISSI","WINBOND","IM"]
["2Gb","128M x 16","AS4C128M16MD4V-062BAN",null,null,null,null,"IS43/46LQ16128AL\nIS43/46LQ16128EA","W66BQ6NBU"]
["4Gb","256M x 16","AS4C256M16MD4V-062BAN","MT53E256M16D1DS\nMT53E256M16D1FW","K4U8E3S4AD-GFCL\nK4U8E3S4AD-GHC","H9HCNNN4KMMLHR","NT6AP256M16AV","IS43/46LQ16256AL\nIS43/46LQ16256EA","W66CQ6NQU","IM4G16L4JCBG"]
["8Gb","256M x 32","AS4C256M32MD4V-062BAN","MT53B256M32D1DS\nMT53E256M32D2DS\nMT53E256M32D2FW","K4U8E3S4Ax",null,"NT6AP256T32AV","IS43/46LQ32256AL\nIS43/46LQ32256EAL","W66DQ2NQU","IM8G32L4JCBG"]
["8Gb","512M x 16","AS4C512M16MD4V-053BIN","MT53D512M16D1DS\nMT53E512M16D1FW",null,null,"NT6AP512M16AV","IS43LQ16512AL",null,"IM8G16L4JCBG-046"]
["16Gb","512M x 32","AS4C512M32MD4V-053BIN","MT53D512M32D2Dx\nMT53D512M32D1ZW\nMT53D512M32D2FW","K4U6E3S4Ax","H9HCNNNBPUMLHR\n","NT6AP512T32BY",null,null,"IMAG32L4JCBG-046"]
["16Gb","512M x 32","AS4C512M32MD4V-046BIN","MT53D512M32D2Dx\nMT53E512M32D2FW\nMT53E512M32D1ZW","K4U6E3S4Ax","H9HCNNNBKMMLXR\nH9HCNNNBPUMLHR","NT6AP512T32BY",null,null,"IMAG32L4JCBG-046"]
["32Gb","1G x 32","AS4C1G32MD4V-046BIN","MT53D1024M32D4Dx\nMT53E1G32D2FW\nMT53E1G32D2Nx","K4UBE3D4Ax","H9HCNNNCPMMLXR\nH9HCNNNCPMMLXR","NT6AP1024F32B"]

{"sheet":"pSRAM","index":16,"n_rows":10,"n_cols":7,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
[]
["pSRAM"]
["DENSITY","ORG","VCC","PACKAGE","TEMPERATURE","SPEED","ALLIANCE MEMORY PART#"]
["8Mb","512K x 16","1.8V","48 FPBGA (6x7mm)","Industrial (-30°C ~+85°C)","70ns","AS1C512K16PL-70BIN"]
["8Mb","512K x 16","3V","48 FPBGA (6x7mm)","Industrial (-40°C~ +85°C)","70ns","AS1C512K16P-70BIN"]
["16Mb","1M x 16","1.8V","48 FPBGA (6x7mm)","Industrial (-40°C~ +85°C)","70ns","AS1C1M16PL-70BIN"]
["16Mb","1M x 16","3V","48 FPBGA (6x7mm)","Industrial (-40°C~ +85°C)","70ns","AS1C1M16P-70BIN"]
["32Mb","2M x 16","3V","48 FPBGA (6x7mm)","Industrial (-40°C~ +85°C)","70ns","AS1C2M16P-70BIN"]
["64Mb","4M x 16","1.8V","49 FBGA (4x4mm)","Industrial (-30°C ~+85°C)","70ns","AS1C4M16PL-70BIN"]
["128Mb\n(*2-stacked die)","8M x 16","1.8V","49 FBGA (4x4mm)","Industrial (-30°C ~+85°C)","70ns","AS1C8M16PL-70BIN"]

{"sheet":"pSRAM Cross Reference","index":17,"n_rows":10,"n_cols":9,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
[]
["pSRAM Cross Reference"]
["ORG","DENSITY","PACKAGE","COMMENTS/ PREV REV","ALLIANCE","JSC/JEJU","ISSI","FIDELIX","AP MEMORY"]
["8Mb","512K x 16","48 FPBGA","page mode & Non-DPD","AS1C512K16PL-70BIN","EM784SP16BPP-70LF","IS66WV51216EALL-70BLI"]
["8Mb","512K x 16","48 FPBGA","Non-page mode & Non-DPD","AS1C512K16P-70BIN","JS784SU16BSP-70LFI","IS66/67WV51216EBLL-70BL","FMP0817CAx"]
["16Mb","1M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C1M16PL-70BIN","EM7164SP16CSP-70LFI","IS66W1M16EALL-70BLI","FMP1617CCx"]
["16Mb","1M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C1M16P-70BIN","JS164SU16BSP-70LFI","IS66/67WV1M16EBLL-70BL","FMP1617CAx"]
["32Mb","2M X16","48 FPBGA","Non-page mode & Non-DPD","AS1C2M16P-70BIN","JS7324SU16BSP-70LFI","IS66WVE2M16EBLL-70B","FMP3217CAx"]
["64Mb","4M X16","49 FBGA","DPD mode","AS1C4M16PL-70BIN","EMC643SP16CKDT-70LF"]
["128Mb\n(*2-stacked die)","8M X16","49 FBGA","DPD mode","AS1C8M16PL-70BIN","JSC283SP16ATDT-70LF",null,null,"APS128XX"]

{"sheet":"Fast Asynchronous SRAM","index":18,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
[]
["5V FAST ASYNCHRONOUS SRAM"]
["DENSITY","ORG","VCC","PACKAGES","TEMPERATURE","SPEED (NS)","ALLIANCE"]
["64Kb","8K x 8","5V","28pin SOJ (300mils),Skinny 28pin PDIP (300mils)","Commercial  0°C ~ +70°C\nIndustrial  -40°C ~ +85°C",15,"AS7C164A"]
["256Kb","32K x 8","5V","28pin SOJ (300mils), 28pin TSOP I (8x13.4mm)","Commercial  0°C ~ +70°C\nIndustrial  -40°C ~ +85°C","10,12,15,20","AS7C256A"]
["256Kb","32K x 8","5V","28pin PDIP (300mils)","Industrial  -40°C ~ +85°C",15,"AS7C256B"]
["512Kb","32K x 16","5V","44pin SOJ (400mils), 44pin TSOP II (400mils)","Commercial  0°C ~ +70°C","12,15","AS7C513B"]
["1Mb","128K x 8","5V","32pin SOJ (300mils & 400mils), 32pin TSOP I (8x13.4mm) Corner Vcc & Gnd","Commercial  0°C ~ +70°C\nIndustrial  -40°C ~ +85°C","12,15,20","AS7C1024B"]
["1Mb","128K x 8","5V","32pin SOJ (300mils & 400mils), Center Vcc & Gnd","Commercial  0°C ~ +70°C\nIndustrial  -40°C ~ +85°C","10,12,15","AS7C1025B"]
["1Mb","64K x 16","5V","44pin SOJ (400mils), 44pin TSOP II (400mils)","Commercial  0°C ~ +70°C\nIndustrial  -40°C ~ +85°C","10,12,15,20","AS7C1026B"]
["4Mb","512K x 8","5V","36pin SOJ (400mils), 44pin TSOP II (400mils)","Commercial  0°C ~ +70°C\nIndustrial  -40°C ~ +85°C","10,12,15,20","AS7C4096A"]
["4Mb","256K x 16","5V","44pin SOJ (400mils), 44pin TSOP II (400mils)","Commercial  0°C ~ +70°C\nIndustrial  -40°C ~ +85°C","10,12,15,20","AS7C4098A"]
["3.3V FAST ASYNCHRONOUS SRAM"]
["DENSITY","ORG","VCC","PACKAGES","TEMPERATURE","SPEED (NS)","ALLIANCE"]
["256Kb","32K x 8","3.3V","28pin SOJ (300mils), 28pin TSOP I (8x13.4mm)","Commercial\nIndustrial","10,12,15,20","AS7C3256A"]
["512Kb","32K x 16","3.3V","44pin SOJ (400mils), 44pin TSOP II (400mils)","Commercial","10,12,15,20","AS7C3513B"]
["1Mb","128K x 8","3.3V","32pin SOJ (300 & 400mils), 32pin TSOP I (8x13.4mm), Corner Vcc & Gnd","Commercial","10,12,15,20","AS7C31024B"]
["1Mb","128K x 8","3.3V","32pin SOJ (300 & 400mils), Center Vcc & Gnd","Commercial\nIndustrial","10,12,15,20","AS7C31025B"]
["1Mb","64K x 16","3.3V","44pin SOJ (400mils), 44pin TSOP II (400mils)","Commercial\nIndustrial","10,12,15,20","AS7C31026B"]
["2Mb","128K x 16","3.3V","44pin TSOP II (400mils)","Commercial\nIndustrial","10,12,15,20","AS7C32098A"]
["2Mb","256K x 8","3.3V","44pin TSOP II (400mils)","Commercial\nIndustrial","10,12,15,20","AS7C32096A"]
["4Mb","512K x 8","3.3V","36pin SOJ (400mils), 44pin TSOP II (400mils), 36b TFBGA (6x8mm)","Commercial\nIndustrial","8,10,12,15,20","AS7C34096A , B"]
["4Mb","256K x 16","3.3V","44pin SOJ (400mils), 44pin TSOP II (400mils), 48b TFBGA (6x8mm, 8x10mm)","Commercial\nIndustrial","8,10,12,15,20","AS7C34098A , B"]
["8Mb","1M x 8","3.3V","44pin TSOP II (400mils), 48b TFBGA (6x8mm)","Industrial",10,"AS7C38096A , B"]
["8Mb","512K x 16","3.3V","44pin TSOP II (400mils), 48b TFBGA (6x8mm)","Industrial",10,"AS7C38098A"]
["8Mb","256K x 32","3.3V","90b TFBGA (8x13mm)","Industrial",10,"AS7C325632"]
["16Mb","512K x32","3.3V","90b TFBGA (9x13mm)","Industrial",10,"AS7C351232"]
["16Mb","1M x 16","3.3V","48b TFBGA (6x8mm), 48pin TSOP I (12x20mm), 54pin TSOP II (400mils)","Industrial",10,"AS7C316098A , B"]
["16Mb","2M x 8","3.3V","48b TFBGA (6x8mm), 48pin TSOP I (12x20mm), 44pin TSOP II, 54pin TSOP II","Industrial",10,"AS7C316096A , B , C"]

{"sheet":"Fast Asyn SRAM Cross Reference","index":19,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[]}
[]
["Fast Asynchronous SRAM Cross Reference"]
["64K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS (EOL)","IDT","ISSI"]
["8K x 8","5V","28pin SOJ (300mil)",15,"AS7C164A-15JxN",null,"CY7C185-15VI (EOL)","IDT7164SXXYG","IS61C64AL-10JLI (EOL)"]
["8K x 8","5V","28pin Skinny PDIP 300mil",15,"AS7C164A-15PxN",null,"CY7C185-20PXC (EOL)"]
["256K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS (EOL)","IDT","ISSI"]
["32K x 8","5V","28pin SOJ","10,12,15,20","AS7C256A-xxJCN/JIN","K6E0808C (EOL)","CY7C199D-XXVXI","IDT71256SAXXYG","IS61C256AL-XXJL (EOL)"]
["32K x 8","5V","28pin TSOP I","10,12,15,20","AS7C256A-xxTCN/TIN",null,"CY7C199D-XXZXI","IDT71256SAXXPZG","IS61C256AL-XXTL"]
["32K x 8","3.3V","28pin SOJ","10,12,15,20","AS7C3256A-xxJCN/JIN","K6E0808V","CY7C1399BN-12VXC","IDT71V256SAXXYG","IS61LV256AL-10JL (EOL)"]
["32K x 8","3.3V","28pin TSOP I","10,12,15,20","AS7C3256A-xxTCN/TIN",null,"CY7C1399BN-XXZXI","IDT71V256SAXXPZG","IS61LV256AL-10TL"]
["32K x 8","5V","28pin DIP",15,"AS7C256B-xxPIN","(EOL)","CY7C199CN-15PXC (EOL)","IDT71256SAXXTPG"]
["512K FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI"]
["32K x 16","5V","44pin SOJ (400mil)",15,"AS7C513B-xxJCN",null,"CY7C1020D-10VXI",null,"IS61C321AL-12KLI (EOL)"]
["32K x 16","5V","44pin TSOP II (400mil)","12,15","AS7C513B-xxTCN",null,"CY7C1020D-10ZSXI",null,"IS61C3216AL-12TLI"]
["32K x 16","3.3V","44pin TSOP II (400mil)","12,15,20","AS7C3513B-xxTCN",null,"CY7C1020DV33-10ZSXI",null,"IS61WV3216BLL-12TLI"]
["32K x 16","3.3V","44pin SOJ (400mil)","10,12,15","AS7C3513B-xxJCN",null,"CY7C1020DV33-10VXI"]
["1M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG (EOL)","CYPRESS","IDT","ISSI"]
["128K x 8","5V","32pin SOJ (400mil)","12,15,20","AS7C1025B-xxJCN/JIN","K6R1008C1D-KI10",null,"IDT71124SXXYG"]
["128K x 8","3.3V","32pin SOJ (400mil)","10,12,15,20","AS7C31025B-xxJCN/JIN","K6R1008V1D-KI10","CY7C1019DV33-10VXI","IDT71V124SAXXYG","IS63WV1024L-10KLI (EOL)"]
["128K x 8","5V","32pin SOJ (300mil)","10,12,15,20","AS7C1025B-xxTJCN",null,"CY7C1019D-10VXI"]
["128K x 8","3.3V","32pin SOJ (400mil)",12,"AS7C31025C-12JIN"]
["128K x 8","3.3V","32pin SOJ (300mil)","10,12,15,20","AS7C31025B-xxTJCN",null,"CY7C1018DV33-10VXI","IDT71V124SAXXTYG","IS63WV1288DBLL-10JLI (EOL)"]
["128K x 8","5V","32pin SOJ (400mil)","12,15,20","AS7C1024B-xxJCN/JIN",null,"CY7C109D-10VXI","IDT71024SXXYG","IS61C1024AL-12KLI (EOL)"]
["128K x 8","5V","32pin TSOP I","12,15,20","AS7C1024B-xxTCN",null,"CY7C109D-10ZXI",null,"IS61C1024AL-12TLI"]
["128K x 8","5V","32pin SOJ (300mil)","12,15,20","AS7C1024B-xxTJCN",null,"CY7C1009D-10VXI","IDT71024SXXTYG","IS61C1024AL-12JLI (EOL)"]
["128K x 8","3.3V","32pin SOJ (400mil)","12,15,20","AS7C31024B-xxJCN",null,"CY1019DV33-10VXI",null,"IS63WV1288DBLL-10KLI (EOL)"]
["128K x 8","3.3V","32pin TSOP I","10,12,15,20","AS7C31024B-xxTCN",null,null,null,"IS63WV1288DBLL-10HLI"]
["128K x 8","3.3V","32pin SOJ (300mil)","10,12,15,20","AS7C31024B-xxTJCN",null,"CY7C1018DV33-10VXI",null,"IS63WV1288DBLL-10JLI"]
["64K x 16","5V","44pin SOJ (400mil)","10,12,15,20","AS7C1026B-xxJCN/JIN","K6R1016C1D-KI10","CY7C1021D-XXVXC","IDT71016SXXYG","IS61C6416AL-12KLI (EOL)"]
["64K x 16","5V","44pin TSOP II (400mil)","10,12,15,20","AS7C1026B-xxTCN/TIN","K6R1016C1D-UI10","CY7C1021D-XXZSXI","IDT71016SXXPHG","IS61C6416AL-12TLI"]
["64K x 16","3.3V","44pin SOJ (400mil)","10,12,15,20","AS7C31026B-xxJCN/TIN","K6R1016V1D-KI10","CY7C1021DV33-XXVXI","IDT71V016SAXXYG","IS61WV6416DBLL-10KLI (EOL)"]
["64K x 16","3.3V","44pin TSOP II (400mil)","10,12,15,20","AS7C31026B-xxTCN/TIN","K6R1016V1D-UI10","CY7C1021DV33-XXZSXI","IDT71V016SAXXPHG","IS61WV6416DBLL-10TLI"]
["2M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["128K x 16","3.3V","44pin TSOP II","10,12,15,20","AS7C32098A-xxTxN",null,"CY7C1011DV33-10ZSXI",null,"IS61WV12816DBLL-10TL","GS72116AGP-XX"]
["256K x 8","3.3V","44pin TSOP II","10,12,15,20","AS7C32096A-xxTxN",null,"CY7C1010DV33-10ZSXI",null,"IS61WV256EDBLL-10TLI","GS72108AGP-XX"]
["4M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI"]
["512K x 8","5V","36pin SOJ (400mil)","10,12,15,20","AS7C4096A-xxJxN","K6R4008C1D-KI10","CY7C1049D-10VXI",null,"IS61C5128AL-10KLI (EOL)"]
["512K x 8","5V","44pin TSOP II (400mil)","10,12,15,20","AS7C4096A-xxTxN","K6R4008C1D-UI10",null,null,"IS61C5128AL-10TLI"]
["512K x 8","3.3V","36pin SOJ (400mil)","8,10,12,15,20","AS7C34096A-xxJxN","K6R4008V1D-KI10","CY7C1049DV33-10VXI","IDT71V424SXXYG","IS61WV5128EDBLL-10KLI (EOL)"]
["512K x 8","3.3V","44pin TSOP II (400mil)","10,12,15,20","AS7C34096A-xxTxN","K6R4008V1D-UI10","CY7C1049DV33-10ZSI","IDT71V424SXXPHG","IS61WV5128EDBLL-10TLI"]
["512K x 8","2.7 ~ 3.6V","44pin TSOP II",10,"AS7C34096B-10TIN"]
["512K x 8","2.7 ~ 3.6V","36ball TFBGA",10,"AS7C34096B-10BIN"]
["256K x 16","5V","44pin SOJ (400mil)","10,12,15,20","AS7C4098A-xxJxN","K6R4016C1D-KI10","CY7C1041D-10VXI",null,"IS61C25616AL-10KLI (EOL)"]
["256K x 16","5V","44pin TSOP II (400mil)","10,12,15,20","AS7C4098A-xxTxN","K6R4016C1D-UI10","CY7C1041D-10ZSXI",null,"IS61C25616AL-10TL"]
["256K x 16","3.3V","44pin SOJ (400mil)","10,12,15,20","AS7C34098A-xxJxN","K6R4016V1D-KI10","CY7C1041DV33-10VXI","IDT71V416SXXYG"]
["256K x 16","3.3V","44pin TSOP II (400mil)","8,10,12,15,20","AS7C34098A-xxTxN","K6R4016V1D-UI10","CY7C1041DV33-10ZSXI","IDT71V416SXXPHG","IS61WV25616EDBLL-10TLI"]
["256K x 16","3.3V","48ball TFBGA",10,"AS7C34098A-xxBIN",null,"CY7C1041DV33-10BVXI","IDT71V416SXXBE","IS61WV25616EDBLL-10BLI"]
["256K x 16","2.7 ~ 3.6V","44pin TSOP II",10,"AS7C34098B-10TIN"]
["256K x 16","2.7 ~ 3.6V","48ball TFBGA",10,"AS7C34098B-10BIN"]
["8M FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["512K x 16","3.3V","44pin TSOP II",10,"AS7C38098A-10TIN",null,"CY7C1051DV33-10ZSXI",null,"IS61WV51216BLL-XXTLI"]
["512K x 16","3.3V","48ball TFBGA",10,"AS7C38098A-10BIN",null,"CY7C1051DV33-10BAXI",null,"IS61WV51216BLL-10MLI"]
["256K x 32","3.3V","90ball TFBGA",10,"AS7C325632-10BIN",null,null,null,"IS61WV25632BLL-10BLI"]
["1M x 8","3.3V","44pin TSOP II",10,"AS7C38096A-10TIN",null,"CY7C1059DV33-10ZSXI",null,"IS61WV10248BLL-10TLI"]
["1M x 8","3.3V","48ball TFBGA (different pinout)",10,"AS7C38096A-10BIN"]
["1M x 8","3.3V","48ball TFBGA (different pinout)",10,"AS7C38096B-10BIN",null,null,null,"IS61WV10248BLL-10MLI"]
["16M  FAST"]
["ORG","VCC","PACKAGE","SPEED (NS)","ALLIANCE","SAMSUNG","CYPRESS","IDT","ISSI","GSI"]
["1M x 16","3.3V","48pin TSOP I",10,"AS7C316098A-10TIN",null,"CY7C1061GN30-10ZXI",null,"IS61WV102416FBLL-10TLI"]
["1M x 16","3.3V","48ball TFBGA",10,"AS7C316098A-10BIN",null,"CY7C1061GN30-10BV1XI",null,"IS61WV102416FBLL-10BLI"]
["1M x 16","3.3V","54pin TSOP II",10,"AS7C316098B-10TIN",null,"CY7C1061GN30-10ZSXI",null,"IS61WV102416FBLL-10T2LI"]
["1M x 16","3.3V","48ball TFBGA",10,"AS7C316098B-10BIN"]
["2M x 8","3.3V","48pin TSOP I",10,"AS7C316096A-10TIN",null,"CY7C1069GN30-10ZSXI",null,"IS61WV20488FBLL-10T2LI"]
["2M x 8","3.3V","54pin TSOP II",10,"AS7C316096B-10TIN",null,"CY7C1069DV33-10ZSXI"]
["2M x 8","3.3V","44pin TSOP II",10,"AS7C316096C-10TIN",null,null,null,"IS61WV20488FBLL-10TLI"]
["2M x 8","3.3V","48ball TFBGA (1CE)",10,"AS7C316096C-10BIN",null,null,null,"IS61WV20488FBLL-10BLI"]
["2M x 8","3.3V","48ball TFBGA (2CE)",10,"AS7C316096B-10BIN",null,"CY7C1069GN30-10BVXI"]
["512K x 32","3.3V","90ball TFBGA",10,"A7C351232-10BIN",null,null,null,"IS61WV51232BLL-10BLI"]

{"sheet":"Low Power Asynchronous SRAM","index":20,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[]}
[]
["2.7V- 3.6V LOW POWER SRAMS"]
["DENSITY","ORG","VCC","PACKAGES","SPEED(NS)","ALLIANCE MEMORY PART#"]
["256Kb","32K x 8","2.5 ~ 3.6V","28pin SOP (330mm)",70,"AS62V256A-70SIN"]
["1Mb","64K x16 with ECC","2.7 ~ 3.6V","44pin TSOP II (400mils)",45,"AS6CE1016A-45ZIN"]
["2Mb","256K x 8","2.7 ~ 3.6V","32pin SOP(450mils), 32pin TSOP I (8x20mm), 32pin STSOP (8x13.4mm), 36ball TFBGA (6x8mm)",55,"AS6C2008"]
["4Mb","256K x 16","2.7 ~ 3.6V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm)",45,"AS6C4016B"]
["4Mb","256K x16 with ECC","2.7 ~ 3.6V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm)",45,"AS6CE4016B"]
["8Mb","1M x 8","2.7 ~ 3.6V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm)","45/55","AS6C8008B"]
["8Mb","512K x 16","2.7 ~ 3.6V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm)","45/55","AS6C8016B"]
["16Mb","1M x 16","2.7 ~ 3.6V","48pin TSOP I (12x20mm)",55,"AS6C1616-55TIN"]
["16Mb","1M x 16","2.7 ~ 3.6V","48pin TSOP I (12x20mm), 48ball TFBGA (6x8mm) ","45/55","AS6C1616B"]
["16Mb","1M x 16 / 2M x 8","2.7 ~ 3.6V","48pin TSOP I (12x20mm)",45,"AS6C1616C-45TIN"]
["16Mb","2M x 8","2.7 ~ 3.6V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm)",45,"AS6C1608B"]
["32Mb","2M x 16 / 4M x8","2.7 ~ 3.6V","48pin TSOP I (12x20mm) , 48ball TFBGA (8x10mm)",55,"AS6C3216A"]
["64Mb","4M x 16 / 8M x8","2.7 ~ 3.6V","48pin TSOP I (12x20mm),  48ball TFBGA (8x10mm) (dual chip select)",55,"AS6C6416"]
["2.7V - 5.5V LOW POWER SRAMS"]
["DENSITY","ORG","VCC","PACKAGES","SPEED (NS)","ALLIANCE MEMORY PART#"]
["64Kb","8K x 8","2.7 ~ 5.5V","28pin PDIP (600mils), 28pin SOP (330mils), 28pin sTSOP (8x13.4mm)",55,"AS6C6264"]
["256Kb","32K x 8","2.7 ~ 5.5V","28pin PDIP (600mils), 28pin SOP (330mils), 28pin sTSOP (8x13.4mm)",55,"AS6C62256"]
["1Mb","64K x 16","2.7 ~ 5.5V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm)",55,"AS6C1016"]
["1Mb","128K x 8","2.7 ~ 5.5V","32p SOP (450mils), 32p TSOP I (8x20mm), 32p sTSOP (8x13.4mm), 36b TFBGA (6x8mm), 32p PDIP (600mils)",55,"AS6C1008"]
["2Mb","256K x 8","2.7 ~ 5.5V","32p SOP (450mils), 32p TSOP I (8x20mm), 32p sTSOP (8x13.4mm), 36b TFBGA (6x8mm)",55,"AS6C2008A"]
["2Mb","128K x 16","2.7 ~ 5.5V","44pin TSOP II (400mils), 48b TFBGA (6x8mm)",55,"AS6C2016"]
["4Mb","512K x 8","2.7 ~ 5.5V","32p SOP (450mils), 32p TSOP I (8x20mm), 32p sTSOP (8x13.4mm), 36b TFBGA (6x8mm), 32p TSOP II (400mils)",55,"AS6C4008"]
["4Mb","512K x 8","2.7 ~ 5.5V","32p SOP (450mils)",70,"AS6C4008-70SAN"]
["4Mb","256K x 16","2.7 ~ 5.5V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm)",55,"AS6C4016"]
["8Mb","1M x 8","2.7 ~ 5.5V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm)",55,"AS6C8008"]
["8Mb","512K x 16","2.7 ~ 5.5V","44pin TSOP II (400mils), 48ball TFBGA (6x8mm) one chip select pins:B5**",55,"AS6C8016"]
["8Mb","512K x 16","2.7 ~ 3.6V","48pin TSOP I (12x20mm)",55,"AS6C8016-55TIN"]

{"sheet":"Low Power Asyn SRAM Cross Refer","index":21,"n_rows":74,"n_cols":11,"rows_kept":74,"cut":false,"hidden":false,"merged":[]}
[]
["Low Power Asynchronous SRAM Cross Reference"]
["64K"]
["ORG","VCC","PACKAGE","ALLIANCE","ZMD","CYPRESS (EOL)","HITACHI (EOL)","NEC (EOL)","HYNIX (EOL)"]
["8K x 8","2.7V ~ 5.5V","28pin 600mil DIP","AS6C6264-55PCN / PIN","U6264BDC07LLG1",null,"HM6264BLP",null,"HY6264P"]
["8K x 8","2.7V ~ 5.5V","28pin 330mil SOP","AS6C6264-55SCN / SIN","U6264BS2C07LLG1","CY6264-55SNXI","HM6264BLFP","uPD4464","HY6264G"]
["8K x 8","2.7V ~ 5.5V","28pin STSOP (8 x 13.4 mm)","AS6C6264-55STCN"]
["256K"]
["ORG","VCC","PACKAGE","ALLIANCE","ZMD","SAMSUNG (EOL)","CYPRESS (EOL)","RENESAS","BRILLIANCE (EOL)","ISSI"]
["32K x 8","2.7V ~ 5.5V","28pin 600mil DIP","AS6C62256-55PCN","U62256ADC07LLG1","K6X0808C1D-DF55","CY62256NLL-70PXC",null,"BS62LV256PCP-55"]
["32K x 8","2.7V ~ 5.5V","28pin 330mil SOP","AS6C62256-55SxN","U62256AS2C07LLG1","K6X0808C1D-BF55","CY62256NLL-55SNXI","R1LP5256ESP-5S","BS62LV256SCP-55","IS62C256AL-45ULI"]
["32K x 8","2.4V ~ 3.6V","28pin 330mil SOP","AS62V256-70SIN",null,null,"CY62256NVLL-70SNXI","R1LV5256ESP-5S","BS62LV256SCP-55","IS62LV256AL-45ULI"]
["32K x 8","2.7V ~ 5.5V","28pin STSOP (8 x 13.4 mm)","AS6C62256-55STxN",null,"K6X0808C1D-LF55","CY62256NLL-55ZRXI","R1LP5256ESA-5S","BS62LV256STCP-55","IS62LV256AL-45TLI"]
["1M"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","RENESAS","BRILLIANCE (EOL)","NEC (EOL)","ISSI"]
["128K x 8","2 .7V ~ 5.5V","32pin 600mil DIP","AS6C1008-55PCN / PIN","K6X1008C2D-DB55",null,null,null,"BS62LV1027PCP-55","uPD431000ACZ-70L"]
["128K x 8","2.7V ~ 5.5V","32pin 450mil SOP","AS6C1008-55SIN","K6X1008C2D-GF55(Lead)/BF","CY62128ELL-45SXI","M5M51008DFP-55HI","R1LP0108ESP-5SI","BS62LV1027SIP-55","uPD431000AGW-70L","IS62C1024AL-35QLI"]
["128K x 8","2.7V ~ 5.5V","32pin TSOP I (8 x 20 mm)","AS6C1008-55TIN","K6X1008C2D-TF55 or PF","CY62128ELL-45ZXI","M5M51008DVP-55HI","R1LP0108ESF-5SI","BS62LV1027TIP-55","uPD431000AGZ-70LL-KKH","IS62C1024AL-35TLI"]
["128K x 8","2.7V ~ 5.5V","32pin STSOP (8 x 13.4 mm)","AS6C1008-55STIN",null,"CY62128ELL-45ZAXI","M5M51008DKV-55HI","R1LP0108ESA-5SI","BS62LV1027STIP-55","uPD431000AGU-B10-9JH","IS62C1024AL-45HLI"]
["64K x 16","2.7V ~ 5.5V","48ball TFBGA","AS6C1016-55BIN","K6F1016U4C-EF55","CY62127DV30LL-55BVXI",null,null,"BS616LV1010AI-70",null,"IS62WV6416DBLL-45BLI"]
["64K x 16","2.7V ~ 5.5V","44pin TSOP II","AS6C1016-55ZIN",null,"CY62126EV30LL-45SXIT",null,null,"BS616LV1010EI-70",null,"IS62WV6416DBLL-45TLI"]
["64K x 16","2.7V ~3.6V","44pin TSOP II","AS6CE1016A-45ZIN",null,"CY62126EV30LL-45ZSXI",null,null,null,null,"IS61WV6416EEBLL"]
["2M"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["256K x 8","2.7V ~ 3.6V","32pin 450mil SOP","AS6C2008-55SIN",null,"CY62138FV30LL-45SXI",null,null,"BS62LV2006SIP-55"]
["256K x 8","2.7V ~ 3.6V","32pin TSOP I (8 x 20 mm)","AS6C2008-55TIN",null,"CY62138FV30LL-45ZXI",null,null,"BS62LV2006TIP-55","IS62WV2568BLL-55TLI"]
["256K x 8","2.7V ~ 3.6V","32pin STSOP (8 x 13.4 mm)","AS6C2008-55STIN","K6F2008V2E-LF70000","CY62138FV30LL-45ZAXI","M5M5V208AKV-55HI","R1LV0208BSA-5SI","BS62LV2006STIP-55","IS62WV2568BLL-55HLI"]
["256K x 8","2.7V ~ 3.6V","36ball TFBGA (6mm x 8mm)","AS6C2008-55BIN",null,"CY62138FV30LL-45BVXI",null,null,null,"IS62WV2568BLL-55B2LI"]
["128K x 16","2.7V ~ 5.5V","44pin TSOP II","AS6C2016-55ZIN",null,"CY62136FVLL-70ZSXI","M5M5V216ATP-70HI","R1LV0216-BSB-5SI","BS616LV2016EIP-55","IS62WV12816BLL-55TLI"]
["128K x 16","2.7V ~ 3.6V","48ball TFBGA","AS6C2016-55BIN","K6F2016U4E-EF55000","CY62136FVLL-70BVXI",null,null,"BS616LV2019AIG-55","IS62WV12816BLL-55B2LI"]
["256K x 8","2.7V ~ 5.5V","32pin 450mil SOP","AS6C2008A-55SIN",null,"CY2138FV30LL-45SXI",null,null,"BS62LV2006SIP-55"]
["256K x 8","2.7V ~ 5.5V","32pin TSOP I (8 x 20mm)","AS6C2008A-55TIN",null,"CY2138FV30LL-45ZXI",null,null,"BS62LV2006TIP-55","IS62WV256BLL-55TLI"]
["256K x 8","2.7V ~ 5.5V","36ball TFBGA (6mm x 8mm)","AS6C2008A-55BIN",null,"CY62138FV30LL-45BVXI",null,null,null,"IS62WV256BLL-55B2LI"]
["4M"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["512K x 8","2.7V ~ 5.5V","32pin 600mil DIP","AS6C4008-55PCN","K4X4008C1F-DB55",null,null,"BS62LV4006PCP-55"]
["512K x 8","2.7V ~ 5.5V","32pin 450mil SOP","AS6C4008-55SIN","K6X4008C1F-GF55 or BF","CY62148ELL-55SXI","R1LV0408CSP-5SI","BS62LV4006SIP-55","IS62C5128BLL-45QLI"]
["512K x 8","2.7V ~ 5.5V","32pin STSOP (8 x 13.4mm)","AS6C4008-55STIN",null,"CY62148ELL-55ZAXI","R1LV0408DSA-5SI","BS62LV4006STIP-55","IS62C512BL-45HLI"]
["512K x 8","2.7V ~ 5.5V","32pin TSOP II","AS6C4008-55ZIN","K6X4008C1F-VF55","CY62148ELL-45ZSXI","R1LV0408DSB-5SI","BS62LV4006ECP55","IS62WV5128DBLL-45T2LI"]
["512K x 8","2.7V ~ 5.5V","36pin TFBGA (6mm x 8mm)","AS6C4008-55BIN",null,"CY62148EV30LL-55BVXI","RILV0408DBG-5SI",null,"IS62WV5128EBLL-45BLI"]
["256K x 16","2.7V ~ 5.5V","44pin TSOP II","AS6C4016-55ZIN","K6X4016C3F-TF70000","CY62146ELL-45ZSXI",null,"BS616LV4017EIP-55","IS62WV5128BLL-55TLI"]
["256K x 16","2.7V ~ 3.6V","44pin TSOP II","AS6C4016B-45ZIN","K6X4016T3F-TF70000","CY62147EV30LL-45ZSXI","R1LV0414DSB-5SI","BS616LV4017EIP-55","IS62C25616BL-45T2LI"]
["256K x 16","2.7V ~ 3.6V","48ball  TFBGA","AS6C4016B-45BIN","K6F4016U6G-EF70000","CY62147EV30LL-45BVXI","RMLV0416EGBG-4S2","BS616LV4017AIP-55","IS62WV25616DBLL-45BLI"]
["256K x 16","2.7V ~ 3.6V","44pin TSOP II","AS6CE4016B-45ZIN","K6X4016T3F-TF70000","CY62147EV30LL-45ZSXI","R1LV0414DSB-5SI","BS616LV4017EIP-55","IS62C25616EDBLL"]
["256K x 16","2.7V ~ 3.6V","48ball  TFBGA","AS6CE4016B-45BIN","K6F4016U6G-EF70000","CY62147EV30LL-45BVXI","RMLV0416EGBG-4S2","BS616LV4017AIP-55","IS62C25616EDFA/BLL"]
["8M"]
["ORG","VCC","PACKAGE","ALLIANCE","SAMSUNG (EOL)","CYPRESS","RENESAS","RENESAS","RENESAS","BRILLIANCE","ISSI"]
["1M x 8","2.7 ~ 5.5V","44pin TSOP II","AS6C8008-55ZIN","K6X8008(C/T)2B-UF55","CY62158EV30LL-45ZSXI",null,"R1LV0808ASB-5SI","HM62V8100LTTI-5SL","BS62LV8001ECP-55","IS62WV1024BLL-55TLI"]
["1M x 8","2.7 ~ 5.5V","44pin TSOP II","AS6C8008B-45/55ZIN","K6X8008(C/T)2B-UF55","CY62158EV30LL-45ZSXI",null,"R1LV0808ASB-5SI","HM62V8100LTTI-5SL","BS62LV8001ECP-55","IS62WV1024BLL-55TLI"]
["1M x 8","2.7 ~ 5.5V","48ball TFBGA","AS6C8008-55BIN",null,"CY62158EV30LL-45BVXI","EOL",null,"HM62V8100LBPI-5SL","BS62LV8001ECP-55","IS62WV1024BLL-55MLI"]
["1M x 8","2.7 ~ 3.6V","48ball TFBGA","AS6C8008B-45BIN",null,"CY62158EV30LL-45BVXI","EOL",null,"HM62V8100LBPI-5SL","BS62LV8001FIP-55","IS62WV1024BLL-55MLI"]
["512K x 16","2.7 ~ 5.5V","48ball TFBGA (6 x 8mm)*","AS6C8016-55BIN*","K6F8016U6G-FF55","CY62157EV30LL-55BVXI","M5M5W816WG-55HI","R1LV0816ABG-5SI",null,"BS616LV8017ECP55","IS62WV51216BLL-55BLI"]
["512K x 16","2.7 ~3.6V","48ball TFBGA (6 x 8mm)**","AS6C8016B-45/55BIN",null,"CY2157EV30LL-45BVXIT"]
["512K x 16","2.7 ~ 5.5V","44pin TSOP II","AS6C8016 -55ZIN","K6X8016(C/T)3B-UF55","CY62157EV30LL-55ZSXI","M5M5W816TP-55HI","R1LV0816ASA-5SI","HM62165I14LTT-5SL","BS616LV8017FCP70","IS62WV51216BLL-55T2LI"]
["512K x 16","2.7 ~3.6V","44pin TSOP II","AS6C8016B-45/55ZIN",null,"CY62157EV30LL-45ZSXIT",null,null,null,null,"IS62WV51216BLL-55T2LI"]
["512K x 16","2.7 ~ 5.5V","48pin TSOP I","AS6C8016-55TIN",null,"CY62157EV30LL-45ZXIT",null,null,null,null,"IS62WV51216GBLL-45TLI"]
["* = one chip select pin:B5 ** = two chip select pins: B5 and A6"]
["16M"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS","BRILLIANCE (EOL)","ISSI"]
["1M x 16","2.7 ~ 3.6V","48pin TSOP I","AS6C1616-55TIN\nAS6C1616B-45/55TIN","CY62167E30LL-45/55ZXI","R1LV1616RSA-5SI","BS6216LV1611TCP55","IS62WV102416xxLL"]
["1M x 16","2.7 ~ 3.6V","48pin TSOP I","AS6C1616C-45TIN","CY62167E30LL-45/55ZXI","R1LV1616RSA-5SI","BS6216LV1611TCP55","IS62WV102416xxLL"]
["1M x 16","2.7 ~ 3.6V","48ball TFBGA","AS6C1616B-45/55BIN","CY62167DV30LL-xxBVXIT","R1LV1616HBG-4SI","BS6216LV1611FCP70","IS62WV102416xxLL-xxBLI"]
["2M x 8","2.7 ~ 3.6V","44pin TSOP I","AS6C1608B-45TIN","CY62168EV30LL-xxZXI",null,"BS6216LV1600EIP55","IS62WV20488xxLL-xxTLI"]
["2M x 8","2.7 ~ 3.6V","48ball TFBGA","AS6C1608B-45BIN","CY62168DV30LL-xxBVI",null,null,"IS62WV20488xxLL-xxBLI"]
["32M"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS"]
["2M x 16","2.7 ~ 3.6V","48pin TSOP I","AS6C3216A-55TIN*","CY62177EV30LL-55ZXI","R1LV3216RSA-5SI"]
["2M x 16","2.7 ~ 3.6V","48ball TFBGA","AS6C3216A-55BIN","CY62177EV30LL-55BAXI","R1LV3216CSA-5SI"]
["*48pin TSOP I (please note: dual chip select 2Mx16 or 4Mx8)"]
["64M"]
["ORG","VCC","PACKAGE","ALLIANCE","CYPRESS","RENESAS"]
["4M x 16","2.7V ~ 3.6V","48pin TSOP I","AS6C6416-55TIN",null,"R1WV6416RSA-5S"]
["4M x 16","2.7V ~ 3.6V","48ball BGA","AS6C6416-55BIN","CY62187EV30LL-55BAXI","R1WV6416RBG-5S"]
["*48pin TSOP I (please note: dual chip select 4Mx16 or 8Mx8)"]

{"sheet":"Parallel 5V NOR Flash","index":22,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[]
["Parallel 5V NOR Flash"]
["DENSITY","BUS WIDTH","VCC","PACKAGES","TEMPERATURE RANGE","SPEED (NS)","ALLIANCE PART#","REMARKS"]
["1Mb","x8","5V","PLCC 32","-40°C to 85°C",55,"AS29CF010-55CCIN","Uniform Sector, Industrial Grade"]
["4Mb","x8","5V","PLCC 32","-40°C to 85°C",55,"AS29CF040-55CCIN","Uniform Sector, Industrial Grade"]
["4Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 85°C",55,"M29F400FT5AN6E2","Top Boot, Automotive Grade3"]
["4Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 125°C",55,"M29F400FB55N3E2 \nM29F400FB55N3F2","Bottom Boot, Automotive Grade1"]
["8Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 85°C",55,"AS29CF800T-55TIN","Top Boot, Industrial Grade"]
["8Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 85°C",55,"AS29CF800B-55TIN","Bottom Boot, Industrial Grade"]
["8Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 85°C",55,"M29F800FB5AN6E2 \nM29F800FB5AN6F2","Bottom Boot, Automotive Grade3"]
["8Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 125°C",55,"M29F800FT55N3E2","Top Boot, Automotive Grade1"]
["16Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 85°C",55,"AS29CF160B-55TIN","Bottom Boot, Industrial Grade"]
["16Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 85°C",55,"AS29CF160T-55TIN","Top Boot, Industrial Grade"]
["16Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 85°C",55,"M29F160FB5AN6F2","Bottom Boot, Automotive Grade3"]
["16Mb","x8 , x16","5V","TSOP(I) 48pin","-40°C to 125°C",55,"M29F160FT55N3E2","Top Boot, Automotive Grade1"]

{"sheet":"Parallel 5V NOR Falsh Cross Ref","index":23,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[]
["Parallel 5V NOR Flash Cross Reference"]
["DENSITY","VCC","PACKAGE","SPEED (NS)","ALLIANCE","MICRON","CYPRESS/SPANSION","MACRONIX"]
["1Mb","5V","PLCC 32",55,"AS29CF010-55CCIN",null,"AM29F010B* (EOL)"]
["4Mb","5V","PLCC 32",55,"AS29CF040-55CCIN","M29F040","AM29F040B","MX29F040C"]
["4Mb","5V","TSOP 48pin",55,"M29F400FB55N3E2 \nM29F400FB55N3F2","M29F400F","AM29F400BB* (EOL)","MX29F400CBT"]
["4Mb","5V","TSOP 48pin",55,"M29F400FT5AN6E2","M29F400F","AM29F400BT* (EOL)","MX29F400CTT"]
["8Mb","5V","TSOP 48pin",55,"AS29CF800T-55TIN","M29F800F","AM29F800BT* (EOL)","MX29F800C T/B"]
["8Mb","5V","TSOP 48pin",55,"AS29CF800B-55TIN","M29F800F","AM29F800BB* (EOL)","MX29F800C T/B"]
["8Mb","5V","TSOP 48pin",55,"M29F800FB5AN6E2\nM29F800FB5AN6F2","M29F800F","AM29F800BB* (EOL)","MX29F800CBT"]
["8Mb","5V","TSOP 48pin",55,"M29F800FT55N3E2","M29F800F","AM29F800BT* (EOL)","MX29F800CTT"]
["16Mb","5V","TSOP 48pin",55,"AS29CF160T-55TIN","M29F160F","AM29F160DT* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"AS29CF160B-55TIN","M29F160F","AM29F160DB* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"M29F160FB5AN6F2","M29F160F","AM29F160DB* (EOL)"]
["16Mb","5V","TSOP 48pin",55,"M29F160FT55N3E2","M29F160F","AM29F160DT* (EOL)"]

{"sheet":"SLC Parallel NAND Flash","index":24,"n_rows":11,"n_cols":8,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
[]
["SLC Parallel NAND Flash"]
["DENSITY","BUS WIDTH","VCC","PACKAGES","TEMPERATURE RANGE","SPEED (NS)","ALLIANCE","REMARKS"]
["1Gb","x8","3.3V","63b FBGA\n(9x11mm)","Industrial\n(-40°C to 85°C)","25ns","AS9F31G08SA-25BIN","4bit ECC, 2K page, 64B Spare"]
["2Gb","x8","3.3V","63b FBGA\n(9x11mm)","Industrial\n(-40°C to 85°C)","25ns","AS9F32G08SA-25BIN","4bit ECC, 2K page, 128B Spare"]
["4Gb","x8","3.3V","63b FBGA\n(9x11mm)","Industrial\n(-40°C to 85°C)","25ns","AS9F34G08SA-25BIN","4bit ECC, 2K page, 128B Spare"]
["8Gb","x8","3.3V","63b FBGA\n(9x11mm)","Industrial\n(-40°C to 85°C)","25ns","AS9F38G08SA-25BIN","4bit ECC, 2K page, 128B Spare"]
["4Gb","x8","1.8V","63b FBGA\n(9x11mm)","Industrial\n(-40°C to 85°C)","45ns","AS9F14G08SA-45BIN","4bit ECC, 2K page, 128B Spare"]
["8Gb","x8","1.8V","63b FBGA\n(9x11mm)","Industrial\n(-40°C to 85°C)","45ns","AS9F18G08SA-45BIN","4bit ECC, 2K page, 128B Spare, DDP"]
["4Gb","x8","1.8V","63b FBGA\n(9x11mm)","Automotive Grade2\n(-40°C to 105°C)","45ns","AS9F14G08SA-45BAN","4bit ECC, 2K page, 64B Spare"]
["8Gb","x8","1.8V","63b FBGA\n(9x11mm)","Automotive Grade2\n(-40°C to 105°C)","45ns","AS9F18G08SA-45BAN","4bit ECC, 2K page, 128B Spare, DDP"]

{"sheet":"SLC Parallel NAND Flash.Cross R","index":25,"n_rows":11,"n_cols":15,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
[]
["SLC Parallel NAND Flash Cross Reference"]
["DENSITY","VCC","BUS WIDTH","PACKAGE","TEMPERATURE","ALLIANCE","MICRON","SKY HIGH","CYPRESS","WINBOND","MACRONIX","KIOXIA","ISSI","GIGA DEVICES","ESMT"]
["1Gb","3.3V","x8","63b FBGA","-40°C to 85°C","AS9F31G08SA-25BIN","MT29F1G08ABADAH4\nMT29F1G08ABAEAH4","S34SL01G200BFI\nS34ML01G200BFI\nS34ML01G300BFI","S34ML01G100BFI","W29N01HV\nW29N01GV","MX30LF1G18AC","TC58NVG0S3HBA","IS34ML01G084","GD9FU1G8F3AL","F59L1G81MB"]
["2Gb","3.3V","x8","63b FBGA","-40°C to 85°C","AS9F32G08SA-25BIN","MT29F2G08ABAEAH4\nMT29F2G08ABAGAH4","S34SL02G200BFI\nS34ML02G200BFI\nS34ML02G300BFI","S34ML02G100BFI","W29N02GV\nW29N02KV","MX30LF2G18AC","TC58NVG1S3HBA","IS34ML02G084","GD9FU2G8F2AL","F59L2G81A\nF59L2G81KA"]
["4Gb","3.3V","x8","63b FBGA","-40°C to 85°C","AS9F34G08SA-25BIN","MT29F4G08ABADAH4\nMT29F4G08ABAEAH4\nMT29F4G08ABAFAH4","S34SL04G200BFI\nS34ML04G200BFI","S34ML04G100BFI","W29N04GV","MX30LF4G18AC","TC58NVG2S0HBA","IS34ML04G084","GD9FU4G8F2AL","F59L4G81XB"]
["8Gb","3.3V","x8","63b FBGA","-40°C to 85°C","AS9F38G08SA-25BIN","MT29F8G08ADACAH4","S34ML08G201BFI","S34ML08G101BFI","W29N08GV","MX60LF8G18AC","TH58NVG3S0HBA","IS34ML08G088\nIS34ML08G168","GD9FU8G8E2AL","F59D4G81XB\nF59D4G-81KA"]
["4Gb","1.8V","x8","63b FBGA","-40°C to 85°C","AS9F14G08SA-45BIN","MT29F4G08ABBDAH4\nMT29F4G08ABBEAH4\nMT29F4G08ABBFAH4","S34MS04G200BFI","S34MS04G100BFI","W29N04GZ\nW29N04GW","MX30UF4G18AC","TC58NYG2S0HBA","IS34MW04G164","GD9FS4G8F2AL","F59D8G81XB"]
["8Gb","1.8V","x8","63b FBGA","-40°C to 85°C","AS9F18G08SA-45BIN","MT29F8G08ADBCAH4\nMT29F8G08ADBDAH4\nMT29F8G08ABBCAH4\nMT29F8G08ABBDAH4","S34MS08G201BFI","S34MS08G101BFI","W29N08GW\nW29N08GZ","MX60UF8G18AC","TH58NYG3S0HBA","IS34MW08G088\nIS34MW08G168","GD9FS8G8E2AL"]
["4Gb","1.8V","x8","63b FBGA","-40°C to 105°C","AS9F14G08SA-45BAN","MT29F4G08ABBDAH4-A\nMT29F4G08ABBEAH4-A","S34MS04G200BFI","S34MS04G100BFV","W29N04GZ\nW29N04GW",null,null,"IS35MW04G084","GD9FS4G8F2AL"]
["8Gb","1.8V","x8","63b FBGA","-40°C to 105°C","AS9F18G08SA-45BAN","MT29F8G08ADBDAH4-A","S34MS08G201BFA","S34MS08G101BFA","W29N08GW\nW29N08GZ",null,null,null,"GD9FS8G8E2AL"]

{"sheet":"Serial NOR Flash","index":26,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
[]
["Serial NOR Flash"]
["DENSITY","BUS WIDTH","VCC","PACKAGES","TEMPERATURE RANGE","SPEED (MHz)","ALLIANCE","REMARKS"]
["2Mb","x1","3.3V","8pin SOIC (150mils)","-40°C to 85°C",75,"M45PE20-VMN6P","PAGE ERASABLE, 2Mb Serial Flash (256K x 8bits, 1024 pages, 4 Sectors), Industrial Grade"]
["8Mb","x1","3.3V","8pin DFN (6x5mm)","-40°C to 85°C",75,"M45PE80-VMP6TG","PAGE ERASABLE 8Mb Serial Flash (1K x 8bits, 4096 pages, 16 Sectors), Industrial Grade, T&R"]
["16Mb","x1","3.3V","8pin SOIC (208mils)","-40°C to 85°C",75,"M45PE16-VMW6TG","PAGE ERASABLE, 16Mb Serial Flash (2K x 8bits, 8192 pages, 32 Sectors), Industrial Grade"]
["4Mb","x1, x2","3.3V","8pin SOIC (150mils)","-40°C to 85°C",104,"AS25F34MD-10S1IN","4Mb, 3.3V Serial NOR Flash, Dual IO, Industrial Grade, 8pin SOIC (150mils) package"]
["16Mb","x1, x2, x4","3.3V","8pin SOIC (150mils)","-40°C to 85°C",104,"AS25F316MQ-10S1IN","16Mb, 3.3V Serial NOR Flash, Multiple IO, Industrial Grade, 8pin SOIC (150mils) Package"]
["32Mb","x1, x2, x4","3.3V","8pin DFN (4x3mm)","-40°C to 125°C",108,"N25Q032A13EF4A0F","32Mb Serial NOR Flash, Multiple IO, 64 Sectors, 4KB Sector Erase, Automotive Grade T&R"]
["32Mb","x1, x2, x4","3.3V","8pin SOIC (150mils)","-40°C to 85°C",108,"N25Q032A13ESC40F","32Mb Serial NOR Flash, Multiple IO, 64 Sectors, 4KB Sector Erase, Industrial Grade, T&R"]
["32Mb","x1, x2, x4","3.3V","8pin SOIC (150mils)","-40°C to 85°C",108,"N25Q032A13ESC40G","32Mb Serial NOR Flash, Multiple IO, 64 Sectors, 4KB Sector Erase, Industrial Grade, Tube"]
["32Mb","x1, x2, x4","3.3V","8pin SOIC (150mils)","-40°C to 125°C",108,"N25Q032A13ESCA0F","32Mb Serial NOR Flash, Multiple IO, 64 Sectors, 4KB Sector Erase, Automotive Grade, T&R"]
["32Mb","x1, x2, x4","3.3V","16pin SOIC (300mils)","-40°C to 125°C",108,"N25Q032A13ESFA0F","32Mb Serial NOR Flash, Multiple IO, 64 Sectors, 4KB Sector Erase, Automotive Grade, T&R"]
["64Mb","x1, x2, x4","1.8V","8pin SOIC (208mils)","-40°C to 125°C",108,"N25Q064A11ESEA0F","64Mb Serial NOR Flash, Multiple IO, 128 Sectors, 4KB Sector Erase, Automotive Grade T&R"]
["64Mb","x1, x2, x4","3.3V","8pin DFN (6x5mm)","-40°C to 85°C",108,"N25Q064A13EF640E","64Mb Serial NOR Flash, Multiple IO, 128 Sectors, 4KB Sector Erase, Industrial Grade, Tray"]
["64Mb","x1, x2, x4","3.3V","8pin DFN (8x6mm)","-40°C to 125°C",108,"N25Q064A13EF8A0E","64Mb Serial NOR Flash, Multiple IO, 128 Sectors,  4KB Sector Erase, Automotive Grade Tray"]
["64Mb","x1, x2, x4","3.3V","8pin DFN (8x6mm)","-40°C to 125°C",108,"N25Q064A13EF8A0F","64Mb Serial NOR Flash, Multiple IO, 128 Sectors, 4KB Sector Erase, Automotive Grade T&R"]
["64Mb","x1, x2, x4","3.3V","8pin DFN (8x6mm)","-40°C to 85°C*",108,"N25Q064A13EF8H0E","64Mb Serial NOR Flash, Multiple IO, 128 Sectors, 4KB Sector Erase, Industrial Grade High Reliability, Tray"]
["64Mb","x1, x2, x4","3.3V","16pin SOIC (300mils)","-40°C to 125°C",108,"N25Q064A13ESFA0F","64Mb Serial NOR Flash, Multiple IO, 128 Sectors, 4KB Sector Erase, Automotive Grade T&R"]
["64Mb","x1, x2, x4","3.3V","8pin SOIC (208mils)","-40°C to 85°C",104,"AS25F364MQ-10SIN","64Mb, 3.3V Serial NOR Flash, Multiple IO, Default Feature1, Industrial Grade, 8SOIC Wide Body Package"]
["64Mb","x1, x2, x4","3.3V","8L WSON (6x5mm)","-40°C to 85°C",104,"AS25F364MQ-10WIN","64Mb, 3.3V Serial NOR Flash, Multiple IO, Default Feature1, Industrial Grade, 8WSON Package"]
["128Mb","x1, x2, x4","1.8V","8pin SOIC (208mils)","-40°C to 85°C",133,"AS25F128MQ-70SIN","128Mb, 1.8V Serial NOR Flash, Multiple IO, Default Feature1, Industrial Grade, 8SOIC Wide Body Package"]
["128Mb","x1, x2, x4","1.8V","8L WSON (6x5mm)","-40°C to 85°C",133,"AS25F128MQ-70WIN","128Mb, 1.8V Serial NOR Flash, Multiple IO, Default Feature1, Industrial Grade, 8WSON Package"]

{"sheet":"Serial NOR Flash Cross Ref","index":27,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[]}
[]
["Serial NOR Flash Cross Reference"]
["DENSITY","VCC","PACKAGES","ALLIANCE","MICRON","ADESTO","SPANSION","WINBOND","MACRONIX","ISSI","GIGA DEVICES"]
["2Mb","3.3V","8pin SOIC (150mils)","M45PE20-VMN6P","M45PE20-VMN6","AT45DB021E"]
["8Mb","3.3V","8pin DFN (6x5mm)","M45PE80-VMP6G","M45PE80-VMP6","AT45DB081E"]
["8Mb","3.3V","8pin DFN (6x5mm)","M45PE80-VMP6TG","M45PE80-VMP6","AT45DB081E"]
["16Mb","3.3V","8pin SOIC (208mils)","M45PE16-VMW6TG","M45PE16-VMW6","AT45DB161E"]
["4Mb","3.3V","8pin SOIC (150mils)","AS25F34MD-10S1IN","M25P40-AVMN6","AT25SF041","S25FL040","W25Q40","MX25L40\nMX25V40","IS25LP040\nIS25LQ040","GD25Q40\nGD25B40\nGD25D40"]
["16Mb","3.3V","8pin SOIC (150mils)","AS25F316MQ-10S1IN","M25P16-AVMN6\nM25PX16","AT25SF161\nAT25FF161","S25FL016","W25Q16","MX25L16\nMX25V16","IS25LP016\nIS25LQ016","GD25Q16\nGD25B16"]
["32Mb","3.3V","8pin DFN (4x3mm)","N25Q032A13EF440F","N25Q032A13EF4","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3.3V","8pin DFN (4x3mm)","N25Q032A13EF4A0F","N25Q032A13EF4","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3.3V","8pin DFN (6x5mm)","N25Q032A13EF640F","N25Q032A13EF6","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3.3V","8pin SOIC (150mils)","N25Q032A13ESC40F","N25Q032A13ESC","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3.3V","8pin SOIC (150mils)","N25Q032A13ESC40G","N25Q032A13ESC","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3.3V","8pin SOIC (150mils)","N25Q032A13ESCA0F","N25Q032A13ESC","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["32Mb","3.3V","16pin SOIC (300mils)","N25Q032A13ESFA0F","N25Q032A13ESF","AT25DF32/AT25SF32","S25FL032A/P","W25Q32","MX25L32","IS25LP032 / IS25LQ032","GD25Q32"]
["64Mb","1.8V","8pin SOIC (208mils)","N25Q064A11ESEA0F","N25Q064A11ESE","AT25SL64/AT25QL64",null,"W25Q64","MX25U64","IS25WP064","GD25LQ64"]
["64Mb","3.3V","8pin DFN (6x5mm)","N25Q064A13EF640E","N25Q064A13EF6","AT25SF64/AT25QF64","S25FL064A/P","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","8pin DFN (8x6mm)","N25Q064A13EF8A0E","N25Q064A13EF8","AT25SF64/AT25QF64","S25FL064A/P","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","8pin DFN (8x6mm)","N25Q064A13EF8A0F","N25Q064A13EF8","AT25SF64/AT25QF64","S25FL064A/P","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","8pin DFN (8x6mm)","N25Q064A13EF8H0E","N25Q064A13EF8","AT25SF64/AT25QF64","S25FL064A/P","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","16pin SOIC (300mils)","N25Q064A13ESFA0F","N25Q064A13ESF","AT25SF64/AT25QF64","S25FL064A/P","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","8pin SOIC (208mils)","AS25F364MQ-10SIN","N25Q064A13ESE","AT25QF64","S25FL064","W25Q64","MX25L64","IS25LP064","GD25Q64"]
["64Mb","3.3V","8L WSON (6x5mm)","AS25F364MQ-10WIN","N25Q064A13EF6","AT25QF64","S25FL064","W25Q64","MX25L64","IS25L064","GD25Q64"]
["128Mb","1.8V","8pin SOIC (208mils)","AS25F1128MQ-70SIN","MT25QU128ABA1ESE","AT25SL128A-SUE","S25FS128SDSMFI","W25Q128JWSIM","MX25U12832FM2I","IS25WP128-JBLE","GD25LB128ESIG"]
["128Mb","1.8V","8L WSON (6x5mm)","AS25F1128MQ-70WIN","MT25QU128ABA1EW7","AT25SL128A-MHE","S25FS128SDSNFI","W25Q128JWPIM","MX25U12832FZNI","IS25WP128-JKLE","GD25LB128EWIG"]

{"sheet":"Serial NAND Flash","index":28,"n_rows":12,"n_cols":8,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
[]
["Serial NAND Flash"]
["DENSITY","BUS WIDTH","SPEED (NS)","VCC","PACKAGES","TEMPERTURE RANGE","TYPE","ALLIANCE PART#"]
["1Gb","x1, x2, x4","120 Mhz","3.3V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","4bit ECC, (2048 + 64) bytes × 64 pages × 1024 blocks","AS5F31G04SND-08LIN"]
["2Gb","x1, x2, x4","100 Mhz","1.8V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","8bit ECC, (2048 + 128) bytes × 64 pages × 2048 blocks","AS5F12G04SND-10LIN"]
["2Gb","x1, x2, x4","120 Mhz","3.3V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","8bit ECC, (2048 + 128) bytes × 64 pages × 2048 blocks","AS5F32G04SNDA-08LIN"]
["2Gb","x1, x2, x4","120 Mhz","3.3V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","4bit ECC, (2048 + 128) bytes × 64 pages × 2048 blocks","AS5F32G04SNDB-08LIN"]
["4Gb","x1, x2, x4","100 Mhz","1.8V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","8bit ECC, (2048 + 128) bytes × 64 pages × 4096 blocks","AS5F14G04SND-10LIN"]
["4Gb","x1, x2, x4","120 Mhz","3.3V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","8bit ECC, (2048 + 128) bytes × 64 pages × 4096 blocks","AS5F34G04SNDA-08LIN"]
["4Gb","x1, x2, x4","120 Mhz","3.3V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","4bit ECC, (2048 + 128) bytes × 64 pages × 4096 blocks","AS5F34G04SNDB-08LIN"]
["8Gb","x1, x2, x4","100 Mhz","1.8V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","8bit ECC, (4096 + 256) bytes × 64 pages × 4096 blocks","AS5F18G04SND-10LIN"]
["8Gb","x1, x2, x4","120 Mhz","3.3V","8pin LGA (8x6mm)","Industrial (-40°C to 85°C)","8bit ECC, (4096 + 256) bytes × 64 pages × 4096 blocks","AS5F38G04SND-08LIN"]

{"sheet":"Serial NAND Flash Cross Ref","index":29,"n_rows":10,"n_cols":10,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
[]
["Serial NAND Flash Cross Reference"]
["DENSITY","SPEED (NS)","VCC","ALLIANCE","MICRON","TOSHIBA/KIOXIA","WINBOND","MACRONIX","GIGA DEVICES","ISSI"]
["1Gb","120Mhz","3V","AS5F31G04SND-08LIN","MT29F1G01ABAFDWB-IT","TC58CVG0S3HRAIJ","W25N01GV\nW25N01KV","MX35LF1GE4AB\nMX35LF1G24AD","GD5F1GQ4Ux\nGD5F1GQ5Ux\nGD5F1GM7Ux","IS37SML01G1-LLI\nIS37SML01G8A-JJLI"]
["2Gb","100Mhz","1.8V","AS5F12G04SND-10LIN","MT29F2G01ABBGDWB-IT:G","TC58CYG1S3HRAIJ","W25N02JW\nW25M02GW","MX35UF2G14AC\nMX35UF2G24AD\nMX35UF2GE4AC\nMX35UF2GE4AD","GD5F2GQ4Rx\nGD5F2GQ5Rx\nGD5F2GM7Rx","IS37SMW02G8A-JJLI"]
["2Gb","120Mhz","3V","AS5F32G04SNDA-08LIN AS5F32G04SNDB-08LIN","MT29F2G01ABAGDWB-IT","TC58CVG1S3HRAIJ","W25M02GV","MX35LF2G14AC\nMX35LF2GE4AD\nMX35LF2G24AD","GD5F2GQ4Ux\nGD5F2GQ5Ux\nGD5F2GM7Ux","IS37SML02G8A-JJLI"]
["4Gb","100Mhz","1.8V","AS5F14G04SND-10LIN","MT29F4G01ABBFDWB-IT","TC58CYG2S0HRAIJ","W25N04KW","MX35UF4G24AD\nMX35UF4GE4AD","GD5F4GQ6Rx\nGD5F4GM8Rx","IS37SMW04G8A-JJLI"]
["4Gb","120Mhz","3V","AS5F34G04SNDA-08LIN AS5F34G04SNDB-08LIN","MT29F4G01ABAFDWB","TC58CVG2S0HRAIJ","W25N04KV","MX35LF4G24AD\nMX35LF4GE4AD","GD5F4GQ6Ux\nGD5F4GM8Ux","IS37SML04G8A-JJLI"]
["8Gb","100Mhz","1.8V","AS5F18G04SND-10LIN",null,"TH58CYG3S0HRAIJ",null,null,null,"IS37SMW08G8A-JJLI"]
["8Gb","120Mhz","3V","AS5F38G04SND-08LIN",null,"TH58CVG3S0HRAIJ",null,null,null,"IS37SML08G8A-JJLI"]

{"sheet":"eMMC","index":30,"n_rows":9,"n_cols":10,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
[]
["eMMC"]
["DENSITY","VCC","VCCQ","BUS WIDTH","MMC INTERFACE","CLOCK FREQUENCY","PACKAGE","NAND TYPE","TEMPERATURE","ALLIANCE"]
["4GB","2.7V~3.6V","1.8V / 3.3V ","x1 , x4 , x8","v5.1","200 MHz","153b FBGA (11.5x13mm)","MLC","Industrial (-40°C to 85°C)","ASFC4G31M-51BIN"]
["8GB","2.7V~3.6V","1.8V / 3.3V ","x1 , x4 , x8","v5.1","200 MHz","153b FBGA (11.5x13mm)","MLC","Industrial (-40°C to 85°C)","ASFC8G31M-51BIN"]
["16GB","2.7V~3.6V","1.8V / 3.3V ","x1 , x4 , x8","v5.1","200 MHz","153b FBGA (11.5x13mm)","MLC","Industrial (-40°C to 85°C)","ASFC16G31M-51BIN"]
["32GB","2.7V~3.6V","1.8V / 3.3V ","x1 , x4 , x8","v5.1","200 MHz","153b FBGA (11.5x13mm)","TLC","Industrial (-40°C to 85°C)","ASFC32G31T3-51BIN"]
["64GB","2.7V~3.6V","1.8V / 3.3V ","x1 , x4 , x8","v5.1","200 MHz","153b FBGA (11.5x13mm)","TLC","Industrial (-40°C to 85°C)","ASFC64G31T5-51BIN"]
["128GB","2.7V~3.6V","1.8V / 3.3V ","x1 , x4 , x8","v5.1","200 MHz","153b FBGA (11.5x13mm)","TLC","Industrial (-40°C to 85°C)","ASFC128G32T5-51BIN"]

{"sheet":"eMMC Cross Reference","index":31,"n_rows":9,"n_cols":13,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
[]
["eMMC Cross Reference"]
["DENSITY","PACKAGETYPE","TEMP GRADE","ALLIANCE","MICRON","SAMSUNG","KINGSTON","KIOXIA","ISSI","SANDISK","SK HYNIX","MACRONIX","SKY-HIGH"]
["4GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC4G31M-51BIN","MTFC4GACAJCN\nMTFC4GMWDM","KLM4G1GXXX","EMMC04GMK27\nEMMC04GM627\nEMMC04G-W627","THGBMNG5D1LBA","IS21ES04G-JCLI\nIS21ES04G-BCLI","X","H26M31001HPR","MX52LM04A11X","S40FC004C1B"]
["8GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC8G31M-51BIN","MTFC8GACAENS\nMTFC8GAKAJCN\nMTFC8GAMALBH\nMTFC8GAMALGT\nMTFC8GLWDM","KLM8G1GEUF\nKLM8G1GESD\nKLM8G1GETF","EMMC08GML36","THGBMJG6C1LBA","IS21ES08GA-JCLI\nIS21ES08GA-BCLI","SDINBDG4-8G","H26M41208HPR","MX52LM08A11X","S40FC008C3B"]
["16GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC16G31M-51BIN","MTFC16GAKAECN\nMTFC16GAKAEJP\nMTFC16GAPALBH","KLMAG1JETD\nKLMAG2GESD\nKLMAG2GEUF","EMMC16G-TB29\nEMMC16G-IB29","THGBMUG7C1LBA\nTHGAMVG7T13BA","IS21TF16G-JCLI\nIS21TF16G-BCLI","SDINBDA6-16G","H26M51002KPR","X","S40FC016C3B"]
["32GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC32G31T3-51BIN","MTFC32GAKAECN\nMTFC32GAKAEJP\nMTFC32GAZAQHD\nMTFC32GAPALBH","KLMBG2JETD\nKLMBG4GESD","EMMC32G-TX29\nEMMC32G-IX29","THGBMUG8C2LBA\nTHGAMVG8T13BA\nTHGBMJG88C4LBA","IS21TF32G-JCLI\nIS21TF32G-BCLI","SDINBDA6-32G\nSDINBDG4-32G","H26M62002JPR\nH26M64208EM","X","X"]
["64GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC64G31T5-51BIN","MTFC64GAZAQHD\nMTFC64GAPALBH","KLMCG2KCTA\nKLMCG2UCTA\nKLMCG2UCTB\nKLMCG4JEUD\nKLMCG8GESD","EMMC64G-TY29\nEMMC64G-IY29","THGAMVG9T23BA\nTHGBMJG9C8LBA","IS21TF64G-JCLI\nIS21TF64G-BCLI","SDINBDA6-64G\nSDINBDG4-64G","H26M74002HMR\nH26M78208CMR","X","X"]
["128GB","153ball FBGA\n(11.5x13mm)","Industrial Grade\n(-40C to 85C)","ASFC128G32T5-51BIN","MTFC128GAPALNS\nMTFC128GAZAQJP","KLMDG4UCTA\nKLMDG4UCTB\nKLMDG8JEUD","EMMC128-TY29\nEMMC128-IY29","THGAMVT0T43BA","IS21TF128G-JCLI\nIS21TF128G-BCLI","SDINBDA6-128G","X","X","X"]

{"sheet":"Alliance Packaging Quantities","index":32,"n_rows":100,"n_cols":8,"rows_kept":100,"cut":false,"hidden":false,"merged":[[61,0,61,4],[66,0,66,4],[72,0,72,4]]}
[]
[]
["FAST SRAM ORDER QTY"]
["PART #","PACKAGESUFFIX","PACKAGE","BOX QTY","QUANTITY PER TRAY/TUBE","REEL SIZE","TAPE WIDTH (mm)","TAPE PITCH (mm)"]
["164A, 256A, 3256A","JxN","28 SOJ - 300mil",2500,"25/Tube",1000,24,12]
["256B","JIN","28 SOJ - 300mil",1080,"27/Tube",1000,24,12]
["3256B","JIN","28 SOJ - 300mil",1352,"26/Tube",1000,24,12]
["256A, 3256A","TxN","28 TSOP I (8x13.4)",2340,"234/Tray",1000,24,12]
["1025B, 31025B, 1024B, 31024B","TJCN","32.3 SOJ - 300mil",2200,"22/Tube",1000,32,12]
["1024C","TJIN","32.3 SOJ - 300mil",920,"23/Tube",1000,32,12]
["31025C","TJIN","32.3 SOJ - 300mil",805,"23/Tube",1000,32,12]
["1025B, 31025B, 1024B, 31024B","JCN","32.4 SOJ - 400mil",2100,"21/Tube",1000,32,16]
["1024C, 1025C, 31025C","JIN","32.4 SOJ - 400mil",805,"23/Tube",1000,32,16]
["513B, 3513B, 1026B, 31026B","JCN","44 SOJ - 400mil - 1 Meg",1600,"16/Tube",500,44,16]
["1026C, 31026C","JIN","44 SOJ - 400mil - 1 Meg",560,"16/Tube",500,44,16]
["1024B, 31024B","TCN","32 TSOP I (8x20)",1560,"156/Tray",1000,32,12]
["31025C","TIN","32 TSOP I (8x20)",805,"23/Tube",1000,32,12]
["513B, 3513B, 1026B, 31026B","TCN","44 TSOP II - 400mil - 1 Meg",1350,"135/Tray",1000,32,16]
["1026C, 31026C","TIN","44 TSOP II - 400mil - 1 Meg",1352,"26/Tube",1500,32,16]
["31026C","BIN","48ball FBGA",3600,"360/Tray",2000,44,16]
["4096A, 34096A, 4098A, 34098A","TxN","44 TSOP II - 400mil - 4 Meg",1350,"135/Tray",1000,32,16]
["4096A, 34096A","JxN","36 SOJ - 400mil",1900,"19/Tube",500,44,16]
["4098A, 34098A","JxN","44 SOJ - 400mil - 4 Meg",1600,"16/Tube",500,44,16]
["34098A","B","48ball BGA",2200,"480/Tray"]
["38096A, 38098A","TIN","44 TSOP II",1350,"135/Tray",1000,44,16]
["38096A, 38098A","B","48ball BGA",4800,"480/Tray",2000,44,16]
["316096A, 316098A","TIN","48 TSOP I",1350,"135/Tray",1000,44,16]
["316098A","B","48ball BGA",4800,"480/Tray",2000,16,16]
[325632351232,"BIN","90ball TFBGA",2400,"240/Tray",2000]
[]
[]
["LOW POWER SRAM ORDER QTY"]
["PART #","PACKAGESUFFIX","PACKAGE","BOX QTY","QUANTITY PER TRAY/TUBE","REEL SIZE","TAPE WIDTH (mm)","TAPE PITCH (mm)"]
["6264/62256","S","28pin 330mil SOP",2500,"25/Tube",1000,24,16]
["6264/62256","P","28pin 600mil DIP",600,"15/Tube"]
["6264/62256","ST","28pin STSOP (8x13.4)",2340,"234/Tray",1500,24,12]
["1008/2008/4008","P","32pin 600mil DIP",520,"13/Tube"]
["1008/2008/4008","S","32pin 450mil SOP",720,"72/Tray",1000,32,16]
["1008/2008/4008","T","32pin TSOP I (8x20)",1560,"156/Tray",1500,32,12]
["1008/2008/4008","ST","32pin STSOP (8x13.4)",2340,"234/Tray",1500,24,12]
["1016/2016/4016/8008/8016","Z","44pin TSOP II 400mil",1350,"135/Tray",1000,32,12]
["1616/6416","T","48pin TSOP I",960,"96/Tray",1500]
["1008/2008/4008/8008/1016/1616/2016/4016/8016/1616/3216","B","36B/48B TFBGA (6x8)","4800 or 3000","480/Tray Or 300/Tray",2000,16,12]
[4008,"Z","32pin TSOP II",1170,"117/Tray",1000,32,16]
[]
[]
[]
["DRAM ORDER QTY"]
["PART# ","PACKAGE","BOX QTY","QUANTITY PER TRAY/REEL","REEL SIZE "]
["SDRAM "]
["AS4C1M16S","50pin TSOP II",1170,"117/Tray",1000]
["AS4C16M16SA-6TAN/AS4C16M16SA-6TCN/AS4C16M16SA-6TIN/\nAS4C16M16SA-7TCN/AS4C16M16SB-6TIN/AS4C16M16SB-7TCN/\nAS4C32M16SB-6TIN/AS4C32M16SB-7TCN/AS4C32M16SB-7TIN/\nAS4C32M16SC-7TIN/AS4C32M8SA-6TIN/AS4C32M8SA-7TCN/\nAS4C4M16SA-5TCN/AS4C4M16SA-6TAN/AS4C4M16SA-6TCN/\nAS4C4M16SA-6TIN/AS4C4M16SA-7TCN/AS4C4M16SB-6TIN/\nAS4C64M4SA-6TIN/AS4C64M4SA-7TCN/AS4C64M8SC-7TIN/\nAS4C8M16SA-6TAN/AS4C8M16SA-6TCN/AS4C8M16SA-6TIN/\nAS4C8M16SA-7TCN/AS4C8M16SB-6TIN","54pin TSOP II",1080,"108/Tray",1000]
["AS4C64M8SD-7TCN","54pin TSOP II",1080,"108/Tray",1500]
["AS4C16M16SA-6BAN/AS4C16M16SA-6BIN/AS4C16M16SA-7BCN/\nAS4C16M16SB-6BIN/AS4C32M16SB-7BIN/AS4C4M16SA-6BAN/\nAS4C4M16SA-6BIN/AS4C4M16SA-7BCN/AS4C8M16SA-6BAN/\nAS4C8M16SA-6BIN/AS4C8M16SA-7BCN","54ball BGA",3480,"348/Tray",2500]
["AS4C4M16SA-7B2CN","60ball FBGA",2860,"286/Tray",2000]
["AS4C4M32SA/AS4C8M32S/AS4C8M32S","86pin TSOP II",1080,"108/Tray",1000]
["AS4C4M32S/AS4C8M32SA","90ball BGA",1900,"190/Tray",2000]
["*Alliance Memory has collaborated with Micron for exclusive rights to continue to provide these Micron marked PARTs"]
[]
[]
["PART #","Package","BOX QTY","QUANTITY PER TRAY/REEL","REEL SIZE"]
["DDR1"]
["AS4C32M16D1A/AS4C4M16D1A/AS4C64M16D1/AS4C64M16D1A/AS4C64M16D1/ AS4C64M16D1A/AS4C64M8D1/AS4C8M16D1A","66pin TSOP II",1080,"108/Tray",1000]
["AS4C64M16D1A","60ball FBGA",2400,"240/Tray",1000]
["AS4C64M8D1/AS4C8M16D1","60ball TFBGA",2400,"240/Tray",2500]
["AS4C4M32D1A","144ball FBGA",1890,"189/Tray",1500]
["DDR2"]
["AS4C128M16D2A /AS4C16M16D2 / AS4C32M16D2A/AS4C32M16D2C/AS4C64M16D2A","84ball FBGA",2090,"209/Tray",2500]
["AS4C64M8D2","60ball FBGA",2640,"264/Tray",2000]
["AS4C64M16D2B","84ball FBGA",2000,"200/Tray",2500]
["AS4C128M16D2","84ball FBGA",1620,"162/Tray",2500]
["AS4C256M8D2","60ball FBGA",1360,"136/Tray",2500]
["DDR3"]
["AS4C32M16D3-12BxN/AS4C32M16D3L-12BxN","96ball FBGA",1900,"190/Tray",1500]
["AS4C64M16D3B","96ball FBGA",1900,"190/Tray",2000]
["AS4C64M16D3LB","96ball FBGA",1900,"190/Tray",2000]
["AS4C128M16D3C","96ball FBGA",2090,"209/Tray",2500]
["AS4C256M16D3C","96ball FBGA",2090,"209/Tray",2000]
["AS4C256M16D3LC","96ball FBGA",2090,"209/Tray",2500]
["AS4C512M16D3LA/AS4C512M16D3LB","96ball FBGA",1800,"180/Tray",2000]
["AS4C512M16D3LC","96ball FBGA",1900,"190/Tray",2000]
[]
[]
["PART#","PACKAGE","BOX QTY","QUANTITY PER TRAY/REEL","REEL SIZE"]
["MOBILE SDRAM"]
["AS4C16M16MSA/AS4C8M16MSA/AS4C16M16MSB/AS4C8M16MSB","54-ball FBGA",3190,"319/Tray",1000]
["AS4C32M16MSA/AS4C32M16MSB","54-ball BGA ",3190,"319/Tray",1000]
["AS4C4M32MSA/AS4C8M32MSA/AS4C8M32MSB","90-ball FBGA","1900 /2400","190/240 Tray","1000/2000"]
["AS4C16M32MSA/AS4C16M32MSB","90-ball BGA",1900,"190/Tray",1500]
["MOBILE LPDDR1"]
["AS4C32M16MD1A","60-ball FPBGA",1600,"160/Tray",2000]
["AS4C64M16MD1A","60-ball FPBGA",3000,"300/Tray",1000]
["AS4C16M32MD1","90-ball FPBGA",1600,"160/Tray",1000]
["AS4C32M32MD1A","90-ball FPBGA",2400,"240/Tray",1000]
["AS4C64M32MD1","90-ball FPBGA",3480,"348/Tray",1000]
["MOBILE LPDDR2"]
["AS4C32M32MD2A-25BIN/AS4C64M16MD2A-25BIN","134ball FBGA (10 x 11.5 x 1.0)",1280,"128/Tray",2000]
["AS4C128M16MD2A-25BIN/AS4C64M32MD2A-25BIN/AS4C8M32MD2A-25BCN","134ball FBGA (10 x 11.5 x 1.0)",1710,"171/Tray",1000]
["AS4C128M32MD2-18/25BIN","134ball FBGA (11.5 x 11.5 x 1.0)",1680,"168/Tray",2000]
["AS4C8M32MD2A-25BPCN","168ball FBGA (12  x 12 x 0.9)",1680,"168/Tray","Do Not Offer"]

{"sheet":"Part Numbering System - SRAM ","index":33,"n_rows":48,"n_cols":2,"rows_kept":48,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Go Back To ","Index"]

{"sheet":"Part Numbering System - DRAM ","index":34,"n_rows":50,"n_cols":2,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Go Back To","Index"]

{"sheet":"Part Numbering System - Paralle","index":35,"n_rows":50,"n_cols":2,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Go Back To","Index"]

{"sheet":"Part Numbering System - S.NAND","index":36,"n_rows":50,"n_cols":2,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Go Back To","Index"]

{"sheet":"Part Numbering System-Serial SL","index":37,"n_rows":50,"n_cols":2,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Go Back To","Index"]

{"sheet":"Part Numbering System-eMMC","index":38,"n_rows":50,"n_cols":2,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Go Back To","Index"]

{"sheet":"Alliance Memory Contact","index":39,"n_rows":21,"n_cols":15,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[]
["Contact Information"]
["US HEADQUARTERS",null,null,null,null,null,null,"ASIA HEADQUARTERS",null,null,null,null,null,null,"EMEA HEADQUARTERS"]
["Alliance Memory , Inc.",null,null,null,null,null,null,"Alliance Memory, Inc.",null,null,null,null,null,null,"Alliance Memory, Inc."]
["12815 NE 124th St, Suite #D,\nKirkland, WA  98034",null,null,null,null,null,null,"NO.22, Xingde Road,Dayuan DIST,",null,null,null,null,null,null,"7 Pauls Field Eversley, Hampshire, RG27, ONE, United Kingdom"]
["- Phone: +1(425) 898 4456",null,null,null,null,null,null,"Taoyuan City 337002, Taiwan",null,null,null,null,null,null,"- Phone: +44(0) 787-634-4055"]
["- Fax: +1(425) 896 8628",null,null,null,null,null,null,"- Phone: +886 3461 4646",null,null,null,null,null,null,"- Email: sue@alliancememory.com"]
["- Email: david@alliancememory.com",null,null,null,null,null,null,"- Email: kelly@alliancememory.com"]
[]
["CANADA SALES OFFICE",null,null,null,null,null,null,"CHINA SALES OFFICE",null,null,null,null,null,null,"INDIA SALES OFFICE"]
["Tom Gargan",null,null,null,null,null,null,"Room1108, 4# Building Excellence Century Center",null,null,null,null,null,null,"Bangalore – INDIA Ramesh Varadharajan"]
["- Phone:+1(514) 442-0677",null,null,null,null,null,null,"Fuhua 3 Road, Futian District 518000 Shenzhen,",null,null,null,null,null,null,"- Phone: +91 96065 00288"]
["- Email: tom@alliancememory.com",null,null,null,null,null,null,"Guangdong, China"]
[null,null,null,null,null,null,null,"- Phone: +86(189) 2600 6867"]
[null,null,null,null,null,null,null,"- Email: mars@alliancememory.com"]
[]
["NORTH AMERICA REP",null,null,null,null,null,null,"JAPAN SALES OFFICE   ",null,null,null,null,null,null,"KOREA SALES OFFICE"]
["Electra Sales Corporation",null,null,null,null,null,null,"3-7-10, Sakurajyousui, Setagaya-Ku",null,null,null,null,null,null,"Linus Park"]
["21 Goodway Drive",null,null,null,null,null,null," Tokyo, Japan 156-0045",null,null,null,null,null,null,"- Email: linus@alliancememory.com"]
["Rochester, NY 14623",null,null,null,null,null,null,"- Phone: +81(90) 3963 0869"]
["-Phone: +1 (585) 217-6496",null,null,null,null,null,null,"- Email: ted@alliancememory.com"]